(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 72)
    (tracks 766)
    (zones 0)
    (modules 40)
    (nets 66)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 22)
  (net 10 7)
  (net 11 6)
  (net 12 5)
  (net 13 OE)
  (net 14 RCLK)
  (net 15 SRCLK)
  (net 16 5V)
  (net 17 24)
  (net 18 25)
  (net 19 26)
  (net 20 23)
  (net 21 8)
  (net 22 10)
  (net 23 11)
  (net 24 12)
  (net 25 14)
  (net 26 15)
  (net 27 16)
  (net 28 17)
  (net 29 18)
  (net 30 19)
  (net 31 20)
  (net 32 21)
  (net 33 "Net-(J3-Pad6)")
  (net 34 +POE)
  (net 35 "Net-(J3-Pad3)")
  (net 36 B)
  (net 37 A)
  (net 38 "Net-(J4-Pad3)")
  (net 39 "Net-(J4-Pad6)")
  (net 40 "Net-(J6-Pad2)")
  (net 41 "Net-(J6-Pad3)")
  (net 42 VIN)
  (net 43 RX2)
  (net 44 DE)
  (net 45 "Net-(U1-Pad18)")
  (net 46 "Net-(U1-Pad15)")
  (net 47 "Net-(U1-Pad34)")
  (net 48 "Net-(U1-Pad35)")
  (net 49 TX1)
  (net 50 RX1)
  (net 51 "Net-(U3-Pad2)")
  (net 52 "Net-(U3-Pad3)")
  (net 53 "Net-(U3-Pad5)")
  (net 54 "Net-(U3-Pad6)")
  (net 55 "Net-(U3-Pad9)")
  (net 56 "Net-(U3-Pad10)")
  (net 57 "Net-(U3-Pad11)")
  (net 58 "Net-(U3-Pad12)")
  (net 59 "Net-(U3-Pad13)")
  (net 60 "Net-(U3-Pad14)")
  (net 61 "Net-(U3-Pad19)")
  (net 62 "Net-(U3-Pad22)")
  (net 63 "Net-(U3-Pad27)")
  (net 64 "Net-(U3-Pad28)")
  (net 65 "Net-(J9-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +POE)
    (add_net 10)
    (add_net 11)
    (add_net 12)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18)
    (add_net 19)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 24)
    (add_net 25)
    (add_net 26)
    (add_net 5)
    (add_net 5V)
    (add_net 6)
    (add_net 7)
    (add_net 8)
    (add_net A)
    (add_net B)
    (add_net DE)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J9-Pad2)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad22)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad9)")
    (add_net OE)
    (add_net RCLK)
    (add_net RX1)
    (add_net RX2)
    (add_net SRCLK)
    (add_net TX1)
    (add_net VCC)
    (add_net VIN)
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 161.925 76.708)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C4124AA)
    (at 110.49 110.49)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C4124AA)
    (at 110.49 69.85)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C4124AA)
    (at 170.18 69.85)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 127 81.574 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 1.25 1.905 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.05 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 149.86 86.146 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.05 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.05 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 153.122 81.534 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.25 -2.05 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.05 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 150.622 77.47)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 4.318 -1.27) (layer F.SilkS))
    (fp_text value "10 uF" (at 1 3.75) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 107.95 80.01)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at -0.635 2.54) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 107.95 86.36)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at -0.635 2.54) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 107.95 92.71)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at -0.635 2.54) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59DE0611)
    (at 111.76 101.6 90)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J0 (at -4.445 -3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 1.27 16.764 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 22))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 7))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 6))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 5))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 OE))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 RCLK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SRCLK))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C414C92)
    (at 133.35 101.6 90)
    (descr "Through hole straight IDC box header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x05 2.54mm double row")
    (fp_text reference J1 (at -2.54 16.51 180) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 1.27 16.764 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SRCLK))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 RCLK))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 OE))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 24))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 25))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 26))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 59DE0251)
    (at 120.65 111.76 90)
    (descr "Through hole straight IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J2 (at -1.905 -6.604 180) (layer F.SilkS))
    (fp_text value Conn_01x20 (at 1.27 29.464 90) (layer F.Fab))
    (fp_text user %R (at 1.27 11.43 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 SRCLK))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 RCLK))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 OE))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 8))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 10))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 11))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 12))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 14))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 15))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 16))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 17))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 18))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 19))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 20))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 21))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 22))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal (layer F.Cu) (tedit 5B103613)
    (at 127 73.66 180)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference J3 (at -4.445 3.175 270) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 4.445 4 180) (layer F.Fab))
    (fp_text user %R (at 4.445 2 180) (layer F.Fab))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 34 +POE))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 34 +POE))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 35 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 36 B))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 37 A))
    (pad "" np_thru_hole circle (at -1.27 6.35 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.16 6.35 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:RJ45_Amphenol_54602-x08_Horizontal (layer F.Cu) (tedit 5B103613)
    (at 144.78 73.66 180)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference J4 (at -4.445 2.54 270) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 4.445 4 180) (layer F.Fab))
    (fp_text user %R (at 4.445 2 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 10.16 6.35 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 37 A))
    (pad 2 thru_hole circle (at 1.27 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 36 B))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 34 +POE))
    (pad 5 thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 34 +POE))
    (pad 6 thru_hole circle (at 6.35 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 39 "Net-(J4-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 8.89 -2.54 180) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C25944D)
    (at 107.696 75.184 90)
    (fp_text reference J5 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 90) (layer F.Fab))
    (fp_text user %R (at 0 1.778 90) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 +POE))
  )
  (module Connector_USB:USB_B_OST_USB-B1HSxx_Horizontal (layer F.Cu) (tedit 5AFE01FF)
    (at 156.21 72.39 90)
    (descr "USB B receptacle, Horizontal, through-hole, http://www.on-shore.com/wp-content/uploads/2015/09/usb-b1hsxx.pdf")
    (tags "USB-B receptacle horizontal through-hole")
    (fp_text reference J6 (at 1.27 8.255 270) (layer F.SilkS))
    (fp_text value USB_B (at 6.76 10.27 90) (layer F.Fab))
    (fp_text user %R (at 6.76 1.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 0 2.5 90) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask)
      (net 40 "Net-(J6-Pad2)"))
    (pad 3 thru_hole circle (at 2 2.5 90) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask)
      (net 41 "Net-(J6-Pad3)"))
    (pad 4 thru_hole circle (at 2 0 90) (size 1.7 1.7) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 4.71 -4.77 90) (size 3.5 3.5) (drill 2.33) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at 4.71 7.27 90) (size 3.5 3.5) (drill 2.33) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_B_OST_USB-B1HSxx_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C25944D)
    (at 164.846 113.03 180)
    (fp_text reference J7 (at 0 1.778 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 180) (layer F.Fab))
    (fp_text user %R (at 0 1.778 180) (layer B.SilkS))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 VIN))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C25944D)
    (at 172.72 76.2 270)
    (fp_text reference J8 (at -3.302 -0.762 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 270) (layer F.Fab))
    (fp_text user %R (at -3.302 -0.762 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 RX2))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391ABA)
    (at 116.84 111.648 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 2.936 0 90) (layer B.SilkS))
    (fp_text value SolderJumper_2_Bridged (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 42 VIN) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
        (gr_poly (pts
           (xy 0.9 0.3) (xy 0.4 0.3) (xy 0.4 -0.3) (xy 0.9 -0.3)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers B.Cu B.Mask)
      (net 16 5V) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 112.522 75.296 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at -2.906 -0.508 270) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 34 +POE) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 16 5V) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.126 86.23 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 VCC))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 OE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 119.126 93.088 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.936 93.088 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 7))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 138.176 93.094 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 25))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 141.986 93.088 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 26))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.746 93.088 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 10))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.556 93.094 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.366 93.094 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 12))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 131.448 78.994 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 3.178 0.254 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 B))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 A))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.17 80.01)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.17 86.36)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 44 DE))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.176 92.71 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module teensy:Teensy_LC (layer F.Cu) (tedit 5BFB0271)
    (at 165.1 96.52 90)
    (fp_text reference U1 (at 0 -10.16 90) (layer F.SilkS))
    (fp_text value Teensy-LC (at 0 10.16 90) (layer F.Fab))
    (pad 17 thru_hole circle (at 16.51 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 18 thru_hole circle (at 16.51 -2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 16.51 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 19 26))
    (pad 20 thru_hole circle (at 16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 44 DE))
    (pad 16 thru_hole circle (at 16.51 2.54 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J9-Pad2)"))
    (pad 15 thru_hole circle (at 16.51 5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U1-Pad15)"))
    (pad 14 thru_hole circle (at 16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 24 12))
    (pad 21 thru_hole circle (at 13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 25 14))
    (pad 22 thru_hole circle (at 11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 26 15))
    (pad 23 thru_hole circle (at 8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 27 16))
    (pad 24 thru_hole circle (at 6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 28 17))
    (pad 25 thru_hole circle (at 3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 29 18))
    (pad 26 thru_hole circle (at 1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 30 19))
    (pad 27 thru_hole circle (at -1.27 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 31 20))
    (pad 28 thru_hole circle (at -3.81 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 32 21))
    (pad 29 thru_hole circle (at -6.35 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 9 22))
    (pad 30 thru_hole circle (at -8.89 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 20 23))
    (pad 31 thru_hole circle (at -11.43 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 32 thru_hole circle (at -13.97 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 33 thru_hole circle (at -16.51 -7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 42 VIN))
    (pad 34 thru_hole circle (at -13.97 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U1-Pad34)"))
    (pad 35 thru_hole circle (at -8.89 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U1-Pad35)"))
    (pad 36 thru_hole circle (at -6.35 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 17 24))
    (pad 37 thru_hole circle (at -3.81 -5.08 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 18 25))
    (pad 13 thru_hole circle (at 13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 23 11))
    (pad 12 thru_hole circle (at 11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 22 10))
    (pad 11 thru_hole circle (at 8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 43 RX2))
    (pad 10 thru_hole circle (at 6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 21 8))
    (pad 9 thru_hole circle (at 3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 10 7))
    (pad 8 thru_hole circle (at 1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 11 6))
    (pad 7 thru_hole circle (at -1.27 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 12 5))
    (pad 6 thru_hole circle (at -3.81 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 13 OE))
    (pad 5 thru_hole circle (at -6.35 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 14 RCLK))
    (pad 4 thru_hole circle (at -8.89 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 15 SRCLK))
    (pad 3 thru_hole circle (at -11.43 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 49 TX1))
    (pad 2 thru_hole circle (at -13.97 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 50 RX1))
    (pad 1 thru_hole rect (at -16.51 7.62 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 131.318 84.074 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -2.921 -3.5 90) (layer F.SilkS))
    (fp_text value SP3485CN (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 RX1))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 DE))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 DE))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 TX1))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 A))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 B))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SSOP-28_5.3x10.2mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 143.51 83.82 180)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at -3.81 -5.715 180) (layer F.SilkS))
    (fp_text value FT232RL (at 0 6.25 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 RX2))
    (pad 2 smd rect (at -3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 5 smd rect (at -3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U3-Pad9)"))
    (pad 10 smd rect (at -3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at -3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad11)"))
    (pad 12 smd rect (at -3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U3-Pad12)"))
    (pad 13 smd rect (at -3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U3-Pad13)"))
    (pad 14 smd rect (at -3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U3-Pad14)"))
    (pad 15 smd rect (at 3.6 4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J6-Pad3)"))
    (pad 16 smd rect (at 3.6 3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J6-Pad2)"))
    (pad 17 smd rect (at 3.6 2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 18 smd rect (at 3.6 2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 3.6 1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U3-Pad19)"))
    (pad 20 smd rect (at 3.6 0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 21 smd rect (at 3.6 0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 3.6 -0.325 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U3-Pad22)"))
    (pad 23 smd rect (at 3.6 -0.975 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 24 smd rect (at 3.6 -1.625 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 3.6 -2.275 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 3.6 -2.925 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 3.6 -3.575 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-Pad27)"))
    (pad 28 smd rect (at 3.6 -4.225 180) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U3-Pad28)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-28_5.3x10.2mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5C4124AA)
    (at 152.4 110.49)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 134.874 85.852 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module AOR_custom:header_01x02 (layer F.Cu) (tedit 5C25944D)
    (at 170.18 76.2 270)
    (fp_text reference J9 (at 0 1.778 270) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -0.5 270) (layer F.Fab))
    (fp_text user %R (at 0 1.778 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 65 "Net-(J9-Pad2)"))
  )
  (gr_text "PANEL 2" (at 145.288 110.49 270) (layer B.SilkS))
  (gr_text "PANEL 1" (at 131.318 100.584 270) (layer B.SilkS))
  (gr_text "PANEL 0" (at 109.728 100.584 270) (layer B.SilkS))
  (gr_text "ACP3-X-CTL-PCB\nREV D, 1-18-2019" (at 152.654 99.314 90) (layer F.SilkS))
  (gr_text "ACP3-X-CTL-PCB\nREV D, 1-18-2019" (at 134.62 90.424) (layer B.SilkS))
  (gr_text A (at 127 71.882) (layer B.SilkS))
  (gr_text G (at 119.38 71.882) (layer B.SilkS))
  (gr_text B (at 125.73 77.978) (layer B.SilkS))
  (gr_text G (at 118.11 77.978) (layer B.SilkS))
  (gr_text +V (at 121.92 71.882) (layer B.SilkS))
  (gr_text +V (at 123.19 77.978) (layer B.SilkS))
  (gr_text G (at 135.89 77.978) (layer B.SilkS))
  (gr_text G (at 137.16 71.882) (layer B.SilkS))
  (gr_text +V (at 140.97 77.978) (layer B.SilkS))
  (gr_text +V (at 139.7 71.882) (layer B.SilkS))
  (gr_text B (at 143.51 77.978) (layer B.SilkS))
  (gr_text A (at 144.78 71.882) (layer B.SilkS))
  (gr_text PWR (at 113.03 80.01) (layer B.SilkS))
  (gr_text RS485 (at 114.3 86.36) (layer B.SilkS))
  (gr_text DMX (at 113.03 92.71) (layer B.SilkS))
  (gr_text 23 (at 143.51 97.155) (layer B.SilkS))
  (gr_text SC (at 135.89 97.155) (layer B.SilkS))
  (gr_text 5V (at 133.35 97.155) (layer B.SilkS))
  (gr_text 3V (at 135.89 103.505) (layer B.SilkS))
  (gr_text 24 (at 140.97 103.505) (layer B.SilkS))
  (gr_text RC (at 138.43 103.505) (layer B.SilkS))
  (gr_text 25 (at 140.97 97.155) (layer B.SilkS))
  (gr_text G (at 133.35 103.505) (layer B.SilkS))
  (gr_text OE (at 138.43 97.155) (layer B.SilkS))
  (gr_text 26 (at 143.51 103.505) (layer B.SilkS))
  (gr_text 22 (at 121.92 97.155) (layer B.SilkS))
  (gr_text 6 (at 119.38 97.155) (layer B.SilkS))
  (gr_text SC (at 114.3 97.155) (layer B.SilkS))
  (gr_text 5V (at 111.76 97.155) (layer B.SilkS))
  (gr_text 3V (at 114.3 103.505) (layer B.SilkS))
  (gr_text RC (at 116.84 103.505) (layer B.SilkS))
  (gr_text G (at 111.76 103.505) (layer B.SilkS))
  (gr_text OE (at 116.84 97.155) (layer B.SilkS))
  (gr_text 5 (at 119.38 103.505) (layer B.SilkS))
  (gr_text 7 (at 121.92 103.505) (layer B.SilkS))
  (gr_text 23 (at 143.51 107.315) (layer B.SilkS))
  (gr_text 21 (at 140.97 107.315) (layer B.SilkS))
  (gr_text 19 (at 138.43 107.315) (layer B.SilkS))
  (gr_text 17 (at 135.89 107.315) (layer B.SilkS))
  (gr_text 15 (at 133.35 107.315) (layer B.SilkS))
  (gr_text 12 (at 130.81 107.315) (layer B.SilkS))
  (gr_text 10 (at 128.27 107.315) (layer B.SilkS))
  (gr_text OE (at 125.73 107.315) (layer B.SilkS))
  (gr_text SC (at 123.19 107.315) (layer B.SilkS))
  (gr_text 22 (at 143.51 113.665) (layer B.SilkS))
  (gr_text 20 (at 140.97 113.665) (layer B.SilkS))
  (gr_text 18 (at 138.43 113.665) (layer B.SilkS))
  (gr_text 16 (at 135.89 113.665) (layer B.SilkS))
  (gr_text 14 (at 133.35 113.665) (layer B.SilkS))
  (gr_text 11 (at 130.81 113.665) (layer B.SilkS))
  (gr_text 8 (at 128.27 113.665) (layer B.SilkS))
  (gr_text RC (at 125.73 113.665) (layer B.SilkS))
  (gr_text 3V (at 123.19 113.665) (layer B.SilkS))
  (gr_text 5V (at 120.65 107.315) (layer B.SilkS))
  (gr_text G (at 120.65 113.665) (layer B.SilkS))
  (gr_text +5V (at 161.29 113.03) (layer B.SilkS))
  (gr_text GND (at 169.545 113.03) (layer B.SilkS))
  (gr_text TEENSY-LC (at 165.1 97.155 90) (layer B.SilkS))
  (gr_text "VIEWSCREEN\nUSB" (at 157.48 66.675) (layer B.SilkS))
  (gr_text RS485 (at 140.335 67.31) (layer B.SilkS))
  (gr_text RS485 (at 122.555 67.31) (layer B.SilkS))
  (gr_text "EXT\nPWR" (at 115.062 75.565 90) (layer B.SilkS))
  (gr_text "USB\nPWR" (at 114.3 111.76 90) (layer B.SilkS))
  (gr_line (start 106.045 114.935) (end 106.045 64.77) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 174.625 114.935) (end 106.045 114.935) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 174.625 64.77) (end 174.625 114.935) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 106.045 64.77) (end 174.625 64.77) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.045 64.77) (xy 174.625 64.77) (xy 174.625 114.935) (xy 106.045 114.935)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.045 64.77) (xy 174.625 64.77) (xy 174.625 114.935) (xy 106.045 114.935)
      )
    )
  )
)
