(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 680)
    (zones 0)
    (modules 41)
    (nets 262)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.016)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.524)
    (user_trace_width 2.032)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.8128)
    (uvia_drill 0.4064)
    (uvias_allowed no)
    (uvia_min_size 0.6858)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad7)")
  (net 6 "Net-(J1-Pad8)")
  (net 7 "Net-(J1-Pad9)")
  (net 8 "Net-(J1-Pad10)")
  (net 9 "Net-(J1-Pad11)")
  (net 10 "Net-(J1-Pad12)")
  (net 11 "Net-(J1-Pad13)")
  (net 12 "Net-(J1-Pad14)")
  (net 13 "Net-(J1-Pad15)")
  (net 14 "Net-(J1-Pad16)")
  (net 15 "Net-(J1-Pad17)")
  (net 16 "Net-(J1-Pad18)")
  (net 17 "Net-(J1-Pad19)")
  (net 18 "Net-(J1-Pad20)")
  (net 19 "Net-(J1-Pad21)")
  (net 20 "Net-(J1-Pad22)")
  (net 21 "Net-(J1-Pad23)")
  (net 22 "Net-(J1-Pad24)")
  (net 23 "Net-(J1-Pad25)")
  (net 24 "Net-(J1-Pad26)")
  (net 25 "Net-(J1-Pad27)")
  (net 26 "Net-(J1-Pad28)")
  (net 27 "Net-(J1-Pad29)")
  (net 28 "Net-(J1-Pad30)")
  (net 29 "Net-(J1-Pad31)")
  (net 30 "Net-(J1-Pad32)")
  (net 31 "Net-(J1-Pad33)")
  (net 32 "Net-(J1-Pad34)")
  (net 33 "Net-(J1-Pad35)")
  (net 34 "Net-(J1-Pad36)")
  (net 35 "Net-(J1-Pad37)")
  (net 36 "Net-(J1-Pad38)")
  (net 37 "Net-(J1-Pad39)")
  (net 38 "Net-(J1-Pad40)")
  (net 39 "Net-(J1-Pad41)")
  (net 40 "Net-(J1-Pad42)")
  (net 41 "Net-(J1-Pad43)")
  (net 42 "Net-(J1-Pad44)")
  (net 43 "Net-(J1-Pad45)")
  (net 44 "Net-(J1-Pad46)")
  (net 45 "Net-(J1-Pad47)")
  (net 46 "Net-(J1-Pad48)")
  (net 47 "Net-(J1-Pad49)")
  (net 48 "Net-(J1-Pad50)")
  (net 49 "Net-(J1-Pad51)")
  (net 50 "Net-(J1-Pad52)")
  (net 51 "Net-(J1-Pad53)")
  (net 52 "Net-(J1-Pad54)")
  (net 53 "Net-(J1-Pad55)")
  (net 54 "Net-(J1-Pad56)")
  (net 55 "Net-(J1-Pad57)")
  (net 56 "Net-(J1-Pad59)")
  (net 57 "Net-(J1-Pad60)")
  (net 58 "Net-(J1-Pad61)")
  (net 59 "Net-(J2-Pad3)")
  (net 60 "Net-(J2-Pad4)")
  (net 61 "Net-(J2-Pad5)")
  (net 62 "Net-(J2-Pad6)")
  (net 63 "Net-(J2-Pad7)")
  (net 64 "Net-(J2-Pad8)")
  (net 65 "Net-(J2-Pad9)")
  (net 66 "Net-(J2-Pad10)")
  (net 67 "Net-(J2-Pad11)")
  (net 68 "Net-(J2-Pad12)")
  (net 69 "Net-(J2-Pad13)")
  (net 70 "Net-(J2-Pad14)")
  (net 71 "Net-(J2-Pad15)")
  (net 72 "Net-(J2-Pad16)")
  (net 73 "Net-(J2-Pad17)")
  (net 74 "Net-(J2-Pad18)")
  (net 75 "Net-(J2-Pad19)")
  (net 76 "Net-(J2-Pad20)")
  (net 77 "Net-(J2-Pad21)")
  (net 78 "Net-(J2-Pad22)")
  (net 79 "Net-(J2-Pad23)")
  (net 80 "Net-(J2-Pad24)")
  (net 81 "Net-(J2-Pad25)")
  (net 82 "Net-(J2-Pad26)")
  (net 83 "Net-(J2-Pad27)")
  (net 84 "Net-(J2-Pad28)")
  (net 85 "Net-(J2-Pad29)")
  (net 86 "Net-(J2-Pad30)")
  (net 87 "Net-(J2-Pad31)")
  (net 88 "Net-(J2-Pad32)")
  (net 89 "Net-(J2-Pad34)")
  (net 90 "Net-(J2-Pad35)")
  (net 91 "Net-(J2-Pad36)")
  (net 92 "Net-(J2-Pad38)")
  (net 93 "Net-(J2-Pad40)")
  (net 94 "Net-(BZ5-Pad1)")
  (net 95 "Net-(BZ5-Pad2)")
  (net 96 GNDREF)
  (net 97 VCC)
  (net 98 "Net-(J3-Pad3)")
  (net 99 "Net-(J3-Pad2)")
  (net 100 "Net-(J3-Pad1)")
  (net 101 "Net-(J4-Pad1)")
  (net 102 "Net-(J4-Pad2)")
  (net 103 "Net-(J4-Pad3)")
  (net 104 "Net-(J6-Pad1)")
  (net 105 "Net-(J8-Pad1)")
  (net 106 "Net-(J8-Pad2)")
  (net 107 "Net-(J8-Pad3)")
  (net 108 "Net-(J8-Pad4)")
  (net 109 "Net-(J8-Pad6)")
  (net 110 "Net-(J8-Pad7)")
  (net 111 "Net-(J8-Pad8)")
  (net 112 "Net-(J8-Pad9)")
  (net 113 "Net-(J8-Pad10)")
  (net 114 "Net-(J10-Pad1)")
  (net 115 "Net-(J10-Pad3)")
  (net 116 "Net-(J10-Pad4)")
  (net 117 "Net-(J10-Pad5)")
  (net 118 "Net-(J10-Pad6)")
  (net 119 "Net-(J10-Pad7)")
  (net 120 "Net-(J10-Pad8)")
  (net 121 "Net-(J10-Pad9)")
  (net 122 "Net-(J10-Pad10)")
  (net 123 "Net-(J10-Pad11)")
  (net 124 "Net-(J10-Pad12)")
  (net 125 "Net-(J10-Pad13)")
  (net 126 "Net-(J10-Pad14)")
  (net 127 "Net-(J10-Pad15)")
  (net 128 "Net-(J10-Pad16)")
  (net 129 "Net-(J10-Pad17)")
  (net 130 "Net-(J10-Pad18)")
  (net 131 "Net-(J10-Pad19)")
  (net 132 "Net-(J10-Pad20)")
  (net 133 "Net-(J10-Pad21)")
  (net 134 "Net-(J10-Pad22)")
  (net 135 "Net-(J10-Pad23)")
  (net 136 "Net-(J10-Pad24)")
  (net 137 "Net-(J10-Pad25)")
  (net 138 "Net-(J10-Pad26)")
  (net 139 "Net-(J10-Pad27)")
  (net 140 "Net-(J10-Pad28)")
  (net 141 "Net-(J10-Pad29)")
  (net 142 "Net-(J10-Pad30)")
  (net 143 "Net-(J10-Pad31)")
  (net 144 "Net-(J10-Pad32)")
  (net 145 "Net-(J10-Pad33)")
  (net 146 "Net-(J10-Pad34)")
  (net 147 "Net-(J10-Pad35)")
  (net 148 "Net-(J10-Pad36)")
  (net 149 "Net-(J10-Pad37)")
  (net 150 "Net-(J10-Pad38)")
  (net 151 "Net-(J10-Pad39)")
  (net 152 "Net-(J10-Pad44)")
  (net 153 "Net-(J12-Pad1)")
  (net 154 "Net-(J12-Pad2)")
  (net 155 "Net-(J12-Pad3)")
  (net 156 "Net-(J12-Pad4)")
  (net 157 "Net-(J12-Pad6)")
  (net 158 "Net-(J12-Pad7)")
  (net 159 "Net-(J12-Pad8)")
  (net 160 "Net-(J12-Pad9)")
  (net 161 "Net-(J12-Pad10)")
  (net 162 "Net-(J13-Pad2)")
  (net 163 "Net-(J13-Pad4)")
  (net 164 "Net-(J13-Pad6)")
  (net 165 "Net-(J13-Pad8)")
  (net 166 "Net-(J13-Pad10)")
  (net 167 "Net-(J13-Pad12)")
  (net 168 "Net-(J13-Pad14)")
  (net 169 "Net-(J13-Pad16)")
  (net 170 "Net-(J13-Pad18)")
  (net 171 "Net-(J13-Pad20)")
  (net 172 "Net-(J13-Pad22)")
  (net 173 "Net-(J13-Pad24)")
  (net 174 "Net-(J13-Pad26)")
  (net 175 "Net-(J13-Pad28)")
  (net 176 "Net-(J13-Pad30)")
  (net 177 "Net-(J13-Pad32)")
  (net 178 "Net-(J13-Pad34)")
  (net 179 "Net-(J14-Pad9)")
  (net 180 "Net-(J14-Pad7)")
  (net 181 "Net-(J14-Pad5)")
  (net 182 "Net-(J14-Pad3)")
  (net 183 "Net-(J14-Pad1)")
  (net 184 "Net-(J15-Pad10)")
  (net 185 "Net-(J15-Pad9)")
  (net 186 "Net-(J15-Pad8)")
  (net 187 "Net-(J15-Pad7)")
  (net 188 "Net-(J15-Pad6)")
  (net 189 "Net-(J15-Pad4)")
  (net 190 "Net-(J15-Pad3)")
  (net 191 "Net-(J15-Pad2)")
  (net 192 "Net-(J15-Pad1)")
  (net 193 "Net-(J16-Pad1)")
  (net 194 "Net-(J16-Pad2)")
  (net 195 "Net-(J16-Pad3)")
  (net 196 "Net-(J16-Pad4)")
  (net 197 "Net-(J16-Pad6)")
  (net 198 "Net-(J16-Pad7)")
  (net 199 "Net-(J16-Pad8)")
  (net 200 "Net-(J16-Pad9)")
  (net 201 "Net-(J16-Pad10)")
  (net 202 "Net-(J17-Pad1)")
  (net 203 "Net-(J17-Pad2)")
  (net 204 "Net-(J17-Pad3)")
  (net 205 "Net-(J17-Pad4)")
  (net 206 "Net-(J17-Pad5)")
  (net 207 "Net-(J17-Pad6)")
  (net 208 "Net-(J17-Pad7)")
  (net 209 "Net-(J17-Pad8)")
  (net 210 "Net-(JA8-Pad10)")
  (net 211 "Net-(JA12-Pad10)")
  (net 212 "Net-(JA14-Pad4)")
  (net 213 "Net-(JA14-Pad9)")
  (net 214 "Net-(JA14-Pad11)")
  (net 215 "Net-(JA14-Pad12)")
  (net 216 "Net-(JA14-Pad15)")
  (net 217 "Net-(JA15-Pad10)")
  (net 218 "Net-(JA16-Pad10)")
  (net 219 VDD)
  (net 220 "Net-(JC20-Pad5)")
  (net 221 "Net-(JC21-Pad3)")
  (net 222 "Net-(JP1-Pad3)")
  (net 223 "Net-(JP1-Pad4)")
  (net 224 "Net-(JP1-Pad5)")
  (net 225 "Net-(JP1-Pad6)")
  (net 226 "Net-(JP1-Pad7)")
  (net 227 "Net-(JP1-Pad8)")
  (net 228 "Net-(JP1-Pad9)")
  (net 229 "Net-(JP1-Pad10)")
  (net 230 "Net-(JP1-Pad11)")
  (net 231 "Net-(JP1-Pad12)")
  (net 232 "Net-(JP1-Pad13)")
  (net 233 "Net-(JP1-Pad14)")
  (net 234 "Net-(JP1-Pad15)")
  (net 235 "Net-(JP1-Pad16)")
  (net 236 "Net-(JP1-Pad17)")
  (net 237 "Net-(JP1-Pad18)")
  (net 238 "Net-(P1-Pad1)")
  (net 239 "Net-(P1-Pad2)")
  (net 240 "Net-(P1-Pad3)")
  (net 241 "Net-(P1-Pad4)")
  (net 242 "Net-(P1-Pad5)")
  (net 243 "Net-(P1-Pad6)")
  (net 244 "Net-(P1-Pad7)")
  (net 245 "Net-(P1-Pad8)")
  (net 246 "Net-(P1-Pad9)")
  (net 247 "Net-(P1-Pad10)")
  (net 248 "Net-(P1-Pad11)")
  (net 249 "Net-(P1-Pad12)")
  (net 250 "Net-(P1-Pad13)")
  (net 251 "Net-(P1-Pad14)")
  (net 252 "Net-(P1-Pad15)")
  (net 253 "Net-(P1-Pad16)")
  (net 254 "Net-(P1-Pad17)")
  (net 255 "Net-(P1-Pad26)")
  (net 256 "Net-(PA1-Pad26)")
  (net 257 "Net-(JA3-Pad6)")
  (net 258 "Net-(JA3-Pad2)")
  (net 259 "Net-(JA4-Pad2)")
  (net 260 "Net-(JA4-Pad6)")
  (net 261 "Net-(J2-Pad33)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.8128)
    (uvia_drill 0.4064)
    (diff_pair_gap 0.254)
    (diff_pair_width 0.254)
    (add_net GNDREF)
    (add_net "Net-(BZ5-Pad1)")
    (add_net "Net-(BZ5-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad27)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J1-Pad29)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad31)")
    (add_net "Net-(J1-Pad32)")
    (add_net "Net-(J1-Pad33)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad39)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad41)")
    (add_net "Net-(J1-Pad42)")
    (add_net "Net-(J1-Pad43)")
    (add_net "Net-(J1-Pad44)")
    (add_net "Net-(J1-Pad45)")
    (add_net "Net-(J1-Pad46)")
    (add_net "Net-(J1-Pad47)")
    (add_net "Net-(J1-Pad48)")
    (add_net "Net-(J1-Pad49)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad50)")
    (add_net "Net-(J1-Pad51)")
    (add_net "Net-(J1-Pad52)")
    (add_net "Net-(J1-Pad53)")
    (add_net "Net-(J1-Pad54)")
    (add_net "Net-(J1-Pad55)")
    (add_net "Net-(J1-Pad56)")
    (add_net "Net-(J1-Pad57)")
    (add_net "Net-(J1-Pad59)")
    (add_net "Net-(J1-Pad60)")
    (add_net "Net-(J1-Pad61)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J10-Pad10)")
    (add_net "Net-(J10-Pad11)")
    (add_net "Net-(J10-Pad12)")
    (add_net "Net-(J10-Pad13)")
    (add_net "Net-(J10-Pad14)")
    (add_net "Net-(J10-Pad15)")
    (add_net "Net-(J10-Pad16)")
    (add_net "Net-(J10-Pad17)")
    (add_net "Net-(J10-Pad18)")
    (add_net "Net-(J10-Pad19)")
    (add_net "Net-(J10-Pad20)")
    (add_net "Net-(J10-Pad21)")
    (add_net "Net-(J10-Pad22)")
    (add_net "Net-(J10-Pad23)")
    (add_net "Net-(J10-Pad24)")
    (add_net "Net-(J10-Pad25)")
    (add_net "Net-(J10-Pad26)")
    (add_net "Net-(J10-Pad27)")
    (add_net "Net-(J10-Pad28)")
    (add_net "Net-(J10-Pad29)")
    (add_net "Net-(J10-Pad3)")
    (add_net "Net-(J10-Pad30)")
    (add_net "Net-(J10-Pad31)")
    (add_net "Net-(J10-Pad32)")
    (add_net "Net-(J10-Pad33)")
    (add_net "Net-(J10-Pad34)")
    (add_net "Net-(J10-Pad35)")
    (add_net "Net-(J10-Pad36)")
    (add_net "Net-(J10-Pad37)")
    (add_net "Net-(J10-Pad38)")
    (add_net "Net-(J10-Pad39)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(J10-Pad44)")
    (add_net "Net-(J10-Pad5)")
    (add_net "Net-(J10-Pad6)")
    (add_net "Net-(J10-Pad7)")
    (add_net "Net-(J10-Pad8)")
    (add_net "Net-(J10-Pad9)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J12-Pad10)")
    (add_net "Net-(J12-Pad2)")
    (add_net "Net-(J12-Pad3)")
    (add_net "Net-(J12-Pad4)")
    (add_net "Net-(J12-Pad6)")
    (add_net "Net-(J12-Pad7)")
    (add_net "Net-(J12-Pad8)")
    (add_net "Net-(J12-Pad9)")
    (add_net "Net-(J13-Pad10)")
    (add_net "Net-(J13-Pad12)")
    (add_net "Net-(J13-Pad14)")
    (add_net "Net-(J13-Pad16)")
    (add_net "Net-(J13-Pad18)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(J13-Pad20)")
    (add_net "Net-(J13-Pad22)")
    (add_net "Net-(J13-Pad24)")
    (add_net "Net-(J13-Pad26)")
    (add_net "Net-(J13-Pad28)")
    (add_net "Net-(J13-Pad30)")
    (add_net "Net-(J13-Pad32)")
    (add_net "Net-(J13-Pad34)")
    (add_net "Net-(J13-Pad4)")
    (add_net "Net-(J13-Pad6)")
    (add_net "Net-(J13-Pad8)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J14-Pad3)")
    (add_net "Net-(J14-Pad5)")
    (add_net "Net-(J14-Pad7)")
    (add_net "Net-(J14-Pad9)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J15-Pad10)")
    (add_net "Net-(J15-Pad2)")
    (add_net "Net-(J15-Pad3)")
    (add_net "Net-(J15-Pad4)")
    (add_net "Net-(J15-Pad6)")
    (add_net "Net-(J15-Pad7)")
    (add_net "Net-(J15-Pad8)")
    (add_net "Net-(J15-Pad9)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J16-Pad10)")
    (add_net "Net-(J16-Pad2)")
    (add_net "Net-(J16-Pad3)")
    (add_net "Net-(J16-Pad4)")
    (add_net "Net-(J16-Pad6)")
    (add_net "Net-(J16-Pad7)")
    (add_net "Net-(J16-Pad8)")
    (add_net "Net-(J16-Pad9)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J17-Pad2)")
    (add_net "Net-(J17-Pad3)")
    (add_net "Net-(J17-Pad4)")
    (add_net "Net-(J17-Pad5)")
    (add_net "Net-(J17-Pad6)")
    (add_net "Net-(J17-Pad7)")
    (add_net "Net-(J17-Pad8)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad10)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(J8-Pad4)")
    (add_net "Net-(J8-Pad6)")
    (add_net "Net-(J8-Pad7)")
    (add_net "Net-(J8-Pad8)")
    (add_net "Net-(J8-Pad9)")
    (add_net "Net-(JA12-Pad10)")
    (add_net "Net-(JA14-Pad11)")
    (add_net "Net-(JA14-Pad12)")
    (add_net "Net-(JA14-Pad15)")
    (add_net "Net-(JA14-Pad4)")
    (add_net "Net-(JA14-Pad9)")
    (add_net "Net-(JA15-Pad10)")
    (add_net "Net-(JA16-Pad10)")
    (add_net "Net-(JA3-Pad2)")
    (add_net "Net-(JA3-Pad6)")
    (add_net "Net-(JA4-Pad2)")
    (add_net "Net-(JA4-Pad6)")
    (add_net "Net-(JA8-Pad10)")
    (add_net "Net-(JC20-Pad5)")
    (add_net "Net-(JC21-Pad3)")
    (add_net "Net-(JP1-Pad10)")
    (add_net "Net-(JP1-Pad11)")
    (add_net "Net-(JP1-Pad12)")
    (add_net "Net-(JP1-Pad13)")
    (add_net "Net-(JP1-Pad14)")
    (add_net "Net-(JP1-Pad15)")
    (add_net "Net-(JP1-Pad16)")
    (add_net "Net-(JP1-Pad17)")
    (add_net "Net-(JP1-Pad18)")
    (add_net "Net-(JP1-Pad3)")
    (add_net "Net-(JP1-Pad4)")
    (add_net "Net-(JP1-Pad5)")
    (add_net "Net-(JP1-Pad6)")
    (add_net "Net-(JP1-Pad7)")
    (add_net "Net-(JP1-Pad8)")
    (add_net "Net-(JP1-Pad9)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad15)")
    (add_net "Net-(P1-Pad16)")
    (add_net "Net-(P1-Pad17)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(PA1-Pad26)")
    (add_net VCC)
    (add_net VDD)
  )
  (module connectors:Mini-DIN-6-PS2-Horizontal (layer F.Cu) (tedit 5C779DF0)
    (at 132.588 95.25 270)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference JA4 (at 0 6 270) (layer F.SilkS))
    (fp_text value KBD (at 6.604 5.969 270) (layer F.SilkS))
    (fp_text user %R (at -4.953 5.969 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 1.24 -3.8 270) (size 4.4196 4.4196) (drill 2.2098) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.99 -3 270) (size 4.4196 4.4196) (drill 2.2098) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.51 -3 270) (size 4.4196 4.4196) (drill 2.2098) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -2.16 2.5 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 101 "Net-(J4-Pad1)"))
    (pad 6 thru_hole circle (at 4.64 2.5 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 260 "Net-(JA4-Pad6)"))
    (pad 3 thru_hole circle (at -2.16 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole circle (at 4.64 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 1 thru_hole rect (at -0.06 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 102 "Net-(J4-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 259 "Net-(JA4-Pad2)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors:Mini-DIN-6-PS2-Horizontal (layer F.Cu) (tedit 5C779DDC)
    (at 132.588 74.93 270)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference JA3 (at 0 6 270) (layer F.SilkS))
    (fp_text value MOUSE (at 5.842 5.969 270) (layer F.SilkS))
    (fp_text user %R (at -4.953 5.969 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 1.24 -3.8 270) (size 4.4196 4.4196) (drill 2.2098) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.99 -3 270) (size 4.4196 4.4196) (drill 2.2098) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.51 -3 270) (size 4.4196 4.4196) (drill 2.2098) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -2.16 2.5 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 100 "Net-(J3-Pad1)"))
    (pad 6 thru_hole circle (at 4.64 2.5 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 257 "Net-(JA3-Pad6)"))
    (pad 3 thru_hole circle (at -2.16 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole circle (at 4.64 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 1 thru_hole rect (at -0.06 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 99 "Net-(J3-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 258 "Net-(JA3-Pad2)"))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors:DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset5.08mm (layer F.Cu) (tedit 5C42EBBB)
    (at 59.817 80.772 270)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 9.4mm")
    (fp_text reference JA14 (at 0 -2.794 270) (layer F.SilkS))
    (fp_text value VGA (at -8.763 -2.794 270) (layer F.SilkS))
    (fp_text user %R (at -4.318 6.985 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 183 "Net-(J14-Pad1)"))
    (pad 2 thru_hole circle (at -2.29 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 182 "Net-(J14-Pad3)"))
    (pad 3 thru_hole circle (at -4.58 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 181 "Net-(J14-Pad5)"))
    (pad 4 thru_hole circle (at -6.87 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 212 "Net-(JA14-Pad4)"))
    (pad 5 thru_hole circle (at -9.16 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole circle (at 1.145 1.98 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 7 thru_hole circle (at -1.145 1.98 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 8 thru_hole circle (at -3.435 1.98 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 9 thru_hole circle (at -5.725 1.98 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 213 "Net-(JA14-Pad9)"))
    (pad 10 thru_hole circle (at -8.015 1.98 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 11 thru_hole circle (at 0 3.96 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 214 "Net-(JA14-Pad11)"))
    (pad 12 thru_hole circle (at -2.29 3.96 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 215 "Net-(JA14-Pad12)"))
    (pad 13 thru_hole circle (at -4.58 3.96 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 180 "Net-(J14-Pad7)"))
    (pad 14 thru_hole circle (at -6.87 3.96 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 179 "Net-(J14-Pad9)"))
    (pad 15 thru_hole circle (at -9.16 3.96 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 216 "Net-(JA14-Pad15)"))
    (pad "" np_thru_hole circle (at 8.165 1.98 270) (size 6.35 6.35) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -16.825 1.98 270) (size 6.35 6.35) (drill 3.2) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Dsub.3dshapes/DSUB-15-HD_Female_Horizontal_P2.29x1.98mm_EdgePinOffset9.40mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors:BarrelJack_CUI_PJ-102AH_Horizontal (layer F.Cu) (tedit 5C42E9BE)
    (at 60.96 120.142 270)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference JC21 (at 5.75 6.604) (layer F.SilkS))
    (fp_text value DC-SRC (at -5.715 5.08) (layer F.SilkS))
    (fp_text user %R (at 0 6.5 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 4.7 3 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 221 "Net-(JC21-Pad3)"))
    (pad 2 thru_hole circle (at 0 6 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 219 VDD))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors:RJ45_Amphenol_54602-x08_Horizontal (layer F.Cu) (tedit 5C42E918)
    (at 64.77 98.044 270)
    (descr "8 Pol Shallow Latch Connector, Modjack, RJ45 (https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/c-bmj-0102.pdf)")
    (tags RJ45)
    (fp_text reference JA17 (at 0 -5.207 270) (layer F.SilkS))
    (fp_text value 8P8C (at 9.271 -5.207 270) (layer F.SilkS))
    (fp_text user %R (at 4.445 2 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 10.16 6.35 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35 270) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 202 "Net-(J17-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 203 "Net-(J17-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 204 "Net-(J17-Pad3)"))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 205 "Net-(J17-Pad4)"))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 206 "Net-(J17-Pad5)"))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 207 "Net-(J17-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 208 "Net-(J17-Pad7)"))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.5 1.5) (drill 0.76) (layers *.Cu *.Mask)
      (net 209 "Net-(J17-Pad8)"))
    (pad "" np_thru_hole circle (at -3.27 10.85 270) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12.16 10.85 270) (size 3.048 3.048) (drill 1.524) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Amphenol_54602-x08_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5C31A30C)
    (at 86.106 106.934)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C305746)
    (at 135.89 141.605)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C305737)
    (at 55.88 141.605)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C30571E)
    (at 59.69 55.88)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C305729)
    (at 133.35 55.88)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.048) (layers *.Cu *.Mask))
  )
  (module Buzzer_Beeper:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5C3454B4)
    (at 82.55 86.36 270)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BZ5 (at 6.731 7.366 270) (layer F.SilkS))
    (fp_text value SPK (at 1.016 7.4 270) (layer F.SilkS))
    (fp_text user + (at -0.01 -2.54 270) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54 270) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(BZ5-Pad1)"))
    (pad 2 thru_hole circle (at 7.6 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(BZ5-Pad2)"))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x32_P2.54mm_Vertical (layer F.Cu) (tedit 5C345AB2)
    (at 57.15 136.525 90)
    (descr "Through hole straight pin header, 2x32, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x32 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value ISA8 (at 1.27 81.07 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 39.37 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J1-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad39)"))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad40)"))
    (pad 41 thru_hole oval (at 0 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad41)"))
    (pad 42 thru_hole oval (at 2.54 50.8 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad42)"))
    (pad 43 thru_hole oval (at 0 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad43)"))
    (pad 44 thru_hole oval (at 2.54 53.34 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad44)"))
    (pad 45 thru_hole oval (at 0 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-Pad45)"))
    (pad 46 thru_hole oval (at 2.54 55.88 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad46)"))
    (pad 47 thru_hole oval (at 0 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J1-Pad47)"))
    (pad 48 thru_hole oval (at 2.54 58.42 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J1-Pad48)"))
    (pad 49 thru_hole oval (at 0 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J1-Pad49)"))
    (pad 50 thru_hole oval (at 2.54 60.96 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J1-Pad50)"))
    (pad 51 thru_hole oval (at 0 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J1-Pad51)"))
    (pad 52 thru_hole oval (at 2.54 63.5 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J1-Pad52)"))
    (pad 53 thru_hole oval (at 0 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J1-Pad53)"))
    (pad 54 thru_hole oval (at 2.54 66.04 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J1-Pad54)"))
    (pad 55 thru_hole oval (at 0 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(J1-Pad55)"))
    (pad 56 thru_hole oval (at 2.54 68.58 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J1-Pad56)"))
    (pad 57 thru_hole oval (at 0 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J1-Pad57)"))
    (pad 58 thru_hole oval (at 2.54 71.12 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 59 thru_hole oval (at 0 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J1-Pad59)"))
    (pad 60 thru_hole oval (at 2.54 73.66 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J1-Pad60)"))
    (pad 61 thru_hole oval (at 0 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J1-Pad61)"))
    (pad 62 thru_hole oval (at 2.54 76.2 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 63 thru_hole oval (at 0 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 64 thru_hole oval (at 2.54 78.74 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x32_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 5C345AAD)
    (at 77.47 141.605 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value ISA16 (at 1.27 50.59 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(J2-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(J2-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(J2-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J2-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J2-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J2-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J2-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(J2-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(J2-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J2-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(J2-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(J2-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(J2-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 261 "Net-(J2-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(J2-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(J2-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(J2-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(J2-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(J2-Pad40)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer B.Cu) (tedit 5C344FF0)
    (at 123.19 71.12 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 2.413 0 270) (layer B.SilkS))
    (fp_text value MOUSE (at 2.413 -9.144 270) (layer B.SilkS))
    (fp_text user %R (at 0 -5.08 90) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer B.Cu) (tedit 5C345011)
    (at 123.19 91.44 180)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J4 (at 2.413 0 270) (layer B.SilkS))
    (fp_text value KBD (at 2.413 -10.287 270) (layer B.SilkS))
    (fp_text user %R (at 0 -5.08 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5C345470)
    (at 72.39 86.995 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at 2.413 0.508 270) (layer B.SilkS))
    (fp_text value SPK (at 2.413 -2.413 270) (layer B.SilkS))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(BZ5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(BZ5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5C34538D)
    (at 66.675 66.675)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at -2.413 0 90) (layer B.SilkS))
    (fp_text value RST (at -2.413 -2.667 90) (layer B.SilkS))
    (fp_text user %R (at 0 -1.27 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x05_P2.00mm_Vertical (layer B.Cu) (tedit 5C345A92)
    (at 132.08 116.205 180)
    (descr "Through hole straight pin header, 2x05, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.00mm double row")
    (fp_text reference J8 (at 1 2.06 180) (layer B.SilkS))
    (fp_text value COM1 (at 1 -10.06 180) (layer B.SilkS))
    (fp_text user %R (at 1 -4 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 105 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 106 "Net-(J8-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 107 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 108 "Net-(J8-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 109 "Net-(J8-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(J8-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(J8-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "Net-(J8-Pad9)"))
    (pad 10 thru_hole oval (at 2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 113 "Net-(J8-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x05_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x22_P2.00mm_Vertical (layer B.Cu) (tedit 5C345862)
    (at 83.693 63.5 270)
    (descr "Through hole straight pin header, 2x22, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x22 2.00mm double row")
    (fp_text reference J10 (at -2.159 -0.127 180) (layer B.SilkS))
    (fp_text value IDE (at -2.159 -41.91 180) (layer B.SilkS))
    (fp_text user %R (at 1 -21 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 114 "Net-(J10-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 115 "Net-(J10-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 116 "Net-(J10-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 "Net-(J10-Pad5)"))
    (pad 6 thru_hole oval (at 2 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 "Net-(J10-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(J10-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 "Net-(J10-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 "Net-(J10-Pad9)"))
    (pad 10 thru_hole oval (at 2 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(J10-Pad10)"))
    (pad 11 thru_hole oval (at 0 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 "Net-(J10-Pad11)"))
    (pad 12 thru_hole oval (at 2 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 "Net-(J10-Pad12)"))
    (pad 13 thru_hole oval (at 0 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 125 "Net-(J10-Pad13)"))
    (pad 14 thru_hole oval (at 2 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 126 "Net-(J10-Pad14)"))
    (pad 15 thru_hole oval (at 0 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 127 "Net-(J10-Pad15)"))
    (pad 16 thru_hole oval (at 2 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 128 "Net-(J10-Pad16)"))
    (pad 17 thru_hole oval (at 0 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 "Net-(J10-Pad17)"))
    (pad 18 thru_hole oval (at 2 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(J10-Pad18)"))
    (pad 19 thru_hole oval (at 0 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(J10-Pad19)"))
    (pad 20 thru_hole oval (at 2 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(J10-Pad20)"))
    (pad 21 thru_hole oval (at 0 -20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(J10-Pad21)"))
    (pad 22 thru_hole oval (at 2 -20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(J10-Pad22)"))
    (pad 23 thru_hole oval (at 0 -22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(J10-Pad23)"))
    (pad 24 thru_hole oval (at 2 -22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 "Net-(J10-Pad24)"))
    (pad 25 thru_hole oval (at 0 -24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "Net-(J10-Pad25)"))
    (pad 26 thru_hole oval (at 2 -24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(J10-Pad26)"))
    (pad 27 thru_hole oval (at 0 -26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(J10-Pad27)"))
    (pad 28 thru_hole oval (at 2 -26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(J10-Pad28)"))
    (pad 29 thru_hole oval (at 0 -28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(J10-Pad29)"))
    (pad 30 thru_hole oval (at 2 -28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(J10-Pad30)"))
    (pad 31 thru_hole oval (at 0 -30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(J10-Pad31)"))
    (pad 32 thru_hole oval (at 2 -30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 144 "Net-(J10-Pad32)"))
    (pad 33 thru_hole oval (at 0 -32 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 145 "Net-(J10-Pad33)"))
    (pad 34 thru_hole oval (at 2 -32 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 146 "Net-(J10-Pad34)"))
    (pad 35 thru_hole oval (at 0 -34 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 147 "Net-(J10-Pad35)"))
    (pad 36 thru_hole oval (at 2 -34 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 148 "Net-(J10-Pad36)"))
    (pad 37 thru_hole oval (at 0 -36 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 149 "Net-(J10-Pad37)"))
    (pad 38 thru_hole oval (at 2 -36 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 150 "Net-(J10-Pad38)"))
    (pad 39 thru_hole oval (at 0 -38 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 151 "Net-(J10-Pad39)"))
    (pad 40 thru_hole oval (at 2 -38 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 41 thru_hole oval (at 0 -40 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 42 thru_hole oval (at 2 -40 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 43 thru_hole oval (at 0 -42 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 44 thru_hole oval (at 2 -42 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 152 "Net-(J10-Pad44)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x22_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x05_P2.00mm_Vertical (layer B.Cu) (tedit 5C345A97)
    (at 119.38 116.205 180)
    (descr "Through hole straight pin header, 2x05, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.00mm double row")
    (fp_text reference J12 (at 1 2.06 180) (layer B.SilkS))
    (fp_text value COM2 (at 1 -10.06 180) (layer B.SilkS))
    (fp_text user %R (at 1 -4 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 153 "Net-(J12-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(J12-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(J12-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 156 "Net-(J12-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 157 "Net-(J12-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 158 "Net-(J12-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 159 "Net-(J12-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 160 "Net-(J12-Pad9)"))
    (pad 10 thru_hole oval (at 2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 161 "Net-(J12-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x05_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x17_P2.00mm_Vertical (layer B.Cu) (tedit 5C3458AE)
    (at 82.042 70.485 270)
    (descr "Through hole straight pin header, 2x17, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x17 2.00mm double row")
    (fp_text reference J13 (at -2.159 -0.254 180) (layer B.SilkS))
    (fp_text value FDD (at -2.159 -31.75 180) (layer B.SilkS))
    (fp_text user %R (at 1 -16 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 162 "Net-(J13-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 2 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 163 "Net-(J13-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 164 "Net-(J13-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 8 thru_hole oval (at 2 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 165 "Net-(J13-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 10 thru_hole oval (at 2 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 166 "Net-(J13-Pad10)"))
    (pad 11 thru_hole oval (at 0 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 12 thru_hole oval (at 2 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 167 "Net-(J13-Pad12)"))
    (pad 13 thru_hole oval (at 0 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 14 thru_hole oval (at 2 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 "Net-(J13-Pad14)"))
    (pad 15 thru_hole oval (at 0 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 16 thru_hole oval (at 2 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 "Net-(J13-Pad16)"))
    (pad 17 thru_hole oval (at 0 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 18 thru_hole oval (at 2 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 "Net-(J13-Pad18)"))
    (pad 19 thru_hole oval (at 0 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 20 thru_hole oval (at 2 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 171 "Net-(J13-Pad20)"))
    (pad 21 thru_hole oval (at 0 -20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 22 thru_hole oval (at 2 -20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 172 "Net-(J13-Pad22)"))
    (pad 23 thru_hole oval (at 0 -22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 24 thru_hole oval (at 2 -22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 173 "Net-(J13-Pad24)"))
    (pad 25 thru_hole oval (at 0 -24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 26 thru_hole oval (at 2 -24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 174 "Net-(J13-Pad26)"))
    (pad 27 thru_hole oval (at 0 -26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 28 thru_hole oval (at 2 -26 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 175 "Net-(J13-Pad28)"))
    (pad 29 thru_hole oval (at 0 -28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 30 thru_hole oval (at 2 -28 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 176 "Net-(J13-Pad30)"))
    (pad 31 thru_hole oval (at 0 -30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 32 thru_hole oval (at 2 -30 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 177 "Net-(J13-Pad32)"))
    (pad 33 thru_hole oval (at 0 -32 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 34 thru_hole oval (at 2 -32 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 178 "Net-(J13-Pad34)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x17_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x05_P2.00mm_Vertical (layer B.Cu) (tedit 5C34525B)
    (at 65.5 80.8)
    (descr "Through hole straight pin header, 2x05, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.00mm double row")
    (fp_text reference J14 (at -2.127 -0.155 90) (layer B.SilkS))
    (fp_text value VGA (at -2.127 -7.648 90) (layer B.SilkS))
    (fp_text user %R (at 1 -4 -90) (layer B.Fab))
    (pad 10 thru_hole oval (at 2 -8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 9 thru_hole oval (at 0 -8) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 179 "Net-(J14-Pad9)"))
    (pad 8 thru_hole oval (at 2 -6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 7 thru_hole oval (at 0 -6) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 180 "Net-(J14-Pad7)"))
    (pad 6 thru_hole oval (at 2 -4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 5 thru_hole oval (at 0 -4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 181 "Net-(J14-Pad5)"))
    (pad 4 thru_hole oval (at 2 -2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 -2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 182 "Net-(J14-Pad3)"))
    (pad 2 thru_hole oval (at 2 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 "Net-(J14-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x05_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x05_P2.00mm_Vertical (layer B.Cu) (tedit 5C345A9D)
    (at 106.68 116.205 180)
    (descr "Through hole straight pin header, 2x05, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.00mm double row")
    (fp_text reference J15 (at 1 2.06 180) (layer B.SilkS))
    (fp_text value COM3 (at 1 -10.06 180) (layer B.SilkS))
    (fp_text user %R (at 1 -4 90) (layer B.Fab))
    (pad 10 thru_hole oval (at 2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 "Net-(J15-Pad10)"))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 "Net-(J15-Pad9)"))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 186 "Net-(J15-Pad8)"))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 187 "Net-(J15-Pad7)"))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 188 "Net-(J15-Pad6)"))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 189 "Net-(J15-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 190 "Net-(J15-Pad3)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 191 "Net-(J15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 192 "Net-(J15-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x05_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x05_P2.00mm_Vertical (layer B.Cu) (tedit 5C345AA3)
    (at 93.98 116.205 180)
    (descr "Through hole straight pin header, 2x05, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.00mm double row")
    (fp_text reference J16 (at 1 2.06 180) (layer B.SilkS))
    (fp_text value COM4 (at 1 -10.06 180) (layer B.SilkS))
    (fp_text user %R (at 1 -4 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 193 "Net-(J16-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 194 "Net-(J16-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 195 "Net-(J16-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 196 "Net-(J16-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 197 "Net-(J16-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 198 "Net-(J16-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 199 "Net-(J16-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 200 "Net-(J16-Pad9)"))
    (pad 10 thru_hole oval (at 2 -8 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 201 "Net-(J16-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x05_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x04_P2.00mm_Vertical (layer B.Cu) (tedit 5C345534)
    (at 75 96.98 180)
    (descr "Through hole straight pin header, 2x04, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x04 2.00mm double row")
    (fp_text reference J17 (at 4.261 -0.175 270) (layer B.SilkS))
    (fp_text value ETH (at 4.134 -5.89 270) (layer B.SilkS))
    (fp_text user %R (at 1 -3 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 202 "Net-(J17-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 203 "Net-(J17-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 204 "Net-(J17-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 205 "Net-(J17-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 206 "Net-(J17-Pad5)"))
    (pad 6 thru_hole oval (at 2 -4 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 207 "Net-(J17-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 208 "Net-(J17-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 180) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 209 "Net-(J17-Pad8)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x04_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5C345705)
    (at 80.01 128.905 270)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J18 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value POWER (at 2.54 16.637 180) (layer F.SilkS))
    (fp_text user %R (at 0 8.89) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad18)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad14)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C345A8B)
    (at 135.89 116.205)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference JA8 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value COM1 (at 1.27 12.49) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(J8-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(J8-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(J8-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(J8-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(J8-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(J8-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(J8-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 210 "Net-(JA8-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 5C345807)
    (at 79.375 56.515 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference JA10 (at -2.54 0.508) (layer F.SilkS))
    (fp_text value IDE (at -2.54 48.387) (layer F.SilkS))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(J10-Pad39)"))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(J10-Pad38)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(J10-Pad37)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(J10-Pad36)"))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(J10-Pad35)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 146 "Net-(J10-Pad34)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 145 "Net-(J10-Pad33)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 "Net-(J10-Pad32)"))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(J10-Pad31)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(J10-Pad30)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(J10-Pad29)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(J10-Pad28)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(J10-Pad27)"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J10-Pad26)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(J10-Pad25)"))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(J10-Pad24)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J10-Pad23)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(J10-Pad22)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(J10-Pad21)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(J10-Pad20)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(J10-Pad19)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(J10-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(J10-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(J10-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(J10-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(J10-Pad14)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(J10-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(J10-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(J10-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(J10-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(J10-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(J10-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(J10-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(J10-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(J10-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(J10-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(J10-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C345A85)
    (at 123.19 116.205)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference JA12 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value COM2 (at 1.27 12.49) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 211 "Net-(JA12-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 160 "Net-(J12-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 "Net-(J12-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 158 "Net-(J12-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 157 "Net-(J12-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 156 "Net-(J12-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 155 "Net-(J12-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(J12-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(J12-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical (layer F.Cu) (tedit 5C345905)
    (at 74.93 80.645 90)
    (descr "Through hole straight pin header, 2x17, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x17 2.54mm double row")
    (fp_text reference JA13 (at 4.953 0.508) (layer F.SilkS))
    (fp_text value FDD (at 5.08 40.513) (layer F.SilkS))
    (fp_text user %R (at 1.27 20.32 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 162 "Net-(J13-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 163 "Net-(J13-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 164 "Net-(J13-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(J13-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 "Net-(J13-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 167 "Net-(J13-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 168 "Net-(J13-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 169 "Net-(J13-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 170 "Net-(J13-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 "Net-(J13-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 172 "Net-(J13-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 173 "Net-(J13-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 174 "Net-(J13-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 175 "Net-(J13-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 176 "Net-(J13-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 177 "Net-(J13-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 178 "Net-(J13-Pad34)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C345A7F)
    (at 110.49 116.205)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference JA15 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value COM3 (at 1.27 12.49) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 192 "Net-(J15-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 191 "Net-(J15-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 190 "Net-(J15-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 189 "Net-(J15-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 188 "Net-(J15-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 187 "Net-(J15-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 186 "Net-(J15-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 185 "Net-(J15-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 217 "Net-(JA15-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C345A77)
    (at 97.79 116.205)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference JA16 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value COM4 (at 1.27 12.49) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 90) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 218 "Net-(JA16-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 200 "Net-(J16-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 199 "Net-(J16-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 198 "Net-(J16-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 197 "Net-(J16-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 196 "Net-(J16-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 195 "Net-(J16-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 194 "Net-(J16-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 193 "Net-(J16-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5C3457BB)
    (at 66.675 53.975 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference JB10 (at -2.54 0.508) (layer F.SilkS))
    (fp_text value IDE (at -2.54 7.874) (layer F.SilkS))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 5C345742)
    (at 86.36 123.825 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference JC20 (at 2.54 0.508 180) (layer F.SilkS))
    (fp_text value DC-REG (at 2.54 8.509 180) (layer F.SilkS))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 219 VDD))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 220 "Net-(JC20-Pad5)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C3456A8)
    (at 67.31 121.285)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JC22 (at 2.54 0.508 90) (layer F.SilkS))
    (fp_text value DC-SRC (at -2.413 1.016 90) (layer F.SilkS))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 219 VDD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 221 "Net-(JC21-Pad3)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x10_P2.00mm_Vertical (layer B.Cu) (tedit 5C345931)
    (at 93.98 86.36 270)
    (descr "Through hole straight pin header, 2x10, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.00mm double row")
    (fp_text reference JP1 (at -2.159 -0.254 180) (layer B.SilkS))
    (fp_text value GPIO (at -2.159 -17.272 180) (layer B.SilkS))
    (fp_text user %R (at 1 -9 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 3 thru_hole oval (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 222 "Net-(JP1-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 223 "Net-(JP1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 224 "Net-(JP1-Pad5)"))
    (pad 6 thru_hole oval (at 2 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 225 "Net-(JP1-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 226 "Net-(JP1-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 227 "Net-(JP1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 228 "Net-(JP1-Pad9)"))
    (pad 10 thru_hole oval (at 2 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 229 "Net-(JP1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 230 "Net-(JP1-Pad11)"))
    (pad 12 thru_hole oval (at 2 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 231 "Net-(JP1-Pad12)"))
    (pad 13 thru_hole oval (at 0 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 232 "Net-(JP1-Pad13)"))
    (pad 14 thru_hole oval (at 2 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 233 "Net-(JP1-Pad14)"))
    (pad 15 thru_hole oval (at 0 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 234 "Net-(JP1-Pad15)"))
    (pad 16 thru_hole oval (at 2 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 235 "Net-(JP1-Pad16)"))
    (pad 17 thru_hole oval (at 0 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 236 "Net-(JP1-Pad17)"))
    (pad 18 thru_hole oval (at 2 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 237 "Net-(JP1-Pad18)"))
    (pad 19 thru_hole oval (at 0 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 20 thru_hole oval (at 2 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x10_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer F.Cu) (tedit 5C345969)
    (at 92.71 95.885 90)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference JPA1 (at 5.08 0.508) (layer F.SilkS))
    (fp_text value GPIO (at 5.08 22.352) (layer F.SilkS))
    (fp_text user %R (at 1.27 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 222 "Net-(JP1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 223 "Net-(JP1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 224 "Net-(JP1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 225 "Net-(JP1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 226 "Net-(JP1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 227 "Net-(JP1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 228 "Net-(JP1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 229 "Net-(JP1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 230 "Net-(JP1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 231 "Net-(JP1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 232 "Net-(JP1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 233 "Net-(JP1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 234 "Net-(JP1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 235 "Net-(JP1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 236 "Net-(JP1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 237 "Net-(JP1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 VCC))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.00mm:PinHeader_2x13_P2.00mm_Vertical (layer B.Cu) (tedit 5C34599D)
    (at 93.98 101.6 270)
    (descr "Through hole straight pin header, 2x13, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x13 2.00mm double row")
    (fp_text reference P1 (at -2.159 0.127 180) (layer B.SilkS))
    (fp_text value PARALLEL (at -2.159 -21.59 180) (layer B.SilkS))
    (fp_text user %R (at 1 -12 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 238 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 239 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 240 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2 -2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 241 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 242 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 2 -4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 243 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 244 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 2 -6 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 245 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 246 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 2 -8 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 247 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 248 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 2 -10 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 249 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 250 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 2 -12 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 251 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 252 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at 2 -14 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 253 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 254 "Net-(P1-Pad17)"))
    (pad 18 thru_hole oval (at 2 -16 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 19 thru_hole oval (at 0 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 20 thru_hole oval (at 2 -18 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 21 thru_hole oval (at 0 -20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 22 thru_hole oval (at 2 -20 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 23 thru_hole oval (at 0 -22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 24 thru_hole oval (at 2 -22 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 25 thru_hole oval (at 0 -24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 26 thru_hole oval (at 2 -24 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 255 "Net-(P1-Pad26)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_2x13_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x13_P2.54mm_Vertical (layer F.Cu) (tedit 5C3459CE)
    (at 92.71 111.125 90)
    (descr "Through hole straight pin header, 2x13, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x13 2.54mm double row")
    (fp_text reference PA1 (at 4.953 0) (layer F.SilkS))
    (fp_text value PARALLEL (at 4.953 28.067) (layer F.SilkS))
    (fp_text user %R (at 1.27 15.24 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 238 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 239 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 240 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 241 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 242 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 243 "Net-(P1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 244 "Net-(P1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 245 "Net-(P1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 246 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 247 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 248 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 249 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 250 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 251 "Net-(P1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 252 "Net-(P1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 253 "Net-(P1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 254 "Net-(P1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 256 "Net-(PA1-Pad26)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x13_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5C345394)
    (at 71.5645 65.0875)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW6 (at 3.2385 -2.0955) (layer F.SilkS))
    (fp_text value RST (at 3.2385 6.7) (layer F.SilkS))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 104 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 104 "Net-(J6-Pad1)"))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 96 GNDREF))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 5C31A31F)
    (at 72.644 122.936)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_text "DARIAN   ICOP 6054VE BACKPLANE   v0.2" (at 102.997 144.907) (layer F.SilkS))
  (gr_line (start 50.8 146.685) (end 50.8 50.8) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 146.685) (end 50.8 146.685) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 50.8) (end 140.97 146.685) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 50.8 50.8) (end 140.97 50.8) (layer Edge.Cuts) (width 0.15))
  (zone (net 96) (net_name GNDREF) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.673 146.812) (xy 50.673 50.673) (xy 141.097 50.673) (xy 141.097 146.812)
      )
    )
  )
  (zone (net 96) (net_name GNDREF) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.673 146.812) (xy 50.673 50.673) (xy 141.097 50.673) (xy 141.097 146.812)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.533 87.757) (xy 73.533 88.773) (xy 78.74 88.773) (xy 78.74 87.757)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63.37294 130.17506) (xy 68.57994 130.17506) (xy 68.57994 131.06406) (xy 67.05594 132.58806) (xy 63.37294 132.58806)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.65 119.761) (xy 120.65 120.523) (xy 121.793 121.666) (xy 121.793 120.777)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.95 119.761) (xy 107.95 120.523) (xy 109.093 121.666) (xy 109.093 120.777)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 119.761) (xy 133.35 120.523) (xy 134.493 121.666) (xy 134.493 120.777)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.25 119.761) (xy 95.25 120.523) (xy 96.393 121.666) (xy 96.393 120.777)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.677 62.103) (xy 82.042 62.738) (xy 77.343 57.912) (xy 78.486 57.912)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.96 72.136) (xy 60.325 72.771) (xy 60.96 73.406)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.762))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.134 70.231) (xy 59.563 70.231) (xy 58.293 71.501) (xy 57.404 71.501)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.786 106.299) (xy 66.294 106.299) (xy 66.294 99.187) (xy 65.786 99.187)
      )
    )
  )
)
