(kicad_pcb (version 4) (host pcbnew 4.0.0-rc1-stable)
  (general
    (links 0)
    (no_connects 0)
    (area -26.999001 -26.999001 26.999001 26.999001)
    (thickness 1.6)
    (drawings 1)
    (tracks 0)
    (zones 0)
    (modules 2)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module junes:LOGO (layer B.Cu) (tedit 0)
    (at -1.195 0.715674 180)
    (fp_text reference G*** (at 0 0 180) (layer B.Mask) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.Mask) hide)
  )
  (module junes:LOGO (layer F.Cu) (tedit 0)
    (at 1.27 1.27)
    (fp_text reference G*** (at 0 0) (layer F.Mask) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (gr_circle (center 0 0) (end 26.924 0) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -29.845 -13.97) (xy -21.59 -13.97) (xy -22.86 13.335) (xy -29.21 11.43)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -13.335 -23.19628) (xy -13.335 -31.45128) (xy 13.97 -30.18128) (xy 12.065 -23.83128)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 2.54)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -13.335 -24.13) (xy 13.335 -24.13) (xy 12.7 -28.575) (xy -13.97 -27.94) (xy -13.97 -24.13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 2.54)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -24.13 12.7) (xy -24.13 -13.97) (xy -28.575 -13.335) (xy -27.94 13.335) (xy -24.13 13.335)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 2.54)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.205 12.145674) (xy 24.205 -14.524326) (xy 28.65 -13.889326) (xy 28.015 12.780674) (xy 24.205 12.780674)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 2.54)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13.41 -24.684326) (xy -13.26 -24.684326) (xy -12.625 -29.129326) (xy 14.045 -28.494326) (xy 14.045 -24.684326)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29.92 -14.524326) (xy 21.665 -14.524326) (xy 22.935 12.780674) (xy 29.285 10.875674)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13.41 -23.750606) (xy 13.41 -32.005606) (xy -13.895 -30.735606) (xy -11.99 -24.385606)
      )
    )
  )
)
