<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="68.5675" y2="0" width="0" layer="20"/>
<wire x1="68.5675" y1="0" x2="68.5675" y2="57.14" width="0" layer="20"/>
<wire x1="68.5675" y1="57.14" x2="0" y2="57.14" width="0" layer="20"/>
<wire x1="0" y1="57.14" x2="0" y2="0" width="0" layer="20"/>
<hole x="12.7" y="48.895" drill="3.2"/>
<hole x="12.7" y="8.255" drill="3.2"/>
<hole x="53.34" y="8.255" drill="3.2"/>
<hole x="53.34" y="48.895" drill="3.2"/>
<text>SR1</text>
<text>MCLK</text>
<text>!MSYNC</text>
<text>RESET</text>
<text>CBLNK</text>
<text>!BUSAK</text>
<text>VCC</text>
<text>GND</text>
<text>EXT. VIDEO II</text>
<text>EXT. AUDIO</text>
<text>EXT. VIDEO</text>
<text>TOP</text>
<text>x6</text>
<text>x6</text>
<text>x6</text>
<text>Inty A/V Tap v.1.0</text>
<text>APR 28 2017</text>
</plain>
<libraries>
<library name="con-cardedge">
<packages>
<package name="CARDEDGE-44M">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X22">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-5MM">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="ptc-ntc">
<description>&lt;b&gt;PTC and NTC Resistors&lt;/b&gt;&lt;p&gt;
Siemens, Philips, Valvo&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P660">
<description>&lt;b&gt;PHILIPS PTC&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE06">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sip">
<description>&lt;B&gt;Bourns 4600X Series - Thick Film Conformal SIPs&lt;/B&gt;&lt;P&gt;

Created by Jeffrey Reuben (JRJJ)&lt;P&gt;</description>
<packages>
<package name="SIP7">
<description>&lt;B&gt;Bourns 4607X-101 Resistor Network&lt;/B&gt;&lt;P&gt;

Source: http://www.bourns.com/data/global/pdfs/4600X.pdf&lt;P&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="con-cardedge" package="CARDEDGE-44M" value="CE-44M"/>
<element name="JP2" library="pinhead" package="2X22" value="CART">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="PWR">
<attribute name="NAME"/>
</element>
<element name="JP3" library="pinhead" package="1X03" value="A/V">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="4.7K">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="AXIAL-0.4" value="1k">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="22pf">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="22pf"/>
<element name="C3" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="22pf"/>
<element name="C4" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="22pf"/>
<element name="C5" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="22pf"/>
<element name="C6" library="SparkFun-Capacitors" package="CAP-PTH-5MM" value="22pf"/>
<element name="D1" library="diode" package="DO35-10" value="1N4148DO35-10">
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D3" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D4" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D5" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D6" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D7" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D8" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D9" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D10" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D11" library="diode" package="DO35-10" value="1N4148DO35-10"/>
<element name="D12" library="diode" package="DO35-10" value="1N4148DO35-10">
<attribute name="VALUE"/>
</element>
<element name="D51" library="diode" package="DO41-10" value="1N4004">
<attribute name="VALUE"/>
</element>
<element name="PTC" library="ptc-ntc" package="P660" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="con-lsta" package="FE06" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-sip" package="SIP7" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="DB0">
<contactref element="U$1" pad="P$33"/>
<contactref element="JP2" pad="33"/>
</signal>
<signal name="DB1">
<contactref element="U$1" pad="P$31"/>
<contactref element="JP2" pad="31"/>
</signal>
<signal name="DB2">
<contactref element="U$1" pad="P$27"/>
<contactref element="JP2" pad="27"/>
</signal>
<signal name="DB3">
<contactref element="U$1" pad="P$21"/>
<contactref element="JP2" pad="21"/>
</signal>
<signal name="DB4">
<contactref element="U$1" pad="P$17"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="DB5">
<contactref element="U$1" pad="P$13"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="DB6">
<contactref element="U$1" pad="P$9"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="DB7">
<contactref element="U$1" pad="P$5"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="DB8">
<contactref element="U$1" pad="P$7"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="DB9">
<contactref element="U$1" pad="P$11"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="DB10">
<contactref element="U$1" pad="P$15"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="DB11">
<contactref element="U$1" pad="P$19"/>
<contactref element="JP2" pad="19"/>
</signal>
<signal name="DB12">
<contactref element="U$1" pad="P$23"/>
<contactref element="JP2" pad="23"/>
</signal>
<signal name="DB13">
<contactref element="U$1" pad="P$25"/>
<contactref element="JP2" pad="25"/>
</signal>
<signal name="DB14">
<contactref element="U$1" pad="P$29"/>
<contactref element="JP2" pad="29"/>
</signal>
<signal name="DB15">
<contactref element="U$1" pad="P$35"/>
<contactref element="JP2" pad="35"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="P$16"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="P$18"/>
<contactref element="JP2" pad="18"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="P$20"/>
<contactref element="JP2" pad="20"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="P$22"/>
<contactref element="JP2" pad="22"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="P$24"/>
<contactref element="JP2" pad="24"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="P$26"/>
<contactref element="JP2" pad="26"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="P$28"/>
<contactref element="JP2" pad="28"/>
</signal>
<signal name="EXTVID2">
<contactref element="U$1" pad="P$2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="EXTVID">
<contactref element="U$1" pad="P$8"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="EXTAUD">
<contactref element="U$1" pad="P$6"/>
<contactref element="R1" pad="P$2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="!BUSAK">
<contactref element="U$1" pad="P$30"/>
<contactref element="JP2" pad="30"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="CBLNK">
<contactref element="U$1" pad="P$4"/>
<contactref element="JP2" pad="4"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="P$12"/>
<contactref element="JP2" pad="12"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="MCLK">
<contactref element="U$1" pad="P$10"/>
<contactref element="JP2" pad="10"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="SR1">
<contactref element="U$1" pad="P$14"/>
<contactref element="JP2" pad="14"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="!MSYNC">
<contactref element="U$1" pad="P$3"/>
<contactref element="JP2" pad="3"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="BC1OUT">
<contactref element="U$1" pad="P$41"/>
<contactref element="JP2" pad="41"/>
</signal>
<signal name="BC2OUT">
<contactref element="U$1" pad="P$39"/>
<contactref element="JP2" pad="39"/>
</signal>
<signal name="BDIROUT">
<contactref element="U$1" pad="P$37"/>
<contactref element="JP2" pad="37"/>
</signal>
<signal name="BC1IN">
<contactref element="U$1" pad="P$32"/>
<contactref element="JP2" pad="32"/>
</signal>
<signal name="BC2IN">
<contactref element="U$1" pad="P$34"/>
<contactref element="JP2" pad="34"/>
</signal>
<signal name="BDIRIN">
<contactref element="U$1" pad="P$36"/>
<contactref element="JP2" pad="36"/>
</signal>
<signal name="BDIRLOOP">
<contactref element="U$1" pad="P$38"/>
<contactref element="JP2" pad="38"/>
</signal>
<signal name="BC2LOOP">
<contactref element="U$1" pad="P$40"/>
<contactref element="JP2" pad="40"/>
</signal>
<signal name="BC1LOOP">
<contactref element="U$1" pad="P$42"/>
<contactref element="JP2" pad="42"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND2">
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="44"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="D7" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="D9" pad="A"/>
<contactref element="D10" pad="A"/>
<contactref element="D11" pad="A"/>
<contactref element="D12" pad="A"/>
<contactref element="U$1" pad="P$44"/>
</signal>
<signal name="!BUSAK_TAP">
<contactref element="C6" pad="1"/>
<contactref element="D6" pad="A"/>
<contactref element="D12" pad="C"/>
<contactref element="R8" pad="P$2"/>
<contactref element="JP4" pad="6"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="CBLNK_TAP">
<contactref element="C5" pad="1"/>
<contactref element="D5" pad="A"/>
<contactref element="D11" pad="C"/>
<contactref element="R6" pad="P$2"/>
<contactref element="JP4" pad="5"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="RESET_TAP">
<contactref element="C4" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="D10" pad="C"/>
<contactref element="R5" pad="P$2"/>
<contactref element="JP4" pad="4"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="!MSYNC_TAP">
<contactref element="C3" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="D9" pad="C"/>
<contactref element="R7" pad="P$2"/>
<contactref element="JP4" pad="3"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="MCLK_TAP">
<contactref element="C2" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="D8" pad="C"/>
<contactref element="R4" pad="P$2"/>
<contactref element="JP4" pad="2"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="SR1_TAP">
<contactref element="C1" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D7" pad="C"/>
<contactref element="R9" pad="P$2"/>
<contactref element="JP4" pad="1"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="JP2" pad="6"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="VCC_FUSE">
<contactref element="JP2" pad="43"/>
<contactref element="JP1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D6" pad="C"/>
<contactref element="PTC" pad="2"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="P$43"/>
<contactref element="D51" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="D51" pad="C"/>
<contactref element="PTC" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
