<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="31.75" y1="15.24" x2="82.5629" y2="15.199359375" width="0" layer="20"/>
<wire x1="82.5629" y1="15.199359375" x2="82.611159375" y2="62.29111875" width="0" layer="20"/>
<wire x1="82.611159375" y1="62.29111875" x2="31.75" y2="62.22" width="0" layer="20"/>
<wire x1="31.75" y1="62.22" x2="31.75" y2="15.24" width="0" layer="20"/>
<text>mettinoktay</text>
</plain>
<libraries>
<library name="Final_Thesis">
<packages>
<package name="ARCH_PRO">
</package>
<package name="ENCODER">
</package>
<package name="GENERATOR">
</package>
<package name="PITOT">
</package>
<package name="SERVO">
</package>
<package name="STEPPER">
</package>
<package name="STEPPER_DRIVER">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="special">
<description>&lt;b&gt;Special Devices&lt;/b&gt;&lt;p&gt;
7-segment displays, switches, heatsinks, crystals, transformers, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="EDG-03">
<description>&lt;b&gt;DIP SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SAP1" library="Final_Thesis" package="ARCH_PRO" value=""/>
<element name="U$1" library="Final_Thesis" package="ENCODER" value="ENCODER"/>
<element name="U$2" library="Final_Thesis" package="GENERATOR" value="GENERATOR"/>
<element name="U$3" library="Final_Thesis" package="PITOT" value="PITOT"/>
<element name="U$4" library="Final_Thesis" package="SERVO" value="SERVO"/>
<element name="U$5" library="Final_Thesis" package="STEPPER" value="STEPPER"/>
<element name="U$6" library="Final_Thesis" package="STEPPER_DRIVER" value="STEPPER_DRIVER"/>
<element name="12V" library="adafruit" package="DCJACK_2MM_PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-100UF-25V" value="100uF"/>
<element name="SW1" library="special" package="EDG-03" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="OUTPUT" library="adafruit" package="DCJACK_2MM_PTH" value=""/>
</elements>
<signals>
<signal name="N$6">
<contactref element="U$2" pad="+"/>
<contactref element="OUTPUT" pad="PWR"/>
</signal>
<signal name="P0_9">
<contactref element="SAP1" pad="P0_9_MOSI"/>
<contactref element="U$1" pad="B"/>
</signal>
<signal name="P0_6">
<contactref element="U$1" pad="A"/>
<contactref element="SAP1" pad="P0_6_SSEL"/>
</signal>
<signal name="12V">
<contactref element="12V" pad="PWR"/>
<contactref element="SAP1" pad="VIN"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="U$6" pad="VMOT"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="VCC"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="GND"/>
<contactref element="12V" pad="GND"/>
<contactref element="12V" pad="GNDBREAK"/>
<contactref element="U$4" pad="GND"/>
<contactref element="U$6" pad="GND"/>
<contactref element="SAP1" pad="GND1"/>
<contactref element="SAP1" pad="GND2"/>
<contactref element="U$6" pad="GND1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$3" pad="GND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="SAP1" pad="GND3"/>
</signal>
<signal name="P0_1">
<contactref element="SAP1" pad="P0_1_SCL1_RXD3"/>
<contactref element="U$2" pad="A"/>
</signal>
<signal name="P0_0">
<contactref element="SAP1" pad="P0_0_SDA1_TXD3"/>
<contactref element="U$2" pad="B"/>
</signal>
<signal name="~P2_5">
<contactref element="SAP1" pad="~P2_5"/>
<contactref element="U$4" pad="SGN"/>
</signal>
<signal name="P0_23">
<contactref element="SAP1" pad="P0_23"/>
<contactref element="U$3" pad="SGN"/>
</signal>
<signal name="5V">
<contactref element="SAP1" pad="5V"/>
<contactref element="U$4" pad="5V"/>
<contactref element="U$6" pad="SLP"/>
<contactref element="U$6" pad="RST"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="6"/>
<contactref element="U$3" pad="5V"/>
</signal>
<signal name="N$1">
<contactref element="U$6" pad="B2"/>
<contactref element="U$5" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U$6" pad="B1"/>
<contactref element="U$5" pad="B"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="A1"/>
<contactref element="U$5" pad="C"/>
</signal>
<signal name="N$4">
<contactref element="U$6" pad="A2"/>
<contactref element="U$5" pad="D"/>
</signal>
<signal name="N$10">
<contactref element="SW1" pad="3"/>
<contactref element="U$6" pad="M0"/>
</signal>
<signal name="N$12">
<contactref element="SW1" pad="2"/>
<contactref element="U$6" pad="M1"/>
</signal>
<signal name="N$13">
<contactref element="SW1" pad="1"/>
<contactref element="U$6" pad="M2"/>
</signal>
<signal name="N$15">
<contactref element="OUTPUT" pad="GNDBREAK"/>
<contactref element="OUTPUT" pad="GND"/>
<contactref element="U$2" pad="-"/>
</signal>
<signal name="~P2_4">
<contactref element="SAP1" pad="~P2_4"/>
<contactref element="U$6" pad="STEP"/>
</signal>
<signal name="P0_4">
<contactref element="SAP1" pad="P0_4"/>
<contactref element="U$6" pad="DIR"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
