(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 65)
    (no_connects 1)
    (area 141.949999 53.949999 185.774801 76.050001)
    (thickness 1.6)
    (drawings 6)
    (tracks 278)
    (zones 0)
    (modules 22)
    (nets 46)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFCFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.200000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 VCC)
  (net 4 "Net-(C3-Pad1)")
  (net 5 /MOSI)
  (net 6 /MISO)
  (net 7 /SCK)
  (net 8 /RESET)
  (net 9 "Net-(IC1-Pad7)")
  (net 10 "Net-(IC1-Pad8)")
  (net 11 /UART_RX)
  (net 12 /UART_TX)
  (net 13 "Net-(IC1-Pad11)")
  (net 14 "Net-(IC1-Pad13)")
  (net 15 "Net-(IC1-Pad14)")
  (net 16 "Net-(IC1-Pad15)")
  (net 17 "Net-(IC1-Pad16)")
  (net 18 /i2c_scl)
  (net 19 /i2c_sda)
  (net 20 "Net-(IC1-Pad21)")
  (net 21 "Net-(IC1-Pad22)")
  (net 22 "Net-(IC1-Pad23)")
  (net 23 "Net-(IC1-Pad24)")
  (net 24 "Net-(IC1-Pad25)")
  (net 25 "Net-(IC1-Pad26)")
  (net 26 "Net-(IC1-Pad30)")
  (net 27 "Net-(IC1-Pad31)")
  (net 28 "Net-(IC1-Pad32)")
  (net 29 "Net-(IC1-Pad34)")
  (net 30 "Net-(IC1-Pad35)")
  (net 31 "Net-(IC1-Pad36)")
  (net 32 "Net-(IC1-Pad37)")
  (net 33 /RFM_DIO2)
  (net 34 /RFM_DIO1)
  (net 35 /RFM_DIO0)
  (net 36 /RFM_RESET)
  (net 37 /RFM_SS)
  (net 38 "Net-(U1-Pad4)")
  (net 39 "Net-(U2-Pad7)")
  (net 40 "Net-(U2-Pad11)")
  (net 41 "Net-(U2-Pad12)")
  (net 42 "Net-(P5-Pad1)")
  (net 43 /DHT22_data)
  (net 44 "Net-(P7-Pad3)")
  (net 45 /DHT22_vcc)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /DHT22_data)
    (add_net /DHT22_vcc)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RFM_DIO0)
    (add_net /RFM_DIO1)
    (add_net /RFM_DIO2)
    (add_net /RFM_RESET)
    (add_net /RFM_SS)
    (add_net /SCK)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net /i2c_scl)
    (add_net /i2c_sda)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad16)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad31)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad34)")
    (add_net "Net-(IC1-Pad35)")
    (add_net "Net-(IC1-Pad36)")
    (add_net "Net-(IC1-Pad37)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad7)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 166.5478 70.6374 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 164.1094 67.691)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 164.084 63.119)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 164.084 65.405 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 154.5082 72.898 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 155.575 64.262)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -7.45) (layer F.SilkS))
    (fp_text value ATMEGA1284P-A (at 0 7.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /MOSI))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /MISO))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCK))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /UART_RX))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /UART_TX))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 /DHT22_data))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad16)"))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /i2c_scl))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /i2c_sda))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad21)"))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad30)"))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad31)"))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad32)"))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /DHT22_vcc))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad34)"))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC1-Pad35)"))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /RFM_DIO2))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /RFM_DIO1))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /RFM_DIO0))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /RFM_RESET))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /RFM_SS))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 163.3982 74.295)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value Battery (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 151.1046 55.0926 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module others:SMA_EDGE (layer F.Cu) (tedit 54067F78)
    (at 167.894 57.3532 270)
    (fp_text reference SMA_E1 (at 0 -6.35 270) (layer F.SilkS) hide)
    (fp_text value SMA_EDGE (at 0 -6.35 450) (layer F.SilkS))
    (pad 2 smd rect (at -2.1463 -2.0955 270) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 270) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.8415 270) (size 1.27 3.683) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at -2.1463 -2.0955 270) (size 1.27 4.191) (layers B.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 270) (size 1.27 4.191) (layers B.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 163.8554 70.739 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -0.05 -2.55 90) (layer F.SilkS))
    (fp_text value LP2985LV (at -0.05 2.35 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module drawn_by_jpmeijers:RFM95 (layer B.Cu) (tedit 575ACF57)
    (at 155.829 64.516)
    (fp_text reference U2 (at 0 -1) (layer B.SilkS))
    (fp_text value RFM95 (at 0 0.5) (layer B.Fab))
    (pad 1 smd rect (at -7.5 7) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -7.5 5) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 /MISO))
    (pad 3 smd rect (at -7.5 3) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 /MOSI))
    (pad 4 smd rect (at -7.5 1) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 /SCK))
    (pad 5 smd rect (at -7.5 -1) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 37 /RFM_SS))
    (pad 6 smd rect (at -7.5 -3) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 36 /RFM_RESET))
    (pad 7 smd rect (at -7.5 -5) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -7.5 -7) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 7.5 -7) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(P5-Pad1)"))
    (pad 10 smd rect (at 7.5 -5) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 7.5 -3) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at 7.5 -1) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at 7.5 1) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 VCC))
    (pad 14 smd rect (at 7.5 3) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 35 /RFM_DIO0))
    (pad 15 smd rect (at 7.5 5) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 34 /RFM_DIO1))
    (pad 16 smd rect (at 7.5 7) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 33 /RFM_DIO2))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 149.225 74.295 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value UART (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /UART_RX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /UART_TX))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 146.558 62.7126)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 156.718 55.753 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 144.145 74.295 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /MOSI))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /MISO))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /SCK))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /RESET))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 159.8168 74.295 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /i2c_sda))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /i2c_scl))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module others:U.FL-COAX (layer F.Cu) (tedit 0)
    (at 169.2148 57.3532 180)
    (attr smd)
    (fp_text reference P5 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value U.FL (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.5 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 0 -1.5 180) (size 2.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.5 180) (size 2.2 1) (layers F.Cu F.Paste F.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 54E9F79C)
    (at 166.7002 57.3532)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 0 -5.1) (layer F.SilkS))
    (fp_text value Antenna (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P5-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module drawn_by_jpmeijers:RESONATOR_CSTCE16M0V53-R0 (layer F.Cu) (tedit 57E915BD)
    (at 147.5994 65.4558 270)
    (fp_text reference Q1 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value RESONATOR (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad7)"))
    (pad 3 smd rect (at 0.95 0 270) (size 0.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad8)"))
  )
  (module "drawn_by_jpmeijers:B3U-1000P(M)-B" (layer F.Cu) (tedit 57E91CBC)
    (at 144.1704 59.0296 270)
    (fp_text reference SW1 (at 0 -2.4 270) (layer F.SilkS))
    (fp_text value RESET (at 0 -3.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.7 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.7 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad "" thru_hole circle (at 0 0 270) (size 0.75 0.75) (drill 0.75) (layers *.Cu *.Paste *.SilkS *.Mask Dwgs.User))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 170.1292 73.9902 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value DHT22 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /DHT22_vcc))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /DHT22_data))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P7-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 167.005 66.9544 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /DHT22_data))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /DHT22_vcc))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 30.175211 (width 0.3) (layer Dwgs.User)
    (gr_text "30,175 mm" (at 157.092582 83.633059 359.9517712) (layer Dwgs.User))
    (feature1 (pts (xy 172.1866 76.0222) (xy 172.179046 84.995759)))
    (feature2 (pts (xy 142.0114 75.9968) (xy 142.003846 84.970359)))
    (crossbar (pts (xy 142.006119 82.27036) (xy 172.181319 82.29576)))
    (arrow1a (pts (xy 172.181319 82.29576) (xy 171.054322 82.881232)))
    (arrow1b (pts (xy 172.181319 82.29576) (xy 171.055309 81.708391)))
    (arrow2a (pts (xy 142.006119 82.27036) (xy 143.132129 82.857729)))
    (arrow2b (pts (xy 142.006119 82.27036) (xy 143.133116 81.684888)))
  )
  (dimension 21.9964 (width 0.3) (layer Dwgs.User)
    (gr_text "21,996 mm" (at 180.5978 64.9986 270) (layer Dwgs.User))
    (feature1 (pts (xy 172.212 75.9968) (xy 181.9478 75.9968)))
    (feature2 (pts (xy 172.212 54.0004) (xy 181.9478 54.0004)))
    (crossbar (pts (xy 179.2478 54.0004) (xy 179.2478 75.9968)))
    (arrow1a (pts (xy 179.2478 75.9968) (xy 178.661379 74.870296)))
    (arrow1b (pts (xy 179.2478 75.9968) (xy 179.834221 74.870296)))
    (arrow2a (pts (xy 179.2478 54.0004) (xy 178.661379 55.126904)))
    (arrow2b (pts (xy 179.2478 54.0004) (xy 179.834221 55.126904)))
  )
  (gr_line (start 142 54) (end 142 76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.2 54) (end 172.2 76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142 76) (end 172.2 76) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142 54) (end 172.2 54) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.0368 54.0258) (xy 172.1612 54.0258) (xy 172.1612 75.9714) (xy 142.0368 75.9714)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 142.0368 54.0258) (xy 172.1612 54.0258) (xy 172.1612 75.9714) (xy 142.0368 75.9714)
      )
    )
  )
)
