<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.99" y2="0" width="0" layer="20"/>
<wire x1="19.99" y1="0" x2="19.99" y2="43.17" width="0" layer="20"/>
<wire x1="19.99" y1="43.17" x2="0" y2="43.17" width="0" layer="20"/>
<wire x1="0" y1="43.17" x2="0" y2="0" width="0" layer="20"/>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>PB</text>
<text>PC</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>Vcc</text>
<text>Gnd</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>PE</text>
<text>PD</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
</plain>
<libraries>
<library name="rcl">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="newchips2">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_LOCK">
</package>
<package name="TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="SIP-100-08-32">
<description>&lt;b&gt;SIP Header&lt;/b&gt; - 0.1", 32 mil drill</description>
</package>
</packages>
</library>
<library name="physnoct">
<packages>
<package name="PHYSNOCT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl" package="C0603" value="27pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0603" value="27pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="newchips2" package="TQFP32-08" value="ATMEGA32832A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun" package="2X3_LOCK" value="AVR_SPI_PRG_62X3_LOCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="con-headers-jp" package="SIP-100-08-32" value="M-1X08-SIP-100-32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="con-headers-jp" package="SIP-100-08-32" value="M-1X08-SIP-100-32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P3" library="con-headers-jp" package="SIP-100-08-32" value="M-1X08-SIP-100-32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P4" library="con-headers-jp" package="SIP-100-08-32" value="M-1X08-SIP-100-32">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun" package="TC38H" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="U$2" library="physnoct" package="PHYSNOCT" value="PHYSNOCT"/>
<element name="C3" library="rcl" package="C0603" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="P4" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="J1" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="IC1" pad="15"/>
<contactref element="P3" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="P3" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="IC1" pad="17"/>
<contactref element="P3" pad="6"/>
</signal>
<signal name="/RESET">
<contactref element="J1" pad="5"/>
<contactref element="IC1" pad="29"/>
<contactref element="P2" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="P3" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="P3" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="30"/>
<contactref element="P1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="31"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="32"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="1"/>
<contactref element="P1" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="2"/>
<contactref element="P1" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="9"/>
<contactref element="P1" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="10"/>
<contactref element="P1" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="11"/>
<contactref element="P1" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="23"/>
<contactref element="P2" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="24"/>
<contactref element="P2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="25"/>
<contactref element="P2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="26"/>
<contactref element="P2" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="27"/>
<contactref element="P2" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="28"/>
<contactref element="P2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="12"/>
<contactref element="P3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="IC1" pad="13"/>
<contactref element="P3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="IC1" pad="14"/>
<contactref element="P3" pad="3"/>
</signal>
<signal name="N$27">
<contactref element="P4" pad="2"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="P4" pad="3"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="P4" pad="4"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="N$30">
<contactref element="P4" pad="5"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="N$31">
<contactref element="P4" pad="6"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="N$32">
<contactref element="P4" pad="7"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="N$33">
<contactref element="P4" pad="8"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="VCC">
<contactref element="P2" pad="8"/>
<contactref element="IC1" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
