(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 55)
    (no_connects 1)
    (area 114.579448 73.828 178.513201 122.460182)
    (thickness 1.6)
    (drawings 29)
    (tracks 116)
    (zones 0)
    (modules 24)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 LED_SIG)
  (net 4 "Net-(R4-Pad2)")
  (net 5 RTC_SDA)
  (net 6 RTC_SCL)
  (net 7 PWR_CTRL)
  (net 8 PCELL)
  (net 9 BUTTON/RST)
  (net 10 LED_SIG_OUT)
  (net 11 +5V)
  (net 12 "Net-(U2-Pad1)")
  (net 13 "Net-(U2-Pad3)")
  (net 14 "Net-(U2-Pad4)")
  (net 15 "Net-(R6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net BUTTON/RST)
    (add_net LED_SIG)
    (add_net LED_SIG_OUT)
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net PCELL)
    (add_net RTC_SCL)
    (add_net RTC_SDA)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net PWR_CTRL)
  )
  (module clock-ws2812-schematic-v2:BatteryHolder_3xAAA_Keystone_2479 locked (layer B.Cu) (tedit 58F26176)
    (at 127.8382 107.9246)
    (descr "3xAAA cell battery holder, Keystone P/N 2479")
    (tags "AAA battery cell holder")
    (fp_text reference BT1 (at 3.048 -3.302 270) (layer B.SilkS))
    (fp_text value Battery (at -0.254 -6.35 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask B.SilkS)
      (net 11 +5V))
    (pad 2 thru_hole circle (at 0 -12.7) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58F1D519)
    (at 127.6604 111.6584)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference REF** (at 0.889 -4.191) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380 (at 0 2.75) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58F1D519)
    (at 151.8412 111.4552)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference REF** (at 0.889 -4.191) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380 (at 0 2.75) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58F1D519)
    (at 128.016 78.994)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference REF** (at 0.889 -4.191) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380 (at 0 2.75) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 58F1D79D)
    (at 127.635 97.8408 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 1.3208 -1.5494 270) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 3.556 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 58F2636C)
    (at 127.635 105.5878 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at -0.3048 1.6764 270) (layer F.SilkS))
    (fp_text value 1uF (at 1.143 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 +5V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58F2AC09)
    (at 129.0828 83.6422)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0.762 9.906 90) (layer F.SilkS) hide)
    (fp_text value I2C (at -0.0508 9.5758 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 RTC_SCL))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 RTC_SDA))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 58F1D153)
    (at 136.4488 87.5284 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -0.127 -2.54 90) (layer F.SilkS) hide)
    (fp_text value ICSP (at 1.143 7.239 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 LED_SIG))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 RTC_SCL))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 RTC_SDA))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 BUTTON/RST))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 58F1D808)
    (at 138.938 79.0956 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at -2.032 -2.286 90) (layer F.SilkS) hide)
    (fp_text value WS2812B_OUT (at 2.0828 2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 LED_SIG_OUT))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 58ED7BE2)
    (at 135.128 99.6696 90)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 2.286 -1.016 90) (layer F.SilkS))
    (fp_text value ATTiny85 (at 3.81 8.89 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 BUTTON/RST))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 PCELL))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PWR_CTRL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 RTC_SDA))
    (pad 6 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 LED_SIG))
    (pad 7 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 RTC_SCL))
    (pad 8 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-16W_7.5x10.3mm_Pitch1.27mm (layer B.Cu) (tedit 58F2AC6D)
    (at 138.2014 106.9594)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0.9906 -1.0414 90) (layer B.SilkS))
    (fp_text value DS3231 (at -0.6604 -1.0414 90) (layer B.SilkS))
    (pad 1 smd rect (at -4.65 4.445) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -4.65 3.175) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 PWR_CTRL))
    (pad 3 smd rect (at -4.65 1.905) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -4.65 0.635) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -4.65 -0.635) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.65 -1.905) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -4.65 -3.175) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at -4.65 -4.445) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.65 -4.445) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 4.65 -3.175) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.65 -1.905) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 4.65 -0.635) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 4.65 0.635) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 4.65 1.905) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 15 smd rect (at 4.65 3.175) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 RTC_SDA))
    (pad 16 smd rect (at 4.65 4.445) (size 1.5 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 RTC_SCL))
    (model __Housings_SOIC.3dshapes/SOIC-16W_7.5x10.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812:WS2812-8mm (layer F.Cu) (tedit 58F1D111)
    (at 149.5044 86.0044 180)
    (fp_text reference LED1 (at 0 3.429 180) (layer F.SilkS))
    (fp_text value WS2812 (at 0 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at -1.905 0 180) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 LED_SIG))
    (pad 2 thru_hole oval (at -0.635 0 180) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 PWR_CTRL))
    (pad 3 thru_hole rect (at 0.635 0 180) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 1.905 0 180) (size 1.016 2.032) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 LED_SIG_OUT))
    (model LEDs.3dshapes/LED_D8.0mm.wrl
      (at (xyz -0.05 0 -0.1))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58F27444)
    (at 133.731 112.141)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at -0.9 -2.7) (layer F.SilkS) hide)
    (fp_text value Hour (at -0.127 -2.5654) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R4-Pad2)"))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 58F27931)
    (at 150.368 92.202 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0.127 270) (layer F.SilkS))
    (fp_text value I2C_PUP (at 2.286 -2.0828 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 RTC_SDA))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Opto-Devices:Resistor_LDR_4.9x4.2_RM2.54 (layer F.Cu) (tedit 58F1CADA)
    (at 134.4168 78.8924 180)
    (descr "Resistor, LDR 4.9x4.2mm")
    (tags "Resistor LDR4.9x4.2")
    (fp_text reference R2 (at 1.27 -1.397 180) (layer F.SilkS))
    (fp_text value "PHOTO CELL" (at 1.17 3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PWR_CTRL))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 PCELL))
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 58F2538F)
    (at 132.6896 82.2452 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 3.8608 -0.0508 450) (layer F.SilkS))
    (fp_text value R_ADC (at 0.4826 -2.2352 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 PCELL))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 58F1D9A5)
    (at 152.8572 105.918 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 9.1948 -0.0508 270) (layer F.SilkS))
    (fp_text value 10K (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 BUTTON/RST))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(R4-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 58F24986)
    (at 145.2372 103.8352)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 6.4008 -1.7272) (layer F.SilkS))
    (fp_text value 2K (at 3.727599 0.0516) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 BUTTON/RST))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 58F24983)
    (at 152.8572 107.95 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 3.7592 -1.778 180) (layer F.SilkS))
    (fp_text value 5K (at 3.81 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 BUTTON/RST))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(R6-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 58F23A5D)
    (at 148.336 92.202 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 3.848599 0.0146 270) (layer F.SilkS))
    (fp_text value I2C_PUP (at 0.635 2.1844 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 RTC_SCL))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58F1D854)
    (at 144.018 112.141 180)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW3 (at 1.778 2.667 180) (layer F.SilkS) hide)
    (fp_text value Minute (at 0 2.54 180) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.7 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R6-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58F1D519)
    (at 151.765 79.121)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference REF** (at 0.889 -4.191) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO7380 (at 0 2.75) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Symbols:OSHW-Symbol_6.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 139.3952 103.9876)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Symbol_6.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing_Handsoldering (layer F.Cu) (tedit 58F2ADB2)
    (at 132.7912 105.1814)
    (descr "SOT89-3, Housing, Handsoldering,")
    (tags "SOT89-3, Housing, Handsoldering,")
    (attr smd)
    (fp_text reference U3 (at -2.2352 -3.9624) (layer F.SilkS))
    (fp_text value MCP1700T (at 0.127 10.9982) (layer F.Fab))
    (pad 1 smd rect (at -1.50114 2.35204) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 2.35204) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 11 +5V))
    (pad 3 smd rect (at 1.50114 2.35204) (size 1.00076 2.5019) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0 -1.6002) (size 1.99898 4.0005) (layers F.Cu F.Paste F.Mask)
      (net 11 +5V))
    (pad 2 smd trapezoid (at 0 0.7493 180) (size 1.50114 0.7493) (rect_delta 0 0.50038 ) (layers F.Cu F.Paste F.Mask)
      (net 11 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 5V (at 126.365 108.331 90) (layer F.SilkS))
  (gr_text "LED Minites Repeater Clock\n Rev 0.2" (at 143.383 95.885) (layer B.SilkS))
  (gr_text https://git.io/vS5e4 (at 144.1704 82.2452) (layer B.SilkS))
  (dimension 37.770107 (width 0.3) (layer Eco2.User)
    (gr_text "37.770 mm" (at 161.418799 95.22151 270.2311855) (layer Eco2.User))
    (feature1 (pts (xy 157.5816 114.1222) (xy 162.844988 114.100963)))
    (feature2 (pts (xy 157.4292 76.3524) (xy 162.692588 76.331163)))
    (crossbar (pts (xy 159.99261 76.342057) (xy 160.14501 114.111857)))
    (arrow1a (pts (xy 160.14501 114.111857) (xy 159.554049 112.987729)))
    (arrow1b (pts (xy 160.14501 114.111857) (xy 160.726881 112.982996)))
    (arrow2a (pts (xy 159.99261 76.342057) (xy 159.410739 77.470918)))
    (arrow2b (pts (xy 159.99261 76.342057) (xy 160.583571 77.466185)))
  )
  (dimension 29.362499 (width 0.3) (layer Eco2.User)
    (gr_text "29.362 mm" (at 139.863152 121.072085 0.1486911355) (layer Eco2.User))
    (feature1 (pts (xy 154.5336 116.8908) (xy 154.547856 122.383981)))
    (feature2 (pts (xy 125.1712 116.967) (xy 125.185456 122.460181)))
    (crossbar (pts (xy 125.178449 119.76019) (xy 154.540849 119.68399)))
    (arrow1a (pts (xy 154.540849 119.68399) (xy 153.415871 120.273332)))
    (arrow1b (pts (xy 154.540849 119.68399) (xy 153.412827 119.100495)))
    (arrow2a (pts (xy 125.178449 119.76019) (xy 126.306471 120.343685)))
    (arrow2b (pts (xy 125.178449 119.76019) (xy 126.303427 119.170848)))
  )
  (gr_text "DO G V DI" (at 149.3012 84.328) (layer F.SilkS))
  (gr_text 5V (at 135.4328 106.9594 90) (layer F.SilkS))
  (gr_text GND (at 130.1496 107.7468 90) (layer F.SilkS))
  (gr_text "3V3  SCL   SDA   GND" (at 126.873 87.757 270) (layer F.SilkS))
  (gr_text 3V3 (at 130.81 102.743 90) (layer F.SilkS))
  (gr_line (start 127.6985 114.2365) (end 152.0825 114.2365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 127.6985 76.1365) (end 152.0825 76.1365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "3V3 DATA GND" (at 141.5288 81.28) (layer F.SilkS))
  (gr_text /10min\ (at 137.8204 108.2802) (layer F.SilkS))
  (gr_text "2017-04-17 @ryo1kato" (at 144.7292 89.8652) (layer B.SilkS))
  (gr_line (start 154.6225 111.6965) (end 154.6225 78.6765) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.1585 78.6765) (end 125.1585 111.6965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.6985 111.6965) (end 127.6985 114.2365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.0825 111.6965) (end 154.6225 111.6965) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.0825 78.6765) (end 152.0825 76.1365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 127.6985 78.6765) (end 125.1585 78.6765) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.6225 76.1365) (xy 154.6225 114.2365) (xy 125.1585 114.4905) (xy 125.1585 76.1365)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.1585 114.4905) (xy 125.1585 76.1365) (xy 154.6225 76.1365) (xy 154.6225 114.2365)
      )
    )
  )
)
