(kicad_pcb (version 20171130) (host pcbnew "(5.1.6-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 23)
    (zones 0)
    (modules 15)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.381)
    (trace_clearance 0.0508)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 GNDD)
  (net_class Default "This is the default net class."
    (clearance 0.0508)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net GNDD)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
  )
  (module myGlobal:DoomyDoomer (layer B.Cu) (tedit 0)
    (at 56.007 41.148 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module kicad:DoomyDoomer_Sig (layer F.Cu) (tedit 0)
    (at 55.88 40.386)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module DoomyDoomer_Legacy:svg2mod (layer F.Cu) (tedit 0)
    (at 48.895 40.64)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module DoomyDoomer_Legacy:svg2mod-rev (layer F.Cu) (tedit 0)
    (at 47.752 33.909)
    (fp_text reference svg2mod-rev (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module DoomyDoomer_Legacy:svg2mod (layer F.Cu) (tedit 0)
    (at 49.657 39.751)
    (fp_text reference svg2mod (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value G*** (at 0 3.048) (layer F.SilkS) hide)
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5F374DA6)
    (at 52.07 41.402)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr smd)
    (fp_text reference SW (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value SW (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 63.5 45.974 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.286 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GNDD))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 53.086 45.1335 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GNDD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5F374DB0)
    (at 63.5 41.402)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr smd)
    (fp_text reference SD (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value GPIO15 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 5 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 3 "Net-(D2-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5F374DAC)
    (at 59.69 41.402)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr smd)
    (fp_text reference PO (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value GPIO14 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 4 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 4 "Net-(D3-Pad2)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5F374DA9)
    (at 55.88 41.402)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr smd)
    (fp_text reference EN (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value EN (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 3 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 2 "Net-(D1-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D2.0mm (layer F.Cu) (tedit 5F374D23)
    (at 48.26 41.402)
    (descr "SMD pad as test Point, diameter 2.0mm")
    (tags "test point SMD pad")
    (attr smd)
    (fp_text reference GND (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value GND (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 5 GNDD))
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 56.388 48.006 90)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D3 (at 0 0) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 60.706 51.054 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 50.038 51.054 270)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer F.SilkS))
    (fp_text value 1N4001 (at 0 2.6 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "R1 = 470\nR2 = 1 K\nD1, D2, D3 = 1N4001\nSW = Switch Leg\nEN = Enable on RetroPSU\nPO = GPIO-PowerOff\nSD = Shutdown GPIO" (at 55.88 46.99) (layer B.SilkS))
  (gr_text "OneForAll Power \nSwitch for RetroPSU " (at 55.372 53.34) (layer B.SilkS))
  (gr_line (start 45.72 40.64) (end 45.72 53.34) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.5 55.88) (end 48.26 55.88) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 66.04 40.64) (end 66.04 53.34) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 63.5 53.34) (end 63.5 55.88) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 48.26 53.34) (end 45.72 53.34) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.5 38.1) (end 48.26 38.1) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 63.5 40.64) (end 66.04 40.64) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 48.26 40.64) (end 48.26 38.1) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.04 55.88) (xy 45.72 55.88) (xy 45.72 38.1) (xy 66.04 38.1)
      )
    )
  )
  (zone (net 5) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.04 55.88) (xy 45.72 55.88) (xy 45.72 38.1) (xy 66.04 38.1)
      )
    )
  )
  (zone (net 5) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.04 38.227) (xy 65.913 55.88) (xy 45.72 55.88) (xy 45.72 38.1) (xy 66.04 38.1)
      )
    )
  )
)
