(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Front Panel for Eurorack Mixer1 Module")
    (date "2022-11-15")
    (rev "1.0")
    (company "Len Popp")
    (comment 1 "Copyright © 2022 Len Popp CC BY")
    (comment 2 "4 HP - Holes match Delptronics panels")
    (comment 3 "NOTE: Holes only. No pads or tracks.")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../gerbers/panel/")
    )
  )
  (net 0 "")
  (footprint "-lmp-holes:MountingHole_Pot_Alpha" locked (layer "F.Cu")
    (tedit 61FF3611)
    (at 150 45.36)
    (descr "Mounting Hole for Alpha RD901F potentiometer")
    (tags "mounting hole Alpha RD901F potentiometer")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pot_Alpha" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole oval locked (at 0 6) (size 3.1 1) (drill oval 3.1 1) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 0 0) (size 7.3 7.3) (drill 7.3) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Panel_3.2mm_M3" locked (layer "F.Cu")
    (tedit 61A52F5F)
    (at 147.5 33)
    (descr "Mounting Hole 3.2mm, no annular, no clearance, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Panel_3.2mm_M3" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Panel_3.2mm_M3" locked (layer "F.Cu")
    (tedit 61A52F5F)
    (at 147.5 155.5)
    (descr "Mounting Hole 3.2mm, no annular, no clearance, M3")
    (tags "mounting hole 3.2mm m3")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Panel_3.2mm_M3" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Pot_Alpha" (layer "F.Cu")
    (tedit 61FF3611)
    (at 150 102.51)
    (descr "Mounting Hole for Alpha RD901F potentiometer")
    (tags "mounting hole Alpha RD901F potentiometer")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pot_Alpha" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 6) (size 3.1 1) (drill oval 3.1 1) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 7.3 7.3) (drill 7.3) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_LED_5mm" locked (layer "F.Cu")
    (tedit 61F1FF03)
    (at 150 116.9)
    (descr "Mounting Hole for LED, 5mm, no bushing")
    (tags "mounting hole led 5mm")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_LED_5mm" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 5.1 5.1) (drill 5.1) (layers F&B.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Jack_3.5mm_PJ398" locked (layer "F.Cu")
    (tedit 61A536EF)
    (at 144.9 128)
    (descr "Mounting Hole for PJ398 3.5mm Jack")
    (tags "mounting hole jack 3.5mm pj398")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Jack_3.5mm_PJ398" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 6.3 6.3) (drill 6.3) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Jack_3.5mm_PJ398" locked (layer "F.Cu")
    (tedit 61A536EF)
    (at 155.1 128)
    (descr "Mounting Hole for PJ398 3.5mm Jack")
    (tags "mounting hole jack 3.5mm pj398")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Jack_3.5mm_PJ398" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 6.3 6.3) (drill 6.3) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Jack_3.5mm_PJ398" (layer "F.Cu")
    (tedit 61A536EF)
    (at 155.1 142)
    (descr "Mounting Hole for PJ398 3.5mm Jack")
    (tags "mounting hole jack 3.5mm pj398")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Jack_3.5mm_PJ398" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 6.3 6.3) (drill 6.3) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Pot_Alpha" (layer "F.Cu")
    (tedit 61FF3611)
    (at 150 83.46)
    (descr "Mounting Hole for Alpha RD901F potentiometer")
    (tags "mounting hole Alpha RD901F potentiometer")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pot_Alpha" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 7.3 7.3) (drill 7.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 0 6) (size 3.1 1) (drill oval 3.1 1) (layers F&B.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Jack_3.5mm_PJ398" (layer "F.Cu")
    (tedit 61A536EF)
    (at 144.9 142)
    (descr "Mounting Hole for PJ398 3.5mm Jack")
    (tags "mounting hole jack 3.5mm pj398")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Jack_3.5mm_PJ398" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 6.3 6.3) (drill 6.3) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-holes:MountingHole_Pot_Alpha" (layer "F.Cu")
    (tedit 61FF3611)
    (at 150 64.41)
    (descr "Mounting Hole for Alpha RD901F potentiometer")
    (tags "mounting hole Alpha RD901F potentiometer")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_Pot_Alpha" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 6) (size 3.1 1) (drill oval 3.1 1) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0) (size 7.3 7.3) (drill 7.3) (layers *.Cu *.Mask))
  )
  (gr_line (start 160 158.5) (end 140 158.5) (layer "Edge.Cuts") (width 0.3556))
  (gr_line (start 140 158.5) (end 140 30) (layer "Edge.Cuts") (width 0.3556))
  (gr_line (start 160 30) (end 160 158.5) (layer "Edge.Cuts") (width 0.3556))
  (gr_line (start 140 30) (end 160 30) (layer "Edge.Cuts") (width 0.3556))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.1 158.6)
        (xy 139.9 158.6)
        (xy 139.9 29.9)
        (xy 160.1 29.9)
      )
    )
  )
)
