(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 64)
    (zones 0)
    (modules 8)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad6)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J2-Pad1)")
  (net 9 "Net-(J2-Pad4)")
  (net 10 "Net-(J2-Pad6)")
  (net 11 "Net-(J2-Pad8)")
  (net 12 "Net-(J2-Pad10)")
  (net 13 "Net-(J2-Pad13)")
  (net 14 "Net-(J2-Pad3)")
  (net 15 "Net-(J1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
  )
  (module myfootprints:MicroD-25-M-upsidedown (layer F.Cu) (tedit 5F4D698C)
    (at 150.0378 68.1736 90)
    (fp_text reference J1 (at -2.1844 14.9098) (layer F.SilkS))
    (fp_text value MicroD-25-M (at -3.81 3.8354) (layer F.Fab))
    (pad 26 thru_hole circle (at 2.54 -8.445 90) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 2.54 16.065 90) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 1.27 -3.17 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 15 thru_hole circle (at 1.27 -1.9 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 16 thru_hole circle (at 1.27 -0.63 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 17 thru_hole circle (at 1.27 0.64 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 18 thru_hole circle (at 1.27 1.91 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 19 thru_hole circle (at 1.27 3.18 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 20 thru_hole circle (at 1.27 4.45 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 21 thru_hole circle (at 1.27 5.72 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 22 thru_hole circle (at 1.27 6.99 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 23 thru_hole circle (at 1.27 8.26 90) (size 1.016 1.016) (drill 0.7112) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 24 thru_hole circle (at 1.27 9.53 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 25 thru_hole circle (at 1.27 10.8 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 1 thru_hole circle (at -1.27 -3.81 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -2.54 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 3 thru_hole circle (at -1.27 -1.27 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 1.27 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad4)"))
    (pad 6 thru_hole circle (at -1.27 2.54 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 3.81 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad6)"))
    (pad 8 thru_hole circle (at -1.27 5.08 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -1.27 6.35 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 thru_hole circle (at -1.27 7.62 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -1.27 8.89 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad10)"))
    (pad 12 thru_hole circle (at -1.27 10.16 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole circle (at -1.27 11.43 90) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad13)"))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/MicroD_381-025-112L565.STEP
      (offset (xyz 7.8486 -3.81 -5.181599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 90))
    )
  )
  (module myfootprints:MicroD-25-M-upsidedown (layer F.Cu) (tedit 5F4D698C)
    (at 157.6456 92.71 270)
    (fp_text reference J2 (at -1.2192 15.7866) (layer F.SilkS))
    (fp_text value MicroD-25-M (at -3.81 3.8354) (layer F.Fab))
    (pad 26 thru_hole circle (at 2.54 -8.445 270) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 0 thru_hole circle (at 2.54 16.065 270) (size 2.79 2.79) (drill 2.79) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 1.27 -3.17 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 15 thru_hole circle (at 1.27 -1.9 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 16 thru_hole circle (at 1.27 -0.63 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 17 thru_hole circle (at 1.27 0.64 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 18 thru_hole circle (at 1.27 1.91 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 19 thru_hole circle (at 1.27 3.18 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 20 thru_hole circle (at 1.27 4.45 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 21 thru_hole circle (at 1.27 5.72 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 22 thru_hole circle (at 1.27 6.99 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 23 thru_hole circle (at 1.27 8.26 270) (size 1.016 1.016) (drill 0.7112) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 24 thru_hole circle (at 1.27 9.53 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 25 thru_hole circle (at 1.27 10.8 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.254))
    (pad 1 thru_hole circle (at -1.27 -3.81 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -1.27 -2.54 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J2-Pad1)"))
    (pad 3 thru_hole circle (at -1.27 -1.27 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 0 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 1.27 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J2-Pad4)"))
    (pad 6 thru_hole circle (at -1.27 2.54 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 3.81 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J2-Pad6)"))
    (pad 8 thru_hole circle (at -1.27 5.08 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at -1.27 6.35 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J2-Pad8)"))
    (pad 10 thru_hole circle (at -1.27 7.62 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at -1.27 8.89 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J2-Pad10)"))
    (pad 12 thru_hole circle (at -1.27 10.16 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole circle (at -1.27 11.43 270) (size 1.016 1.016) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J2-Pad13)"))
    (model /Users/smb2/Documents/PCB/Kicad/Footprints.pretty/3D/MicroD_381-025-112L565.STEP
      (offset (xyz 7.8486 -3.81 -5.181599999999999))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 153.8478 86.8348 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.0254 2.7862) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad6)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 148.9124 86.868 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.043 2.8194) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad10)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.8008 73.8632)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.2032 2.6162) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 153.3828 73.914)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -0.1446 2.5654) (layer F.SilkS))
    (fp_text value R (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 147.1676 73.8124)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q1 (at -0.762 2.9464) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad3)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:SOT65P210X110-3N (layer F.Cu) (tedit 5E7BCFFD)
    (at 159.115 87.4014 180)
    (descr DMN62D0UW-7-1)
    (tags "MOSFET (N-Channel)")
    (attr smd)
    (fp_text reference Q2 (at -0.397 3.2512) (layer F.SilkS))
    (fp_text value DMN62D0UW-7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at -1 0.65 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad1)"))
    (pad 1 smd rect (at -1 -0.65 270) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad3)"))
    (model DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${DMN}/DMN62D0UW-7.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Sonia Buckley 20200908" (at 171.7802 80.6704 90) (layer F.SilkS))
  (gr_text Trout04 (at 135.8646 80.3148 90) (layer F.SilkS))
  (gr_line (start 133.604 60.0964) (end 133.604 100.711) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.1932 60.0964) (end 133.604 60.0964) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.1932 100.711) (end 174.1932 60.0964) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133.604 100.711) (end 174.1932 100.711) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 176.8348 103.8352) (xy 131.318 104.4956) (xy 131.2418 58.9788) (xy 131.2672 59.0042) (xy 176.7332 58.9026)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 176.0728 102.7938) (xy 131.5466 102.9208) (xy 131.6228 59.4868) (xy 176.0728 59.4868)
      )
    )
  )
)
