(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 48)
    (no_connects 10)
    (area 168.072999 62.916999 198.195001 85.419001)
    (thickness 1.6)
    (drawings 36)
    (tracks 169)
    (zones 0)
    (modules 22)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.125)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.4)
    (user_via 0.6 0.5)
    (user_via 0.7 0.6)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.9 0.8)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12L)
  (net 2 GND)
  (net 3 +5P)
  (net 4 "Net-(C2-Pad2)")
  (net 5 +12P)
  (net 6 "Net-(R1-Pad1)")
  (net 7 +3V3)
  (net 8 "Net-(R2-Pad1)")
  (net 9 /TI)
  (net 10 "Net-(R4-Pad2)")
  (net 11 /CANH)
  (net 12 /RTHI)
  (net 13 /CANL)
  (net 14 /RTLI)
  (net 15 /EI)
  (net 16 /RI)
  (net 17 /5)
  (net 18 /8)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12L)
    (add_net +12P)
    (add_net +3V3)
    (add_net +5P)
    (add_net /5)
    (add_net /8)
    (add_net /CANH)
    (add_net /CANL)
    (add_net /EI)
    (add_net /RI)
    (add_net /RTHI)
    (add_net /RTLI)
    (add_net /TI)
    (add_net GND)
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad2)")
  )
  (net_class 50 ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Power ""
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.7)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA863)
    (at 170.942 73.914 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C1 (at 0.254 2.54 270) (layer F.SilkS))
    (fp_text value 10n (at -2.286 -1.778 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5P))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA853)
    (at 178.816 74.93)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.508 12.192) (layer F.SilkS))
    (fp_text value 10n (at 0 1.524) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA83B)
    (at 187.96 64.516 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.54 0.254 90) (layer F.SilkS))
    (fp_text value 10n (at 0.762 -2.286 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +12L))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 581DA843)
    (at 186.055 67.056)
    (attr smd)
    (fp_text reference C4 (at 0.127 5.08) (layer F.SilkS))
    (fp_text value 20u (at -0.635 -2.032) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +12L))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 581DA847)
    (at 184.277 69.85 180)
    (attr smd)
    (fp_text reference C5 (at -2.921 -3.81 180) (layer F.SilkS))
    (fp_text value 20u (at 2.159 -3.302 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 +5P))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA83F)
    (at 187.96 69.596 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference C6 (at 6.096 -2.794 270) (layer F.SilkS))
    (fp_text value 10n (at 1.016 -2.032 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5P))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 174.752 64.516 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 3k (at 5.842 -0.254 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA86C)
    (at 172.974 64.516 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.794 0 90) (layer F.SilkS))
    (fp_text value 3k (at 0.508 -2.032 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA837)
    (at 181.61 65.786 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 3.81 0.254 90) (layer F.SilkS))
    (fp_text value 10k (at 2.032 0.254 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA84C)
    (at 181.102 75.438 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0.762 4.064 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +12L))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA858)
    (at 175.006 75.184 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.032 -10.414 180) (layer F.SilkS))
    (fp_text value >500 (at 3.302 -1.27 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /CANH))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /RTHI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 581DA85C)
    (at 175.768 76.962 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -8.636 180) (layer F.SilkS))
    (fp_text value >500 (at 3.302 -1.27 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /CANL))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /RTLI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 176.53 64.516 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3.302 0 90) (layer F.SilkS))
    (fp_text value 3k (at 6.096 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 /EI))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 178.308 64.516 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 3.302 0 90) (layer F.SilkS))
    (fp_text value 3k (at 6.35 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /RI))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 581DA868)
    (at 176.276 70.104 180)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 3.81 1.524 180) (layer F.SilkS))
    (fp_text value TJA1055/3 (at -0.254 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 /TI))
    (pad 3 smd rect (at -1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 /RI))
    (pad 4 smd rect (at 0 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 15 /EI))
    (pad 5 smd rect (at 1.27 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R1-Pad1)"))
    (pad 6 smd rect (at 2.54 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R2-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 8 smd rect (at 3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 /RTHI))
    (pad 9 smd rect (at 2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 /RTLI))
    (pad 11 smd rect (at 0 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 /CANH))
    (pad 12 smd rect (at -1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 /CANL))
    (pad 13 smd rect (at -2.54 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -3.81 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 10 smd rect (at 1.27 -3.048 180) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +5P))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 552FF239)
    (at 181.864 80.772 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value D (at 5.334 0.508 270) (layer F.Fab))
    (fp_text user K (at 6.35 0.508 270) (layer F.SilkS))
    (fp_text user A (at 2.9 2.9 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +12L))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 +12P))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 0)
    (at 193.548 67.056 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0 -0.762 360) (layer F.SilkS))
    (fp_text value V_REG_MIC2920 (at 5.334 -1.524 360) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 270) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.286 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 +5P))
    (pad 1 smd rect (at -2.286 3.302 270) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +12L))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_SMD_5x10mm (layer F.Cu) (tedit 581DA850)
    (at 185.166 81.026)
    (descr "Wire Pad, Square, SMD Pad,  5mm x 10mm,")
    (tags "MesurementPoint Square SMDPad 5mmx10mm ")
    (attr smd)
    (fp_text reference W1 (at 3.556 -2.032) (layer F.SilkS))
    (fp_text value 12V (at -0.254 3.048) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2 3) (layers F.Cu F.Paste F.Mask)
      (net 5 +12P))
  )
  (module usb:so8_4pins (layer F.Cu) (tedit 581D0FD1)
    (at 175.98644 81.253 90)
    (descr Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A)
    (tags Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A)
    (fp_text reference JP2 (at -4.853 2.06756 180) (layer F.SilkS))
    (fp_text value 4-PIN (at 0.227 2.57556 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0.735 0.03556 180) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 11 /CANH))
    (pad 1 thru_hole oval (at -2.105 0.03556 180) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 17 /5))
    (pad 4 thru_hole oval (at 2.105 0.03556 180) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 18 /8))
    (pad 2 thru_hole oval (at -0.735 0.03556 180) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 13 /CANL))
    (model TO_SOT_Packages_THT.3dshapes/Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb:so8_4pins (layer F.Cu) (tedit 581D0FD1)
    (at 169.45356 81.253 270)
    (descr Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A)
    (tags Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A)
    (fp_text reference JP1 (at 1.551 2.32156 270) (layer F.SilkS))
    (fp_text value 4-PIN (at -2.767 2.32156 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 0.735 0.03556) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 +3V3))
    (pad 1 thru_hole oval (at -2.105 0.03556) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 /TI))
    (pad 4 thru_hole oval (at 2.105 0.03556) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 16 /RI))
    (pad 2 thru_hole oval (at -0.735 0.03556) (size 1.5 0.8) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model TO_SOT_Packages_THT.3dshapes/Pentawatt_Neutral_Straight_Vertical_TO220-5-T05A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 552FF239)
    (at 193.548 67.08902 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 -3.81 270) (layer F.SilkS))
    (fp_text value D (at -5.11302 -0.254 270) (layer F.Fab))
    (fp_text user K (at -2.9 2.95 270) (layer F.SilkS))
    (fp_text user A (at 2.76098 -6.604 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +12L))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +5P))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 0)
    (at 183.134 95.419001)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value MCP2551-I/SN (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 /8))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 /CANH))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 /CANL))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 17 /5))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 /RI))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 +3V3))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 /TI))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text *4 (at 171.196 65.278) (layer F.SilkS))
  (gr_line (start 186.69 85.09) (end 186.436 85.344) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 71.12) (end 198.12 63.246) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.866 62.992) (end 183.642 62.992) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 75.946) (end 183.642 75.946) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.418 63.246) (end 169.418 77.724) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.418 78.232) (end 169.418 77.47) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.148 78.232) (end 169.418 78.232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.148 84.328) (end 168.148 78.232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.292 84.328) (end 168.148 84.328) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.292 78.232) (end 177.292 84.328) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 78.232) (end 177.292 78.232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 85.344) (end 179.578 78.232) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.642 71.374) (end 183.642 75.946) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 63.246) (end 197.866 62.992) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 71.12) (end 197.866 71.374) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.642 71.374) (end 197.866 71.374) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.436 75.946) (end 186.69 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.69 85.09) (end 186.69 76.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 85.344) (end 186.436 85.344) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.418 63.246) (end 169.672 62.992) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.642 62.992) (end 169.672 62.992) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 169.672 62.992) (xy 198.12 62.992) (xy 198.12 71.374) (xy 183.642 71.374) (xy 183.642 75.946)
        (xy 186.69 75.946) (xy 186.69 85.344) (xy 179.578 85.344) (xy 179.578 78.232) (xy 176.022 78.232)
        (xy 176.022 84.328) (xy 169.418 84.328) (xy 169.418 78.232) (xy 169.418 70.612) (xy 169.418 63.246)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 183.642 71.374) (xy 198.12 71.374) (xy 198.12 62.992) (xy 169.672 62.992) (xy 169.418 63.246)
        (xy 169.418 84.328) (xy 176.022 84.328) (xy 176.022 78.232) (xy 179.578 78.232) (xy 179.578 85.344)
        (xy 186.69 85.344) (xy 186.69 85.344) (xy 186.69 75.946) (xy 186.69 75.946) (xy 183.642 75.946)
      )
    )
  )
)
