(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 2770)
    (zones 0)
    (modules 63)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.44)
    (user_trace_width 0.38)
    (user_trace_width 0.44)
    (user_trace_width 2.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.8)
    (uvia_drill 0.4)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.44 0.44)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 154.05 179.45)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 "Net-(D5-Pad2)")
  (net 7 "Net-(D6-Pad2)")
  (net 8 "Net-(F1-Pad2)")
  (net 9 Pout)
  (net 10 "Net-(F2-Pad2)")
  (net 11 "Net-(F3-Pad2)")
  (net 12 "Net-(F4-Pad2)")
  (net 13 "Net-(F5-Pad2)")
  (net 14 "Net-(F6-Pad2)")
  (net 15 L-6_Enet_Rx+)
  (net 16 L-6_Enet_Tx+)
  (net 17 L-6_Enet_Rx-)
  (net 18 L-6_Enet_Tx-)
  (net 19 GPS_Pulse)
  (net 20 L-1_Enet_Tx+)
  (net 21 L-1_Enet_Tx-)
  (net 22 L-1_Enet_Rx-)
  (net 23 L-1_Enet_Rx+)
  (net 24 L-2_Enet_Tx+)
  (net 25 L-2_Enet_Tx-)
  (net 26 L-2_Enet_Rx-)
  (net 27 L-2_Enet_Rx+)
  (net 28 L-3_Enet_Tx+)
  (net 29 L-3_Enet_Tx-)
  (net 30 L-3_Enet_Rx-)
  (net 31 L-3_Enet_Rx+)
  (net 32 L-4_Enet_Tx+)
  (net 33 L-4_Enet_Tx-)
  (net 34 L-4_Enet_Rx-)
  (net 35 L-4_Enet_Rx+)
  (net 36 L-5_Enet_Tx+)
  (net 37 L-5_Enet_Tx-)
  (net 38 L-5_Enet_Rx-)
  (net 39 L-5_Enet_Rx+)
  (net 40 "Net-(J7-Pad2)")
  (net 41 "Net-(R1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.8)
    (uvia_drill 0.4)
    (add_net GND)
    (add_net GPS_Pulse)
    (add_net L-1_Enet_Rx+)
    (add_net L-1_Enet_Rx-)
    (add_net L-1_Enet_Tx+)
    (add_net L-1_Enet_Tx-)
    (add_net L-2_Enet_Rx+)
    (add_net L-2_Enet_Rx-)
    (add_net L-2_Enet_Tx+)
    (add_net L-2_Enet_Tx-)
    (add_net L-3_Enet_Rx+)
    (add_net L-3_Enet_Rx-)
    (add_net L-3_Enet_Tx+)
    (add_net L-3_Enet_Tx-)
    (add_net L-4_Enet_Rx+)
    (add_net L-4_Enet_Rx-)
    (add_net L-4_Enet_Tx+)
    (add_net L-4_Enet_Tx-)
    (add_net L-5_Enet_Rx+)
    (add_net L-5_Enet_Rx-)
    (add_net L-5_Enet_Tx+)
    (add_net L-5_Enet_Tx-)
    (add_net L-6_Enet_Rx+)
    (add_net L-6_Enet_Rx-)
    (add_net L-6_Enet_Tx+)
    (add_net L-6_Enet_Tx-)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad2)")
    (add_net "Net-(F3-Pad2)")
    (add_net "Net-(F4-Pad2)")
    (add_net "Net-(F5-Pad2)")
    (add_net "Net-(F6-Pad2)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net Pout)
  )
  (module Connector:MD-80SM (layer F.Cu) (tedit 5DB8C23B)
    (at 86.03996 114.654584 90)
    (fp_text reference J5 (at 0.6858 -0.6604 90) (layer F.SilkS))
    (fp_text value MD-80SM (at 0 0.9906 90) (layer F.Fab))
    (fp_text user "ENET TX-" (at 1.05 12.175 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at -1.075 12.125 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at -3.425 12.15 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at 3.625 12.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 1.275 7.425 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -3.302 7.5184 90) (layer F.SilkS))
    (fp_text user 12V (at 3.425 7.325 90) (layer F.SilkS))
    (fp_text user GND (at -1.2192 7.493 90) (layer F.SilkS))
    (fp_text user Shield (at 6.5532 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at 0.0254 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at -6.2484 3.7084 90) (layer F.SilkS))
    (pad 11 thru_hole rect (at 6.7437 5.5118) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole rect (at -6.7437 5.5118 180) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole rect (at 0 4.699 90) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 32 L-4_Enet_Tx+))
    (pad 7 thru_hole circle (at 0.889 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 33 L-4_Enet_Tx-))
    (pad 6 thru_hole circle (at -3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 34 L-4_Enet_Rx-))
    (pad 5 thru_hole circle (at 3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 12 "Net-(F4-Pad2)"))
    (pad 4 thru_hole circle (at -1.2954 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 35 L-4_Enet_Rx+))
    (pad 3 thru_hole circle (at -3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 19 GPS_Pulse))
    (pad 2 thru_hole circle (at 1.27 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.2954 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector:T3507900U (layer F.Cu) (tedit 5DB3C253)
    (at 73.64476 159.98952 270)
    (fp_text reference J1 (at 0.6858 0.9144 90) (layer F.SilkS))
    (fp_text value T3507900U (at 1.143 -0.7874 90) (layer F.Fab))
    (fp_text user SHIELD (at -7.493 -8.1534 90) (layer F.SilkS))
    (fp_text user SHIELD (at 7.6708 -8.255 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at 7.675 -16.15 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at 0.05 -18.625 90) (layer F.SilkS))
    (fp_text user "ENET TX-" (at -2.5 -16.2 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at -7.4 -16.25 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 2.5908 -16.2814 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -4.9276 -13.7414 90) (layer F.SilkS))
    (fp_text user 12V+ (at 0.0254 -13.6652 90) (layer F.SilkS))
    (fp_text user GND (at 5.08 -13.6906 90) (layer F.SilkS))
    (pad GND thru_hole circle (at -7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad GND thru_hole circle (at 7.5057 -10.1092 270) (size 3.2766 3.2766) (drill 2.5146) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 0 -20.0914 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 15 L-6_Enet_Rx+))
    (pad 7 thru_hole circle (at -7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 16 L-6_Enet_Tx+))
    (pad 6 thru_hole circle (at 7.5057 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 17 L-6_Enet_Rx-))
    (pad 5 thru_hole circle (at -2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 18 L-6_Enet_Tx-))
    (pad 4 thru_hole circle (at 2.5019 -17.6022 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 19 GPS_Pulse))
    (pad 2 thru_hole circle (at 0 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 14 "Net-(F6-Pad2)"))
    (pad 1 thru_hole circle (at 4.9911 -15.113 270) (size 2.1844 2.1844) (drill 1.4224) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 144.65 180.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 82 179.95)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 92.7 21.15)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 144.65 21.1)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD909E)
    (at 94.5 146.9)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "GPS PULSE" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 19 GPS_Pulse))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FD7)
    (at 127 146 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L5 Rx-" (at -0.15748 1.56972) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 38 L-5_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FCB)
    (at 125.2 141.8)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L5 Rx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 39 L-5_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FE6)
    (at 126.2 136.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L5 Tx-" (at 0.09652 1.37668) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 37 L-5_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FF2)
    (at 128.4 137.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L5 Tx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 36 L-5_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FC2)
    (at 121.6 124.8)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L4 Rx-" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 34 L-4_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FB1)
    (at 119.2 120.8)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L4 Rx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 35 L-4_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9023)
    (at 126.15 114.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L4 Tx-" (at -0.03556 1.56464) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 33 L-4_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9028)
    (at 128.3 115.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L4 Tx+" (at 0.03556 -1.5494) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 32 L-4_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9031)
    (at 120.1 100.65)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L3 Rx-" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 30 L-3_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9039)
    (at 118.3 97.85)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L3 Rx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 31 L-3_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9041)
    (at 128.5 95)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L3 Tx-" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 29 L-3_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9046)
    (at 127.25 92.6)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L3 Tx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 28 L-3_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9058)
    (at 118.95 78.2 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L2 Rx-" (at -0.05 -1.9) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 26 L-2_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD905F)
    (at 117.8 75.8)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L2 Rx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 27 L-2_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9065)
    (at 128.3 73.8)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L2 TX-" (at 0.04572 1.56464) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 25 L-2_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD906C)
    (at 126.55 72)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L2 Tx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 24 L-2_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9082)
    (at 122.05 61.45)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L1 Rx-" (at 0.00508 1.57988) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 22 L-1_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9078)
    (at 119.60104 57.9)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L1 Rx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 23 L-1_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9088)
    (at 125.85 52.3)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L1 Tx-" (at -0.26416 1.46304) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 21 L-1_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9090)
    (at 127.95 53.35)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L1 Tx+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 20 L-1_Enet_Tx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9012)
    (at 127.5 169.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L6 Rx-" (at -2.47904 -0.3302) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 17 L-6_Enet_Rx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD900B)
    (at 125.66396 168.35628)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L6 Rx+" (at -2.35712 -0.32512) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 15 L-6_Enet_Rx+))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD9007)
    (at 124.02312 165.51656)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L6 Tx-" (at -0.16764 1.41732) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 18 L-6_Enet_Tx-))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5DBD8FFC)
    (at 121.83872 164.80028)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference "L6 TX+" (at 0 -1.448) (layer F.SilkS))
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 0.44 0.44) (layers F.Cu F.Mask)
      (net 16 L-6_Enet_Tx+))
  )
  (module Diode_SMD:MMSZ5242B-TP (layer F.Cu) (tedit 5DAFB067)
    (at 119.22656 38.42664 90)
    (fp_text reference U2 (at 1.625 1.05 90) (layer F.SilkS))
    (fp_text value MMSZ5242B-TP (at 1.55 -1.075 90) (layer F.Fab))
    (fp_text user Cathode (at 2.6 0.025) (layer F.SilkS))
    (fp_text user Anode (at 0.7 0.025) (layer F.SilkS))
    (pad 2 smd rect (at 3.2766 0 180) (size 1.2192 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at 0 0 180) (size 1.2192 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 9 Pout))
  )
  (module Package_TO_SOT_THT:FQP47P06 (layer F.Cu) (tedit 5DB39E0F)
    (at 123.3312 36.2778 270)
    (fp_text reference U1 (at 0 -3.15 90) (layer F.SilkS))
    (fp_text value FQP47P06 (at 0 1.725 90) (layer F.Fab))
    (fp_text user Drain (at 0 -1.55 90) (layer F.SilkS))
    (fp_text user Source (at 2.675 -1.55 90) (layer F.SilkS))
    (fp_text user Gate (at -2.7 -1.575 90) (layer F.SilkS))
    (pad 3 thru_hole rect (at 2.67 0) (size 2 2.125) (drill 1.62) (layers *.Cu *.Mask)
      (net 9 Pout))
    (pad 2 thru_hole rect (at 0 0 270) (size 2.125 2.125) (drill 1.62) (layers *.Cu *.Mask)
      (net 40 "Net-(J7-Pad2)"))
    (pad 1 thru_hole rect (at -2.67 0 270) (size 2.125 2.125) (drill 1.62) (layers *.Cu *.Mask)
      (net 41 "Net-(R1-Pad2)"))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 104.65816 147.27936 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(F6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 104.65816 128.54432 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(F5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 104.45 106.49 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(F4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 104.65816 84.836 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(F3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 104.65816 65.8622 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(F2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 104.65816 44.03344 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.27 -2.37 90) (layer F.SilkS))
    (fp_text value 560 (at 1.27 2.37 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 125.85088 29.27756 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 120K (at 1.27 2.37) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 170.6104 90)
    (fp_text reference J13 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 16 L-6_Enet_Tx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 18 L-6_Enet_Tx-))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 15 L-6_Enet_Rx+))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 17 L-6_Enet_Rx-))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 149.308944 90)
    (fp_text reference J12 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 36 L-5_Enet_Tx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 37 L-5_Enet_Tx-))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 39 L-5_Enet_Rx+))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 38 L-5_Enet_Rx-))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 128.007488 90)
    (fp_text reference J11 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 32 L-4_Enet_Tx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 33 L-4_Enet_Tx-))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 35 L-4_Enet_Rx+))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 34 L-4_Enet_Rx-))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 106.706032 90)
    (fp_text reference J10 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 28 L-3_Enet_Tx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 29 L-3_Enet_Tx-))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 31 L-3_Enet_Rx+))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 30 L-3_Enet_Rx-))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 85.404576 90)
    (fp_text reference J9 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 24 L-2_Enet_Tx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 25 L-2_Enet_Tx-))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 27 L-2_Enet_Rx+))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 26 L-2_Enet_Rx-))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector_RJ:SS-60300-004_1 (layer F.Cu) (tedit 5DB3A5DE)
    (at 133.55444 64.10312 90)
    (fp_text reference J8 (at 6.2 2.6 90) (layer F.SilkS))
    (fp_text value RJ45_Shielded (at 5.8 -5.4 90) (layer F.Fab))
    (fp_text user "Enet- TX+" (at 8.575 -0.225 90) (layer F.SilkS))
    (fp_text user "Enet- TX-" (at 10.225 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX+" (at 7.875 -3.75 90) (layer F.SilkS))
    (fp_text user "Enet- RX-" (at 4.625 -0.3 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 8.509 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 20 L-1_Enet_Tx+))
    (pad 2 thru_hole circle (at 9.525 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 21 L-1_Enet_Tx-))
    (pad 3 thru_hole circle (at 7.493 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 23 L-1_Enet_Rx+))
    (pad 4 thru_hole circle (at 5.461 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 6.477 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.445 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 22 L-1_Enet_Rx-))
    (pad 7 thru_hole circle (at 2.413 -1.27 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 3.429 -2.794 90) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 0 90) (size 3.429 3.429) (drill 3.2512) (layers *.Cu *.Mask))
    (pad SH thru_hole circle (at -1.905 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad SH thru_hole circle (at 13.843 3.175 90) (size 2.4384 2.4384) (drill 1.6764) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector:0768250002 (layer F.Cu) (tedit 5DB3ADC9)
    (at 133.87728 30.49168)
    (fp_text reference J7 (at 0 16.35) (layer F.SilkS))
    (fp_text value 76825-0002 (at 0 -4.95) (layer F.Fab))
    (fp_text user +12V (at -0.1 10.425) (layer F.SilkS))
    (fp_text user GND (at 0.025 4.85) (layer F.SilkS))
    (fp_text user foot (at 0 3.55) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 12.8) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 40 "Net-(J7-Pad2)"))
    (pad 3 thru_hole circle (at 0 7.3) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 0 0) (size 6.2 6.2) (drill 3.1) (layers *.Cu *.Mask))
  )
  (module Connector:MD-80SM (layer F.Cu) (tedit 5DB8C23B)
    (at 86.03996 136.013952 90)
    (fp_text reference J6 (at 0.6858 -0.6604 90) (layer F.SilkS))
    (fp_text value MD-80SM (at 0 0.9906 90) (layer F.Fab))
    (fp_text user "ENET TX-" (at 1.05 12.175 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at -1.075 12.125 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at -3.425 12.15 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at 3.625 12.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 1.275 7.425 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -3.302 7.5184 90) (layer F.SilkS))
    (fp_text user 12V (at 3.425 7.325 90) (layer F.SilkS))
    (fp_text user GND (at -1.2192 7.493 90) (layer F.SilkS))
    (fp_text user Shield (at 6.5532 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at 0.0254 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at -6.2484 3.7084 90) (layer F.SilkS))
    (pad 11 thru_hole rect (at 6.7437 5.5118) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole rect (at -6.7437 5.5118 180) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole rect (at 0 4.699 90) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 36 L-5_Enet_Tx+))
    (pad 7 thru_hole circle (at 0.889 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 37 L-5_Enet_Tx-))
    (pad 6 thru_hole circle (at -3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 38 L-5_Enet_Rx-))
    (pad 5 thru_hole circle (at 3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 13 "Net-(F5-Pad2)"))
    (pad 4 thru_hole circle (at -1.2954 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 39 L-5_Enet_Rx+))
    (pad 3 thru_hole circle (at -3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 19 GPS_Pulse))
    (pad 2 thru_hole circle (at 1.27 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.2954 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector:MD-80SM (layer F.Cu) (tedit 5DB8C23B)
    (at 86.03996 93.295216 90)
    (fp_text reference J4 (at 0.6858 -0.6604 90) (layer F.SilkS))
    (fp_text value MD-80SM (at 0 0.9906 90) (layer F.Fab))
    (fp_text user "ENET TX-" (at 1.05 12.175 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at -1.075 12.125 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at -3.425 12.15 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at 3.625 12.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 1.275 7.425 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -3.302 7.5184 90) (layer F.SilkS))
    (fp_text user 12V (at 3.425 7.325 90) (layer F.SilkS))
    (fp_text user GND (at -1.2192 7.493 90) (layer F.SilkS))
    (fp_text user Shield (at 6.5532 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at 0.0254 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at -6.2484 3.7084 90) (layer F.SilkS))
    (pad 11 thru_hole rect (at 6.7437 5.5118) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole rect (at -6.7437 5.5118 180) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole rect (at 0 4.699 90) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 28 L-3_Enet_Tx+))
    (pad 7 thru_hole circle (at 0.889 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 29 L-3_Enet_Tx-))
    (pad 6 thru_hole circle (at -3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 30 L-3_Enet_Rx-))
    (pad 5 thru_hole circle (at 3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 11 "Net-(F3-Pad2)"))
    (pad 4 thru_hole circle (at -1.2954 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 31 L-3_Enet_Rx+))
    (pad 3 thru_hole circle (at -3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 19 GPS_Pulse))
    (pad 2 thru_hole circle (at 1.27 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.2954 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector:MD-80SM (layer F.Cu) (tedit 5DB8C23B)
    (at 86.03996 71.935848 90)
    (fp_text reference J3 (at 0.6858 -0.6604 90) (layer F.SilkS))
    (fp_text value MD-80SM (at 0 0.9906 90) (layer F.Fab))
    (fp_text user "ENET TX-" (at 1.05 12.175 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at -1.075 12.125 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at -3.425 12.15 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at 3.625 12.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 1.275 7.425 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -3.302 7.5184 90) (layer F.SilkS))
    (fp_text user 12V (at 3.425 7.325 90) (layer F.SilkS))
    (fp_text user GND (at -1.2192 7.493 90) (layer F.SilkS))
    (fp_text user Shield (at 6.5532 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at 0.0254 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at -6.2484 3.7084 90) (layer F.SilkS))
    (pad 11 thru_hole rect (at 6.7437 5.5118) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole rect (at -6.7437 5.5118 180) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole rect (at 0 4.699 90) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 24 L-2_Enet_Tx+))
    (pad 7 thru_hole circle (at 0.889 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 25 L-2_Enet_Tx-))
    (pad 6 thru_hole circle (at -3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 26 L-2_Enet_Rx-))
    (pad 5 thru_hole circle (at 3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 10 "Net-(F2-Pad2)"))
    (pad 4 thru_hole circle (at -1.2954 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 27 L-2_Enet_Rx+))
    (pad 3 thru_hole circle (at -3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 19 GPS_Pulse))
    (pad 2 thru_hole circle (at 1.27 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.2954 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Connector:MD-80SM (layer F.Cu) (tedit 5DB8C23B)
    (at 86.03996 50.57648 90)
    (fp_text reference J2 (at 0.6858 -0.6604 90) (layer F.SilkS))
    (fp_text value MD-80SM (at 0 0.9906 90) (layer F.Fab))
    (fp_text user "ENET TX-" (at 1.05 12.175 90) (layer F.SilkS))
    (fp_text user "ENET RX+" (at -1.075 12.125 90) (layer F.SilkS))
    (fp_text user "ENET RX-" (at -3.425 12.15 90) (layer F.SilkS))
    (fp_text user "ENET TX+" (at 3.625 12.2 90) (layer F.SilkS))
    (fp_text user "GPS RX" (at 1.275 7.425 90) (layer F.SilkS))
    (fp_text user "GPS PULSE" (at -3.302 7.5184 90) (layer F.SilkS))
    (fp_text user 12V (at 3.425 7.325 90) (layer F.SilkS))
    (fp_text user GND (at -1.2192 7.493 90) (layer F.SilkS))
    (fp_text user Shield (at 6.5532 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at 0.0254 3.683 90) (layer F.SilkS))
    (fp_text user Shield (at -6.2484 3.7084 90) (layer F.SilkS))
    (pad 11 thru_hole rect (at 6.7437 5.5118) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole rect (at -6.7437 5.5118 180) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole rect (at 0 4.699 90) (size 2.794 1.524) (drill oval 2.0066 0.7366) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 8 thru_hole circle (at 3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 20 L-1_Enet_Tx+))
    (pad 7 thru_hole circle (at 0.889 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 21 L-1_Enet_Tx-))
    (pad 6 thru_hole circle (at -3.4036 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 22 L-1_Enet_Rx-))
    (pad 5 thru_hole circle (at 3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad2)"))
    (pad 4 thru_hole circle (at -1.2954 10.9982 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 23 L-1_Enet_Rx+))
    (pad 3 thru_hole circle (at -3.4036 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 19 GPS_Pulse))
    (pad 2 thru_hole circle (at 1.27 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.2954 8.509 90) (size 1.524 1.524) (drill 0.871982) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.81052 149.85492 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F6 (at 11.25 -6) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(F6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 Pout))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.81052 131.13512 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F5 (at 11.25 -6) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(F5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 Pout))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.7 107.94 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F4 (at 11.25 -6) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(F4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 Pout))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.81052 87.36584 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F3 (at 11.25 -6) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(F3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 Pout))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.81052 68.49364 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F2 (at 11.25 -6) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(F2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 Pout))
  )
  (module "480 Component Footprints:Fuseholder" (layer F.Cu) (tedit 5DBB5C63)
    (at 124.81052 46.37532 180)
    (descr "Fuseholder horizontal open 5x20 Schurter 0031.8201, https://www.schurter.com/en/datasheet/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F1 (at 11.25 -6) (layer F.SilkS))
    (fp_text value Fuse (at 11.25 6) (layer F.Fab))
    (fp_text user %R (at 11.25 4) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.5 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 15 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 Pout))
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 104.65816 141.78788 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 104.65816 122.64136 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 104.45 100.82 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 104.65816 79.10068 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 104.65816 59.88812 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "480 Component Footprints:LED_D3.0mm" (layer F.Cu) (tedit 5DBB5A9D)
    (at 104.65816 38.31844 270)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 87.4 144.15) (end 87.35 16.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76 144.15) (end 87.4 144.15) (layer Edge.Cuts) (width 0.05))
  (gr_text "LIDAR 6" (at 102.6 158.4 90) (layer F.SilkS))
  (gr_text "LIDAR 5" (at 100.65 134.25 90) (layer F.SilkS))
  (gr_text "LIDAR 4" (at 101.2 112.8 90) (layer F.SilkS))
  (gr_text "LIDAR 3" (at 100.3 93.2 90) (layer F.SilkS))
  (gr_text "LIDAR 2" (at 100.24996 70.80744 90) (layer F.SilkS))
  (gr_text "LIDAR 1" (at 100.20424 49.6848 90) (layer F.SilkS))
  (gr_text "GPS PULSE" (at 93.75648 36.91128) (layer F.SilkS))
  (gr_line (start 150 16.21536) (end 150 186) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 87.35 16.25) (end 150 16.21536) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76.1 186) (end 76 144.15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 150 186) (end 76.1 186) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 78 145.55) (xy 78 184.55) (xy 149 184.55) (xy 149.1 16.7) (xy 88 16.7)
        (xy 87.8 144.85) (xy 78 144.85)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 78 145.55) (xy 78 184.55) (xy 149 184.55) (xy 149.1 16.7) (xy 88 16.7)
        (xy 87.8 144.85) (xy 78 144.85)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 78 170.35) (xy 91.4 184.55) (xy 78 184.55)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 134.8 184.55) (xy 149 171.15) (xy 149 184.55)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 149.1 30.9) (xy 135.7 16.7) (xy 149.1 16.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 1) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 102.2 16.7) (xy 88 30.1) (xy 88 16.7)
      )
    )
  )
)
