(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001330_80000001)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory "meta/")
    )
  )
  (net 0 "")
  (net 1 "Net-(C2-Pad1)")
  (net 2 "Net-(C2-Pad2)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "GND")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "unconnected-(J1-Pad2)")
  (net 8 "unconnected-(J1-Pad3)")
  (net 9 "unconnected-(J1-Pad4)")
  (net 10 "unconnected-(J1-Pad5)")
  (net 11 "unconnected-(J1-Pad7)")
  (net 12 "TX_PI")
  (net 13 "unconnected-(J1-Pad9)")
  (net 14 "RX_PI")
  (net 15 "RTS_PI")
  (net 16 "unconnected-(J1-Pad12)")
  (net 17 "unconnected-(J1-Pad13)")
  (net 18 "unconnected-(J1-Pad14)")
  (net 19 "unconnected-(J1-Pad15)")
  (net 20 "unconnected-(J1-Pad16)")
  (net 21 "unconnected-(J1-Pad17)")
  (net 22 "unconnected-(J1-Pad18)")
  (net 23 "unconnected-(J1-Pad19)")
  (net 24 "unconnected-(J1-Pad20)")
  (net 25 "unconnected-(J1-Pad21)")
  (net 26 "unconnected-(J1-Pad22)")
  (net 27 "unconnected-(J1-Pad23)")
  (net 28 "unconnected-(J1-Pad24)")
  (net 29 "unconnected-(J1-Pad25)")
  (net 30 "unconnected-(J1-Pad26)")
  (net 31 "unconnected-(J1-Pad27)")
  (net 32 "unconnected-(J1-Pad28)")
  (net 33 "unconnected-(J1-Pad29)")
  (net 34 "unconnected-(J1-Pad30)")
  (net 35 "unconnected-(J1-Pad31)")
  (net 36 "unconnected-(J1-Pad32)")
  (net 37 "unconnected-(J1-Pad33)")
  (net 38 "unconnected-(J1-Pad34)")
  (net 39 "unconnected-(J1-Pad35)")
  (net 40 "CTS_PI")
  (net 41 "unconnected-(J1-Pad37)")
  (net 42 "unconnected-(J1-Pad38)")
  (net 43 "unconnected-(J1-Pad39)")
  (net 44 "unconnected-(J1-Pad40)")
  (net 45 "unconnected-(J2-Pad1)")
  (net 46 "RXD_232")
  (net 47 "TXD_232")
  (net 48 "unconnected-(J2-Pad4)")
  (net 49 "unconnected-(J2-Pad6)")
  (net 50 "RTS_232")
  (net 51 "CTS_232")
  (net 52 "unconnected-(J2-Pad9)")
  (net 53 "TX_3232")
  (net 54 "RX_3232")
  (net 55 "RTS_3232")
  (net 56 "CTS_3232")
  (net 57 "unconnected-(J3-Pad1)")
  (net 58 "Net-(C1-Pad1)")
  (net 59 "Net-(C1-Pad2)")
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217C7B)
    (at 74 28)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217CA2)
    (at 16 28)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217CCB)
    (at 74 51)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217CCB)
    (at 16 51)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 26.67 39.37 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 2.54 -2.54 90) (layer "F.Fab"))
    (fp_text user "0.1uF" (at 2.54 -2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 50.815 40.8 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 8.875 90) (layer "F.SilkS"))
    (fp_text value "SP3232E" (at 3.81 20.11 90) (layer "F.Fab"))
    (fp_text user "SP3232E" (at 3.97 -2.555 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C1-Pad1)") (pinfunction "C1+") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)") (pinfunction "VS+") (pintype "power_out"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C1-Pad2)") (pinfunction "C1-") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C2-Pad1)") (pinfunction "C2+") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)") (pinfunction "C2-") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)") (pinfunction "VS-") (pintype "power_out"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "RTS_3232") (pinfunction "T2OUT") (pintype "output"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "CTS_3232") (pinfunction "R2IN") (pintype "input"))
    (pad "9" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "CTS_PI") (pinfunction "R2OUT") (pintype "output"))
    (pad "10" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "RTS_PI") (pinfunction "T2IN") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "TX_PI") (pinfunction "T1IN") (pintype "input"))
    (pad "12" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "RX_PI") (pinfunction "R1OUT") (pintype "output"))
    (pad "13" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "RX_3232") (pinfunction "R1IN") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "TX_3232") (pinfunction "T1OUT") (pintype "output"))
    (pad "15" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "16" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 48.895 46.564669)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.84mm, pin-PCB-offset 4.9399999999999995mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 7.4799999999999995mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.84mm pin-PCB-offset 4.9399999999999995mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 5.54 -3.7) (layer "F.SilkS"))
    (fp_text value "DB9_Male" (at 5.54 15.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.54 11.18) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -6.96 0.3) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle (at 18.04 0.3) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.77 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 46 "RXD_232") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.54 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 47 "TXD_232") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 8.31 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J2-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 11.08 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 1.385 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 49 "unconnected-(J2-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 4.155 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 50 "RTS_232") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 6.925 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 51 "CTS_232") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 9.695 2.84) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 52 "unconnected-(J2-Pad9)") (pinfunction "9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset7.48mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 29.96 52.5 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 7.318228 270) (layer "F.SilkS"))
    (fp_text value "Conn_02x02_Counter_Clockwise" (at -4.65 8.775) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "unconnected-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "RXD_232") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "TXD_232") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "CTS_232") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "RTS_232") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 31.79 45.72)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 2.54 -2.54 180) (layer "F.Fab"))
    (fp_text user "0.1uF" (at 2.5 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_CuK_JS202011AQN_DPDT_Angled" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 17.025 38 -90)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 2.64 1.785 -90) (layer "F.SilkS"))
    (fp_text value "SW_DPDT_x2" (at 2.25 6.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 1.75 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "RXD_232") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "TX_3232") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "TXD_232") (pinfunction "C") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 3.3 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "TXD_232") (pinfunction "A") (pintype "passive"))
    (pad "5" thru_hole circle (at 2.5 3.3 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "RX_3232") (pinfunction "B") (pintype "passive"))
    (pad "6" thru_hole circle (at 5 3.3 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "RXD_232") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_CuK_JS202011AQN_DPDT_Angled.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 20.87 29.27 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -2.48 -0.55 180) (layer "F.SilkS"))
    (fp_text value "Raspberry_Pi_2_3" (at -2.73 43.13 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 24.13 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)") (pinfunction "3V3") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J1-Pad2)") (pinfunction "5V") (pintype "power_in"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J1-Pad3)") (pinfunction "SDA/GPIO2") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J1-Pad4)") (pinfunction "5V") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J1-Pad5)") (pinfunction "SCL/GPIO3") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J1-Pad7)") (pinfunction "GCLK0/GPIO4") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "TX_PI") (pinfunction "GPIO14/TXD") (pintype "bidirectional"))
    (pad "9" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J1-Pad9)") (pinfunction "GND") (pintype "power_in"))
    (pad "10" thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "RX_PI") (pinfunction "GPIO15/RXD") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "RTS_PI") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J1-Pad12)") (pinfunction "GPIO18/PWM0") (pintype "bidirectional"))
    (pad "13" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-Pad13)") (pinfunction "GPIO27") (pintype "bidirectional"))
    (pad "14" thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J1-Pad14)") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J1-Pad15)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J1-Pad16)") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J1-Pad17)") (pinfunction "3V3") (pintype "power_in"))
    (pad "18" thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J1-Pad18)") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "19" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J1-Pad19)") (pinfunction "MOSI0/GPIO10") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J1-Pad20)") (pinfunction "GND") (pintype "power_in"))
    (pad "21" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J1-Pad21)") (pinfunction "MISO0/GPIO9") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J1-Pad22)") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "23" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J1-Pad23)") (pinfunction "SCLK0/GPIO11") (pintype "bidirectional"))
    (pad "24" thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J1-Pad24)") (pinfunction "~{CE0}/GPIO8") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J1-Pad25)") (pinfunction "GND") (pintype "power_in"))
    (pad "26" thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "unconnected-(J1-Pad26)") (pinfunction "~{CE1}/GPIO7") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "unconnected-(J1-Pad27)") (pinfunction "ID_SD/GPIO0") (pintype "bidirectional"))
    (pad "28" thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "unconnected-(J1-Pad28)") (pinfunction "ID_SC/GPIO1") (pintype "bidirectional"))
    (pad "29" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "unconnected-(J1-Pad29)") (pinfunction "GCLK1/GPIO5") (pintype "bidirectional"))
    (pad "30" thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J1-Pad30)") (pinfunction "GND") (pintype "power_in"))
    (pad "31" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "unconnected-(J1-Pad31)") (pinfunction "GCLK2/GPIO6") (pintype "bidirectional"))
    (pad "32" thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(J1-Pad32)") (pinfunction "PWM0/GPIO12") (pintype "bidirectional"))
    (pad "33" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J1-Pad33)") (pinfunction "PWM1/GPIO13") (pintype "bidirectional"))
    (pad "34" thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J1-Pad34)") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "unconnected-(J1-Pad35)") (pinfunction "GPIO19/MISO1") (pintype "bidirectional"))
    (pad "36" thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "CTS_PI") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "37" thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "unconnected-(J1-Pad37)") (pinfunction "GPIO26") (pintype "bidirectional"))
    (pad "38" thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "unconnected-(J1-Pad38)") (pinfunction "GPIO20/MOSI1") (pintype "bidirectional"))
    (pad "39" thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "unconnected-(J1-Pad39)") (pinfunction "GND") (pintype "power_in"))
    (pad "40" thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "unconnected-(J1-Pad40)") (pinfunction "GPIO21/SCLK1") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 39.37 34.5 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 2.33 2.54 90) (layer "F.Fab"))
    (fp_text user "0.1uF" (at 2.33 2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_CuK_JS202011AQN_DPDT_Angled" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 73 42 90)
    (descr "CuK sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
    (tags "switch DPDT")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 2.63 1.93 270) (layer "F.SilkS"))
    (fp_text value "SW_DPDT_x2" (at 2.25 6.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 1.75 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "CTS_232") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "RTS_3232") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "RTS_232") (pinfunction "C") (pintype "passive"))
    (pad "4" thru_hole circle (at 0 3.3 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "RTS_232") (pinfunction "A") (pintype "passive"))
    (pad "5" thru_hole circle (at 2.5 3.3 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "CTS_3232") (pinfunction "B") (pintype "passive"))
    (pad "6" thru_hole circle (at 5 3.3 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "CTS_232") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_CuK_JS202011AQN_DPDT_Angled.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 45.72 34.5 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 2.33 2.54 90) (layer "F.Fab"))
    (fp_text user "0.1uF" (at 2.33 2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 33.02 39.33 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "PiRS232.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 2.5 -2.54 270) (layer "F.Fab"))
    (fp_text user "0.1uF" (at 2.5 -2.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 15.5 54.5) (mid 13.37868 53.62132) (end 12.5 51.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 77.5 51.5) (mid 76.62132 53.62132) (end 74.5 54.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 74.5 24.5) (mid 76.62132 25.37868) (end 77.5 27.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 15.5 24.5) (end 74.5 24.5) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 12.5 27.5) (mid 13.37868 25.37868) (end 15.5 24.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 77.5 27.5) (end 77.5 51.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 15.5 54.5) (end 74.5 54.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 12.5 27.5) (end 12.5 51.5) (layer "Edge.Cuts") (width 0.1))
  (gr_text "©2022 Orange Tentacle" (at 59.69 52.07) (layer "B.SilkS"))
  (gr_text "RTS:RTS\nCTS:CTS" (at 74.583189 45.79916) (layer "F.SilkS"))
  (gr_text "RTS:CTS\nCTS:RTS" (at 74.661257 33.53255) (layer "F.SilkS"))
  (gr_text "TX:RX\nRX:TX" (at 15.363415 34.266923) (layer "F.SilkS"))
  (gr_text "TX:TX\nRX:RX" (at 15.446165 46.491688) (layer "F.SilkS"))
  (gr_text "Select one of these board edges depending \nupon the type of socket that is used." (at 20.5 9.5) (layer "Cmts.User"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 20 54.5) (xy 20 51))
    (height 2.5)
    (gr_text "3.5000 mm" (at 20.85 52.75 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 16.068883 55.2811) (xy 12.568883 55.2811))
    (height -3)
    (gr_text "3.5000 mm" (at 14.318883 56.6311) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 78.5 54.5) (xy 78.5 24.5))
    (height 3.5)
    (gr_text "30.0000 mm" (at 80.35 39.5 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 45 32) (xy 16 32))
    (height -2.499999)
    (gr_text "29.0000 mm" (at 30.5 32.849999) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 11.5 28) (xy 11.5 51))
    (height 2.5)
    (gr_text "23.0000 mm" (at 7.35 39.5 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 78.5 54.5) (xy 78.5 24))
    (height 8.5)
    (gr_text "30.5000 mm" (at 85.35 39.25 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 74 23) (xy 16 23))
    (height 2.5)
    (gr_text "58.0000 mm" (at 45 18.85) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 77.5 23) (xy 12.5 23))
    (height 7)
    (gr_text "65.0000 mm" (at 45 14.35) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 4) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.74 55.88)
        (xy 11.43 55.88)
        (xy 11.43 24.13)
        (xy 78.74 24.13)
      )
    )
  )
  (zone (net 4) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.74 55.88)
        (xy 11.43 55.88)
        (xy 11.43 24.13)
        (xy 78.74 24.13)
      )
    )
  )
)
