(kicad_pcb (version 20171130) (host pcbnew "(6.0.0-rc1-dev-1481-g5e705347b)")
  (general
    (thickness 1.6)
    (drawings 108)
    (tracks 736)
    (zones 0)
    (modules 60)
    (nets 79)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.1524)
    (zone_clearance 0.1)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1 0.5)
    (user_via 1.5 0.8)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (grid_origin 146.077733 100.4697)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x0100c_7ffffff8)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Plots/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 VCC)
  (net 5 BOOT1)
  (net 6 "Net-(U2-Pad52)")
  (net 7 "Net-(U2-Pad51)")
  (net 8 "Net-(U2-Pad50)")
  (net 9 "Net-(U2-Pad49)")
  (net 10 "Net-(U2-Pad46)")
  (net 11 "Net-(U2-Pad41)")
  (net 12 "Net-(U2-Pad33)")
  (net 13 "Net-(U2-Pad30)")
  (net 14 "Net-(U2-Pad29)")
  (net 15 "Net-(U2-Pad27)")
  (net 16 "Net-(U2-Pad25)")
  (net 17 "Net-(U2-Pad15)")
  (net 18 "Net-(U2-Pad9)")
  (net 19 "Net-(U2-Pad8)")
  (net 20 NRST)
  (net 21 "Net-(U2-Pad6)")
  (net 22 "Net-(U2-Pad5)")
  (net 23 "Net-(U2-Pad4)")
  (net 24 BLUE)
  (net 25 RED)
  (net 26 "Net-(U1-Pad7)")
  (net 27 SDCARD_CS)
  (net 28 MISO1)
  (net 29 SCK1)
  (net 30 MOSI1)
  (net 31 "Net-(D3-Pad2)")
  (net 32 "Net-(C8-Pad1)")
  (net 33 "Net-(J1-Pad1)")
  (net 34 "Net-(J1-Pad8)")
  (net 35 PWM1)
  (net 36 PWM2)
  (net 37 PWM3)
  (net 38 PWM4)
  (net 39 USBDP)
  (net 40 USBDM)
  (net 41 RX1)
  (net 42 TX1)
  (net 43 "Net-(D2-Pad1)")
  (net 44 BMP280_CS)
  (net 45 "Net-(D1-Pad1)")
  (net 46 TX2)
  (net 47 RX2)
  (net 48 RCIN)
  (net 49 TX3)
  (net 50 "Net-(J10-Pad4)")
  (net 51 USBDM1)
  (net 52 USBDP1)
  (net 53 +5V_MIX)
  (net 54 MOSI2)
  (net 55 SCK2)
  (net 56 MISO2)
  (net 57 I2C1_SDA)
  (net 58 I2C1_SCL)
  (net 59 "Net-(FB1-Pad2)")
  (net 60 BUZZER)
  (net 61 COIL)
  (net 62 SERVO_PWR)
  (net 63 CURR)
  (net 64 VOLT)
  (net 65 BOOT1_PD)
  (net 66 "Net-(Q1-Pad1)")
  (net 67 VOLTO)
  (net 68 "Net-(R15-Pad1)")
  (net 69 "Net-(U2-Pad54)")
  (net 70 "Net-(U2-Pad53)")
  (net 71 RX6)
  (net 72 TX6)
  (net 73 VBUS_O)
  (net 74 VBUS)
  (net 75 "Net-(C4-Pad2)")
  (net 76 "Net-(U1-Pad21)")
  (net 77 MPU9250_CS)
  (net 78 INT_MPU9250)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +5V_MIX)
    (add_net BLUE)
    (add_net BMP280_CS)
    (add_net BOOT1)
    (add_net BOOT1_PD)
    (add_net BUZZER)
    (add_net COIL)
    (add_net CURR)
    (add_net GND)
    (add_net I2C1_SCL)
    (add_net I2C1_SDA)
    (add_net INT_MPU9250)
    (add_net MISO1)
    (add_net MISO2)
    (add_net MOSI1)
    (add_net MOSI2)
    (add_net MPU9250_CS)
    (add_net NRST)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(FB1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J10-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad46)")
    (add_net "Net-(U2-Pad49)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad50)")
    (add_net "Net-(U2-Pad51)")
    (add_net "Net-(U2-Pad52)")
    (add_net "Net-(U2-Pad53)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net PWM1)
    (add_net PWM2)
    (add_net PWM3)
    (add_net PWM4)
    (add_net RCIN)
    (add_net RED)
    (add_net RX1)
    (add_net RX2)
    (add_net RX6)
    (add_net SCK1)
    (add_net SCK2)
    (add_net SDCARD_CS)
    (add_net SERVO_PWR)
    (add_net TX1)
    (add_net TX2)
    (add_net TX3)
    (add_net TX6)
    (add_net USBDM)
    (add_net USBDM1)
    (add_net USBDP)
    (add_net USBDP1)
    (add_net VBUS)
    (add_net VBUS_O)
    (add_net VCC)
    (add_net VOLT)
    (add_net VOLTO)
  )
  (module "Kicad Library:Pin_Header_Straight_1x06_Pitch1.27mm" (layer F.Cu) (tedit 5C5E337A)
    (at 155.3972 103.3018 180)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (fp_text reference J12 (at 0 -1.695 180) (layer Dwgs.User))
    (fp_text value CONN_1.27_6 (at 0 8.045 180) (layer F.Fab))
    (fp_text user %R (at 0 -3.175) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 6.35 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 63 CURR))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 64 VOLT))
    (pad 4 thru_hole oval (at 0 3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 61 COIL))
    (pad 2 thru_hole oval (at 0 1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 57 I2C1_SDA))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 58 I2C1_SCL))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:SDM1U20CSP-7" (layer F.Cu) (tedit 5C5E2DC7)
    (at 142.1384 92.6719 180)
    (fp_text reference D4 (at 0.599976 -0.849966 180) (layer Dwgs.User))
    (fp_text value SDM1U20CSP-7 (at 0.449982 -1.649934 180) (layer F.Fab))
    (pad 2 smd rect (at 0.51998 0 270) (size 0.58 0.84) (layers F.Cu F.Paste F.Mask)
      (net 74 VBUS))
    (pad 1 smd rect (at -0.259996 0 270) (size 0.58 0.304) (layers F.Cu F.Paste F.Mask)
      (net 53 +5V_MIX))
    (model C:/Users/mookie/Documents/Kicad3D/SDM1U40CSP.STEP
      (offset (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "Kicad Library:SDM1U20CSP-7" (layer F.Cu) (tedit 5C5E2DC7)
    (at 150.108004 107.5309 180)
    (fp_text reference D5 (at 0.599976 -0.849966 180) (layer Dwgs.User))
    (fp_text value SDM1U20CSP-7 (at 0.449982 -1.649934 180) (layer F.Fab))
    (pad 2 smd rect (at 0.51998 0 270) (size 0.58 0.84) (layers F.Cu F.Paste F.Mask)
      (net 62 SERVO_PWR))
    (pad 1 smd rect (at -0.259996 0 270) (size 0.58 0.304) (layers F.Cu F.Paste F.Mask)
      (net 53 +5V_MIX))
    (model C:/Users/mookie/Documents/Kicad3D/SDM1U40CSP.STEP
      (offset (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C5A)
    (at 136.935801 114.554 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 180) (layer Dwgs.User))
    (fp_text value PIN_2.54x3_VRT (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 PWM1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C5A)
    (at 139.475801 114.554 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer Dwgs.User))
    (fp_text value PIN_2.54x3_VRT (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 PWM2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C5A)
    (at 142.015801 114.554 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer Dwgs.User))
    (fp_text value PIN_2.54x3_VRT (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 PWM3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x03_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C5A)
    (at 144.555801 114.554 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 180) (layer Dwgs.User))
    (fp_text value PIN_2.54x3_VRT (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 PWM4))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x04_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C7D)
    (at 154.715801 112.014 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 270) (layer Dwgs.User))
    (fp_text value PIN_2.54x4_VRT (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 RX2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 TX2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x04_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C7D)
    (at 154.715801 114.554 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 270) (layer Dwgs.User))
    (fp_text value PIN_2.54x4_VRT (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 RX1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 TX1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x04_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C7D)
    (at 154.715801 109.474 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 270) (layer Dwgs.User))
    (fp_text value PIN_2.54x4_VRT (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 RCIN))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 TX3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:Pin_Header_Straight_1x04_Pitch2.54mm" (layer F.Cu) (tedit 5C5E2C7D)
    (at 136.4869 87.3506 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 90) (layer Dwgs.User))
    (fp_text value PIN_2.54x4_VRT (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 -180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 SERVO_PWR))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 RX6))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 TX6))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE801E5)
    (at 150.070801 89.485201 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.27 270) (layer Dwgs.User))
    (fp_text value 0402_10nF_X5R (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE801E5)
    (at 152.920801 93.2268 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.27 90) (layer Dwgs.User))
    (fp_text value 0402_100nF_X5R (at 0 1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:MPU9250" (layer F.Cu) (tedit 5BF9DECD)
    (at 152.720801 89.935201)
    (descr "24-Lead Plastic QFN (3mm x 3mm); Pitch 0.4mm; EP 1.7x1.54mm; for InvenSense motion sensors; keepout area marked (Package see: https://store.invensense.com/datasheets/invensense/MPU9250REV1.0.pdf; See also https://www.invensense.com/wp-content/uploads/2015/02/InvenSense-MEMS-Handling.pdf)")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U1 (at 0 -3.25) (layer Dwgs.User))
    (fp_text value MPU9250 (at 0 3.25) (layer F.Fab))
    (fp_text user Component (at 0 0.55) (layer Cmts.User))
    (fp_text user "Directly Below" (at 0 0.25) (layer Cmts.User))
    (fp_text user "No Copper" (at 0 -0.1) (layer Cmts.User))
    (fp_text user KEEPOUT (at 0 -0.5) (layer Cmts.User))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 24 smd roundrect (at -1 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 MOSI1))
    (pad 23 smd roundrect (at -0.6 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 SCK1))
    (pad 22 smd roundrect (at -0.2 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 MPU9250_CS))
    (pad 21 smd roundrect (at 0.2 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 "Net-(U1-Pad21)"))
    (pad 20 smd roundrect (at 0.6 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 19 smd roundrect (at 1 -1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 18 smd roundrect (at 1.5 -1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at 1.5 -0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at 1.5 -0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at 1.5 0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at 1.5 0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 1.5 1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 12 smd roundrect (at 1 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 INT_MPU9250))
    (pad 11 smd roundrect (at 0.6 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 smd roundrect (at 0.2 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 "Net-(C4-Pad2)"))
    (pad 9 smd roundrect (at -0.2 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 MISO1))
    (pad 8 smd roundrect (at -0.6 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (pad 7 smd roundrect (at -1 1.5 90) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad7)"))
    (pad 6 smd roundrect (at -1.5 1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 5 smd roundrect (at -1.5 0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -1.5 0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 3 smd roundrect (at -1.5 -0.2) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 2 smd roundrect (at -1.5 -0.6) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.5 -1) (size 0.55 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24_3x3mm_P0.4mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_2K" (layer F.Cu) (tedit 5BEB4D57)
    (at 136.779 92.456 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R19 (at 0 -1.35 180) (layer Dwgs.User))
    (fp_text value 0402_2K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 74 VBUS))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 VBUS_O))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_2K" (layer F.Cu) (tedit 5BEB4D57)
    (at 137.414 94.615 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R18 (at 0 -1.35 180) (layer Dwgs.User))
    (fp_text value 0402_2K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 73 VBUS_O))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE855ED)
    (at 151.5745 96.8629 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -1.27 180) (layer Dwgs.User))
    (fp_text value 0402_100nF_X5R (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:EVPBB2A9B000" (layer F.Cu) (tedit 5BE8596E)
    (at 154.4701 95.1992)
    (descr EVPBB2A9B000)
    (tags Switch)
    (attr smd)
    (fp_text reference S1 (at 0.049998 -1.949922) (layer Dwgs.User))
    (fp_text value EVPBB2A9B000 (at 0.399984 2.699892) (layer Dwgs.User))
    (pad 1 smd rect (at -1.075 -0.375 90) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 BOOT1))
    (pad 2 smd rect (at -1.075 0.375 90) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 BOOT1))
    (pad 3 smd rect (at 1.575 0.375 90) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 4 smd rect (at 1.575 -0.375 90) (size 0.55 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model C:/Users/mookie/Documents/Kicad3D/EVPBB2A9B000.STEP
      (offset (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "Kicad Library:WURTH_USB_VRT" (layer F.Cu) (tedit 5C28F167)
    (at 139.9921 90.8431 180)
    (descr 614105150621)
    (tags Connector)
    (fp_text reference J10 (at 2.399904 -1.849926 180) (layer Dwgs.User))
    (fp_text value USB_A_VRT_WURTH (at -0.1016 -0.9144 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -1.3 0.065 270) (size 0.9 0.9) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 74 VBUS))
    (pad 2 thru_hole circle (at -0.65 1.065 270) (size 0.9 0.9) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 40 USBDM))
    (pad 3 thru_hole circle (at 0 0.065 270) (size 0.9 0.9) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 39 USBDP))
    (pad 4 thru_hole circle (at 0.65 1.065 270) (size 0.9 0.9) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(J10-Pad4)"))
    (pad 5 thru_hole circle (at 1.3 0.065 270) (size 0.9 0.9) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at -3.575 0.285 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole circle (at 3.575 0.285 270) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model C:/Users/mookie/Documents/Kicad3D/USB_61410515062_WURTH_V.STEP
      (offset (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE859BA)
    (at 139.6619 92.6719 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.27 180) (layer Dwgs.User))
    (fp_text value 0402_2.2uF_X5R (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE859E7)
    (at 136.2075 103.8606 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27 270) (layer Dwgs.User))
    (fp_text value 0402_2.2uF_X5R (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE85605)
    (at 155.520801 91.585201 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at 0 -1.27 270) (layer Dwgs.User))
    (fp_text value 0402_100nF_X5R (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:STM32F405RGT6" (layer F.Cu) (tedit 5BE85A24)
    (at 143.4442 100.0654 180)
    (descr "64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 0 -7.2 180) (layer Dwgs.User))
    (fp_text value STM32F405RGT6 (at 0 7.2 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 64 smd rect (at -3.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 63 smd rect (at -3.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 62 smd rect (at -2.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 I2C1_SDA))
    (pad 61 smd rect (at -2.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 I2C1_SCL))
    (pad 60 smd rect (at -1.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 BOOT1))
    (pad 59 smd rect (at -1.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 RX1))
    (pad 58 smd rect (at -0.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 TX1))
    (pad 57 smd rect (at -0.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 PWM4))
    (pad 56 smd rect (at 0.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 PWM3))
    (pad 55 smd rect (at 0.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 RCIN))
    (pad 54 smd rect (at 1.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U2-Pad54)"))
    (pad 53 smd rect (at 1.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U2-Pad53)"))
    (pad 52 smd rect (at 2.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U2-Pad52)"))
    (pad 51 smd rect (at 2.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U2-Pad51)"))
    (pad 50 smd rect (at 3.25 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U2-Pad50)"))
    (pad 49 smd rect (at 3.75 -5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U2-Pad49)"))
    (pad 48 smd rect (at 5.7 -3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 47 smd rect (at 5.7 -3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 46 smd rect (at 5.7 -2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U2-Pad46)"))
    (pad 45 smd rect (at 5.7 -2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 USBDP1))
    (pad 44 smd rect (at 5.7 -1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 USBDM1))
    (pad 43 smd rect (at 5.7 -1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 PWM1))
    (pad 42 smd rect (at 5.7 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 VBUS_O))
    (pad 41 smd rect (at 5.7 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-Pad41)"))
    (pad 40 smd rect (at 5.7 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 BUZZER))
    (pad 39 smd rect (at 5.7 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 SDCARD_CS))
    (pad 38 smd rect (at 5.7 1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 RX6))
    (pad 37 smd rect (at 5.7 1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 TX6))
    (pad 36 smd rect (at 5.7 2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 MOSI2))
    (pad 35 smd rect (at 5.7 2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 MISO2))
    (pad 34 smd rect (at 5.7 3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 SCK2))
    (pad 33 smd rect (at 5.7 3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad33)"))
    (pad 32 smd rect (at 3.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 31 smd rect (at 3.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 30 smd rect (at 2.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad30)"))
    (pad 29 smd rect (at 2.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad29)"))
    (pad 28 smd rect (at 1.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 BOOT1_PD))
    (pad 27 smd rect (at 1.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad27)"))
    (pad 26 smd rect (at 0.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 PWM2))
    (pad 25 smd rect (at 0.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad25)"))
    (pad 24 smd rect (at -0.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 MPU9250_CS))
    (pad 23 smd rect (at -0.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 MOSI1))
    (pad 22 smd rect (at -1.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 MISO1))
    (pad 21 smd rect (at -1.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 SCK1))
    (pad 20 smd rect (at -2.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 BMP280_CS))
    (pad 19 smd rect (at -2.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 18 smd rect (at -3.25 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 17 smd rect (at -3.75 5.7 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 RX2))
    (pad 16 smd rect (at -5.7 3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 TX2))
    (pad 15 smd rect (at -5.7 3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad15)"))
    (pad 14 smd rect (at -5.7 2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 INT_MPU9250))
    (pad 13 smd rect (at -5.7 2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(FB1-Pad2)"))
    (pad 12 smd rect (at -5.7 1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -5.7 1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(R15-Pad1)"))
    (pad 10 smd rect (at -5.7 0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 VOLTO))
    (pad 9 smd rect (at -5.7 0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad9)"))
    (pad 8 smd rect (at -5.7 -0.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad8)"))
    (pad 7 smd rect (at -5.7 -0.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 NRST))
    (pad 6 smd rect (at -5.7 -1.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -5.7 -1.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -5.7 -2.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -5.7 -2.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 BLUE))
    (pad 2 smd rect (at -5.7 -3.25 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 RED))
    (pad 1 smd rect (at -5.7 -3.75 180) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CSTCE16M0V53A-R0" (layer F.Cu) (tedit 5BE85A65)
    (at 151.5364 98.575126 90)
    (descr "SMD Resomator/Filter Murata SFECV, http://cdn-reichelt.de/documents/datenblatt/B400/SFECV-107.pdf, 6.9x2.9mm^2 package")
    (tags "SMD SMT ceramic resonator filter filter")
    (attr smd)
    (fp_text reference Y1 (at -1.549938 -2.049918 90) (layer Dwgs.User))
    (fp_text value CSTCE16M0V53A-R0 (at -1.399944 2.149914 90) (layer F.Fab))
    (fp_text user %R (at -1.549938 0 90) (layer F.Fab))
    (pad 3 smd rect (at -0.649974 0 90) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U2-Pad6)"))
    (pad 2 smd rect (at -1.74993 0 90) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.85 0 90) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U2-Pad5)"))
    (model C:/Users/mookie/Documents/Kicad3D/SW3dPS-CSTCE_V-1.STEP
      (offset (xyz -2.7 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:RED_LED_0603" (layer F.Cu) (tedit 5BE855B3)
    (at 153.4287 101.3333 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25 90) (layer Dwgs.User))
    (fp_text value Red_LED_0402 (at 1.016 4.2799 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model C:/Users/mookie/Documents/Kicad3D/0603_RED_LED.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module "Kicad Library:BLUE_LED_0603" (layer F.Cu) (tedit 5BE855AB)
    (at 153.4922 98.0058 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.25 90) (layer Dwgs.User))
    (fp_text value Blue_LED_0402 (at -0.1143 7.1374 90) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model C:/Users/mookie/Documents/Kicad3D/0603_BLUE_LED.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Kicad Library:GREEN_LED_0603" (layer F.Cu) (tedit 5BE85F35)
    (at 152.545801 86.785201)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.25) (layer Dwgs.User) hide)
    (fp_text value Green_LED_0402 (at 0 1.35) (layer F.Fab))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D3-Pad2)"))
    (model C:/Users/mookie/Documents/Kicad3D/0603_GREEN_LED.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1.1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Kicad Library:0402_330R" (layer F.Cu) (tedit 5BE851B7)
    (at 150.7308 103.5558 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -0.0254 -2.5654 180) (layer Dwgs.User))
    (fp_text value 0402_330R (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 RED))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_330R" (layer F.Cu) (tedit 5BE851BF)
    (at 150.7181 102.5017 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at -1.8161 0.6604 180) (layer Dwgs.User))
    (fp_text value 0402_330R (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 BLUE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_330R" (layer F.Cu) (tedit 5BE9F12F)
    (at 155.045801 87.235201 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 0 -1.35 90) (layer Dwgs.User))
    (fp_text value 0402_330R (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_10K" (layer F.Cu) (tedit 5BE9F0B9)
    (at 151.58 98.0948 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 0 -1.35 180) (layer Dwgs.User))
    (fp_text value 0402_10K (at 0 1.45 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 NRST))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0603_100nF" (layer F.Cu) (tedit 5BE84E92)
    (at 155.3845 105.549 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5 90) (layer Dwgs.User))
    (fp_text value 0603_100nF_X7R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 53 +5V_MIX))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402_10nF" (layer F.Cu) (tedit 5BE84EFC)
    (at 155.3806 107.5055)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -1.27) (layer Dwgs.User))
    (fp_text value 0402_10nF_X5R (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0603_100nF" (layer F.Cu) (tedit 5BE850D8)
    (at 153.0216 103.6447)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.5) (layer Dwgs.User))
    (fp_text value 0603_100nF_X7R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:REG113NA_3_3_250" (layer F.Cu) (tedit 5BE84E33)
    (at 152.5803 105.9991)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 -2.9) (layer Dwgs.User))
    (fp_text value REG113NA-3.3_250 (at 0.1348 4.379) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(C8-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 +5V_MIX))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 +5V_MIX))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE85984)
    (at 147.7264 91.0463 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 -1.27 180) (layer Dwgs.User))
    (fp_text value 0402_100nF_X5R (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:BMP280_P" (layer F.Cu) (tedit 5BE85AFD)
    (at 147.7646 89.1003 90)
    (descr "LGA-8, https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BMP280-DS001-18.pdf")
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U4 (at 0 -3.1 90) (layer Dwgs.User))
    (fp_text value BMP280_P (at 0 3.1 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.975 -0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0.975 0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 28 MISO1))
    (pad 6 smd rect (at 0.325 0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 7 smd rect (at -0.325 0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.975 -0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 29 SCK1))
    (pad 3 smd rect (at 0.325 -0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 30 MOSI1))
    (pad 2 smd rect (at -0.325 -0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 44 BMP280_CS))
    (pad 8 smd rect (at -0.975 0.8 180) (size 0.5 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model C:/Users/mookie/Documents/Kicad3D/BMP280.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "Kicad Library:JST_SDCARD" locked (layer B.Cu) (tedit 5BE85AD3)
    (at 143.611894 99.967706 90)
    (fp_text reference J1 (at 10.449182 5.736314 90) (layer Dwgs.User))
    (fp_text value SD_CARD_JST (at 0.24959 8.136218 90) (layer B.Fab))
    (pad 1 smd rect (at 3.649454 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 2.549498 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 27 SDCARD_CS))
    (pad 3 smd rect (at 1.449542 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 54 MOSI2))
    (pad 4 smd rect (at 0.349586 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 5 smd rect (at -0.75037 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 55 SCK2))
    (pad 6 smd rect (at -1.850326 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -2.950282 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 56 MISO2))
    (pad 8 smd rect (at -4.050238 -6.09001 90) (size 0.5 0.7) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -5.150194 -6.489994 90) (size 0.8 1.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -6.150154 -4.240084 90) (size 0.5 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -6.400144 -2.390158 90) (size 0.5 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 12 smd rect (at -6.400144 2.209658 90) (size 0.5 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -5.950162 6.58628 90) (size 1.15 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -0.699693 6.60899 90) (size 1.2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 3.650133 6.609482 90) (size 1.2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 16 smd rect (at 7.349985 3.40961 90) (size 0.5 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 17 smd rect (at 7.349985 -2.590642 90) (size 0.5 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 18 smd rect (at 6.627087 -7.63872 90) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model C:/Users/mookie/Documents/Kicad3D/JST_SDCARD.STEP
      (offset (xyz 0.07000000000000001 -0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "Kicad Library:0402_10K" (layer F.Cu) (tedit 5BE85965)
    (at 155.3718 93.8276)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R5 (at 0 -1.35) (layer Dwgs.User))
    (fp_text value 0402_10K (at 0 1.45) (layer F.Fab))
    (fp_text user %R (at 0 -1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 BOOT1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_22R" (layer F.Cu) (tedit 5BE859D0)
    (at 135.7757 95.3461 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0 -1.35 90) (layer Dwgs.User))
    (fp_text value 0402_22R (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 USBDP))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 USBDP1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_22R" (layer F.Cu) (tedit 5BE859D7)
    (at 136.4361 96.97 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 0 -1.35 90) (layer Dwgs.User))
    (fp_text value 0402_22R (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 USBDM1))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 USBDM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0603" (layer F.Cu) (tedit 5BE8597B)
    (at 147.6495 92.9259)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.5) (layer Dwgs.User))
    (fp_text value 0603_4.7uF_X5R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE83759)
    (at 146.6303 107.2388 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0 -1.27 180) (layer Cmts.User))
    (fp_text value 0402_100nF_X7R (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE859EE)
    (at 137.2616 105.6298 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0 -1.27 270) (layer Dwgs.User))
    (fp_text value 0402_100nF_X7R (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE859C7)
    (at 137.922 93.599 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 0 -1.27 180) (layer Dwgs.User))
    (fp_text value 0402_100nF_X7R (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE851A2)
    (at 149.1742 105.5282 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 0 -1.27 270) (layer Dwgs.User))
    (fp_text value 0402_100nF_X7R (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0603" (layer F.Cu) (tedit 5BE859DF)
    (at 136.4488 99.7846 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.5 270) (layer Dwgs.User))
    (fp_text value 0603_4.7uF_X5R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:CAP_0402" (layer F.Cu) (tedit 5BE85A54)
    (at 151.5745 95.7199)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 0 -1.27) (layer Dwgs.User))
    (fp_text value 0402_100nF_X7R (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:FERRITE_0805" (layer F.Cu) (tedit 5BE83B5E)
    (at 150.6855 94.1959 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference FB1 (at 0 -1.5 180) (layer Dwgs.User))
    (fp_text value Ferrite_Bead_0805_Wurth (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(FB1-Pad2)"))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:NFET_CSD13383F4" (layer F.Cu) (tedit 5BE9D2B5)
    (at 138.049 107.5563)
    (fp_text reference Q1 (at 0.56 -0.719992) (layer Dwgs.User))
    (fp_text value NFET_CSD13383F4_MICRO (at 0.4 -1.479992) (layer F.Fab))
    (pad 3 smd rect (at 0.55 -0.029992) (size 0.25 0.5) (layers F.Cu F.Paste F.Mask)
      (net 61 COIL))
    (pad 2 smd rect (at -0.099996 0.149994 180) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.1 -0.199992) (size 0.25 0.15) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(Q1-Pad1)"))
    (model C:/Users/mookie/Documents/Kicad3D/CSD13383F4_NFET.STEP
      (offset (xyz 0.73 0.33 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module "Kicad Library:0402_10K" (layer B.Cu) (tedit 5BE9F4C8)
    (at 145.6381 91.3638)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at 0 1.35) (layer Dwgs.User))
    (fp_text value 0402_10K (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 65 BOOT1_PD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_10K" (layer B.Cu) (tedit 5BE9F66A)
    (at 145.6364 90.297 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R9 (at 0 1.35 180) (layer Dwgs.User))
    (fp_text value 0402_10K (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 BMP280_CS))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_10K" (layer B.Cu) (tedit 5BE9F660)
    (at 151.670801 92.885201 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R10 (at 0 1.35 180) (layer Dwgs.User))
    (fp_text value 0402_10K (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 27 SDCARD_CS))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_10K" (layer B.Cu) (tedit 5BE9FA5F)
    (at 145.6381 89.2429 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R11 (at 0 1.35 180) (layer Dwgs.User))
    (fp_text value 0402_10K (at 0 -1.45 180) (layer B.Fab))
    (fp_text user %R (at 0 1.35 180) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 77 MPU9250_CS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_4K7" (layer B.Cu) (tedit 5BEA060B)
    (at 151.670801 102.5525)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R12 (at 0 1.35) (layer Dwgs.User))
    (fp_text value 0402_4k7 (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 57 I2C1_SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_4K7" (layer B.Cu) (tedit 5BEA060B)
    (at 151.670801 103.6193)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R13 (at 0 1.35) (layer Dwgs.User))
    (fp_text value 0402_4k7 (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 58 I2C1_SCL))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_1K1" (layer B.Cu) (tedit 5BEB4D6A)
    (at 151.7269 98.4885 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R14 (at 0 1.35 90) (layer Dwgs.User))
    (fp_text value 0402_1K1 (at 0 -1.45 90) (layer B.Fab))
    (fp_text user %R (at 0 1.35 90) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 VOLTO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_1K" (layer B.Cu) (tedit 5BEB4D3C)
    (at 153.3216 97.9424)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R15 (at 0 1.35) (layer Dwgs.User))
    (fp_text value 0402_1K (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 63 CURR))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_9K1" (layer B.Cu) (tedit 5BEB4D7B)
    (at 153.3216 98.9965)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R16 (at 0 1.35) (layer Dwgs.User))
    (fp_text value 0402_9K1 (at 0 -1.45) (layer B.Fab))
    (fp_text user %R (at 0 1.35) (layer B.Fab))
    (pad 2 smd rect (at 0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 64 VOLT))
    (pad 1 smd rect (at -0.45 0) (size 0.4 0.6) (layers B.Cu B.Paste B.Mask)
      (net 67 VOLTO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Kicad Library:0402_2K" (layer F.Cu) (tedit 5BEB4D57)
    (at 138.4427 106.1013 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R17 (at 0 -1.35 90) (layer Dwgs.User))
    (fp_text value 0402_2K (at 0 1.45 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 BUZZER))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 155.85411 85.965865) (end 155.685729 85.920757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.378096 86.405547) (end 156.278132 86.262763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.67005 85.965865) (end 135.512084 86.039527) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.451777 115.247577) (end 156.496886 115.079196) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.512088 114.905551) (end 156.512088 114.625551) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.512088 114.625551) (end 156.512088 86.905559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.146064 86.405547) (end 135.072383 86.563533) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.072383 86.563533) (end 135.027274 86.731914) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.317083 115.905555) (end 155.512084 115.905555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.3693 86.13951) (end 135.246028 86.262763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.451777 86.563533) (end 156.378096 86.405547) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.012076 85.905555) (end 135.838431 85.920757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.512084 115.905555) (end 155.685729 115.890353) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.15486 86.13951) (end 156.012076 86.039527) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.512088 86.905559) (end 156.496886 86.731914) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.012076 115.771583) (end 156.15486 115.6716) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.012076 86.039527) (end 155.85411 85.965865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.012072 87.185559) (end 135.012072 114.905551) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.246028 86.262763) (end 135.146064 86.405547) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.496886 115.079196) (end 156.512088 114.905551) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.246028 115.548347) (end 135.3693 115.6716) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.15486 115.6716) (end 156.278132 115.548347) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.3693 115.6716) (end 135.512084 115.771583) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.838431 85.920757) (end 135.67005 85.965865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.027274 86.731914) (end 135.012072 86.905559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.67005 115.845245) (end 135.838431 115.890353) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.685729 85.920757) (end 155.512084 85.905555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.027274 115.079196) (end 135.072383 115.247577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.278132 86.262763) (end 156.15486 86.13951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.838431 115.890353) (end 136.012076 115.905555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.512084 115.771583) (end 135.67005 115.845245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.512084 85.905555) (end 136.207077 85.905555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.072383 115.247577) (end 135.146064 115.405563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.207077 85.905555) (end 136.012076 85.905555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.146064 115.405563) (end 135.246028 115.548347) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.496886 86.731914) (end 156.451777 86.563533) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.85411 115.845245) (end 156.012076 115.771583) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.378096 115.405563) (end 156.451777 115.247577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.012072 86.905559) (end 135.012072 87.185559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.512084 86.039527) (end 135.3693 86.13951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.278132 115.548347) (end 156.378096 115.405563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.012224 114.907288) (end 135.027274 115.079196) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.685729 115.890353) (end 155.85411 115.845245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.012076 115.905555) (end 155.317083 115.905555) (layer Edge.Cuts) (width 0.1))
  (gr_text "RCIN\nTELM1\nGPS1" (at 152.7302 105.5878) (layer B.SilkS))
  (gr_text "U6 TELM2" (at 147.5232 87.3506 180) (layer B.SilkS))
  (gr_text "U3R\nU2\nU1" (at 155.2067 105.5878) (layer B.SilkS))
  (gr_text "USART 1,2,6" (at 151.4602 89.9668 180) (layer B.SilkS))
  (gr_text MPU9250 (at 151.4602 89.2048 180) (layer B.SilkS))
  (gr_text BMP280 (at 151.4602 88.4428 180) (layer B.SilkS))
  (gr_text GND (at 136.4615 88.773 180) (layer B.SilkS))
  (gr_text PWR (at 139.0015 88.773 180) (layer B.SilkS))
  (gr_text RX (at 141.5415 88.773 180) (layer B.SilkS))
  (gr_text TX (at 144.0815 88.773 180) (layer B.SilkS))
  (gr_text GND (at 154.7495 107.7468) (layer B.SilkS))
  (gr_text PWR (at 152.2095 107.7468) (layer B.SilkS))
  (gr_text RX (at 149.6695 107.7468) (layer B.SilkS))
  (gr_text TX (at 147.1295 107.7468) (layer B.SilkS))
  (gr_text 4 (at 144.5895 107.4039) (layer F.SilkS))
  (gr_text 3 (at 142.0495 107.4039) (layer F.SilkS))
  (gr_text 2 (at 139.5095 107.4039) (layer F.SilkS))
  (gr_text 4 (at 144.6022 107.7468) (layer B.SilkS))
  (gr_text 3 (at 142.0622 107.7468) (layer B.SilkS))
  (gr_text 2 (at 139.5222 107.7468) (layer B.SilkS))
  (gr_text 1 (at 136.9822 107.7468) (layer B.SilkS))
  (gr_text PWR (at 153.4922 100.1268) (layer B.SilkS))
  (gr_text VOLT (at 153.3652 96.9518) (layer B.SilkS))
  (gr_text CURR (at 153.2382 96.3168) (layer B.SilkS))
  (gr_text BUZ (at 153.4922 100.7618) (layer B.SilkS))
  (gr_text SDA (at 153.4922 102.0318) (layer B.SilkS))
  (gr_text SCL (at 153.4922 103.3018) (layer B.SilkS))
  (gr_text 1 (at 136.8171 107.3785) (layer F.SilkS))
  (gr_text Emma (at 155.9052 93.3323 90) (layer B.SilkS))
  (gr_text qUark_Nano9_V1.0 (at 152.235801 86.674 180) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 119.323885 74.674765) (xy 167.025085 75.220865) (xy 169.145985 123.264965) (xy 127.147085 122.058465) (xy 120.238285 120.039165)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 115.6081 69.2658) (xy 174.0535 69.6468) (xy 174.0027 128.1049) (xy 115.9891 127.2286)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.936 77.216) (xy 162.179 78.232) (xy 164.973 115.57) (xy 162.941 118.999) (xy 153.797 120.65)
        (xy 124.206 119.761)
      )
    )
  )
  (zone (net 4) (net_name VCC) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.1)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 159.385 117.475) (xy 130.556 117.729) (xy 131.064 80.899) (xy 160.02 80.899)
      )
    )
  )
  (zone (net 53) (net_name +5V_MIX) (layer In2.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 151.485801 104.724) (xy 144.535801 98.574) (xy 143.935801 92.074) (xy 142.335801 92.074) (xy 142.735801 98.874)
        (xy 147.835801 103.074) (xy 150.385801 105.824)
      )
    )
  )
  (zone (net 53) (net_name +5V_MIX) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 142.135801 92.174) (xy 143.835801 92.174) (xy 143.835801 93.174) (xy 142.135801 93.174)
      )
    )
  )
  (zone (net 53) (net_name +5V_MIX) (layer F.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 152.135801 104.574) (xy 152.135801 105.474) (xy 149.835801 105.474) (xy 149.835801 104.274) (xy 152.135801 104.274)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F.Cu In1.Cu In2.Cu B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.1))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.620801 88.835201) (xy 153.820801 88.835201) (xy 153.820801 91.035201) (xy 151.620801 91.035201)
      )
    )
  )
)
