(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6002)
    (drawings 29)
    (tracks 838)
    (zones 0)
    (modules 105)
    (nets 106)
  )
  (page A4)
  (layers
    (0 Front signal)
    (31 Back signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.127)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.127)
    (pad_size 2.6 2.6)
    (pad_drill 1.6)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +12V)
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 VBUS)
  (net 9 "Net-(D2-Pad2)")
  (net 10 "Net-(D2-Pad1)")
  (net 11 "Net-(J1-PadB5)")
  (net 12 "Net-(J1-PadB8)")
  (net 13 "Net-(J1-PadA8)")
  (net 14 "Net-(J1-PadA5)")
  (net 15 /RST)
  (net 16 /MOSI)
  (net 17 /SCK)
  (net 18 /MISO)
  (net 19 /M1)
  (net 20 /M2)
  (net 21 /M3)
  (net 22 /M4)
  (net 23 /SDA)
  (net 24 /SCL)
  (net 25 "Net-(U1-Pad5)")
  (net 26 "Net-(U1-Pad3)")
  (net 27 "Net-(U1-Pad2)")
  (net 28 "Net-(U1-Pad1)")
  (net 29 "Net-(U2-Pad41)")
  (net 30 "Net-(U2-Pad40)")
  (net 31 "Net-(U2-Pad39)")
  (net 32 "Net-(U2-Pad38)")
  (net 33 "Net-(U2-Pad37)")
  (net 34 "Net-(U2-Pad36)")
  (net 35 "Net-(U2-Pad33)")
  (net 36 "Net-(U2-Pad32)")
  (net 37 "Net-(U2-Pad31)")
  (net 38 "Net-(U2-Pad30)")
  (net 39 "Net-(U2-Pad29)")
  (net 40 "Net-(U2-Pad28)")
  (net 41 "Net-(U2-Pad27)")
  (net 42 "Net-(U2-Pad26)")
  (net 43 "Net-(U2-Pad25)")
  (net 44 "Net-(U2-Pad21)")
  (net 45 "Net-(U2-Pad20)")
  (net 46 "Net-(U2-Pad12)")
  (net 47 "Net-(U2-Pad8)")
  (net 48 "Net-(U2-Pad1)")
  (net 49 /M8)
  (net 50 /M7)
  (net 51 /M6)
  (net 52 /M5)
  (net 53 "Net-(U3-Pad8)")
  (net 54 "Net-(U3-Pad7)")
  (net 55 /M9)
  (net 56 /M10)
  (net 57 /M11)
  (net 58 /M12)
  (net 59 /M13)
  (net 60 /M14)
  (net 61 /M15)
  (net 62 /M16)
  (net 63 /M17)
  (net 64 /M18)
  (net 65 /M19)
  (net 66 /M20)
  (net 67 /M21)
  (net 68 /M22)
  (net 69 /M23)
  (net 70 /M24)
  (net 71 "Net-(U4-Pad8)")
  (net 72 "Net-(U4-Pad7)")
  (net 73 "Net-(U5-Pad8)")
  (net 74 "Net-(U5-Pad7)")
  (net 75 /SWITCH_OUT)
  (net 76 /D+)
  (net 77 /D-)
  (net 78 "/Motor Channel 1/DRAIN")
  (net 79 "/Motor Channel 2/DRAIN")
  (net 80 "/Motor Channel 3/DRAIN")
  (net 81 "/Motor Channel 4/DRAIN")
  (net 82 "/Motor Channel 5/DRAIN")
  (net 83 "/Motor Channel 6/DRAIN")
  (net 84 "/Motor Channel 7/DRAIN")
  (net 85 "/Motor Channel 8/DRAIN")
  (net 86 "/Motor Channel 9/DRAIN")
  (net 87 "/Motor Channel 10/DRAIN")
  (net 88 "/Motor Channel 11/DRAIN")
  (net 89 "/Motor Channel 12/DRAIN")
  (net 90 "/Motor Channel 13/DRAIN")
  (net 91 "/Motor Channel 14/DRAIN")
  (net 92 "/Motor Channel 15/DRAIN")
  (net 93 "/Motor Channel 16/DRAIN")
  (net 94 "/Motor Channel 17/DRAIN")
  (net 95 "/Motor Channel 18/DRAIN")
  (net 96 "/Motor Channel 19/DRAIN")
  (net 97 "/Motor Channel 20/DRAIN")
  (net 98 "/Motor Channel 21/DRAIN")
  (net 99 "/Motor Channel 22/DRAIN")
  (net 100 "/Motor Channel 23/DRAIN")
  (net 101 "/Motor Channel 24/DRAIN")
  (net 102 "Net-(J27-Pad3)")
  (net 103 /FUSE)
  (net 104 /MCU_D-)
  (net 105 /MCU_D+)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net /M1)
    (add_net /M10)
    (add_net /M11)
    (add_net /M12)
    (add_net /M13)
    (add_net /M14)
    (add_net /M15)
    (add_net /M16)
    (add_net /M17)
    (add_net /M18)
    (add_net /M19)
    (add_net /M2)
    (add_net /M20)
    (add_net /M21)
    (add_net /M22)
    (add_net /M23)
    (add_net /M24)
    (add_net /M3)
    (add_net /M4)
    (add_net /M5)
    (add_net /M6)
    (add_net /M7)
    (add_net /M8)
    (add_net /M9)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-PadA5)")
    (add_net "Net-(J1-PadA8)")
    (add_net "Net-(J1-PadB5)")
    (add_net "Net-(J1-PadB8)")
    (add_net "Net-(J27-Pad3)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U5-Pad7)")
    (add_net "Net-(U5-Pad8)")
  )
  (net_class Motor ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net "/Motor Channel 1/DRAIN")
    (add_net "/Motor Channel 10/DRAIN")
    (add_net "/Motor Channel 11/DRAIN")
    (add_net "/Motor Channel 12/DRAIN")
    (add_net "/Motor Channel 13/DRAIN")
    (add_net "/Motor Channel 14/DRAIN")
    (add_net "/Motor Channel 15/DRAIN")
    (add_net "/Motor Channel 16/DRAIN")
    (add_net "/Motor Channel 17/DRAIN")
    (add_net "/Motor Channel 18/DRAIN")
    (add_net "/Motor Channel 19/DRAIN")
    (add_net "/Motor Channel 2/DRAIN")
    (add_net "/Motor Channel 20/DRAIN")
    (add_net "/Motor Channel 21/DRAIN")
    (add_net "/Motor Channel 22/DRAIN")
    (add_net "/Motor Channel 23/DRAIN")
    (add_net "/Motor Channel 24/DRAIN")
    (add_net "/Motor Channel 3/DRAIN")
    (add_net "/Motor Channel 4/DRAIN")
    (add_net "/Motor Channel 5/DRAIN")
    (add_net "/Motor Channel 6/DRAIN")
    (add_net "/Motor Channel 7/DRAIN")
    (add_net "/Motor Channel 8/DRAIN")
    (add_net "/Motor Channel 9/DRAIN")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net +12V)
    (add_net +3V3)
    (add_net /FUSE)
    (add_net /SWITCH_OUT)
    (add_net GND)
    (add_net VBUS)
  )
  (net_class USB ""
    (clearance 0.1524)
    (trace_width 0.9652)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.4064)
    (diff_pair_gap 0.1524)
    (add_net /D+)
    (add_net /D-)
    (add_net /MCU_D+)
    (add_net /MCU_D-)
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580 (layer Front) (tedit 56D1B4CB)
    (at 93.98 101.6)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580 (layer Front) (tedit 56D1B4CB)
    (at 93.98 139.7)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580 (layer Front) (tedit 56D1B4CB)
    (at 35.56 139.7)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO14580")
    (tags "mounting hole 3.2mm no annular m3 iso14580")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.75) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO14580 (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_BarrelJack:BarrelJack_CUI_PJ-102AH_Horizontal (layer Front) (tedit 6189968D)
    (at 56.7055 110.998 180)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J27 (at 0.1905 -2.54 180) (layer F.SilkS))
    (fp_text value Barrel_Jack_Switch (at -5.5 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 3 thru_hole circle (at 4.7 3 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 102 "Net-(J27-Pad3)"))
    (pad 2 thru_hole circle (at 0 6 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer Front) (tedit 5D9F72B1)
    (at 54.1655 129.413 270)
    (descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U5 (at 0 -6.72 90) (layer F.SilkS))
    (fp_text value MCP23008-xSO (at 0 6.72 90) (layer F.Fab))
    (fp_text user %R (at 6.858 -5.2705 180) (layer F.Fab))
    (pad 18 smd roundrect (at 4.65 -5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 17 smd roundrect (at 4.65 -3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 /M6))
    (pad 16 smd roundrect (at 4.65 -2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 /M12))
    (pad 15 smd roundrect (at 4.65 -1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 /M18))
    (pad 14 smd roundrect (at 4.65 0 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /M24))
    (pad 13 smd roundrect (at 4.65 1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 /M5))
    (pad 12 smd roundrect (at 4.65 2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 /M11))
    (pad 11 smd roundrect (at 4.65 3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /M17))
    (pad 10 smd roundrect (at 4.65 5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 /M23))
    (pad 9 smd roundrect (at -4.65 5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -4.65 3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(U5-Pad8)"))
    (pad 7 smd roundrect (at -4.65 2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 "Net-(U5-Pad7)"))
    (pad 6 smd roundrect (at -4.65 1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at -4.65 0 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -4.65 -1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 3 smd roundrect (at -4.65 -2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -4.65 -3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /SDA))
    (pad 1 smd roundrect (at -4.65 -5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /SCL))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer Front) (tedit 5D9F72B1)
    (at 41.4655 129.413 270)
    (descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U4 (at 0 -6.72 90) (layer F.SilkS))
    (fp_text value MCP23008-xSO (at 0 6.72 90) (layer F.Fab))
    (fp_text user %R (at 6.858 -5.1435 180) (layer F.Fab))
    (pad 18 smd roundrect (at 4.65 -5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 17 smd roundrect (at 4.65 -3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /M4))
    (pad 16 smd roundrect (at 4.65 -2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 /M10))
    (pad 15 smd roundrect (at 4.65 -1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 /M16))
    (pad 14 smd roundrect (at 4.65 0 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 /M22))
    (pad 13 smd roundrect (at 4.65 1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /M3))
    (pad 12 smd roundrect (at 4.65 2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /M9))
    (pad 11 smd roundrect (at 4.65 3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 /M15))
    (pad 10 smd roundrect (at 4.65 5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 /M21))
    (pad 9 smd roundrect (at -4.65 5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -4.65 3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(U4-Pad8)"))
    (pad 7 smd roundrect (at -4.65 2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(U4-Pad7)"))
    (pad 6 smd roundrect (at -4.65 1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at -4.65 0 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 4 smd roundrect (at -4.65 -1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -4.65 -2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -4.65 -3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /SDA))
    (pad 1 smd roundrect (at -4.65 -5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /SCL))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 104.3305 180.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R32 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 70 /M24))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 89.7255 180.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R31 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 69 /M23))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 75.1205 180.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R30 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 68 /M22))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 60.5155 180.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R29 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 67 /M21))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 45.9105 180.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R28 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 66 /M20))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 31.3055 180.848 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R27 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 65 /M19))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 104.3305 168.148 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 64 /M18))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 89.7255 168.148 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 63 /M17))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 75.1205 168.148 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 62 /M16))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 60.5155 168.148 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 61 /M15))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 45.9105 168.148 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 60 /M14))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 31.3055 168.148 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 59 /M13))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 104.3305 155.448 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 58 /M12))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 89.7255 155.448 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 57 /M11))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 75.1205 155.448 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 56 /M10))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 60.5155 155.448 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 55 /M9))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 45.9105 155.448 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 49 /M8))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 31.3055 155.448 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 50 /M7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 104.3305 142.748 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 51 /M6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 89.7255 142.748 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 52 /M5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 101.1555 180.213 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q24 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 101 "/Motor Channel 24/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 70 /M24))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 86.5505 180.213 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q23 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 100 "/Motor Channel 23/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 69 /M23))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 71.9455 180.213 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q22 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 99 "/Motor Channel 22/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 68 /M22))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 57.3405 180.213 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q21 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 98 "/Motor Channel 21/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 67 /M21))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 42.7355 180.213 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q20 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 97 "/Motor Channel 20/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 66 /M20))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 28.1305 180.213 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q19 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 96 "/Motor Channel 19/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 65 /M19))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 101.1555 167.513 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q18 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 95 "/Motor Channel 18/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 64 /M18))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 86.5505 167.513 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q17 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 94 "/Motor Channel 17/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 63 /M17))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 71.9455 167.513 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q16 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 93 "/Motor Channel 16/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 62 /M16))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 57.3405 167.513 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q15 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 92 "/Motor Channel 15/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 61 /M15))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 42.7355 167.513 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q14 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 91 "/Motor Channel 14/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 60 /M14))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 28.1305 167.513 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q13 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 90 "/Motor Channel 13/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 59 /M13))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 101.1555 154.813 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q12 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 89 "/Motor Channel 12/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 58 /M12))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 86.5505 154.813 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q11 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 88 "/Motor Channel 11/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 57 /M11))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 71.9455 154.813 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q10 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 87 "/Motor Channel 10/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 56 /M10))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 57.3405 154.813 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q9 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 86 "/Motor Channel 9/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 55 /M9))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 42.7355 154.813 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q8 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 85 "/Motor Channel 8/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 49 /M8))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 28.1305 154.813 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q7 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 84 "/Motor Channel 7/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 50 /M7))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 101.1555 142.113 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q6 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 83 "/Motor Channel 6/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 51 /M6))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 86.5505 142.113 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q5 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 82 "/Motor Channel 5/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 52 /M5))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 99.2505 185.928)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J26 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 101 "/Motor Channel 24/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 84.6455 185.928)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J25 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 100 "/Motor Channel 23/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 70.0405 185.928)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J24 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 99 "/Motor Channel 22/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 55.4355 185.928)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J23 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 98 "/Motor Channel 21/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 40.8305 185.928)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J22 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 97 "/Motor Channel 20/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 26.2255 185.928)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J21 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 96 "/Motor Channel 19/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 99.2505 173.228)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J20 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 95 "/Motor Channel 18/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 84.6455 173.228)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J19 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 94 "/Motor Channel 17/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 70.0405 173.228)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J18 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 93 "/Motor Channel 16/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 55.4355 173.228)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J17 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 92 "/Motor Channel 15/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 40.8305 173.228)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J16 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 91 "/Motor Channel 14/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 26.2255 173.228)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J15 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 90 "/Motor Channel 13/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 99.2505 160.528)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J14 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 89 "/Motor Channel 12/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 84.6455 160.528)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J13 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 88 "/Motor Channel 11/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 70.0405 160.528)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J12 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 87 "/Motor Channel 10/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 55.4355 160.528)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J11 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 86 "/Motor Channel 9/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 40.8305 160.528)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J10 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 85 "/Motor Channel 8/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 26.2255 160.528)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J9 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 84 "/Motor Channel 7/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 99.2505 147.828)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J8 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 83 "/Motor Channel 6/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 84.6455 147.828)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J7 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 82 "/Motor Channel 5/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_HC49-SD_HandSoldering (layer Front) (tedit 5A1AD52C)
    (at 67.7545 126.3965 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, hand-soldering, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 0 -3.55 90) (layer F.SilkS))
    (fp_text value Crystal (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at -7.493 -3.4925 90) (layer F.Fab))
    (pad 2 smd rect (at 5.9375 0 90) (size 7.875 2) (layers Front F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at -5.9375 0 90) (size 7.875 2) (layers Front F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm (layer Front) (tedit 5D9F72B1)
    (at 28.7655 129.413 270)
    (descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0 -6.72 90) (layer F.SilkS))
    (fp_text value MCP23008-xSO (at 0 6.72 90) (layer F.Fab))
    (fp_text user %R (at 6.985 5.1435 180) (layer F.Fab))
    (pad 18 smd roundrect (at 4.65 -5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 17 smd roundrect (at 4.65 -3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /M2))
    (pad 16 smd roundrect (at 4.65 -2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 /M8))
    (pad 15 smd roundrect (at 4.65 -1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 /M14))
    (pad 14 smd roundrect (at 4.65 0 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /M20))
    (pad 13 smd roundrect (at 4.65 1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /M1))
    (pad 12 smd roundrect (at 4.65 2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /M7))
    (pad 11 smd roundrect (at 4.65 3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 /M13))
    (pad 10 smd roundrect (at 4.65 5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 /M19))
    (pad 9 smd roundrect (at -4.65 5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 8 smd roundrect (at -4.65 3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U3-Pad8)"))
    (pad 7 smd roundrect (at -4.65 2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(U3-Pad7)"))
    (pad 6 smd roundrect (at -4.65 1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at -4.65 0 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 4 smd roundrect (at -4.65 -1.27 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -4.65 -2.54 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -4.65 -3.81 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /SDA))
    (pad 1 smd roundrect (at -4.65 -5.08 270) (size 2.05 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /SCL))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-18W_7.5x11.6mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer Front) (tedit 5A02F146)
    (at 78.9305 128.778 270)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (clearance 0.1524)
    (attr smd)
    (fp_text reference U2 (at 0 -7.45 90) (layer F.SilkS))
    (fp_text value ATmega32U4RC-AU (at 0 7.45 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0.1905 180) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 48 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -5.7 -3.2 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 8 VBUS))
    (pad 3 smd rect (at -5.7 -2.4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 104 /MCU_D-))
    (pad 4 smd rect (at -5.7 -1.6 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 105 /MCU_D+))
    (pad 5 smd rect (at -5.7 -0.8 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -5.7 0 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 7 smd rect (at -5.7 0.8 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 8 VBUS))
    (pad 8 smd rect (at -5.7 1.6 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 47 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -5.7 2.4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 17 /SCK))
    (pad 10 smd rect (at -5.7 3.2 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 16 /MOSI))
    (pad 11 smd rect (at -5.7 4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 18 /MISO))
    (pad 12 smd rect (at -4 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 46 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at -3.2 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 15 /RST))
    (pad 14 smd rect (at -2.4 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at -1.6 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.8 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 17 smd rect (at 0 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 18 smd rect (at 0.8 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 24 /SCL))
    (pad 19 smd rect (at 1.6 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 23 /SDA))
    (pad 20 smd rect (at 2.4 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 45 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 3.2 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 44 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 4 5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 23 smd rect (at 5.7 4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 24 smd rect (at 5.7 3.2 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 3 +3V3))
    (pad 25 smd rect (at 5.7 2.4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 43 "Net-(U2-Pad25)"))
    (pad 26 smd rect (at 5.7 1.6 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 42 "Net-(U2-Pad26)"))
    (pad 27 smd rect (at 5.7 0.8 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 41 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 5.7 0 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 40 "Net-(U2-Pad28)"))
    (pad 29 smd rect (at 5.7 -0.8 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 39 "Net-(U2-Pad29)"))
    (pad 30 smd rect (at 5.7 -1.6 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 38 "Net-(U2-Pad30)"))
    (pad 31 smd rect (at 5.7 -2.4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 37 "Net-(U2-Pad31)"))
    (pad 32 smd rect (at 5.7 -3.2 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 36 "Net-(U2-Pad32)"))
    (pad 33 smd rect (at 5.7 -4 270) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 35 "Net-(U2-Pad33)"))
    (pad 34 smd rect (at 4 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 3 +3V3))
    (pad 35 smd rect (at 3.2 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 2.4 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 34 "Net-(U2-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 33 "Net-(U2-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 32 "Net-(U2-Pad38)"))
    (pad 39 smd rect (at 0 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 31 "Net-(U2-Pad39)"))
    (pad 40 smd rect (at -0.8 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 30 "Net-(U2-Pad40)"))
    (pad 41 smd rect (at -1.6 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 29 "Net-(U2-Pad41)"))
    (pad 42 smd rect (at -2.4 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 43 smd rect (at -3.2 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 44 smd rect (at -4 -5.7) (size 1.5 0.55) (layers Front F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer Front) (tedit 5D9F72B1)
    (at 35.7505 110.363 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -4.445 0 180) (layer F.SilkS))
    (fp_text value LM2594M-3.3 (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(U1-Pad1)"))
    (pad 2 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(U1-Pad2)"))
    (pad 3 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(U1-Pad3)"))
    (pad 4 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 5 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 "Net-(U1-Pad5)"))
    (pad 6 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +12V))
    (pad 8 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /SWITCH_OUT))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_Push_1P1T_NO_6x6mm_H9.5mm (layer Front) (tedit 5CA1CA7F)
    (at 99.8855 130.683)
    (descr "tactile push button, 6x6mm e.g. PTS645xx series, height=9.5mm")
    (tags "tact sw push 6mm smd")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.05) (layer F.SilkS))
    (fp_text value SW_Push (at 0 4.15) (layer F.Fab))
    (fp_text user %R (at 0 -4.05) (layer F.Fab))
    (pad 2 smd rect (at 3.975 2.25) (size 1.55 1.3) (layers Front F.Paste F.Mask)
      (net 15 /RST))
    (pad 1 smd rect (at 3.975 -2.25) (size 1.55 1.3) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.975 -2.25) (size 1.55 1.3) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.975 2.25) (size 1.55 1.3) (layers Front F.Paste F.Mask)
      (net 15 /RST))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_PUSH_6mm_H9.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 75.1205 142.748 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 22 /M4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 60.5155 142.748 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 21 /M3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 45.9105 142.748 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 20 /M2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 31.3055 142.748 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -2.81 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 19 /M1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 103.0605 123.698 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 9 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1 0 270) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 60.5155 120.523 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 24 /SCL))
    (pad 1 smd roundrect (at -1 0 180) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 56.0705 120.523)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 1.905) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 23 /SDA))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 102.6955 136.398)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at -0.27 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 15 /RST))
    (pad 1 smd roundrect (at -1 0) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 66.8655 109.728 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 76 /D+))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 105 /MCU_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 69.4055 109.728 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 77 /D-))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 104 /MCU_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 64.3255 109.728 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 11 "Net-(J1-PadB5)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder (layer Front) (tedit 5F68FEEE)
    (at 71.9455 109.728 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 5.1K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 14 "Net-(J1-PadA5)"))
    (pad 1 smd roundrect (at -1 0 90) (size 1.2 1.4) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 71.9455 142.113 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q4 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 81 "/Motor Channel 4/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 22 /M4))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 57.3405 142.113 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q3 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 80 "/Motor Channel 3/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 21 /M3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 42.7355 142.113 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q2 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 79 "/Motor Channel 2/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 20 /M2))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-323_SC-70 (layer Front) (tedit 5A02FF57)
    (at 28.1305 142.113 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference Q1 (at 3.175 0) (layer F.SilkS))
    (fp_text value BSS214NW (at -0.05 2.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 78 "/Motor Channel 1/DRAIN"))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers Front F.Paste F.Mask)
      (net 19 /M1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Bourns_SRR1210A (layer Front) (tedit 5B853E9E)
    (at 26.2255 110.363 270)
    (descr "Bourns SRR1210A series SMD inductor https://www.bourns.com/docs/Product-Datasheets/SRR1210A.pdf")
    (tags "Bourns SRR1210A SMD inductor")
    (attr smd)
    (fp_text reference L1 (at -7.366 5.2705 90) (layer F.SilkS))
    (fp_text value 150uH (at 0 7.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -5.05 0 270) (size 2.8 5.3) (layers Front F.Paste F.Mask)
      (net 75 /SWITCH_OUT))
    (pad 2 smd rect (at 5.05 0 270) (size 2.8 5.3) (layers Front F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Bourns_SRR1210A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 70.0405 147.828)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J6 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 81 "/Motor Channel 4/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 55.4355 147.828)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J5 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 80 "/Motor Channel 3/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 40.8305 147.828)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J4 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 79 "/Motor Channel 2/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Hirose_Mark:Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical (layer Front) (tedit 617508FB)
    (at 26.2255 147.828)
    (descr "Hirose  series connector, DF3EA-02P-2V (https://www.hirose.com/en/product/document?clcode=CL0543-0315-0-21&productname=DF3EA-2P-2V(21)&series=DF3&documenttype=2DDrawing&lang=en&documentid=0001162002), generated with kicad-footprint-generator")
    (tags "connector Hirose  vertical")
    (attr smd)
    (fp_text reference J3 (at -6.35 -5.08) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.92) (layer F.Fab))
    (fp_text user ${REFERENCE} (at 0 1.92) (layer F.Fab))
    (pad MP smd roundrect (at 5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad MP smd roundrect (at -5.52 2.05) (size 2.3 3.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.108695652173913))
    (pad 2 smd roundrect (at 1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 78 "/Motor Channel 1/DRAIN"))
    (pad 1 smd roundrect (at -1 -2.4) (size 1.2 2.6) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2083325)
      (net 2 +12V))
    (model ${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF3EA-02P-2V_1x02-1MP_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer Front) (tedit 59FED5CC)
    (at 97.3455 117.983 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /RST))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /MOSI))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCK))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /MISO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_C_Receptacle_GCT_USB4085 (layer Front) (tedit 5BCCCD93)
    (at 72.5805 105.918 180)
    (descr "USB 2.0 Type C Receptacle, https://gct.co/Files/Drawings/USB4085.pdf")
    (tags "USB Type-C Receptacle Through-hole Right angle")
    (clearance 0.1016)
    (fp_text reference J1 (at -3.6195 1.016) (layer F.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0 (at 2.975 9.925) (layer F.Fab))
    (fp_text user %R (at 2.975 4.025) (layer F.Fab))
    (fp_text user "PCB Edge" (at 2.975 6.1) (layer Dwgs.User))
    (pad S1 thru_hole oval (at 7.3 4.36 180) (size 0.9 1.7) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -1.35 4.36 180) (size 0.9 1.7) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at 7.3 0.98 180) (size 0.9 2.4) (drill oval 0.6 2.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S1 thru_hole oval (at -1.35 0.98 180) (size 0.9 2.4) (drill oval 0.6 2.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B6 thru_hole circle (at 3.4 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 76 /D+))
    (pad B1 thru_hole circle (at 5.95 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B4 thru_hole circle (at 5.1 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 103 /FUSE))
    (pad B5 thru_hole circle (at 4.25 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-PadB5)"))
    (pad B12 thru_hole circle (at 0 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B8 thru_hole circle (at 1.7 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-PadB8)"))
    (pad B7 thru_hole circle (at 2.55 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 77 /D-))
    (pad B9 thru_hole circle (at 0.85 1.35 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 103 /FUSE))
    (pad A12 thru_hole circle (at 5.95 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A9 thru_hole circle (at 5.1 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 103 /FUSE))
    (pad A8 thru_hole circle (at 4.25 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadA8)"))
    (pad A7 thru_hole circle (at 3.4 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 77 /D-))
    (pad A6 thru_hole circle (at 2.55 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 76 /D+))
    (pad A5 thru_hole circle (at 1.7 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-PadA5)"))
    (pad A4 thru_hole circle (at 0.85 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 103 /FUSE))
    (pad A1 thru_hole circle (at 0 0 180) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4085.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer Front) (tedit 5F68FEF1)
    (at 74.4855 109.728 90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (attr smd)
    (fp_text reference F1 (at -3.429 0.0635 90) (layer F.SilkS))
    (fp_text value Fuse (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 103 /FUSE))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 8 VBUS))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_PLCC-2 (layer Front) (tedit 59959404)
    (at 99.2505 123.698)
    (descr "LED PLCC-2 SMD package")
    (tags "LED PLCC-2 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value LED (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0) (size 1.5 2.6) (layers Front F.Paste F.Mask)
      (net 9 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.5 0) (size 1.5 2.6) (layers Front F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_PLCC-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer Front) (tedit 58645DC7)
    (at 35.1155 102.743)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS))
    (fp_text value B130-E3 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers Front F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers Front F.Paste F.Mask)
      (net 75 /SWITCH_OUT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 87.8205 131.953 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 84.6455 119.253)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 8 VBUS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 76.3905 119.253 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.68) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 87.8205 126.238 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 1.905 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 63.9445 122.809 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at -3.048 -0.0635 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder (layer Front) (tedit 5F68FEEF)
    (at 63.9445 130.429 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at -3.048 -0.0635 90) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.68 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2127659574468085)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_10x10 (layer Front) (tedit 5BCA39D1)
    (at 44.6405 116.078 90)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 10.0x10.0mm")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at 0 -6.2 90) (layer F.SilkS))
    (fp_text value 220uF (at 0 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 4 0 90) (size 4 2.5) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 1 smd roundrect (at -4 0 90) (size 4 2.5) (layers Front F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_Elec_8x10.2 (layer Front) (tedit 5BC8D926)
    (at 44.6405 103.378 270)
    (descr "SMD capacitor, aluminum electrolytic nonpolar, 8.0x10.2mm")
    (tags "capacitor electrolyic nonpolar")
    (attr smd)
    (fp_text reference C1 (at 0 -5.2 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 5.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 3.6 0 270) (size 4.5 2.1) (layers Front F.Paste F.Mask) (roundrect_rratio 0.119047619047619)
      (net 1 GND))
    (pad 1 smd roundrect (at -3.6 0 270) (size 4.5 2.1) (layers Front F.Paste F.Mask) (roundrect_rratio 0.119047619047619)
      (net 2 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_Elec_8x10.2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Steve PCB III" (at 91.44 108.966) (layer F.SilkS))
  (gr_text 21 (at 94.996 183.769) (layer F.SilkS))
  (gr_text 17 (at 80.391 183.769) (layer F.SilkS))
  (gr_text 13 (at 65.786 183.769) (layer F.SilkS))
  (gr_text 9 (at 51.181 183.769) (layer F.SilkS))
  (gr_text 5 (at 36.576 183.769) (layer F.SilkS))
  (gr_text 1 (at 21.971 183.769) (layer F.SilkS))
  (gr_text 22 (at 94.996 171.069) (layer F.SilkS))
  (gr_text 18 (at 80.391 171.069) (layer F.SilkS))
  (gr_text 14 (at 65.786 171.069) (layer F.SilkS))
  (gr_text 10 (at 51.181 171.069) (layer F.SilkS))
  (gr_text 6 (at 36.576 171.069) (layer F.SilkS))
  (gr_text 2 (at 21.971 171.069) (layer F.SilkS))
  (gr_text 23 (at 94.996 158.369) (layer F.SilkS))
  (gr_text 19 (at 80.391 158.369) (layer F.SilkS))
  (gr_text 15 (at 65.786 158.369) (layer F.SilkS))
  (gr_text 11 (at 51.181 158.369) (layer F.SilkS))
  (gr_text 7 (at 36.576 158.369) (layer F.SilkS))
  (gr_text 3 (at 21.971 158.369) (layer F.SilkS))
  (gr_text 24 (at 94.996 145.669) (layer F.SilkS))
  (gr_text 20 (at 80.391 145.669) (layer F.SilkS))
  (gr_text 16 (at 65.786 145.669) (layer F.SilkS))
  (gr_text 12 (at 51.181 145.669) (layer F.SilkS))
  (gr_text 8 (at 36.576 145.669) (layer F.SilkS))
  (gr_text 4 (at 21.971 145.669) (layer F.SilkS))
  (gr_line (start 107.315 97.155) (end 18.415 97.155) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 107.315 191.77) (end 107.315 97.155) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 18.415 191.77) (end 107.315 191.77) (layer Edge.Cuts) (width 0.0381))
  (gr_line (start 18.415 191.77) (end 18.415 97.155) (layer Edge.Cuts) (width 0.0381))
  (zone (net 75) (net_name /SWITCH_OUT) (layer Front) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.4805 109.093) (xy 33.2105 109.093) (xy 33.2105 104.013) (xy 28.7655 104.013) (xy 28.7655 107.188)
        (xy 23.0505 107.188) (xy 23.0505 102.108) (xy 34.4805 102.108)
      )
    )
  )
  (zone (net 2) (net_name +12V) (layer Front) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45.592108 97.843502) (xy 59.4995 109.728) (xy 59.4995 112.268) (xy 57.9755 114.046) (xy 49.8475 114.046)
        (xy 48.0695 112.268) (xy 48.0695 104.394) (xy 45.5295 101.854) (xy 45.5295 101.6) (xy 35.8775 101.6)
        (xy 35.8775 106.172) (xy 35.3695 106.934) (xy 35.3695 108.712) (xy 34.8615 108.712) (xy 34.913555 101.6)
        (xy 22.611723 101.6635) (xy 22.600278 143.7005) (xy 106.68 143.637) (xy 106.68 191.135) (xy 19.05 191.135)
        (xy 19.05 97.79) (xy 45.593 97.79)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer Front) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.1635 114.046) (xy 38.1635 118.11) (xy 45.7835 118.11) (xy 45.7835 121.92) (xy 23.6855 121.92)
        (xy 23.6855 114.046) (xy 28.7655 114.046) (xy 28.7655 118.11) (xy 37.1475 118.11) (xy 37.1475 114.046)
        (xy 37.6555 113.538)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.2115 104.902) (xy 45.7835 104.902) (xy 45.7835 114.046) (xy 43.4975 114.046) (xy 39.9415 111.252)
        (xy 36.1315 111.252) (xy 36.1315 106.934) (xy 36.3855 106.68) (xy 36.3855 102.362) (xy 36.6395 102.235)
        (xy 38.6715 102.235)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.8825 153.9875) (xy 75.8825 154.8765) (xy 75.565 155.194) (xy 73.5965 155.194) (xy 72.5805 154.3685)
        (xy 72.5805 153.9875) (xy 73.2155 153.3525) (xy 75.2475 153.3525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.4875 153.9875) (xy 90.4875 154.8765) (xy 90.17 155.194) (xy 88.2015 155.194) (xy 87.1855 154.3685)
        (xy 87.1855 153.9875) (xy 87.8205 153.3525) (xy 89.8525 153.3525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.0925 153.9875) (xy 105.0925 154.8765) (xy 104.775 155.194) (xy 102.8065 155.194) (xy 101.7905 154.3685)
        (xy 101.7905 153.9875) (xy 102.4255 153.3525) (xy 104.4575 153.3525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.0675 166.6875) (xy 32.0675 167.5765) (xy 31.75 167.894) (xy 29.7815 167.894) (xy 28.7655 167.0685)
        (xy 28.7655 166.6875) (xy 29.4005 166.0525) (xy 31.4325 166.0525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.6725 166.6875) (xy 46.6725 167.5765) (xy 46.355 167.894) (xy 44.3865 167.894) (xy 43.3705 167.0685)
        (xy 43.3705 166.6875) (xy 44.0055 166.0525) (xy 46.0375 166.0525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.2775 166.6875) (xy 61.2775 167.5765) (xy 60.96 167.894) (xy 58.9915 167.894) (xy 57.9755 167.0685)
        (xy 57.9755 166.6875) (xy 58.6105 166.0525) (xy 60.6425 166.0525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.8825 166.6875) (xy 75.8825 167.5765) (xy 75.565 167.894) (xy 73.5965 167.894) (xy 72.5805 167.0685)
        (xy 72.5805 166.6875) (xy 73.2155 166.0525) (xy 75.2475 166.0525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.4875 166.6875) (xy 90.4875 167.5765) (xy 90.17 167.894) (xy 88.2015 167.894) (xy 87.1855 167.0685)
        (xy 87.1855 166.6875) (xy 87.8205 166.0525) (xy 89.8525 166.0525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.0925 166.6875) (xy 105.0925 167.5765) (xy 104.775 167.894) (xy 102.8065 167.894) (xy 101.7905 167.0685)
        (xy 101.7905 166.6875) (xy 102.4255 166.0525) (xy 104.4575 166.0525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.0675 179.3875) (xy 32.0675 180.2765) (xy 31.75 180.594) (xy 29.7815 180.594) (xy 28.7655 179.7685)
        (xy 28.7655 179.3875) (xy 29.4005 178.7525) (xy 31.4325 178.7525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.6725 141.2875) (xy 46.6725 142.1765) (xy 46.355 142.494) (xy 44.3865 142.494) (xy 43.3705 141.6685)
        (xy 43.3705 141.2875) (xy 44.0055 140.6525) (xy 46.0375 140.6525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.6725 179.3875) (xy 46.6725 180.2765) (xy 46.355 180.594) (xy 44.3865 180.594) (xy 43.3705 179.7685)
        (xy 43.3705 179.3875) (xy 44.0055 178.7525) (xy 46.0375 178.7525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.2775 179.3875) (xy 61.2775 180.2765) (xy 60.96 180.594) (xy 58.9915 180.594) (xy 57.9755 179.7685)
        (xy 57.9755 179.3875) (xy 58.6105 178.7525) (xy 60.6425 178.7525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.8825 179.3875) (xy 75.8825 180.2765) (xy 75.565 180.594) (xy 73.5965 180.594) (xy 72.5805 179.7685)
        (xy 72.5805 179.3875) (xy 73.2155 178.7525) (xy 75.2475 178.7525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.4875 179.3875) (xy 90.4875 180.2765) (xy 90.17 180.594) (xy 88.2015 180.594) (xy 87.1855 179.7685)
        (xy 87.1855 179.3875) (xy 87.8205 178.7525) (xy 89.8525 178.7525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.0925 179.3875) (xy 105.0925 180.2765) (xy 104.775 180.594) (xy 102.8065 180.594) (xy 101.7905 179.7685)
        (xy 101.7905 179.3875) (xy 102.4255 178.7525) (xy 104.4575 178.7525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.2775 141.2875) (xy 61.2775 142.1765) (xy 60.96 142.494) (xy 58.9915 142.494) (xy 57.9755 141.6685)
        (xy 57.9755 141.2875) (xy 58.6105 140.6525) (xy 60.6425 140.6525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75.8825 141.2875) (xy 75.8825 142.1765) (xy 75.565 142.494) (xy 73.5965 142.494) (xy 72.5805 141.6685)
        (xy 72.5805 141.2875) (xy 73.2155 140.6525) (xy 75.2475 140.6525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.4875 141.2875) (xy 90.4875 142.1765) (xy 90.17 142.494) (xy 88.2015 142.494) (xy 87.1855 141.6685)
        (xy 87.1855 141.2875) (xy 87.8205 140.6525) (xy 89.8525 140.6525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.0925 141.2875) (xy 105.0925 142.1765) (xy 104.775 142.494) (xy 102.8065 142.494) (xy 101.7905 141.6685)
        (xy 101.7905 141.2875) (xy 102.4255 140.6525) (xy 104.4575 140.6525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.0675 153.9875) (xy 32.0675 154.8765) (xy 31.75 155.194) (xy 29.7815 155.194) (xy 28.7655 154.3685)
        (xy 28.7655 153.9875) (xy 29.4005 153.3525) (xy 31.4325 153.3525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.6725 153.9875) (xy 46.6725 154.8765) (xy 46.355 155.194) (xy 44.3865 155.194) (xy 43.3705 154.3685)
        (xy 43.3705 153.9875) (xy 44.0055 153.3525) (xy 46.0375 153.3525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61.2775 153.9875) (xy 61.2775 154.8765) (xy 60.96 155.194) (xy 58.9915 155.194) (xy 57.9755 154.3685)
        (xy 57.9755 153.9875) (xy 58.6105 153.3525) (xy 60.6425 153.3525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Front) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.0675 141.2875) (xy 32.0675 142.1765) (xy 31.75 142.494) (xy 29.7815 142.494) (xy 28.7655 141.6685)
        (xy 28.7655 141.2875) (xy 29.4005 140.6525) (xy 31.4325 140.6525)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.68 191.135) (xy 19.05 191.135) (xy 19.05 97.79) (xy 106.68 97.79)
      )
    )
  )
)
