(kicad_pcb (version 20171130) (host pcbnew 5.1.3-ffb9f22~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 36)
    (tracks 84)
    (zones 0)
    (modules 17)
    (nets 19)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.1524)
    (zone_clearance 0.4064)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.8 0.4)
    (user_via 1.6 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.51 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDA)
  (net 2 VCCA)
  (net 3 "/Child Board/CLK_A")
  (net 4 "/Child Board/LATCH_A")
  (net 5 "/Child Board/SLOW_DATA_A")
  (net 6 "/Child Board/FAST_DATA_A")
  (net 7 "/Child Board/CLK_B")
  (net 8 "/Child Board/LATCH_B")
  (net 9 "/Child Board/SLOW_DATA_B")
  (net 10 "/Child Board/FAST_DATA_B")
  (net 11 "/Child Board/S_OR_NES_A")
  (net 12 "/Child Board/S_OR_NES_B")
  (net 13 "/Child Board/ENABLE_B")
  (net 14 "/Child Board/ENABLE_A")
  (net 15 "Net-(U3-Pad8)")
  (net 16 "Net-(JP9-Pad2)")
  (net 17 "Net-(JP8-Pad2)")
  (net 18 "Net-(U4-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/Child Board/CLK_A")
    (add_net "/Child Board/CLK_B")
    (add_net "/Child Board/ENABLE_A")
    (add_net "/Child Board/ENABLE_B")
    (add_net "/Child Board/FAST_DATA_A")
    (add_net "/Child Board/FAST_DATA_B")
    (add_net "/Child Board/LATCH_A")
    (add_net "/Child Board/LATCH_B")
    (add_net "/Child Board/SLOW_DATA_A")
    (add_net "/Child Board/SLOW_DATA_B")
    (add_net "/Child Board/S_OR_NES_A")
    (add_net "/Child Board/S_OR_NES_B")
    (add_net "Net-(JP8-Pad2)")
    (add_net "Net-(JP9-Pad2)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U4-Pad8)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.5)
    (via_dia 1.6)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDA)
    (add_net VCCA)
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58E0A804)
    (at 128.825 128.27)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 9 "/Child Board/SLOW_DATA_B"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:square_logo (layer Top) (tedit 0)
    (at 148.59 132.461)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module controllerpro:PinHeader_1x08_P2.54mm_Vertical (layer Bottom) (tedit 59FED5CC)
    (at 179.705 137.795 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P2 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x08_Male (at 0 -20.11 270) (layer B.Fab))
    (fp_text user %R (at 0 -8.89 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/Child Board/FAST_DATA_A"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/Child Board/S_OR_NES_A"))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/Child Board/SLOW_DATA_A"))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/Child Board/LATCH_A"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/Child Board/CLK_A"))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/Child Board/ENABLE_A"))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCCA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t32_ref:SOLDERJUMPER (layer Top) (tedit 0)
    (at 137.795 128.27)
    (fp_text reference JP7 (at 0 0) (layer F.Fab))
    (fp_text value SolderJumper_2_Open (at -1.524 1.651) (layer F.Fab))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 1 GNDA) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 12 "/Child Board/S_OR_NES_B") (solder_mask_margin 0.1016))
  )
  (module t32_ref:SOLDERJUMPER (layer Top) (tedit 0)
    (at 134.493 128.27)
    (fp_text reference JP6 (at 0 0) (layer F.Fab))
    (fp_text value SolderJumper_2_Open (at -1.524 1.651) (layer F.Fab))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 12 "/Child Board/S_OR_NES_B") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 2 VCCA) (solder_mask_margin 0.1016))
  )
  (module logos:qrcode (layer Bottom) (tedit 0)
    (at 147.828 132.334 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module t32_ref:SOLDERJUMPER (layer Top) (tedit 0)
    (at 183.642 128.27)
    (fp_text reference JP4 (at 0 0) (layer F.Fab))
    (fp_text value SolderJumper_2_Open (at -1.524 1.651) (layer F.Fab))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 1 GNDA) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 11 "/Child Board/S_OR_NES_A") (solder_mask_margin 0.1016))
  )
  (module t32_ref:SOLDERJUMPER (layer Bottom) (tedit 0)
    (at 111.76 136.398 270)
    (fp_text reference JP5 (at 0 0 270) (layer B.Fab))
    (fp_text value SolderJumper_2_Bridged (at -1.524 -1.651 270) (layer B.Fab))
    (pad 1 smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 12 "/Child Board/S_OR_NES_B") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 12 "/Child Board/S_OR_NES_B") (solder_mask_margin 0.1016))
  )
  (module t32_ref:SOLDERJUMPER (layer Bottom) (tedit 0)
    (at 157.48 136.525 270)
    (fp_text reference JP2 (at 0 0 270) (layer B.Fab))
    (fp_text value SolderJumper_2_Bridged (at -1.524 -1.651 270) (layer B.Fab))
    (pad 2 smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 11 "/Child Board/S_OR_NES_A") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 11 "/Child Board/S_OR_NES_A") (solder_mask_margin 0.1016))
  )
  (module t32_ref:SOLDERJUMPER (layer Top) (tedit 0)
    (at 180.34 128.27)
    (fp_text reference JP3 (at 0 0) (layer F.Fab))
    (fp_text value SolderJumper_2_Open (at -1.524 1.651) (layer F.Fab))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 11 "/Child Board/S_OR_NES_A") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers Top F.Mask)
      (net 2 VCCA) (solder_mask_margin 0.1016))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer Bottom) (tedit 59FED5CC)
    (at 133.985 137.795 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference P1 (at 0 2.33 90) (layer B.SilkS))
    (fp_text value Conn_01x08_Male (at 0 -20.11 90) (layer B.Fab))
    (fp_text user %R (at 0 -8.89 180) (layer B.Fab))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCCA))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/Child Board/ENABLE_B"))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/Child Board/CLK_B"))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/Child Board/LATCH_B"))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/Child Board/SLOW_DATA_B"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/Child Board/S_OR_NES_B"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/Child Board/FAST_DATA_B"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Top) (tedit 58E0A804)
    (at 174.625 128.27)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 5 "/Child Board/SLOW_DATA_A"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers Top F.Paste F.Mask)
      (net 1 GNDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t32_ref:SOLDERJUMPER (layer Bottom) (tedit 0)
    (at 112.903 128.905 180)
    (fp_text reference JP9 (at 0 0) (layer B.Fab))
    (fp_text value SolderJumper_2_Open (at -1.524 -1.651) (layer B.Fab))
    (pad 2 smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 16 "Net-(JP9-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 13 "/Child Board/ENABLE_B") (solder_mask_margin 0.1016))
  )
  (module controllerpro:NINTENDO-MULTI (layer Top) (tedit 5C8B19A0)
    (at 169.545 132.715)
    (fp_text reference U3 (at 22.86 -10.16 180) (layer F.Fab))
    (fp_text value NINTENDO-MULTI_LARGE (at -5.08 8.89 180) (layer F.Fab))
    (fp_text user "(N64)" (at 8.382 1.778) (layer F.SilkS))
    (fp_text user DAT (at 10.16 -1.905) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 23.7744 0) (layer Cmts.User))
    (fp_text user GND (at 14.224 -1.905) (layer F.SilkS))
    (fp_text user VCC (at 6.35 -1.905) (layer F.SilkS))
    (fp_text user VCC (at -11.938 2.159) (layer F.SilkS))
    (fp_text user GND (at -11.938 -1.905) (layer F.SilkS))
    (fp_text user VCC (at -7.874 -6.096) (layer F.SilkS))
    (fp_text user DAT (at -0.127 -1.905) (layer F.SilkS))
    (fp_text user LAT (at -3.937 -1.905) (layer F.SilkS))
    (fp_text user CLK (at -8.001 -1.905) (layer F.SilkS))
    (fp_text user X (at -3.937 -6.096) (layer F.SilkS))
    (fp_text user X (at 0 -6.096) (layer F.SilkS))
    (fp_text user "(SNES)" (at -9.652 1.778) (layer F.SilkS))
    (pad 1 thru_hole circle (at -11.8872 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 11 "/Child Board/S_OR_NES_A"))
    (pad 2 thru_hole circle (at -7.9248 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "/Child Board/CLK_A"))
    (pad 3 thru_hole circle (at -3.9624 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 "/Child Board/LATCH_A"))
    (pad 4 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 "/Child Board/SLOW_DATA_A"))
    (pad 5 thru_hole circle (at 6.35 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 VCCA))
    (pad 6 thru_hole circle (at 10.3124 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 6 "/Child Board/FAST_DATA_A"))
    (pad 7 thru_hole circle (at 14.2748 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 8 thru_hole circle (at 0 -4.064) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 15 "Net-(U3-Pad8)"))
    (pad 9 thru_hole circle (at -3.9624 -3.9624) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 17 "Net-(JP8-Pad2)"))
    (pad 10 thru_hole circle (at -7.9248 -3.9624) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 14 "/Child Board/ENABLE_A"))
  )
  (module logos:nes_advantage (layer Bottom) (tedit 0)
    (at 133.858 128.778 180)
    (fp_text reference G*** (at 0.635 1.27) (layer B.SilkS) hide)
    (fp_text value LOGO (at 1.385 1.27) (layer B.SilkS) hide)
  )
  (module controllerpro:NINTENDO-MULTI (layer Top) (tedit 5C8B19A0)
    (at 123.825 132.715)
    (fp_text reference U4 (at 22.86 -10.16 180) (layer F.Fab))
    (fp_text value NINTENDO-MULTI_LARGE (at -5.08 8.89 180) (layer F.Fab))
    (fp_text user "(N64)" (at 8.382 1.778) (layer F.SilkS))
    (fp_text user DAT (at 10.16 -1.905) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 23.7744 0) (layer Cmts.User))
    (fp_text user GND (at 14.224 -1.905) (layer F.SilkS))
    (fp_text user VCC (at 6.35 -1.905) (layer F.SilkS))
    (fp_text user VCC (at -11.938 2.159) (layer F.SilkS))
    (fp_text user GND (at -11.938 -1.905) (layer F.SilkS))
    (fp_text user VCC (at -7.874 -6.096) (layer F.SilkS))
    (fp_text user DAT (at -0.127 -1.905) (layer F.SilkS))
    (fp_text user LAT (at -3.937 -1.905) (layer F.SilkS))
    (fp_text user CLK (at -8.001 -1.905) (layer F.SilkS))
    (fp_text user X (at -3.937 -6.096) (layer F.SilkS))
    (fp_text user X (at 0 -6.096) (layer F.SilkS))
    (fp_text user "(SNES)" (at -9.652 1.778) (layer F.SilkS))
    (pad 1 thru_hole circle (at -11.8872 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 12 "/Child Board/S_OR_NES_B"))
    (pad 2 thru_hole circle (at -7.9248 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 "/Child Board/CLK_B"))
    (pad 3 thru_hole circle (at -3.9624 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 8 "/Child Board/LATCH_B"))
    (pad 4 thru_hole circle (at 0 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 9 "/Child Board/SLOW_DATA_B"))
    (pad 5 thru_hole circle (at 6.35 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 VCCA))
    (pad 6 thru_hole circle (at 10.3124 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 10 "/Child Board/FAST_DATA_B"))
    (pad 7 thru_hole circle (at 14.2748 0) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 GNDA))
    (pad 8 thru_hole circle (at 0 -4.064) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 18 "Net-(U4-Pad8)"))
    (pad 9 thru_hole circle (at -3.9624 -3.9624) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 16 "Net-(JP9-Pad2)"))
    (pad 10 thru_hole circle (at -7.9248 -3.9624) (size 2.286 2.286) (drill 1.52) (layers *.Cu *.Mask)
      (net 13 "/Child Board/ENABLE_B"))
  )
  (module t32_ref:SOLDERJUMPER (layer Bottom) (tedit 0)
    (at 158.115 128.905 180)
    (fp_text reference JP8 (at 0 0 180) (layer B.Fab))
    (fp_text value SolderJumper_2_Open (at -1.524 -1.651 180) (layer B.Fab))
    (pad 2 smd rect (at 0.762 0 180) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 17 "Net-(JP8-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.762 0 180) (size 1.1684 1.6002) (layers Bottom B.Mask)
      (net 14 "/Child Board/ENABLE_A") (solder_mask_margin 0.1016))
  )
  (gr_text NES (at 137.16 126.365) (layer F.SilkS))
  (gr_line (start 186.69 136.525) (end 187.96 136.525) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 136.525) (end 107.95 136.525) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 124.46) (end 107.95 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 124.46) (end 187.96 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 134.62) (end 107.95 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.96 124.46) (end 107.95 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_text 2019-10-11 (at 174.625 128.905) (layer B.SilkS))
  (gr_text "SNES\n" (at 135.89 126.365) (layer F.SilkS))
  (gr_text "SNES\n" (at 181.61 125.73) (layer F.SilkS))
  (gr_text SNES+NES (at 158.75 135.255) (layer B.SilkS))
  (gr_line (start 186.69 134.62) (end 187.96 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.69 136.525) (end 186.69 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.22 136.525) (end 109.22 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 140.335) (end 187.96 140.335) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 136.525) (end 107.95 140.335) (layer Edge.Cuts) (width 0.15))
  (gr_text NES (at 182.88 125.73) (layer F.SilkS))
  (gr_text "Side Board v0.9" (at 178.435 127.635) (layer B.SilkS))
  (gr_text SNES+NES (at 113.03 135.255) (layer B.SilkS))
  (dimension 4 (width 0.3) (layer Cmts.User)
    (gr_text "4.000 mm" (at 102.15 130.75 270) (layer Cmts.User))
    (feature1 (pts (xy 115.9 132.75) (xy 100.8 132.75)))
    (feature2 (pts (xy 115.9 128.75) (xy 100.8 128.75)))
    (crossbar (pts (xy 103.5 128.75) (xy 103.5 132.75)))
    (arrow1a (pts (xy 103.5 132.75) (xy 102.913579 131.623496)))
    (arrow1b (pts (xy 103.5 132.75) (xy 104.086421 131.623496)))
    (arrow2a (pts (xy 103.5 128.75) (xy 102.913579 129.876504)))
    (arrow2b (pts (xy 103.5 128.75) (xy 104.086421 129.876504)))
  )
  (gr_line (start 187.96 136.525) (end 187.96 140.335) (layer Edge.Cuts) (width 0.15))
  (dimension 22.86 (width 0.15) (layer Cmts.User)
    (gr_text "22.860 mm" (at 159.385 79.345) (layer Cmts.User))
    (feature1 (pts (xy 147.955 93.98) (xy 147.955 80.058579)))
    (feature2 (pts (xy 170.815 93.98) (xy 170.815 80.058579)))
    (crossbar (pts (xy 170.815 80.645) (xy 147.955 80.645)))
    (arrow1a (pts (xy 147.955 80.645) (xy 149.081504 80.058579)))
    (arrow1b (pts (xy 147.955 80.645) (xy 149.081504 81.231421)))
    (arrow2a (pts (xy 170.815 80.645) (xy 169.688496 80.058579)))
    (arrow2b (pts (xy 170.815 80.645) (xy 169.688496 81.231421)))
  )
  (dimension 17.78 (width 0.3) (layer Cmts.User)
    (gr_text "0.7000 in" (at 170.815 59.61) (layer Cmts.User))
    (feature1 (pts (xy 179.705 103.505) (xy 179.705 58.26)))
    (feature2 (pts (xy 161.925 103.505) (xy 161.925 58.26)))
    (crossbar (pts (xy 161.925 60.96) (xy 179.705 60.96)))
    (arrow1a (pts (xy 179.705 60.96) (xy 178.578496 61.546421)))
    (arrow1b (pts (xy 179.705 60.96) (xy 178.578496 60.373579)))
    (arrow2a (pts (xy 161.925 60.96) (xy 163.051504 61.546421)))
    (arrow2b (pts (xy 161.925 60.96) (xy 163.051504 60.373579)))
  )
  (gr_text BlueSMiRF (at 191.135 107.95 -90) (layer Cmts.User))
  (dimension 17.78 (width 0.3) (layer Cmts.User)
    (gr_text "0.7000 in" (at 125.095 148.67) (layer Cmts.User))
    (feature1 (pts (xy 133.985 73.025) (xy 133.985 150.02)))
    (feature2 (pts (xy 116.205 73.025) (xy 116.205 150.02)))
    (crossbar (pts (xy 116.205 147.32) (xy 133.985 147.32)))
    (arrow1a (pts (xy 133.985 147.32) (xy 132.858496 147.906421)))
    (arrow1b (pts (xy 133.985 147.32) (xy 132.858496 146.733579)))
    (arrow2a (pts (xy 116.205 147.32) (xy 117.331504 147.906421)))
    (arrow2b (pts (xy 116.205 147.32) (xy 117.331504 146.733579)))
  )
  (dimension 46.355 (width 0.3) (layer Cmts.User)
    (gr_text "1.8250 in" (at 124.7775 58.34) (layer Cmts.User))
    (feature1 (pts (xy 147.955 93.345) (xy 147.955 56.99)))
    (feature2 (pts (xy 101.6 93.345) (xy 101.6 56.99)))
    (crossbar (pts (xy 101.6 59.69) (xy 147.955 59.69)))
    (arrow1a (pts (xy 147.955 59.69) (xy 146.828496 60.276421)))
    (arrow1b (pts (xy 147.955 59.69) (xy 146.828496 59.103579)))
    (arrow2a (pts (xy 101.6 59.69) (xy 102.726504 60.276421)))
    (arrow2b (pts (xy 101.6 59.69) (xy 102.726504 59.103579)))
  )
  (dimension 17.78 (width 0.3) (layer Cmts.User)
    (gr_text "0.7000 in" (at 170.815 145.495) (layer Cmts.User))
    (feature1 (pts (xy 179.705 116.205) (xy 179.705 146.845)))
    (feature2 (pts (xy 161.925 116.205) (xy 161.925 146.845)))
    (crossbar (pts (xy 161.925 144.145) (xy 179.705 144.145)))
    (arrow1a (pts (xy 179.705 144.145) (xy 178.578496 144.731421)))
    (arrow1b (pts (xy 179.705 144.145) (xy 178.578496 143.558579)))
    (arrow2a (pts (xy 161.925 144.145) (xy 163.051504 144.731421)))
    (arrow2b (pts (xy 161.925 144.145) (xy 163.051504 143.558579)))
  )
  (dimension 13.97 (width 0.3) (layer Cmts.User)
    (gr_text "0.5500 in" (at 154.94 82.482) (layer Cmts.User))
    (feature1 (pts (xy 161.925 93.345) (xy 161.925 83.995579)))
    (feature2 (pts (xy 147.955 93.345) (xy 147.955 83.995579)))
    (crossbar (pts (xy 147.955 84.582) (xy 161.925 84.582)))
    (arrow1a (pts (xy 161.925 84.582) (xy 160.798496 85.168421)))
    (arrow1b (pts (xy 161.925 84.582) (xy 160.798496 83.995579)))
    (arrow2a (pts (xy 147.955 84.582) (xy 149.081504 85.168421)))
    (arrow2b (pts (xy 147.955 84.582) (xy 149.081504 83.995579)))
  )
  (zone (net 1) (net_name GNDA) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.6096)
    (fill yes (arc_segments 32) (thermal_gap 0.6596) (thermal_bridge_width 0.6596))
    (polygon
      (pts
        (xy 109.22 127) (xy 110.49 125.73) (xy 185.42 125.73) (xy 186.69 127) (xy 186.69 137.795)
        (xy 185.42 139.065) (xy 110.49 139.065) (xy 109.22 137.795)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.6096)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.6596) (thermal_bridge_width 0.6596))
    (polygon
      (pts
        (xy 110.49 134.62) (xy 109.22 133.35) (xy 107.95 133.35) (xy 107.95 137.795) (xy 109.22 137.795)
        (xy 110.49 136.525)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.6096)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.6596) (thermal_bridge_width 0.6596))
    (polygon
      (pts
        (xy 185.42 134.62) (xy 186.69 133.35) (xy 187.96 133.35) (xy 187.96 137.16) (xy 187.96 137.795)
        (xy 186.69 137.795) (xy 185.42 136.525)
      )
    )
  )
  (zone (net 2) (net_name VCCA) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.4064))
    (min_thickness 0.6096)
    (fill yes (arc_segments 32) (thermal_gap 0.6596) (thermal_bridge_width 0.6596))
    (polygon
      (pts
        (xy 109.22 127) (xy 110.49 125.73) (xy 185.42 125.73) (xy 186.69 127) (xy 186.69 137.795)
        (xy 185.42 139.065) (xy 110.49 139.065) (xy 109.22 137.795)
      )
    )
  )
)
