(kicad_pcb (version 20171130) (host pcbnew "(5.1.8)-1")
  (general
    (thickness 1.6)
    (drawings 31)
    (tracks 246)
    (zones 0)
    (modules 21)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (trace_clearance 0.16)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.155)
    (via_size 0.504)
    (via_drill 0.254)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (user_via 0.504 0.254)
    (user_via 0.8 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.65)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J2-Pad3)")
  (net 3 "Net-(U1-Pad8)")
  (net 4 "Net-(U1-Pad7)")
  (net 5 "Net-(U3-Pad10)")
  (net 6 "Net-(U3-Pad2)")
  (net 7 "Net-(U3-Pad3)")
  (net 8 VIN)
  (net 9 "Net-(C2-Pad1)")
  (net 10 VCC)
  (net 11 "Net-(C4-Pad1)")
  (net 12 "Net-(TP5-Pad1)")
  (net 13 "Net-(U1-Pad20)")
  (net 14 "Net-(U1-Pad18)")
  (net 15 "Net-(TP11-Pad1)")
  (net 16 "Net-(J2-Pad4)")
  (net 17 /SPI_INT)
  (net 18 /SPI_MISO)
  (net 19 /SPI_CLK)
  (net 20 /SPI_CS)
  (net 21 /SPI_MOSI)
  (net 22 /RSTN)
  (net 23 /RX)
  (net 24 /TX)
  (net 25 /SWDCLK)
  (net 26 /SWDIO)
  (net 27 "Net-(TP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.2)
    (via_dia 0.504)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RSTN)
    (add_net /RX)
    (add_net /SPI_CLK)
    (add_net /SPI_CS)
    (add_net /SPI_INT)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(TP1-Pad1)")
    (add_net "Net-(TP11-Pad1)")
    (add_net "Net-(TP5-Pad1)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad3)")
    (add_net VCC)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C2-Pad1)")
    (add_net VIN)
  )
  (module -DaleFootprints:TestPoint_D1.0mm_Drill0.65mm (layer F.Cu) (tedit 602D9047)
    (at 137.3 106.1)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP11 (at -4.8 0.6) (layer F.SilkS) hide)
    (fp_text value spare (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 "Net-(TP11-Pad1)"))
  )
  (module -DaleFootprints:TestPoint_D1.0mm_Drill0.65mm (layer F.Cu) (tedit 602D9047)
    (at 145.5 109)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP5 (at 1 4.4) (layer F.SilkS) hide)
    (fp_text value 32k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 "Net-(TP5-Pad1)"))
  )
  (module -DaleFootprints:TestPoint_D1.0mm_Drill0.65mm (layer F.Cu) (tedit 602D9047)
    (at 147.7 107.6)
    (descr "THT pad as test Point, diameter 1.0mm, hole diameter 0.5mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP1 (at 4.2 4.8) (layer F.SilkS) hide)
    (fp_text value D (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 "Net-(TP1-Pad1)"))
  )
  (module -DaleFootprints:JST_SH_Dale_1x04_P1.00mm_H_and_V (layer F.Cu) (tedit 602C8DED)
    (at 152.2 102.3)
    (descr "Through hole angled pin header, 1x04, 1.00mm pitch, 2.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.00mm single row")
    (fp_text reference J2 (at 0.6 -6.4) (layer F.SilkS) hide)
    (fp_text value RS-485 (at 4.7072 1.251 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.75 1.5 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 3) (size 0.75 0.75) (drill 0.4) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2) (size 0.75 0.75) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 1) (size 0.75 0.75) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 VIN))
    (pad "" thru_hole circle (at 0.3 -1.3) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.7 -1.3) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 3.1 -1.3) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0.3 4.3) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.7 4.3) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 3.1 4.3) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 3 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 VIN))
    (pad 2 thru_hole oval (at 3 1) (size 0.75 0.75) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 3 2) (size 0.75 0.75) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 3 3) (size 0.75 0.75) (drill 0.4) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x04_P1.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 150.4 104.9 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 2.2 0 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(J2-Pad4)"))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -DaleFootprints:MAX32660_QFN20 (layer F.Cu) (tedit 602C73B0)
    (at 141.8 103.1 270)
    (attr smd)
    (fp_text reference U1 (at 9.6 6.2 270) (layer F.SilkS) hide)
    (fp_text value MAX32660GTP+ (at 0.5 8.7 270) (layer F.SilkS) hide)
    (pad 21 smd rect (at 0 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd roundrect (at 1.945 -1 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 /RX))
    (pad 14 smd rect (at 1.945 -0.5 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 18 /SPI_MISO))
    (pad 13 smd rect (at 1.945 0 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 21 /SPI_MOSI))
    (pad 12 smd rect (at 1.945 0.5 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(TP11-Pad1)"))
    (pad 11 smd roundrect (at 1.945 1 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /SPI_INT))
    (pad 5 smd roundrect (at -1.945 1 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /RSTN))
    (pad 4 smd rect (at -1.945 0.5 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 19 /SPI_CLK))
    (pad 3 smd rect (at -1.945 0 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 20 /SPI_CS))
    (pad 2 smd rect (at -1.945 -0.5 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 26 /SWDIO))
    (pad 1 smd roundrect (at -1.945 -1 270) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /SWDCLK))
    (pad 20 smd roundrect (at -1 -1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(U1-Pad20)"))
    (pad 19 smd rect (at -0.5 -1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(TP5-Pad1)"))
    (pad 18 smd rect (at 0 -1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad18)"))
    (pad 17 smd rect (at 0.5 -1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(TP1-Pad1)"))
    (pad 16 smd roundrect (at 1 -1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /TX))
    (pad 10 smd roundrect (at 1 1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at 0.5 1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 8 smd rect (at 0 1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at -0.5 1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad7)"))
    (pad 6 smd roundrect (at -1 1.945) (size 0.84 0.27) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 21 thru_hole circle (at 0 0 270) (size 1 1) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module -DaleFootprints:ICM-42688-P (layer F.Cu) (tedit 5FFDCDB2)
    (at 142.1 108.2)
    (fp_text reference U3 (at 0.1 5.2) (layer F.SilkS) hide)
    (fp_text value ICM-42688-P (at 0 3.9) (layer F.SilkS) hide)
    (fp_text user * (at -2.032 -1) (layer F.SilkS))
    (fp_text user * (at -2.032 -1) (layer F.SilkS))
    (pad 1 smd rect (at -1.1303 -0.750001 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 18 /SPI_MISO))
    (pad 2 smd rect (at -1.1303 -0.25 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U3-Pad2)"))
    (pad 3 smd rect (at -1.1303 0.25 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -1.1303 0.750001 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 17 /SPI_INT))
    (pad 5 smd rect (at -0.499999 0.889) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 6 smd rect (at 0 0.889) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.499999 0.889) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 1.1303 0.750001 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 9 smd rect (at 1.1303 0.25 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(TP5-Pad1)"))
    (pad 10 smd rect (at 1.1303 -0.25 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U3-Pad10)"))
    (pad 11 smd rect (at 1.1303 -0.750001 90) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 0.499999 -0.889) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 20 /SPI_CS))
    (pad 13 smd rect (at 0 -0.889) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 19 /SPI_CLK))
    (pad 14 smd rect (at -0.499999 -0.889) (size 0.28 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 21 /SPI_MOSI))
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 135.5 101.2)
    (descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x06 1.27mm single row")
    (fp_text reference J3 (at -1.6 -1.8) (layer F.SilkS) hide)
    (fp_text value SPI_Debug (at 0 8.045) (layer F.Fab))
    (fp_text user %R (at 0 3.175 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 6.35) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /SPI_INT))
    (pad 5 thru_hole oval (at 0 5.08) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /SPI_MISO))
    (pad 4 thru_hole oval (at 0 3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 21 /SPI_MOSI))
    (pad 3 thru_hole oval (at 0 2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 /SPI_CS))
    (pad 2 thru_hole oval (at 0 1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /SPI_CLK))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical (layer F.Cu) (tedit 59FED6E3)
    (at 144.5 98 270)
    (descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 1.27mm double row")
    (fp_text reference J1 (at -4 2.4 90) (layer F.SilkS) hide)
    (fp_text value "DAPLink Debug" (at 0.635 6.775 90) (layer F.Fab))
    (fp_text user %R (at 0.635 2.54) (layer F.Fab))
    (pad 10 thru_hole oval (at 1.27 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 /RSTN))
    (pad 9 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 1.27 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 /RX))
    (pad 7 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 1.27 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 /TX))
    (pad 5 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 1.27 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 /SWDCLK))
    (pad 3 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 /SWDIO))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.9 101.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2 0) (layer F.SilkS))
    (fp_text value C (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module -DaleFootprints:MountingHole_1.8mm locked (layer F.Cu) (tedit 602BE91F)
    (at 136.5 98.5)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask)
      (clearance 0.7))
  )
  (module -DaleFootprints:MountingHole_1.8mm locked (layer F.Cu) (tedit 602BE91F)
    (at 154.5 98.5)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask)
      (clearance 0.7))
  )
  (module -DaleFootprints:MountingHole_1.8mm locked (layer F.Cu) (tedit 602BE91F)
    (at 154.5 109.6)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask)
      (clearance 0.7))
  )
  (module -DaleFootprints:MountingHole_1.8mm locked (layer F.Cu) (tedit 602BE91F)
    (at 136.5 109.6)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr virtual)
    (fp_text reference " " (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask)
      (clearance 0.7))
  )
  (module -DaleFootprints:THVD1450DRBR_VSON (layer F.Cu) (tedit 602B21F2)
    (at 147.7 104.8)
    (fp_text reference U2 (at 1.4 7.7) (layer F.SilkS) hide)
    (fp_text value THVD1450DGK (at -5.5 -9.2) (layer F.SilkS) hide)
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (fp_text user * (at 0 0) (layer F.SilkS) hide)
    (fp_text user * (at 0 0) (layer F.Fab))
    (fp_text user .Designator (at 0 2.54) (layer F.Fab))
    (fp_text user .Designator (at -1.27 2.54) (layer Dwgs.User))
    (pad 1 smd rect (at -1.4 -0.975002 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(TP1-Pad1)"))
    (pad 2 smd rect (at -1.4 -0.325001 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad20)"))
    (pad 3 smd rect (at -1.4 0.324998 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad18)"))
    (pad 4 smd rect (at -1.4 0.974999 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(TP1-Pad1)"))
    (pad 5 smd rect (at 1.4 0.974999 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.4 0.324998 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad4)"))
    (pad 7 smd rect (at 1.4 -0.325001 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 8 smd rect (at 1.4 -0.975002 90) (size 0.299999 0.599999) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 9 smd rect (at 0.000003 0) (size 1.599999 2.4) (layers F.Cu F.Paste F.Mask))
    (pad V thru_hole circle (at -0.549999 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
    (pad V thru_hole circle (at 0.549999 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
    (pad V thru_hole circle (at 0 -0.950001) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
    (pad V thru_hole circle (at 0 0.950001) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 149 98.8 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at -2 3.5) (layer F.SilkS) hide)
    (fp_text value LP2985-3.3 (at -4.2 3.1) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 VCC))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 VIN))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 VIN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 138.3 102.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -2.1 -6.8 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.475 110.4 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.425 -3.1) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 137.1 101.7 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 -5.5 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 148.1 102.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2 0) (layer F.SilkS))
    (fp_text value C (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 146.4 98.7 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -3.6 -2.4 90) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text P8 (at 137.6 107.4) (layer F.SilkS))
  (gr_text D (at 148.8 107.5) (layer F.SilkS))
  (gr_text Rev2 (at 150.9 109) (layer F.SilkS))
  (gr_text 32k (at 145.4 107.8) (layer F.SilkS))
  (gr_text IMU/RS485 (at 149.3 110.4) (layer F.SilkS))
  (gr_text Rst (at 138 99.5) (layer B.SilkS))
  (gr_text Rx (at 140.5 100.5) (layer B.SilkS))
  (gr_text Tx (at 142 100.5) (layer B.SilkS))
  (gr_text K (at 143.4 100.5) (layer B.SilkS))
  (gr_text G (at 138.4 97.7) (layer B.SilkS))
  (gr_text V+ (at 146 98) (layer B.SilkS))
  (gr_text D (at 144.9 100.4) (layer B.SilkS))
  (gr_text A (at 153.7 105.4) (layer B.SilkS))
  (gr_text B (at 153.7 104.4) (layer B.SilkS))
  (gr_text GND (at 153.7 103.3) (layer B.SilkS))
  (gr_text VIN (at 153.6 102.3) (layer B.SilkS))
  (gr_text INT (at 139.6 109.1) (layer B.SilkS))
  (gr_text MISO (at 138.6 107.4) (layer B.SilkS))
  (gr_text P8 (at 138.9 106.1) (layer B.SilkS))
  (gr_text MOSI (at 137.9 104.9) (layer B.SilkS))
  (gr_text CS (at 137.1 103.8) (layer B.SilkS))
  (gr_text CLK (at 137.6 102.3) (layer B.SilkS))
  (gr_text GND (at 137.7 100.8) (layer B.SilkS))
  (gr_text "IMU RS-485\nRev2\nFeb 2021\nDale Roberts" (at 150.8 107.2) (layer B.SilkS))
  (gr_text + (at 145.1102 99.3394) (layer F.SilkS))
  (gr_line (start 135 111.1) (end 135 97) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156 111.1) (end 135 111.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156 97) (end 156 111.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135 97) (end 156 97) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 156 111.1) (xy 135 111.1) (xy 135 97.028) (xy 156 97)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 156 111.1) (xy 135 111.1) (xy 135 97) (xy 156 97)
      )
    )
  )
)
