(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 36)
    (no_connects 0)
    (area 9.201367 9.576999 71.916143 43.921)
    (thickness 1.6)
    (drawings 11)
    (tracks 210)
    (zones 0)
    (modules 17)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.254)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 12.192 40.64)
    (grid_origin 12.192 40.64)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(JP1-Pad1)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(R3-Pad1)")
  (net 7 "Net-(R3-Pad2)")
  (net 8 "Net-(SW1-Pad2)")
  (net 9 "Net-(SW1-Pad5)")
  (net 10 "Net-(R4-Pad1)")
  (net 11 "Net-(R5-Pad2)")
  (net 12 "Net-(U2-Pad3)")
  (net 13 "Net-(U2-Pad4)")
  (net 14 "Net-(U2-Pad5)")
  (net 15 "Net-(U2-Pad6)")
  (net 16 "Net-(U2-Pad7)")
  (net 17 "Net-(U2-Pad8)")
  (net 18 "Net-(JP2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(SW1-Pad5)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 581FE305)
    (at 19.304 37.338)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 581FE308)
    (at 62.23 37.592)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference REF** (at 0 -0.254) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 581FDEA0)
    (at 20.32 15.748 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 2.286 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 581FDE56)
    (at 25.908 16.256 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 581FE30B)
    (at 15.24 33.528 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference JP1 (at 0 -2.286 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 581FE2DD)
    (at 25.908 33.528 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference JP2 (at 0.762 2.032 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 581FDEA9)
    (at 14.3637 15.1003)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.1463 6.4897 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 20.828 30.988 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.3 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(JP2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 581FDE95)
    (at 20.828 27.94 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 581FDAA1)
    (at 59.436 14.732)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 4.572 0.254) (layer F.SilkS))
    (fp_text value 120 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 581FE44B)
    (at 57.404 36.068 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -1.27 -2.032 270) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 581FDE8D)
    (at 29.464 33.528 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at -4.826 0 90) (layer F.SilkS))
    (fp_text value 1k (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 581FDE9D)
    (at 20.32 21.59)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 4.318 0.254) (layer F.SilkS))
    (fp_text value SN65HVD3082ED (at 0 1.27) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(SW1-Pad5)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(SW1-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad4)"))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(JP1-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:ETH-AMPHENOL-2LED (layer F.Cu) (tedit 581FDE4C)
    (at 41.148 37.592)
    (fp_text reference U3 (at 3.556 0.254) (layer F.SilkS))
    (fp_text value ETH-JACK-2LED (at 3.302 2.921) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.79 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 7.11 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 "Net-(SW1-Pad5)"))
    (pad 2 thru_hole circle (at 6.09 -4.32) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at 4.06 -4.32) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at 3.05 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at 2.03 -4.32) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at 1.02 -2.54) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at 0 -4.32) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad8)"))
    (pad "" np_thru_hole circle (at 9.91 0) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 10.42 -9.14) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 10 "Net-(R4-Pad1)"))
    (pad 10 thru_hole circle (at 8.13 -9.14) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 11 thru_hole circle (at -1.01 -9.14) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 11 "Net-(R5-Pad2)"))
    (pad 12 thru_hole circle (at -3.3 -9.14) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad4)"))
  )
  (module Custom_Footprints:ETH-AMPHENOL (layer F.Cu) (tedit 581FDE51)
    (at 48.26 15.24 180)
    (fp_text reference U2 (at 3.556 0.508 180) (layer F.SilkS))
    (fp_text value ETH-JACK (at 3.302 2.921 180) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.79 0 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 7.11 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 9 "Net-(SW1-Pad5)"))
    (pad 2 thru_hole circle (at 6.09 -4.32 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 8 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 12 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at 4.06 -4.32 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 13 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at 3.05 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 14 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at 2.03 -4.32 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 15 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at 1.02 -2.54 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 16 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at 0 -4.32 180) (size 1.524 1.524) (drill 0.89) (layers *.Cu *.Mask)
      (net 17 "Net-(U2-Pad8)"))
    (pad "" np_thru_hole circle (at 9.91 0 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Custom_Footprints:DPDT-MS-100738 (layer F.Cu) (tedit 581FDADF)
    (at 57.15 24.13)
    (fp_text reference SW1 (at 2.54 -2.032) (layer F.SilkS))
    (fp_text value DPDT (at 2.794 -2.286) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -4.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(SW1-Pad2)"))
    (pad 3 thru_hole circle (at 0 4.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 4.83 4.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 4.83 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(SW1-Pad5)"))
    (pad 4 thru_hole circle (at 4.83 -4.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(R3-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4 (layer F.Cu) (tedit 581FE302)
    (at 32.258 24.384)
    (descr "Mounting Hole 4.3mm, no annular, M4")
    (tags "mounting hole 4.3mm no annular m4")
    (fp_text reference REF** (at 0 -0.254) (layer F.SilkS) hide)
    (fp_text value MountingHole_4.3mm_M4 (at 0 5.3) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 4.3 4.3) (drill 4.3) (layers *.Cu *.Mask))
  )
  (gr_text Power (at 54.356 40.132 90) (layer F.SilkS))
  (gr_text "Data LED" (at 34.798 35.306 90) (layer F.SilkS))
  (gr_text "M4\nHoles" (at 27.94 26.416) (layer F.SilkS))
  (gr_text "GND\nNC\n(5v/3.3v) VCC\nTX\nRX\nNC" (at 16.256 21.336) (layer B.SilkS))
  (gr_text "▼Term On" (at 59.182 31.496) (layer F.SilkS))
  (gr_text "▲Term Off" (at 59.436 16.764) (layer F.SilkS))
  (gr_text "Next House\nParty Light Adapter\nUART to RS-485\nRyan Fish\n11/2/2016" (at 35.814 15.494) (layer B.Cu))
  (gr_line (start 12.192 40.64) (end 12.192 12.192) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.532 40.64) (end 12.192 40.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.532 12.192) (end 65.532 40.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 12.192 12.192) (end 65.532 12.192) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1778) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 66.04 40.64) (xy 10.16 40.64) (xy 10.16 10.16) (xy 66.04 10.16) (xy 66.04 40.64)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.1778) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 66.04 40.64) (xy 10.16 40.64) (xy 10.16 10.16) (xy 66.04 10.16) (xy 66.04 40.64)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35.814 18.034) (xy 27.94 18.034) (xy 27.94 16.256) (xy 26.416 14.732) (xy 26.416 12.446)
        (xy 35.814 12.446) (xy 35.814 18.034)
      )
    )
  )
)
