(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 4)
    (no_connects 0)
    (area 126.574999 98.124999 155.343958 117.275001)
    (thickness 1.6002)
    (drawings 4)
    (tracks 10)
    (zones 0)
    (modules 2)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 RX-)
  (net 2 RX+)
  (net 3 TX-)
  (net 4 TX+)
  (net 5 "Net-(J2-Pad9)")
  (net 6 "Net-(J2-Pad10)")
  (net 7 "Net-(J2-Pad11)")
  (net 8 "Net-(J2-Pad12)")
  (net 9 "Net-(J2-Pad8)")
  (net 10 "Net-(J2-Pad4)")
  (net 11 "Net-(J2-Pad5)")
  (net 12 "Net-(J2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net RX+)
    (add_net RX-)
    (add_net TX+)
    (add_net TX-)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B2DD42E)
    (at 146 103.75)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 2.2489 6.9964 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 RX-))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 RX+))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 TX-))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 TX+))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Connect:RJHSE538X (layer F.Cu) (tedit 5B2DDA11)
    (at 135.25 111.25 90)
    (descr "mod. jack, ethernet, 8P8C, RJ45 connector, 2 leds, shielded")
    (tags "RJHSE538X 8P8C RJ45 ethernet jack")
    (fp_text reference RJHSE538x (at 3.5 -3.5 90) (layer F.SilkS))
    (fp_text value RJ45_LEDS (at 3.937 9.2075 90) (layer F.Fab))
    (pad "" thru_hole circle (at 11.684 0.889 90) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -3.302 6.604 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at -1.016 6.604 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 8.128 6.604 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at 10.414 6.604 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad12)"))
    (pad 8 thru_hole circle (at 7.112 1.778 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 6 thru_hole circle (at 5.08 1.778 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 RX-))
    (pad 4 thru_hole circle (at 3.048 1.778 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad4)"))
    (pad 2 thru_hole circle (at 1.016 1.778 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 3 TX-))
    (pad 5 thru_hole circle (at 4.064 0 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (pad 3 thru_hole circle (at 2.032 0 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 RX+))
    (pad 7 thru_hole circle (at 6.096 0 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.50114 1.50114) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 TX+))
    (pad "" thru_hole circle (at -2.794 -2.54 90) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 9.906 -2.54 90) (size 3.3 3.3) (drill 3.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -4.572 0.889 90) (size 2 2) (drill 1.57) (layers *.Cu *.Mask))
    (model Connect.3dshapes/RJHSE538X.wrl
      (at (xyz 0.138 0.06 0.125))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz -90 0 180))
    )
  )
  (gr_line (start 148 117.25) (end 130.5 117.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.5 117.25) (end 130.5 98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148 98) (end 148 117.25) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.5 98) (end 148 98) (layer Edge.Cuts) (width 0.15))
)
