(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "LOGO" (layer "F.Cu")
    (at 175.25 91.4)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at -10.16 -7.62) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (gr_line (start 182.7 76.7) (end 167.700001 76.700001)
    (layer "Edge.Cuts"))
  (gr_line (start 184.3 103.6) (end 184.3 78.3)
    (layer "Edge.Cuts"))
  (gr_arc (start 182.7 76.7) (mid 183.831371 77.168629) (end 184.3 78.3)
    (layer "Edge.Cuts"))
  (gr_arc (start 184.3 103.6) (mid 183.831371 104.731371) (end 182.7 105.2)
    (layer "Edge.Cuts"))
  (gr_line (start 166.100001 78.300001) (end 166.100001 103.599999)
    (layer "Edge.Cuts"))
  (gr_line (start 167.700001 105.199999) (end 182.7 105.2)
    (layer "Edge.Cuts"))
  (gr_arc (start 166.100001 78.300001) (mid 166.56863 77.16863) (end 167.700001 76.700001)
    (layer "Edge.Cuts"))
  (gr_arc (start 167.700001 105.199999) (mid 166.56863 104.73137) (end 166.100001 103.599999)
    (layer "Edge.Cuts"))
  (gr_text "Rocket pin\nCC-BY-NC-SA 4.0\nby ripper" (at 175.2 85.4) (layer "B.SilkS"))
  (gr_text "chaos.social/@ripper\nko-fi/rippervie\n" (at 175.4 99.4) (layer "B.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.15 91.95)
        (xy 173.4 91.95)
        (xy 173.4 92.15)
        (xy 173.15 92.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.05) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 178.03 102.99)
        (xy 178.355 103.615)
        (xy 178.83 104.14)
        (xy 179.28 104.415)
        (xy 178.93 104.415)
        (xy 178.605 104.315)
        (xy 178.805 104.665)
        (xy 179.155 104.89)
        (xy 179.43 104.965)
        (xy 179.08 105.015)
        (xy 175.755 104.99)
        (xy 176.005 104.84)
        (xy 176.18 104.665)
        (xy 176.455 104.265)
        (xy 176.055 104.415)
        (xy 175.705 104.465)
        (xy 175.98 104.265)
        (xy 176.305 103.84)
        (xy 176.58 102.94)
        (xy 176.88 103.115)
        (xy 177.13 103.19)
        (xy 177.405 103.215)
        (xy 177.655 103.165)
        (xy 177.855 103.09)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 177.125 91.675)
        (xy 177.375 91.675)
        (xy 177.375 91.875)
        (xy 177.125 91.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.45 91.95)
        (xy 173.7 91.95)
        (xy 173.7 92.15)
        (xy 173.45 92.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 176.825 91.95)
        (xy 177.075 91.95)
        (xy 177.075 92.15)
        (xy 176.825 92.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads (clearance 0.5))
    (min_thickness 0.05) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 174.08 87)
        (xy 174.09 86.16)
        (xy 174.5 86.04)
        (xy 175.09 85.96)
        (xy 175.53 85.97)
        (xy 176.08 86.05)
        (xy 176.43 86.15)
        (xy 176.44 86.39)
        (xy 176.47 87.03)
        (xy 176.15 86.94)
        (xy 175.71 86.88)
        (xy 175.24 86.88)
        (xy 174.88 86.89)
        (xy 174.36 86.96)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 176.825 91.675)
        (xy 177.075 91.675)
        (xy 177.075 91.875)
        (xy 176.825 91.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 177.125 91.95)
        (xy 177.375 91.95)
        (xy 177.375 92.15)
        (xy 177.125 92.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.05) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 172.475 103)
        (xy 172.15 103.625)
        (xy 171.675 104.15)
        (xy 171.225 104.425)
        (xy 171.575 104.425)
        (xy 171.9 104.325)
        (xy 171.7 104.675)
        (xy 171.35 104.9)
        (xy 171.075 104.975)
        (xy 171.425 105.025)
        (xy 174.75 105)
        (xy 174.5 104.85)
        (xy 174.325 104.675)
        (xy 174.05 104.275)
        (xy 174.45 104.425)
        (xy 174.8 104.475)
        (xy 174.525 104.275)
        (xy 174.2 103.85)
        (xy 173.925 102.95)
        (xy 173.625 103.125)
        (xy 173.375 103.2)
        (xy 173.1 103.225)
        (xy 172.85 103.175)
        (xy 172.65 103.1)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.1) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.15 91.4)
        (xy 173.7 91.4)
        (xy 173.7 92.15)
        (xy 173.15 92.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads (clearance 0.5))
    (min_thickness 0.1) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 174.1 83.55)
        (xy 174.1 85.58)
        (xy 174.87 85.42)
        (xy 175.67 85.41)
        (xy 176.22 85.52)
        (xy 176.44 85.62)
        (xy 176.44 83.59)
        (xy 175.98 83.44)
        (xy 175.44 83.38)
        (xy 174.88 83.39)
        (xy 174.49 83.44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 177.125 91.4)
        (xy 177.375 91.4)
        (xy 177.375 91.6)
        (xy 177.125 91.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads (clearance 0.5))
    (min_thickness 0.05) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 174.74 102.32)
        (xy 174.63 102.72)
        (xy 174.51 102.87)
        (xy 174.32 103.04)
        (xy 174.18 103.12)
        (xy 174.29 103.14)
        (xy 174.47 103.12)
        (xy 174.57 103.08)
        (xy 174.43 103.33)
        (xy 174.32 103.48)
        (xy 174.25 103.53)
        (xy 174.33 103.71)
        (xy 174.39 103.83)
        (xy 174.52 103.96)
        (xy 174.56 103.95)
        (xy 174.6 103.94)
        (xy 174.77 103.87)
        (xy 174.76 104.11)
        (xy 174.69 104.19)
        (xy 174.86 104.36)
        (xy 174.92 104.34)
        (xy 174.98 104.31)
        (xy 175.08 104.23)
        (xy 175.03 104.62)
        (xy 175.09 104.78)
        (xy 175.21 104.95)
        (xy 175.32 104.84)
        (xy 175.43 104.62)
        (xy 175.42 104.3)
        (xy 175.56 104.34)
        (xy 175.62 104.36)
        (xy 175.74 104.28)
        (xy 175.85 104.19)
        (xy 175.79 104.16)
        (xy 175.74 104.1)
        (xy 175.63 103.85)
        (xy 175.8 103.89)
        (xy 175.94 103.96)
        (xy 176.01 103.98)
        (xy 176.16 103.79)
        (xy 176.24 103.57)
        (xy 176.19 103.51)
        (xy 176.05 103.34)
        (xy 175.95 103.08)
        (xy 176.16 103.21)
        (xy 176.26 103.24)
        (xy 176.35 103.24)
        (xy 176.23 103.1)
        (xy 176.12 102.89)
        (xy 175.95 102.55)
        (xy 175.92 102.32)
        (xy 175.73 102.42)
        (xy 175.48 102.5)
        (xy 175.17 102.5)
        (xy 174.89 102.43)
        (xy 174.76 102.36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.45 91.4)
        (xy 173.7 91.4)
        (xy 173.7 91.6)
        (xy 173.45 91.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.15 91.675)
        (xy 173.4 91.675)
        (xy 173.4 91.875)
        (xy 173.15 91.875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.1) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 176.825 91.4)
        (xy 177.375 91.4)
        (xy 177.375 92.15)
        (xy 176.825 92.15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 173.45 91.675)
        (xy 173.7 91.675)
        (xy 173.7 91.875)
        (xy 173.45 91.875)
      )
    )
  )
)
