<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<hole x="6.5" y="32.6" drill="1.6"/>
<hole x="17.7" y="1.8" drill="1.6"/>
<text>G</text>
<text>W</text>
<text>D</text>
<text>A</text>
<text>B</text>
<text>WHITE</text>
<text>RGB</text>
<text>GND</text>
<text>DATA</text>
<text>VCCB</text>
<text>VCCA</text>
<text>WHITE</text>
<hole x="28.5" y="29.7" drill="1.6"/>
<hole x="28.5" y="21.8" drill="1.6"/>
<hole x="28.5" y="17.1" drill="1.6"/>
<hole x="28.5" y="3.1" drill="1.6"/>
<text>electricity for progress 2015</text>
<hole x="36.5" y="32.6" drill="1.6"/>
<hole x="47.7" y="1.8" drill="1.6"/>
<text>G</text>
<text>W</text>
<text>D</text>
<text>A</text>
<text>B</text>
<text>WHITE</text>
<text>RGB</text>
<text>GND</text>
<text>DATA</text>
<text>VCCB</text>
<text>VCCA</text>
<text>WHITE</text>
<hole x="58.5" y="29.7" drill="1.6"/>
<hole x="58.5" y="21.8" drill="1.6"/>
<hole x="58.5" y="17.1" drill="1.6"/>
<hole x="58.5" y="3.1" drill="1.6"/>
<text>electricity for progress 2015</text>
<hole x="6.5" y="67.4" drill="1.6"/>
<hole x="17.7" y="36.6" drill="1.6"/>
<text>G</text>
<text>W</text>
<text>D</text>
<text>A</text>
<text>B</text>
<text>WHITE</text>
<text>RGB</text>
<text>GND</text>
<text>DATA</text>
<text>VCCB</text>
<text>VCCA</text>
<text>WHITE</text>
<hole x="28.5" y="64.5" drill="1.6"/>
<hole x="28.5" y="56.6" drill="1.6"/>
<hole x="28.5" y="51.9" drill="1.6"/>
<hole x="28.5" y="37.9" drill="1.6"/>
<text>electricity for progress 2015</text>
<hole x="36.6" y="67.4" drill="1.6"/>
<hole x="47.8" y="36.6" drill="1.6"/>
<text>G</text>
<text>W</text>
<text>D</text>
<text>A</text>
<text>B</text>
<text>WHITE</text>
<text>RGB</text>
<text>GND</text>
<text>DATA</text>
<text>VCCB</text>
<text>VCCA</text>
<text>WHITE</text>
<hole x="58.6" y="64.5" drill="1.6"/>
<hole x="58.6" y="56.6" drill="1.6"/>
<hole x="58.6" y="51.9" drill="1.6"/>
<hole x="58.6" y="37.9" drill="1.6"/>
<text>electricity for progress 2015</text>
<wire x1="0.6" y1="99" x2="60" y2="99" width="0.4064" layer="20"/>
<wire x1="60" y1="99" x2="60" y2="0.1" width="0.4064" layer="20"/>
<wire x1="60" y1="0.1" x2="0.5" y2="0.1" width="0.4064" layer="20"/>
<wire x1="0.6" y1="0" x2="0.6" y2="99" width="0.4064" layer="20"/>
<wire x1="30" y1="34.8" x2="30" y2="44.3" width="0.254" layer="20"/>
<wire x1="30" y1="44.3" x2="30.6" y2="44.3" width="0.254" layer="20"/>
<wire x1="30.6" y1="44.3" x2="30.6" y2="34.8" width="0.254" layer="20"/>
<wire x1="30.6" y1="34.8" x2="42.2" y2="34.8" width="0.254" layer="20"/>
<wire x1="42.2" y1="34.8" x2="42.2" y2="34.1" width="0.254" layer="20"/>
<wire x1="42.2" y1="34.1" x2="30.6" y2="34.1" width="0.254" layer="20"/>
<wire x1="30.6" y1="34.1" x2="30.6" y2="26.3" width="0.254" layer="20"/>
<wire x1="30.6" y1="26.3" x2="29.9" y2="26.3" width="0.254" layer="20"/>
<wire x1="29.9" y1="26.3" x2="29.9" y2="34.1" width="0.254" layer="20"/>
<wire x1="29.9" y1="34.1" x2="22.7" y2="34.1" width="0.254" layer="20"/>
<wire x1="22.7" y1="34.1" x2="22.7" y2="34.8" width="0.254" layer="20"/>
<wire x1="22.7" y1="34.8" x2="30" y2="34.8" width="0.254" layer="20"/>
<wire x1="29.9" y1="67.1" x2="30.6" y2="67.1" width="0.254" layer="20"/>
<wire x1="30.6" y1="67.1" x2="30.6" y2="47.1" width="0.254" layer="20"/>
<wire x1="30.6" y1="47" x2="29.9" y2="47" width="0.254" layer="20"/>
<wire x1="29.9" y1="47" x2="29.9" y2="67.1" width="0.254" layer="20"/>
<wire x1="30.1" y1="20" x2="30.1" y2="3" width="0.254" layer="20"/>
<wire x1="30.1" y1="3" x2="30.8" y2="3" width="0.254" layer="20"/>
<wire x1="30.8" y1="3" x2="30.8" y2="20" width="0.254" layer="20"/>
<wire x1="30.8" y1="20" x2="30.1" y2="20" width="0.254" layer="20"/>
<wire x1="2.4" y1="34.8" x2="2.4" y2="34.1" width="0.254" layer="20"/>
<wire x1="2.4" y1="34.1" x2="19.1" y2="34.1" width="0.254" layer="20"/>
<wire x1="19.1" y1="34.1" x2="19.1" y2="34.8" width="0.254" layer="20"/>
<wire x1="19.1" y1="34.8" x2="2.5" y2="34.8" width="0.254" layer="20"/>
<wire x1="44.7" y1="34" x2="56.9" y2="34" width="0.254" layer="20"/>
<wire x1="56.9" y1="34" x2="56.9" y2="34.8" width="0.254" layer="20"/>
<wire x1="56.9" y1="34.8" x2="44.7" y2="34.8" width="0.254" layer="20"/>
<wire x1="44.7" y1="34.8" x2="44.7" y2="34" width="0.254" layer="20"/>
<text>GND</text>
<text>electricity for progress 2015</text>
<text>BedLite v001</text>
<wire x1="4" y1="70" x2="4" y2="69" width="0.254" layer="20"/>
<wire x1="4" y1="69" x2="20" y2="69" width="0.254" layer="20"/>
<wire x1="20" y1="69" x2="20" y2="70" width="0.254" layer="20"/>
<wire x1="20" y1="70" x2="4" y2="70" width="0.254" layer="20"/>
<wire x1="22" y1="70" x2="39" y2="70" width="0.254" layer="20"/>
<wire x1="39" y1="70" x2="39" y2="69" width="0.254" layer="20"/>
<wire x1="39" y1="69" x2="22" y2="69" width="0.254" layer="20"/>
<wire x1="22" y1="69" x2="22" y2="70" width="0.254" layer="20"/>
<wire x1="42" y1="70" x2="56" y2="70" width="0.254" layer="20"/>
<wire x1="56" y1="70" x2="56" y2="69" width="0.254" layer="20"/>
<wire x1="56" y1="69" x2="42" y2="69" width="0.254" layer="20"/>
<wire x1="42" y1="69" x2="42" y2="70" width="0.254" layer="20"/>
<hole x="53.6" y="95.4" drill="1.6"/>
<hole x="4.6" y="95.4" drill="1.6"/>
<hole x="29.4" y="71.6" drill="1.6"/>
<hole x="34.8" y="84.7" drill="1.6"/>
</plain>
<libraries>
<library name="onShore-Terminal">
<packages>
<package name="TERM-5">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="TT5D9">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
diameter 9 mm, grid 5.08 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="1X03-CLEANBIG">
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="AVRISP">
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="78MXXS">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="6410-02">
<description>&lt;b&gt;MOLEX 2.54mm KK  CONNECTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TERM_11" library="onShore-Terminal" package="TERM-5" value=""/>
<element name="TP1" library="testpad" package="P1-13Y" value="VCCA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="P1-13Y" value="VCCB">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="P1-13Y" value="DATA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="P1-13Y" value="WGND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="P1-13Y" value="GND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TERM_12" library="onShore-Terminal" package="TERM-5" value=""/>
<element name="TP6" library="testpad" package="P1-13Y" value="VCCA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="P1-13Y" value="VCCB">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="P1-13Y" value="DATA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="P1-13Y" value="WGND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="P1-13Y" value="GND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TERM_13" library="onShore-Terminal" package="TERM-5" value=""/>
<element name="TP11" library="testpad" package="P1-13Y" value="VCCA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="testpad" package="P1-13Y" value="VCCB">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="testpad" package="P1-13Y" value="DATA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="testpad" package="P1-13Y" value="WGND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="testpad" package="P1-13Y" value="GND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TERM_14" library="onShore-Terminal" package="TERM-5" value=""/>
<element name="TP16" library="testpad" package="P1-13Y" value="VCCA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP17" library="testpad" package="P1-13Y" value="VCCB">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP18" library="testpad" package="P1-13Y" value="DATA">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP19" library="testpad" package="P1-13Y" value="WGND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP20" library="testpad" package="P1-13Y" value="GND">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="atmel" package="DIL08" value="ATTINY85">
<attribute name="OC_NEWARK" value="96K6521"/>
<attribute name="MPN" value="ATTINY13-20PU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9171550"/>
</element>
<element name="JP1" library="adafruit" package="1X03-CLEANBIG" value="JPpir1">
<attribute name="VALUE"/>
</element>
<element name="JP10" library="adafruit" package="1X03-CLEANBIG" value="JPpir2">
<attribute name="VALUE"/>
</element>
<element name="J1" library="con-molex" package="6410-02" value="JPLDR">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="Q11" library="adafruit" package="TO220V" value=""/>
<element name="J2" library="con-molex" package="6410-02" value="LEDstrip">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="0207/2V" value=""/>
<element name="5V1" library="wirepad" package="2,15/1,0" value=""/>
<element name="IC3" library="v-reg" package="78MXXS" value=""/>
<element name="VREGIN1" library="wirepad" package="2,15/1,0" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="TT5D9" value=""/>
<element name="C5" library="adafruit" package="TT5D9" value=""/>
<element name="C6" library="adafruit" package="C050-030X075" value=""/>
<element name="J3" library="con-molex" package="6410-02" value="POWER">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
</elements>
<signals>
<signal name="N$40">
</signal>
<signal name="N$28">
<contactref element="TERM_11" pad="2"/>
<contactref element="TERM_11" pad="12"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="DATA11">
<contactref element="TERM_11" pad="3"/>
<contactref element="TERM_11" pad="13"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="VCCA01">
<contactref element="TERM_11" pad="15"/>
<contactref element="TERM_11" pad="5"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="VCCB01">
<contactref element="TERM_11" pad="4"/>
<contactref element="TERM_11" pad="14"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="GND01">
<contactref element="TERM_11" pad="1"/>
<contactref element="TERM_11" pad="11"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$30">
<contactref element="TERM_12" pad="2"/>
<contactref element="TERM_12" pad="12"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="DATA12">
<contactref element="TERM_12" pad="3"/>
<contactref element="TERM_12" pad="13"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="VCCA02">
<contactref element="TERM_12" pad="15"/>
<contactref element="TERM_12" pad="5"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="VCCB02">
<contactref element="TERM_12" pad="4"/>
<contactref element="TERM_12" pad="14"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="GND02">
<contactref element="TERM_12" pad="1"/>
<contactref element="TERM_12" pad="11"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="N$31">
<contactref element="TERM_13" pad="2"/>
<contactref element="TERM_13" pad="12"/>
<contactref element="TP14" pad="TP"/>
</signal>
<signal name="DATA13">
<contactref element="TERM_13" pad="3"/>
<contactref element="TERM_13" pad="13"/>
<contactref element="TP13" pad="TP"/>
</signal>
<signal name="VCCA03">
<contactref element="TERM_13" pad="15"/>
<contactref element="TERM_13" pad="5"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="VCCB03">
<contactref element="TERM_13" pad="4"/>
<contactref element="TERM_13" pad="14"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="GND03">
<contactref element="TERM_13" pad="1"/>
<contactref element="TERM_13" pad="11"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="N$32">
<contactref element="TERM_14" pad="2"/>
<contactref element="TERM_14" pad="12"/>
<contactref element="TP19" pad="TP"/>
</signal>
<signal name="DATA14">
<contactref element="TERM_14" pad="3"/>
<contactref element="TERM_14" pad="13"/>
<contactref element="TP18" pad="TP"/>
</signal>
<signal name="VCCA04">
<contactref element="TERM_14" pad="15"/>
<contactref element="TERM_14" pad="5"/>
<contactref element="TP16" pad="TP"/>
</signal>
<signal name="VCCB04">
<contactref element="TERM_14" pad="4"/>
<contactref element="TERM_14" pad="14"/>
<contactref element="TP17" pad="TP"/>
</signal>
<signal name="GND04">
<contactref element="TERM_14" pad="1"/>
<contactref element="TERM_14" pad="11"/>
<contactref element="TP20" pad="TP"/>
</signal>
<signal name="VCC12">
<contactref element="J2" pad="1"/>
<contactref element="IC3" pad="IN"/>
<contactref element="VREGIN1" pad="1"/>
<contactref element="C4" pad="+"/>
</signal>
<signal name="N$27">
<contactref element="J2" pad="2"/>
<contactref element="Q11" pad="2"/>
</signal>
<signal name="VCC5">
<contactref element="IC2" pad="8"/>
<contactref element="5V1" pad="1"/>
<contactref element="IC3" pad="OUT"/>
<contactref element="C5" pad="+"/>
<contactref element="C6" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="ISP1" pad="2"/>
<contactref element="JP10" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="LDR">
<contactref element="J1" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="PWM">
<contactref element="Q11" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="GND00">
<contactref element="IC2" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP10" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="-"/>
<contactref element="IC3" pad="GND"/>
<contactref element="C4" pad="-"/>
<contactref element="R11" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="Q11" pad="3"/>
<contactref element="ISP1" pad="6"/>
</signal>
<signal name="RST">
<contactref element="ISP1" pad="5"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="PIR2">
<contactref element="JP10" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="PIR1">
<contactref element="JP1" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
