(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 31)
    (no_connects 0)
    (area 143.468952 46.4344 217.880001 106.120001)
    (thickness 1.6)
    (drawings 6)
    (tracks 118)
    (zones 0)
    (modules 11)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 GND)
  (net 4 "Net-(R1-Pad1)")
  (net 5 /5VDD)
  (net 6 "Net-(SHIELD1-PadAD5)")
  (net 7 "Net-(SHIELD1-PadAD4)")
  (net 8 "Net-(SHIELD1-PadAD3)")
  (net 9 "Net-(SHIELD1-PadAD0)")
  (net 10 "Net-(SHIELD1-PadAD1)")
  (net 11 "Net-(SHIELD1-PadAD2)")
  (net 12 "Net-(SHIELD1-PadGND2)")
  (net 13 /3_3VDD)
  (net 14 "Net-(SHIELD1-PadRST)")
  (net 15 "Net-(SHIELD1-Pad0)")
  (net 16 "Net-(SHIELD1-Pad1)")
  (net 17 /D2)
  (net 18 /D3)
  (net 19 /D4)
  (net 20 /D5)
  (net 21 /D6)
  (net 22 /D7)
  (net 23 /D8)
  (net 24 "Net-(SHIELD1-Pad9)")
  (net 25 /SS)
  (net 26 "Net-(SHIELD1-Pad11)")
  (net 27 /MISO)
  (net 28 /SCLK)
  (net 29 "Net-(SHIELD1-PadGND3)")
  (net 30 "Net-(SHIELD1-PadAREF)")
  (net 31 /Vout)
  (net 32 "Net-(U1-Pad5)")
  (net 33 "Net-(U1-Pad7)")
  (net 34 "Net-(U1-Pad8)")
  (net 35 "Net-(U1-Pad9)")
  (net 36 "Net-(U1-Pad10)")
  (net 37 "Net-(U2-Pad8)")
  (net 38 "Net-(U2-Pad7)")
  (net 39 "Net-(U2-Pad6)")
  (net 40 /S1)
  (net 41 "Net-(U5-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3_3VDD)
    (add_net /5VDD)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /MISO)
    (add_net /S1)
    (add_net /SCLK)
    (add_net /SS)
    (add_net /Vout)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(SHIELD1-Pad0)")
    (add_net "Net-(SHIELD1-Pad1)")
    (add_net "Net-(SHIELD1-Pad11)")
    (add_net "Net-(SHIELD1-Pad9)")
    (add_net "Net-(SHIELD1-PadAD0)")
    (add_net "Net-(SHIELD1-PadAD1)")
    (add_net "Net-(SHIELD1-PadAD2)")
    (add_net "Net-(SHIELD1-PadAD3)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadGND2)")
    (add_net "Net-(SHIELD1-PadGND3)")
    (add_net "Net-(SHIELD1-PadRST)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U5-Pad3)")
  )
  (net_class class1 ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Diodes_SMD:D_MELF-RM10_Universal_Handsoldering (layer F.Cu) (tedit 5905D8D3)
    (at 176.276 91.186)
    (descr "Diode, Universal, MELF, RM10, Handsoldering, SMD, Thruhole,")
    (tags "Diode Universal MELF RM10 Handsoldering SMD Thruhole ")
    (fp_text reference D1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value D (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -5 0) (size 4.5 2.7) (drill 1.19888 (offset 1.1 0)) (layers *.Cu *.Mask)
      (net 5 /5VDD))
    (pad 2 thru_hole rect (at 5 0 180) (size 4.5 2.7) (drill 1.19888 (offset 1.1 0)) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 0)
    (at 155.194 58.166 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J2 (at 1.75 -4.3 270) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 162.306 64.262 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value R (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /D2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "arduino_shields:ARDUINO SHIELD" (layer F.Cu) (tedit 4CD6A37D)
    (at 148.5011 105.0036)
    (fp_text reference SHIELD1 (at 2.54 -57.15) (layer F.SilkS))
    (fp_text value ARDUINO_SHIELD (at 5.08 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(SHIELD1-PadAD3)"))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(SHIELD1-PadAD0)"))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(SHIELD1-PadAD1)"))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(SHIELD1-PadAD2)"))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /S1))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(SHIELD1-PadGND2)"))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /3_3VDD))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(SHIELD1-PadRST)"))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(SHIELD1-Pad0)"))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(SHIELD1-Pad1)"))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D2))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D3))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D4))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D5))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D6))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D7))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /D8))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(SHIELD1-Pad9)"))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SS))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(SHIELD1-Pad11)"))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /MISO))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /SCLK))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(SHIELD1-PadGND3)"))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /5VDD))
    (pad "" thru_hole circle (at 66.04 -7.62 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 66.04 -35.56 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 15.24 -50.8 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 13.97 -2.54 90) (size 3.937 3.937) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
  )
  (module Transistors_OldSowjetAera:OldSowjetaera_Transistor_Type-II_SmallPads (layer F.Cu) (tedit 0)
    (at 170.688 65.532)
    (fp_text reference T1 (at 0 -7.1) (layer F.SilkS))
    (fp_text value TRANSISTOR-NPN-BIPOLAR_EN60617_Derived05-05-02_Date20130304 (at 0.1 7.6) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(R1-Pad1)"))
    (pad 1 thru_hole circle (at -2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 2 0) (size 1.4 1.4) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Transistors_OldSowjetAera.3dshapes/OldSowjetaera_Transistor_Type-II_SmallPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 208.28 97.282 180)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference U1 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value 16x2_LCD (at 0 40.43 180) (layer F.Fab))
    (fp_text user %R (at 0 19.05 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5VDD))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /Vout))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D8))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D7))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D6))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D5))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D4))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D3))
    (pad 15 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5VDD))
    (pad 16 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PB:JZC-11F (layer F.Cu) (tedit 5A8279B4)
    (at 163.576 80.518 90)
    (fp_text reference U5 (at 0 8.89 90) (layer F.SilkS))
    (fp_text value RELAY (at 0 -11.43 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.81 6.35 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 /5VDD))
    (pad 2 thru_hole circle (at 3.81 6.35 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at -3.81 -3.81 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 41 "Net-(U5-Pad3)"))
    (pad 4 thru_hole circle (at -3.81 -8.89 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 /S1))
    (pad 5 thru_hole circle (at 3.81 -6.35 90) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module PB:Potentiometer_Trimmer_Bourns_3006P (layer F.Cu) (tedit 58826B0A)
    (at 194.056 95.25 270)
    (descr "Spindle Trimmer Potentiometer, Bourns 3006P, http://www.bourns.com/docs/Product-Datasheets/3006.pdf?sfvrsn=0")
    (tags "Spindle Trimmer Potentiometer   Bourns 3006P")
    (fp_text reference U3 (at -7.235 -4.935 270) (layer F.SilkS))
    (fp_text value Potentiometer (at -7.235 2.395 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5VDD))
    (pad 2 thru_hole circle (at -7.62 -2.54 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 31 /Vout))
    (pad 3 thru_hole circle (at -12.7 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_Bourns_3006P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PB:robosub_logo-medium (layer F.Cu) (tedit 0)
    (at 183.134 61.722)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module PB:Barrel_Jack (layer F.Cu) (tedit 5A9DEDB3)
    (at 153.924 94.488 180)
    (fp_text reference J1 (at 0 5.08 180) (layer F.SilkS))
    (fp_text value Barrel_Jack (at 0 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.9 -2.4 180) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 40 /S1))
    (pad 2 thru_hole circle (at -2.9 -2.4 180) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 3 thru_hole circle (at 0 2.4 180) (size 2.4 2.4) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module PB:HSCDAND015PDSA3 (layer F.Cu) (tedit 5A9DEE58)
    (at 183.642 74.93 270)
    (fp_text reference U2 (at 0 6.35 270) (layer F.SilkS))
    (fp_text value HSC_Sensor (at 0 -7.62 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.65 -3.81 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at -6.65 -1.27 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 /3_3VDD))
    (pad 3 thru_hole circle (at -6.65 1.27 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 /MISO))
    (pad 4 thru_hole circle (at -6.65 3.81 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 28 /SCLK))
    (pad 8 thru_hole circle (at 6.65 -3.81 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad8)"))
    (pad 7 thru_hole circle (at 6.65 -1.27 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 38 "Net-(U2-Pad7)"))
    (pad 6 thru_hole circle (at 6.65 1.27 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-Pad6)"))
    (pad 5 thru_hole circle (at 6.65 3.81 270) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 /SS))
  )
  (gr_line (start 147.574 106.68) (end 147.574 50.292) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.678 106.68) (end 147.574 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.678 50.292) (end 217.678 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 216.916 50.292) (end 217.678 50.292) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.574 50.292) (end 216.916 50.292) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "N. Heitman\nL. Riske\nH. Reaves\nT. Huynh\nRev. 0\n02/2018" (at 202.692 65.786) (layer F.SilkS))
)
