(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 1041)
    (zones 0)
    (modules 82)
    (nets 97)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.161)
    (zone_clearance 0.204)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.25 3.25)
    (pad_drill 3.25)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 GND)
  (net 4 /MON_VSYS)
  (net 5 /USB_VBUS)
  (net 6 "Net-(C4-Pad2)")
  (net 7 /BATT_LOAD)
  (net 8 +3V3)
  (net 9 /CHG_LDO)
  (net 10 +BATT)
  (net 11 "Net-(C13-Pad2)")
  (net 12 +5V)
  (net 13 /IR_SUPPLY)
  (net 14 "Net-(D1-Pad2)")
  (net 15 "Net-(J2-PadB8)")
  (net 16 "Net-(J2-PadA7)")
  (net 17 "Net-(J2-PadA6)")
  (net 18 "Net-(J2-PadB5)")
  (net 19 "Net-(J2-PadA8)")
  (net 20 "Net-(J2-PadA5)")
  (net 21 /IRRECV)
  (net 22 /PER_1)
  (net 23 "Net-(J4-Pad1)")
  (net 24 /TRIGGER)
  (net 25 /SLIDE)
  (net 26 /CLIP)
  (net 27 /SPEAKER_N)
  (net 28 /SPEAKER_P)
  (net 29 /PER_6)
  (net 30 /PER_5)
  (net 31 /PER_4)
  (net 32 /PER_3)
  (net 33 /PER_2)
  (net 34 "Net-(L2-Pad2)")
  (net 35 "Net-(PS1-Pad4)")
  (net 36 "Net-(Q1-Pad1)")
  (net 37 "Net-(Q2-Pad1)")
  (net 38 "Net-(R1-Pad1)")
  (net 39 "Net-(R3-Pad2)")
  (net 40 "Net-(R4-Pad1)")
  (net 41 "Net-(R5-Pad2)")
  (net 42 /CHG_INT)
  (net 43 "Net-(R8-Pad2)")
  (net 44 "Net-(R10-Pad2)")
  (net 45 "Net-(R11-Pad2)")
  (net 46 "Net-(R12-Pad2)")
  (net 47 /SCL)
  (net 48 /SDA)
  (net 49 "Net-(R16-Pad2)")
  (net 50 /IRTRIG)
  (net 51 "Net-(U1-Pad7)")
  (net 52 "Net-(U2-Pad28)")
  (net 53 "Net-(U2-Pad27)")
  (net 54 /UART_TX)
  (net 55 /UART_RX)
  (net 56 "Net-(U2-Pad24)")
  (net 57 "Net-(U2-Pad23)")
  (net 58 "Net-(U2-Pad22)")
  (net 59 "Net-(U2-Pad21)")
  (net 60 "Net-(U2-Pad20)")
  (net 61 "Net-(U2-Pad19)")
  (net 62 "Net-(U2-Pad18)")
  (net 63 "Net-(U2-Pad17)")
  (net 64 "Net-(U2-Pad16)")
  (net 65 "Net-(U2-Pad15)")
  (net 66 "Net-(U2-Pad14)")
  (net 67 "Net-(U2-Pad13)")
  (net 68 "Net-(U2-Pad12)")
  (net 69 "Net-(U2-Pad10)")
  (net 70 /USB_DM)
  (net 71 /USB_DP)
  (net 72 "Net-(U2-Pad2)")
  (net 73 "Net-(U2-Pad1)")
  (net 74 /SD_8)
  (net 75 /SD_7)
  (net 76 /SD_5)
  (net 77 /SD_2)
  (net 78 /SD_1)
  (net 79 /SD_3)
  (net 80 "Net-(U4-Pad9)")
  (net 81 "Net-(U4-Pad11)")
  (net 82 "Net-(U4-Pad4)")
  (net 83 "Net-(U5-Pad32)")
  (net 84 /A_BCLK)
  (net 85 /A_LRCK)
  (net 86 /A_DIN)
  (net 87 "Net-(U5-Pad22)")
  (net 88 "Net-(U5-Pad21)")
  (net 89 "Net-(U5-Pad20)")
  (net 90 "Net-(U5-Pad19)")
  (net 91 "Net-(U5-Pad18)")
  (net 92 "Net-(U5-Pad17)")
  (net 93 "Net-(U5-Pad5)")
  (net 94 "Net-(U5-Pad4)")
  (net 95 "Net-(U8-Pad1)")
  (net 96 "Net-(D2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.161)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net /A_BCLK)
    (add_net /A_DIN)
    (add_net /A_LRCK)
    (add_net /BATT_LOAD)
    (add_net /CHG_INT)
    (add_net /CHG_LDO)
    (add_net /CLIP)
    (add_net /IRRECV)
    (add_net /IRTRIG)
    (add_net /IR_SUPPLY)
    (add_net /MON_VSYS)
    (add_net /PER_1)
    (add_net /PER_2)
    (add_net /PER_3)
    (add_net /PER_4)
    (add_net /PER_5)
    (add_net /PER_6)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SD_1)
    (add_net /SD_2)
    (add_net /SD_3)
    (add_net /SD_5)
    (add_net /SD_7)
    (add_net /SD_8)
    (add_net /SLIDE)
    (add_net /SPEAKER_N)
    (add_net /SPEAKER_P)
    (add_net /TRIGGER)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net /USB_DM)
    (add_net /USB_DP)
    (add_net /USB_VBUS)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad8)")
    (add_net "Net-(J2-PadA5)")
    (add_net "Net-(J2-PadA6)")
    (add_net "Net-(J2-PadA7)")
    (add_net "Net-(J2-PadA8)")
    (add_net "Net-(J2-PadB5)")
    (add_net "Net-(J2-PadB8)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(PS1-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad9)")
    (add_net "Net-(U5-Pad17)")
    (add_net "Net-(U5-Pad18)")
    (add_net "Net-(U5-Pad19)")
    (add_net "Net-(U5-Pad20)")
    (add_net "Net-(U5-Pad21)")
    (add_net "Net-(U5-Pad22)")
    (add_net "Net-(U5-Pad32)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U8-Pad1)")
  )
  (net_class +3.3v ""
    (clearance 0.161)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class +5v ""
    (clearance 0.161)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class USB_VBUS ""
    (clearance 0.161)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module PL_Footprints:USB_C_Receptacle_Amphenol_12401610E4-2A_CircularHoles (layer F.Cu) (tedit 5E6F5599)
    (at 72 122.92)
    (descr "USB TYPE C, RA RCPT PCB, SMT, https://www.amphenolcanada.com/StockAvailabilityPrice.aspx?From=&PartNum=12401610E4%7e2A")
    (tags "USB C Type-C Receptacle SMD")
    (attr smd)
    (fp_text reference J2 (at -4.6 -6.52) (layer F.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0 (at 0 6.14) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad B12 smd rect (at -3 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad B11 smd rect (at -2.5 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad B10 smd rect (at -2 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad B9 smd rect (at -1.5 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /USB_VBUS))
    (pad B8 smd rect (at -1 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-PadB8)"))
    (pad B7 smd rect (at -0.5 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-PadA7)"))
    (pad B6 smd rect (at 0 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-PadA6)"))
    (pad B5 smd rect (at 0.5 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-PadB5)"))
    (pad B4 smd rect (at 1 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /USB_VBUS))
    (pad B3 smd rect (at 1.5 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad B2 smd rect (at 2 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at -3.6 -4.36) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.6 -4.36) (size 0.95 0.95) (drill 0.95) (layers *.Cu *.Mask))
    (pad S1 thru_hole circle (at -4.49 2.84) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad S1 thru_hole circle (at 4.49 2.84) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad S1 thru_hole circle (at 4.13 -3.11) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad B1 smd rect (at 2.5 -3.32) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A11 smd rect (at 2.25 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A8 smd rect (at 0.75 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J2-PadA8)"))
    (pad A9 smd rect (at 1.25 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /USB_VBUS))
    (pad A10 smd rect (at 1.75 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A12 smd rect (at 2.75 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A7 smd rect (at 0.25 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-PadA7)"))
    (pad A6 smd rect (at -0.25 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-PadA6)"))
    (pad A5 smd rect (at -0.75 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J2-PadA5)"))
    (pad A4 smd rect (at -1.25 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /USB_VBUS))
    (pad A3 smd rect (at -1.75 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A2 smd rect (at -2.25 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask))
    (pad A1 smd rect (at -2.75 -5.02) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad S1 thru_hole circle (at -4.13 -3.11) (size 1.4 1.4) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_C_Receptacle_Amphenol_12401610E4-2A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${PL_Models}/12401610E4#2A.STEP
      (offset (xyz 0 -5.25 1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module PL_Footprints:Logo (layer F.Cu) (tedit 0)
    (at 133.33 101.17 270)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 67.7 92.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5E6FD23C)
    (at 137.2 92.6)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Package_DFN_QFN:UDFN-9_1.0x3.8mm_P0.5mm (layer F.Cu) (tedit 5CD213F6)
    (at 86.3 122.18 90)
    (descr "9-pin UDFN package, 1.0x3.8mm, (Ref: https://katalog.we-online.de/pbs/datasheet/824014881.pdf)")
    (tags "UDFN SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -2.9 90) (layer F.SilkS))
    (fp_text value DT1240A-08LP3810 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 9 smd rect (at 0.475 -1.3 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 77 /SD_2))
    (pad 8 smd rect (at 0.475 -0.4 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(D2-Pad8)"))
    (pad 7 smd rect (at 0.475 0.4 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 6 smd rect (at 0.475 1.3 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 75 /SD_7))
    (pad 5 smd rect (at -0.475 1.7 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 74 /SD_8))
    (pad 4 smd rect (at -0.475 0.8 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 76 /SD_5))
    (pad 3 smd rect (at -0.475 0 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -0.475 -0.8 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 79 /SD_3))
    (pad 1 smd rect (at -0.475 -1.7 90) (size 0.6 0.2) (layers F.Cu F.Paste F.Mask)
      (net 78 /SD_1))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UDFN-9_1.0x3.8mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PL_Footprints:TPS61022RWUR (layer F.Cu) (tedit 5E6CF1CB)
    (at 92.2884 117.8347 90)
    (descr TPS61022RWUR-2)
    (tags "Power Supply")
    (attr smd)
    (fp_text reference PS1 (at -2.8829 -0.7112) (layer F.SilkS))
    (fp_text value TPS61022RWUR (at 0 -2.54 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0127 -1.6764 90) (layer F.Fab))
    (pad 7 smd rect (at 0.975 -0.75 180) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /BATT_LOAD))
    (pad 6 smd rect (at 0.975 -0.25 180) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at 0.975 0.25 180) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /BATT_LOAD))
    (pad 4 smd rect (at 0.975 0.75 180) (size 0.25 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(PS1-Pad4)"))
    (pad 3 smd rect (at -0.625 0.55 180) (size 0.35 1.15) (layers F.Cu F.Paste F.Mask)
      (net 12 +5V))
    (pad 2 smd rect (at -0.475 0 180) (size 0.2 1.45) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(L2-Pad2)"))
    (pad 1 smd rect (at -0.625 -0.55 180) (size 0.35 1.15) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model TPS61022RWUR.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${PL_Models}/TPS61230ARNS.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 73.882 114.284 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U10 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value USBLC6-2SC6 (at 7.6454 6.985 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /USB_VBUS))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-PadA6)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-PadA7)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 70 /USB_DM))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 71 /USB_DP))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:Texas_R-PDSO-G6 (layer F.Cu) (tedit 5A02FF57)
    (at 128.2595 123.95)
    (descr "R-PDSO-G6, http://www.ti.com/lit/ds/slis144b/slis144b.pdf")
    (tags "R-PDSO-G6 SC-70-6")
    (attr smd)
    (fp_text reference U9 (at -0.127 2.032) (layer F.SilkS))
    (fp_text value TPL0401B-10-Q1 (at -2.6035 2.921 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 1.1 -0.65) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /IR_SUPPLY))
    (pad 4 smd rect (at 1.1 0.65) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 48 /SDA))
    (pad 2 smd rect (at -1.1 0) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 5 smd rect (at 1.1 0) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U8-Pad1)"))
    (pad 3 smd rect (at -1.1 0.65) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 /SCL))
    (pad 1 smd rect (at -1.1 -0.65) (size 0.9 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 129.085 115.047)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U8 (at 0 -4.5) (layer F.SilkS))
    (fp_text value AMS1117 (at 5.207 -1.397 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 95 "Net-(U8-Pad1)"))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 +5V))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /IR_SUPPLY))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 13 /IR_SUPPLY))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PL_Footprints:MAX98357AETE+T (layer F.Cu) (tedit 5E6CEE15)
    (at 97.9674 107.0754 270)
    (descr "QFN, 16 Pin (https://www.nxp.com/docs/en/package-information/98ASA00525D.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U7 (at 2.8246 1.2674 180) (layer F.SilkS))
    (fp_text value MAX98357A (at 3.0226 2.8194 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 17 smd roundrect (at 0 0 270) (size 1.9 1.9) (layers F.Cu F.Mask) (roundrect_rratio 0.131579)
      (net 3 GND))
    (pad "" smd roundrect (at -0.475 -0.475 270) (size 0.77 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.475 0.475 270) (size 0.77 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.475 -0.475 270) (size 0.77 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.475 0.475 270) (size 0.77 0.77) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.5125 -0.75 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 /A_DIN))
    (pad 2 smd roundrect (at -1.5125 -0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(R16-Pad2)"))
    (pad 3 smd roundrect (at -1.5125 0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 4 smd roundrect (at -1.5125 0.75 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 5 smd roundrect (at -0.75 1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 6 smd roundrect (at -0.25 1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at 0.25 1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 8 smd roundrect (at 0.75 1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 9 smd roundrect (at 1.5125 0.75 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /SPEAKER_P))
    (pad 10 smd roundrect (at 1.5125 0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /SPEAKER_N))
    (pad 11 smd roundrect (at 1.5125 -0.25 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 12 smd roundrect (at 1.5125 -0.75 270) (size 0.675 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 0.75 -1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at 0.25 -1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 /A_LRCK))
    (pad 15 smd roundrect (at -0.25 -1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 16 smd roundrect (at -0.75 -1.5125 270) (size 0.25 0.675) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 /A_BCLK))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${PL_Models}/MAX98357AETE+T.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 84.0272 108.9844 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U6 (at 2.9972 -2.794) (layer F.SilkS))
    (fp_text value AP7361C-33E (at 5.2832 1.6764 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 +5V))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 +3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RF_Module:ESP32-WROOM-32U (layer B.Cu) (tedit 5B5B4734)
    (at 114.7816 112.676)
    (descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip with U.FL connector, https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32d_esp32-wroom-32u_datasheet_en.pdf")
    (tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
    (attr smd)
    (fp_text reference U5 (at -7.58 10.5 -180) (layer B.SilkS))
    (fp_text value ESP32-WROOM-32U (at 1.9304 10.668) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 38 smd rect (at 8.5 8.255) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 37 smd rect (at 8.5 6.985) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 /TRIGGER))
    (pad 36 smd rect (at 8.5 5.715) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 /SCL))
    (pad 35 smd rect (at 8.5 4.445) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 55 /UART_RX))
    (pad 34 smd rect (at 8.5 3.175) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 54 /UART_TX))
    (pad 33 smd rect (at 8.5 1.905) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 48 /SDA))
    (pad 32 smd rect (at 8.5 0.635) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(U5-Pad32)"))
    (pad 31 smd rect (at 8.5 -0.635) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 84 /A_BCLK))
    (pad 30 smd rect (at 8.5 -1.905) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 85 /A_LRCK))
    (pad 29 smd rect (at 8.5 -3.175) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 86 /A_DIN))
    (pad 28 smd rect (at 8.5 -4.445) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 50 /IRTRIG))
    (pad 27 smd rect (at 8.5 -5.715) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 /IRRECV))
    (pad 26 smd rect (at 8.5 -6.985) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 74 /SD_8))
    (pad 25 smd rect (at 8.5 -8.255) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 /SLIDE))
    (pad 24 smd rect (at 5.715 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 75 /SD_7))
    (pad 23 smd rect (at 4.445 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 79 /SD_3))
    (pad 22 smd rect (at 3.175 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(U5-Pad22)"))
    (pad 21 smd rect (at 1.905 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 88 "Net-(U5-Pad21)"))
    (pad 20 smd rect (at 0.635 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 89 "Net-(U5-Pad20)"))
    (pad 19 smd rect (at -0.635 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(U5-Pad19)"))
    (pad 18 smd rect (at -1.905 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(U5-Pad18)"))
    (pad 17 smd rect (at -3.175 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(U5-Pad17)"))
    (pad 16 smd rect (at -4.445 -9.255 270) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 77 /SD_2))
    (pad 15 smd rect (at -5.715 -9.255 90) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 14 smd rect (at -8.5 -8.255) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 78 /SD_1))
    (pad 13 smd rect (at -8.5 -6.985) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 76 /SD_5))
    (pad 12 smd rect (at -8.5 -5.715) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 /PER_1))
    (pad 11 smd rect (at -8.5 -4.445) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 33 /PER_2))
    (pad 10 smd rect (at -8.5 -3.175) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 26 /CLIP))
    (pad 9 smd rect (at -8.5 -1.905) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 32 /PER_3))
    (pad 8 smd rect (at -8.5 -0.635) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 /PER_4))
    (pad 7 smd rect (at -8.5 0.635) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 /PER_5))
    (pad 6 smd rect (at -8.5 1.905) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 /PER_6))
    (pad 5 smd rect (at -8.5 3.175) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(U5-Pad5)"))
    (pad 4 smd rect (at -8.5 4.445) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(U5-Pad4)"))
    (pad 3 smd rect (at -8.5 5.715) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(R11-Pad2)"))
    (pad 2 smd rect (at -8.5 6.985) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
    (pad 1 smd rect (at -8.5 8.255) (size 2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 39 smd rect (at -1 0.755) (size 5 5) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32U.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SON:Texas_S-PDSO-N12 (layer F.Cu) (tedit 5A02F1D8)
    (at 75.3966 95.8457)
    (descr http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf)
    (tags "SON thermal pads")
    (attr smd)
    (fp_text reference U4 (at -1.778 -2.4765) (layer F.SilkS))
    (fp_text value BQ27441-G1 (at -1.6764 -5.6261 180) (layer F.Fab))
    (fp_text user %R (at -0.000701 0.002607) (layer F.Fab))
    (pad 13 smd rect (at -1.1 1.365 270) (size 0.575 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at -1.1 -1.365 270) (size 0.575 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 1.1 -1.365 270) (size 0.575 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 1.1 1.365 270) (size 0.575 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 0.65 0.4875 90) (size 0.975 1.3) (layers F.Cu F.Paste)
      (net 3 GND) (solder_paste_margin -0.1))
    (pad 13 smd rect (at -0.65 0.4875 90) (size 0.975 1.3) (layers F.Cu F.Paste)
      (net 3 GND) (solder_paste_margin -0.1))
    (pad 13 smd rect (at -0.65 -0.4875 90) (size 0.975 1.3) (layers F.Cu F.Paste)
      (net 3 GND) (solder_paste_margin -0.1))
    (pad 13 smd rect (at 0.65 -0.4875 90) (size 0.975 1.3) (layers F.Cu F.Paste)
      (net 3 GND) (solder_paste_margin -0.1))
    (pad 13 smd rect (at 0 0 270) (size 1.95 2.6) (layers B.Cu F.Mask)
      (net 3 GND))
    (pad 13 thru_hole circle (at 0 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 13 thru_hole circle (at 0 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 13 thru_hole circle (at -0.9 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 13 thru_hole circle (at 0.9 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 13 thru_hole circle (at 0.9 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 13 thru_hole circle (at -0.9 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 3 GND))
    (pad 7 smd rect (at 2.3 1) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /MON_VSYS) (solder_mask_margin 0.05))
    (pad 8 smd rect (at 2.3 0.6) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT) (solder_mask_margin 0.05))
    (pad 9 smd rect (at 2.3 0.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U4-Pad9)") (solder_mask_margin 0.05))
    (pad 10 smd rect (at 2.3 -0.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R10-Pad2)") (solder_mask_margin 0.05))
    (pad 11 smd rect (at 2.3 -0.6) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U4-Pad11)") (solder_mask_margin 0.05))
    (pad 12 smd rect (at 2.3 -1) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R12-Pad2)") (solder_mask_margin 0.05))
    (pad 1 smd rect (at -2.3 -1) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 48 /SDA) (solder_mask_margin 0.05))
    (pad 2 smd rect (at -2.3 -0.6) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 47 /SCL) (solder_mask_margin 0.05))
    (pad 6 smd rect (at -2.3 1) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT) (solder_mask_margin 0.05))
    (pad 5 smd rect (at -2.3 0.6) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C13-Pad2)") (solder_mask_margin 0.05))
    (pad 4 smd rect (at -2.3 0.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U4-Pad4)") (solder_mask_margin 0.05))
    (pad 7 smd oval (at 1.975 1) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /MON_VSYS) (solder_mask_margin 0.05))
    (pad 8 smd oval (at 1.975 0.6) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT) (solder_mask_margin 0.05))
    (pad 9 smd oval (at 1.975 0.2) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(U4-Pad9)") (solder_mask_margin 0.05))
    (pad 10 smd oval (at 1.975 -0.2) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R10-Pad2)") (solder_mask_margin 0.05))
    (pad 11 smd oval (at 1.975 -0.6) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(U4-Pad11)") (solder_mask_margin 0.05))
    (pad 12 smd oval (at 1.975 -1) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R12-Pad2)") (solder_mask_margin 0.05))
    (pad 6 smd oval (at -1.975 1) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 +BATT) (solder_mask_margin 0.05))
    (pad 5 smd oval (at -1.975 0.6) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C13-Pad2)") (solder_mask_margin 0.05))
    (pad 4 smd oval (at -1.975 0.2) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(U4-Pad4)") (solder_mask_margin 0.05))
    (pad 1 smd oval (at -1.975 -1) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 48 /SDA) (solder_mask_margin 0.05))
    (pad 2 smd oval (at -1.975 -0.6) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 47 /SCL) (solder_mask_margin 0.05))
    (pad 3 smd oval (at -1.975 -0.2) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 3 smd rect (at -2.3 -0.2) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND) (solder_mask_margin 0.05))
    (pad 13 smd rect (at -1.1 -1.3125 270) (size 0.675 0.4) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 1.1 -1.3125 270) (size 0.675 0.4) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 1.1 1.3125 270) (size 0.675 0.4) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at -1.1 1.3125 270) (size 0.675 0.4) (layers F.Cu F.Mask)
      (net 3 GND))
    (pad 13 smd rect (at 0 0 270) (size 1.95 2.6) (layers F.Cu F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Package_SON.3dshapes/Texas_S-PDSO-N12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm (layer F.Cu) (tedit 5C1FD453)
    (at 75.2061 104.8479)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=283), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U2 (at 0 -3.8) (layer F.SilkS))
    (fp_text value CP2102N-A01-GQFN28 (at 5.48894 5.15874 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 29 smd roundrect (at 0 0) (size 3.35 3.35) (layers F.Cu F.Mask) (roundrect_rratio 0.074627)
      (net 3 GND))
    (pad "" smd roundrect (at -1.12 -1.12) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 0) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 1.12) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.12) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 1.12) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 -1.12) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 0) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 1.12) (size 0.9 0.9) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.45 -1.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(U2-Pad1)"))
    (pad 2 smd roundrect (at -2.45 -1) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 "Net-(U2-Pad2)"))
    (pad 3 smd roundrect (at -2.45 -0.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 4 smd roundrect (at -2.45 0) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /USB_DP))
    (pad 5 smd roundrect (at -2.45 0.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 /USB_DM))
    (pad 6 smd roundrect (at -2.45 1) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 7 smd roundrect (at -2.45 1.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 8 smd roundrect (at -1.5 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R1-Pad1)"))
    (pad 9 smd roundrect (at -1 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R3-Pad2)"))
    (pad 10 smd roundrect (at -0.5 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 "Net-(U2-Pad10)"))
    (pad 11 smd roundrect (at 0 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R8-Pad2)"))
    (pad 12 smd roundrect (at 0.5 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(U2-Pad12)"))
    (pad 13 smd roundrect (at 1 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(U2-Pad13)"))
    (pad 14 smd roundrect (at 1.5 2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(U2-Pad14)"))
    (pad 15 smd roundrect (at 2.45 1.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(U2-Pad15)"))
    (pad 16 smd roundrect (at 2.45 1) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(U2-Pad16)"))
    (pad 17 smd roundrect (at 2.45 0.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(U2-Pad17)"))
    (pad 18 smd roundrect (at 2.45 0) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(U2-Pad18)"))
    (pad 19 smd roundrect (at 2.45 -0.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(U2-Pad19)"))
    (pad 20 smd roundrect (at 2.45 -1) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(U2-Pad20)"))
    (pad 21 smd roundrect (at 2.45 -1.5) (size 0.8 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(U2-Pad21)"))
    (pad 22 smd roundrect (at 1.5 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(U2-Pad22)"))
    (pad 23 smd roundrect (at 1 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U2-Pad23)"))
    (pad 24 smd roundrect (at 0.5 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(U2-Pad24)"))
    (pad 25 smd roundrect (at 0 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 /UART_RX))
    (pad 26 smd roundrect (at -0.5 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /UART_TX))
    (pad 27 smd roundrect (at -1 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U2-Pad27)"))
    (pad 28 smd roundrect (at -1.5 -2.45) (size 0.25 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(U2-Pad28)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm (layer F.Cu) (tedit 5C1BF39E)
    (at 85.5091 97.4586)
    (descr "VQFN, 24 Pin (http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "VQFN DFN_QFN")
    (attr smd)
    (fp_text reference U1 (at -3.302 1.7145 90) (layer F.SilkS))
    (fp_text value BQ24250RGE (at -4.7879 -1.9558 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 25 smd roundrect (at 0 0) (size 2.45 2.45) (layers F.Cu F.Mask) (roundrect_rratio 0.102041)
      (net 3 GND))
    (pad "" smd roundrect (at -0.82 -0.82) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.82 0) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.82 0.82) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -0.82) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0.82) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.82 -0.82) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.82 0) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.82 0.82) (size 0.66 0.66) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.9875 -1.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at -1.9875 -0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 3 smd roundrect (at -1.9875 -0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 4 smd roundrect (at -1.9875 0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 5 smd roundrect (at -1.9875 0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /SDA))
    (pad 6 smd roundrect (at -1.9875 1.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /SCL))
    (pad 7 smd roundrect (at -1.25 1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(U1-Pad7)"))
    (pad 8 smd roundrect (at -0.75 1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /CHG_INT))
    (pad 9 smd roundrect (at -0.25 1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R4-Pad1)"))
    (pad 10 smd roundrect (at 0.25 1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R5-Pad2)"))
    (pad 11 smd roundrect (at 0.75 1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /MON_VSYS))
    (pad 12 smd roundrect (at 1.25 1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /MON_VSYS))
    (pad 13 smd roundrect (at 1.9875 1.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /BATT_LOAD))
    (pad 14 smd roundrect (at 1.9875 0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /BATT_LOAD))
    (pad 15 smd roundrect (at 1.9875 0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 16 smd roundrect (at 1.9875 -0.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 17 smd roundrect (at 1.9875 -0.75) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 18 smd roundrect (at 1.9875 -1.25) (size 0.775 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (pad 19 smd roundrect (at 1.25 -1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /USB_VBUS))
    (pad 20 smd roundrect (at 0.75 -1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad2)"))
    (pad 21 smd roundrect (at 0.25 -1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 22 smd roundrect (at -0.25 -1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 23 smd roundrect (at -0.75 -1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 24 smd roundrect (at -1.25 -1.9875) (size 0.25 0.775) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /CHG_LDO))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PL_Footprints:SW_SPST_B3U-3000P (layer F.Cu) (tedit 5E6CEFB6)
    (at 131.3 91.89)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW2 (at -0.04 2.38 180) (layer F.SilkS))
    (fp_text value Boot (at 4.1656 -0.762) (layer F.Fab))
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 2 smd rect (at 1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.7 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 /SLIDE))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-3000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${PL_Models}/B3U-3000P.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module PL_Footprints:SW_SPST_B3U-3000P (layer F.Cu) (tedit 5E6CEFB6)
    (at 107.4156 124.868 180)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Side-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at -3.1844 0.168 90) (layer F.SilkS))
    (fp_text value EN (at 3.6576 -0.762) (layer F.Fab))
    (fp_text user %R (at 0 -3) (layer F.Fab))
    (pad 2 smd rect (at 1.7 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R11-Pad2)"))
    (pad 1 smd rect (at -1.7 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-3000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${PL_Models}/B3U-3000P.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 122.2 95.55 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -2.95 0) (layer F.SilkS))
    (fp_text value 10k (at 0.0255 -2.794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /CLIP))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 118.55 118.15 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10k (at 0 -2.794 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /TRIGGER))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.5 118.8 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 5.1k (at 3.15966 -1.48082 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J2-PadB5)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 70.4 115.4)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 5.1k (at 3.0606 -1.4351) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(J2-PadA5)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 136.416 123.848)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -0.0255 1.486) (layer F.SilkS))
    (fp_text value 100k (at 3.086 1.486) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /IRTRIG))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 99.05 96.95)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(J4-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 134.05 122.25 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.922 0.0225 90) (layer F.SilkS))
    (fp_text value 100k (at 3.264 -1.5875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.35 105.23 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0.1 1.4 90) (layer F.SilkS))
    (fp_text value 10k (at 2.8448 -1.3716 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /IRRECV))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.184 115.3328 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100k (at -0.8128 -2.794 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(PS1-Pad4)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.184 118.4824 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 732k (at -0.1524 -2.794 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(PS1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.4 104.15)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100k (at -2.3368 -1.0922 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(R16-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.3 115.1 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 0.1 -1.4 90) (layer F.SilkS))
    (fp_text value 10k (at 3.048 -0.0508 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 /SDA))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 121.3 118.2 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 0 1.3 90) (layer F.SilkS))
    (fp_text value 10k (at 3.048 -0.1016 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /SCL))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 125.5 105.25 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10k (at 2.8956 -1.27 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /SLIDE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 76.5141 93.1152)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at -2.6923 -1.4986) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 110.1 117.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -0.0508 1.4224) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.9526 94.6012 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10k (at -2.8576 -1.397 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 78.9526 97.7127 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 10M (at 3.0479 -0.0254 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /MON_VSYS))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 76.3617 108.7976 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -0.82052 -1.49606) (layer F.SilkS))
    (fp_text value 10k (at 1.26482 -1.45034) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(R8-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 81.8261 101.7511 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.5145 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 /CHG_INT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 85.0011 101.7511 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 2.5655 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /CHG_LDO))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 87.3251 104.1261 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.4249 -0.1239) (layer F.SilkS))
    (fp_text value 500 (at -0.0255 -2.7051) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 83.4136 101.7511 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2.5655 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(R4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 73.2629 108.7976)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -0.51298 1.51892) (layer F.SilkS))
    (fp_text value 2k (at -2.324 1.4859) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 69.4285 107.5982)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.4385 0.0635) (layer F.SilkS))
    (fp_text value 47.5k (at -5.29092 -0.03302) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 69.441 109.1857 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.3875 -0.0635) (layer F.SilkS))
    (fp_text value 22.1k (at 5.42788 -0.02794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /USB_VBUS))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 136.6445 121.2065 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 2.413 90) (layer F.SilkS))
    (fp_text value BC817 (at -1.5875 4.3815) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 136.6 117.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value AO3401A (at -0.6985 5.207) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 /IR_SUPPLY))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PL_Footprints:XAL7030-102 (layer F.Cu) (tedit 5E6CE8DF)
    (at 85.786 116.46 270)
    (fp_text reference L2 (at -0.01 0.011 270) (layer F.SilkS))
    (fp_text value 1u (at 4.572 -1.27) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 2 smd rect (at 2.36 0 270) (size 1.78 6.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(L2-Pad2)"))
    (pad 1 smd rect (at -2.36 0 270) (size 1.78 6.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /BATT_LOAD))
    (model ${PL_Models}/Coilcraft-XAL7030-102.STEP
      (offset (xyz 0 0 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module PL_Footprints:XAL7030-102 (layer F.Cu) (tedit 5E6CE8DF)
    (at 92.8751 97.4586 270)
    (fp_text reference L1 (at -4.4086 -3.0249) (layer F.SilkS))
    (fp_text value 1u (at -4.5466 0.9271 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.SilkS))
    (pad 2 smd rect (at 2.36 0 270) (size 1.78 6.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /BATT_LOAD))
    (pad 1 smd rect (at -2.36 0 270) (size 1.78 6.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${PL_Models}/Coilcraft-XAL7030-102.STEP
      (offset (xyz 0 0 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 102.45 101.94)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J10 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Peripheral (at 2.7686 15.494 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PER_6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /PER_5))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /PER_4))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /PER_3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /PER_2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PER_1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 99.858 123.6992 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 2.3992 -1.008) (layer F.SilkS))
    (fp_text value Speaker (at 2.4892 0 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SPEAKER_N))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /SPEAKER_P))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 67.9 98.31)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0.7 4.64) (layer F.SilkS))
    (fp_text value BATT (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.3368 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +BATT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 122.515 92.9008 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0.1008 5.235 180) (layer F.SilkS))
    (fp_text value Clip (at -2.4892 2.921 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /CLIP))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 122.65 100.25 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J6 (at -2.5 3.7 180) (layer F.SilkS))
    (fp_text value Slide (at -2.4892 2.413 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /SLIDE))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 116.01 123.58 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at -2.5492 1.575 180) (layer F.SilkS))
    (fp_text value Trigger (at -2.4892 2.921 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /TRIGGER))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 98.8396 93.0008 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at -2.5492 6.0604 180) (layer F.SilkS))
    (fp_text value G_IR (at -2.4892 3.4544 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IRRECV))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module PL_Footprints:95501-6669 (layer F.Cu) (tedit 5E6FD242)
    (at 113.2 94.1 180)
    (descr 95501-6669)
    (tags Connector)
    (fp_text reference J3 (at -0.631 1.994) (layer F.SilkS))
    (fp_text value IRConnector (at -0.631 1.994) (layer F.SilkS) hide)
    (fp_text user %R (at -0.631 1.994) (layer F.Fab))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 6 smd rect (at 3.175 -10.225 180) (size 0.76 6.35) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.905 -10.225 180) (size 0.76 6.35) (layers F.Cu F.Paste F.Mask)
      (net 33 /PER_2))
    (pad 4 smd rect (at 0.635 -10.225 180) (size 0.76 6.35) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -0.635 -10.225 180) (size 0.76 6.35) (layers F.Cu F.Paste F.Mask)
      (net 21 /IRRECV))
    (pad 2 smd rect (at -1.905 -10.225 180) (size 0.76 6.35) (layers F.Cu F.Paste F.Mask)
      (net 12 +5V))
    (pad 1 smd rect (at -3.175 -10.225 180) (size 0.76 6.35) (layers F.Cu F.Paste F.Mask))
    (model ${PL_Models}/95501-6669.stp
      (offset (xyz 0 -7.85 5.8))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module PL_Footprints:microSD_HC_Molex_104031-0811 (layer B.Cu) (tedit 5E6CEB17)
    (at 87.695 120.01)
    (descr "1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)")
    (tags "microSD SD molex")
    (attr smd)
    (fp_text reference J1 (at 0 7.18) (layer B.SilkS))
    (fp_text value Micro_SD_Card (at 7.62 0.635 -90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.105 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 78 /SD_1))
    (pad 8 smd rect (at 4.545 5.45) (size 0.75 1.1) (layers B.Cu B.Paste B.Mask)
      (net 74 /SD_8))
    (pad 2 smd rect (at -2.005 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 77 /SD_2))
    (pad 3 smd rect (at -0.905 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 79 /SD_3))
    (pad 4 smd rect (at 0.195 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 8 +3V3))
    (pad 5 smd rect (at 1.295 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 76 /SD_5))
    (pad 6 smd rect (at 2.395 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 7 smd rect (at 3.495 5.45) (size 0.85 1.1) (layers B.Cu B.Paste B.Mask)
      (net 75 /SD_7))
    (pad 11 smd rect (at 5.755 5.1) (size 1.17 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -5.565 5.325) (size 1.55 1.35) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -5.74 -4.4) (size 1.2 1) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -5.74 -0.7) (size 1.2 1) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 11 smd rect (at -2.24 -5.375) (size 1.9 1.35) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 3.73 -5.375) (size 1.9 1.35) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Molex_104031-0811.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${PL_Models}/104031-0811.stp
      (offset (xyz 44.5 -1.5 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LED_THT:LED_D5.0mm_IRGrey (layer F.Cu) (tedit 5A6C9BB8)
    (at 135.5 111.9)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 3.55 4.25 270) (layer F.SilkS))
    (fp_text value TSAL6100 (at -2.9845 -0.1905 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm_IRGrey.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 99.05 98.85 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C25 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 77 114.7665 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C24 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 0.1u (at -0.00498 -2.7051 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /USB_VBUS))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 128.2745 121.27 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C23 (at -0.4295 1.778) (layer F.SilkS))
    (fp_text value 10u (at 2.3645 1.778) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 132.006 119.8095)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at -0.256 1.4605) (layer F.SilkS))
    (fp_text value 4.7u (at 2.286 0.1905 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /IR_SUPPLY))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 96.962 121.9368 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at -3.2004 0.0508 90) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 89.3 107.35 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at 0.05 1.45 90) (layer F.SilkS))
    (fp_text value 4.7u (at 2.1844 -0.508 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 94.93 121.9368 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -3.2004 0 90) (layer F.SilkS))
    (fp_text value 10u (at -0.4572 -1.524 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 125.65 120.4 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -2.9 0 90) (layer F.SilkS))
    (fp_text value 4.7u (at 3.2385 -1.397 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 93.691 107.5496 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at -0.009 -1.6004) (layer F.SilkS))
    (fp_text value 10u (at 2.159 2.8956 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 89.3104 110.5084 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 93.691 105.7208)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 0.1u (at -2.413 5.0292 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +5V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 91.4756 114.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -2.3876 0.254 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /BATT_LOAD))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 71.9041 97.7887 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.0255 -1.397 90) (layer F.SilkS))
    (fp_text value 0.47u (at 3.4797 -1.3843 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C13-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 110.7 120.3625 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 0.0375 -1.6 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 108.6 120.4 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 74.2537 98.5381 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -0.0255 -1.4605) (layer F.SilkS))
    (fp_text value 1u (at -2.4637 -1.4351) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +BATT))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 88.9 125.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -2.425 0.2 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 82.4611 93.1026 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.0575 0.1905 180) (layer F.SilkS))
    (fp_text value 1u (at -3.3656 0.7239) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /CHG_LDO))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 69.4284 105.9472)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.502 0.127) (layer F.SilkS))
    (fp_text value 0.1u (at -5.07746 0.02794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 69.4284 104.3216 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.451 -0.0635) (layer F.SilkS))
    (fp_text value 4.7u (at 4.99618 -0.0127) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 90.7646 102.5386)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.6854 0.0114) (layer F.SilkS))
    (fp_text value 22u (at 0.142 3.0988) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /BATT_LOAD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 85.7631 92.8151 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.0151 0.0635 180) (layer F.SilkS))
    (fp_text value 1u (at -3.2765 -0.5461 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.4141 93.1151 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.0575 -0.0635 180) (layer F.SilkS))
    (fp_text value 2.2u (at -3.2765 -1.3843 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /USB_VBUS))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 87.3126 101.0146)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0.6874 1.4354) (layer F.SilkS))
    (fp_text value 1u (at 1.054 1.4732) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /MON_VSYS))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 84.1121 92.8026 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.0026 0.0635 180) (layer F.SilkS))
    (fp_text value 33n (at -3.2894 0.0381 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 74.5 (width 0.15) (layer Dwgs.User)
    (gr_text "74.500 mm" (at 102.45 80) (layer Dwgs.User))
    (feature1 (pts (xy 139.7 90.1) (xy 139.7 80.713579)))
    (feature2 (pts (xy 65.2 90.1) (xy 65.2 80.713579)))
    (crossbar (pts (xy 65.2 81.3) (xy 139.7 81.3)))
    (arrow1a (pts (xy 139.7 81.3) (xy 138.573496 81.886421)))
    (arrow1b (pts (xy 139.7 81.3) (xy 138.573496 80.713579)))
    (arrow2a (pts (xy 65.2 81.3) (xy 66.326504 81.886421)))
    (arrow2b (pts (xy 65.2 81.3) (xy 66.326504 80.713579)))
  )
  (dimension 36.5 (width 0.15) (layer Dwgs.User)
    (gr_text "36.500 mm" (at 151.199922 108.35 90) (layer Dwgs.User))
    (feature1 (pts (xy 139.7 90.1) (xy 150.486343 90.1)))
    (feature2 (pts (xy 139.7 126.6) (xy 150.486343 126.6)))
    (crossbar (pts (xy 149.899922 126.6) (xy 149.899922 90.1)))
    (arrow1a (pts (xy 149.899922 90.1) (xy 150.486343 91.226504)))
    (arrow1b (pts (xy 149.899922 90.1) (xy 149.313501 91.226504)))
    (arrow2a (pts (xy 149.899922 126.6) (xy 150.486343 125.473496)))
    (arrow2b (pts (xy 149.899922 126.6) (xy 149.313501 125.473496)))
  )
  (gr_line (start 65.2 126.6) (end 65.2 90.1) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.7 126.6) (end 65.2 126.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.7 90.1) (end 139.7 126.6) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.2 90.1) (end 139.7 90.1) (layer Edge.Cuts) (width 0.05))
  (gr_text "LT-Gun-G2.5\nBy Ethan Johnston" (at 138.15 102.35 90) (layer F.SilkS))
  (gr_text Clip (at 122.6 91.05) (layer F.SilkS))
  (gr_text Slide (at 122.5 98.2) (layer F.SilkS))
  (gr_text Trigger (at 114.74 125.64) (layer F.SilkS))
  (gr_text IR (at 102.55 96.15) (layer F.SilkS))
  (gr_text Speaker (at 100.95 125.75) (layer F.SilkS))
  (gr_text - (at 66.9 103.15) (layer F.SilkS))
  (gr_text + (at 67 95.75) (layer F.SilkS))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.204))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.204) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 126.6) (xy 65.2 126.6) (xy 65.2 90.1) (xy 139.7 90.1)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.204))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.204) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 126.6) (xy 65.2 126.6) (xy 65.2 90.1) (xy 139.7 90.1)
      )
    )
  )
)
