(kicad_pcb (version 20171130) (host pcbnew 6.0.0-rc1-unknown-32d262b~66~ubuntu14.04.1)
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 133)
    (zones 0)
    (modules 16)
    (nets 23)
  )
  (page A)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.048 1.7272)
    (pad_drill 1.2192)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/"))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad5)")
  (net 2 "Net-(J2-Pad3)")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(J2-Pad4)")
  (net 6 "Net-(J3-Pad3)")
  (net 7 "Net-(J3-Pad4)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad7)")
  (net 10 "Net-(J1-Pad6)")
  (net 11 "Net-(J1-Pad5)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 "Net-(J1-Pad2)")
  (net 14 "Net-(J1-Pad1)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J4-Pad8)")
  (net 17 "Net-(J4-Pad6)")
  (net 18 "Net-(J4-Pad5)")
  (net 19 "Net-(J4-Pad3)")
  (net 20 "Net-(J4-Pad2)")
  (net 21 "Net-(J4-Pad1)")
  (net 22 "Net-(J4-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad8)")
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer B.Cu) (tedit 5BB39807)
    (at 173.4185 46.2595 90)
    (fp_text reference SW5 (at 0 0.762 90) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -1.016 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)"))
    (pad 2 thru_hole oval (at 6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (pad 1 thru_hole oval (at -6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)"))
    (pad 2 thru_hole oval (at -6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_12mm.step
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer B.Cu) (tedit 5BB39807)
    (at 159.28975 59.15 90)
    (fp_text reference SW4 (at 0 0.762 90) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -1.016 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (pad 2 thru_hole oval (at 6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (pad 1 thru_hole oval (at -6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (pad 2 thru_hole oval (at -6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_12mm.step
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer B.Cu) (tedit 5BB39807)
    (at 159.28975 33.7 90)
    (fp_text reference SW3 (at 0 0.762 90) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -1.016 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (pad 1 thru_hole oval (at -6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at -6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_12mm.step
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer B.Cu) (tedit 5BB39807)
    (at 145.161 46.2595 90)
    (fp_text reference SW2 (at 0 0.762 90) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -1.016 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at 6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (pad 1 thru_hole oval (at -6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 2 thru_hole oval (at -6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_12mm.step
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH-12mm (layer B.Cu) (tedit 5BB39807)
    (at 123.444 46.2595 90)
    (fp_text reference SW1 (at 0 0.762 90) (layer B.SilkS))
    (fp_text value SW_Push (at 0 -1.016 90) (layer B.Fab))
    (pad 1 thru_hole oval (at 6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (pad 1 thru_hole oval (at -6.35 2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at -6.35 -2.54 270) (size 3.048 1.7272) (drill 1.2192) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_12mm.step
      (offset (xyz 0 0 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer F.Cu) (tedit 0)
    (at 141.12 23.92)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J6 (at 8.89 -4.50088) (layer F.SilkS))
    (fp_text value Digital_Pins_8_13_GND_AREF (at 8.89 4.50088) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 20 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer F.Cu) (tedit 0)
    (at 119.4 24.03)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J5 (at 8.89 -4.50088) (layer F.SilkS))
    (fp_text value Digital_0_7 (at 8.89 4.50088) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer F.Cu) (tedit 0)
    (at 141.14 21.03)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J4 (at 8.89 -4.50088) (layer F.SilkS))
    (fp_text value Digital_Pins_8_13_GND_AREF (at 8.89 4.50088) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 20 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (offset (xyz 8.890000000000001 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer F.Cu) (tedit 0)
    (at 136.88 69.34)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J3 (at 8.89 -4.50088) (layer F.SilkS))
    (fp_text value Power (at 8.89 4.50088) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (offset (xyz 8.890000000000001 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_6pol (layer F.Cu) (tedit 0)
    (at 119.27 69.31)
    (descr "6-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 6.35 -4.50088) (layer F.SilkS))
    (fp_text value Analog_0_5 (at 6.35 4.50088) (layer F.Fab))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_6pol.wrl
      (offset (xyz 6.349999904632568 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_8pol (layer F.Cu) (tedit 0)
    (at 119.3 21.04)
    (descr "8-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 8.89 -4.50088) (layer F.SilkS))
    (fp_text value Digital_0_7 (at 8.89 4.50088) (layer F.Fab))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_8pol.wrl
      (offset (xyz 8.889999866485596 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 132.207 42.5765 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 2.31 270) (layer B.SilkS))
    (fp_text value R (at 3.81 -2.31 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 136.271 42.5765 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 2.31 270) (layer B.SilkS))
    (fp_text value R (at 3.81 -2.31 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 153.8605 43.021 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 2.31 270) (layer B.SilkS))
    (fp_text value R (at 3.81 -2.31 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 158.97225 43.0845 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 2.31 270) (layer B.SilkS))
    (fp_text value R (at 3.81 -2.31 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer B.Cu) (tedit 5874F706)
    (at 164.084 43.021 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 2.31 270) (layer B.SilkS))
    (fp_text value R (at 3.81 -2.31 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad5)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad3)"))
    (model Resistors_ThroughHole.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text v0.1 (at 174.498 32.988) (layer B.SilkS))
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 111.48 19.76 270) (layer Dwgs.User))
    (feature1 (pts (xy 114.54 21.03) (xy 112.193579 21.03)))
    (feature2 (pts (xy 114.54 18.49) (xy 112.193579 18.49)))
    (crossbar (pts (xy 112.78 18.49) (xy 112.78 21.03)))
    (arrow1a (pts (xy 112.78 21.03) (xy 112.193579 19.903496)))
    (arrow1b (pts (xy 112.78 21.03) (xy 113.366421 19.903496)))
    (arrow2a (pts (xy 112.78 18.49) (xy 112.193579 19.616504)))
    (arrow2b (pts (xy 112.78 18.49) (xy 113.366421 19.616504)))
  )
  (dimension 4.06 (width 0.15) (layer Dwgs.User)
    (gr_text "4.060 mm" (at 139.12 13.52) (layer Dwgs.User))
    (feature1 (pts (xy 141.15 15.81) (xy 141.15 14.233579)))
    (feature2 (pts (xy 137.09 15.81) (xy 137.09 14.233579)))
    (crossbar (pts (xy 137.09 14.82) (xy 141.15 14.82)))
    (arrow1a (pts (xy 141.15 14.82) (xy 140.023496 15.406421)))
    (arrow1b (pts (xy 141.15 14.82) (xy 140.023496 14.233579)))
    (arrow2a (pts (xy 137.09 14.82) (xy 138.216504 15.406421)))
    (arrow2b (pts (xy 137.09 14.82) (xy 138.216504 14.233579)))
  )
  (dimension 2.54 (width 0.12) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 118.03 14.529478) (layer Dwgs.User))
    (feature1 (pts (xy 119.3 16.64) (xy 119.3 15.213057)))
    (feature2 (pts (xy 116.76 16.64) (xy 116.76 15.213057)))
    (crossbar (pts (xy 116.76 15.799478) (xy 119.3 15.799478)))
    (arrow1a (pts (xy 119.3 15.799478) (xy 118.173496 16.385899)))
    (arrow1b (pts (xy 119.3 15.799478) (xy 118.173496 15.213057)))
    (arrow2a (pts (xy 116.76 15.799478) (xy 117.886504 16.385899)))
    (arrow2b (pts (xy 116.76 15.799478) (xy 117.886504 15.213057)))
  )
  (dimension 10 (width 0.12) (layer F.SilkS)
    (gr_text "10.000 mm" (at 174.3 65.684997) (layer F.SilkS))
    (feature1 (pts (xy 179.3 69.3) (xy 179.3 66.368576)))
    (feature2 (pts (xy 169.3 69.3) (xy 169.3 66.368576)))
    (crossbar (pts (xy 169.3 66.954997) (xy 179.3 66.954997)))
    (arrow1a (pts (xy 179.3 66.954997) (xy 178.173496 67.541418)))
    (arrow1b (pts (xy 179.3 66.954997) (xy 178.173496 66.368576)))
    (arrow2a (pts (xy 169.3 66.954997) (xy 170.426504 67.541418)))
    (arrow2b (pts (xy 169.3 66.954997) (xy 170.426504 66.368576)))
  )
  (dimension 4.318 (width 0.12) (layer Cmts.User)
    (gr_text "4.318 mm" (at 139.319 12.954) (layer Cmts.User))
    (feature1 (pts (xy 141.478 15.24) (xy 141.478 13.637579)))
    (feature2 (pts (xy 137.16 15.24) (xy 137.16 13.637579)))
    (crossbar (pts (xy 137.16 14.224) (xy 141.478 14.224)))
    (arrow1a (pts (xy 141.478 14.224) (xy 140.351496 14.810421)))
    (arrow1b (pts (xy 141.478 14.224) (xy 140.351496 13.637579)))
    (arrow2a (pts (xy 137.16 14.224) (xy 138.286504 14.810421)))
    (arrow2b (pts (xy 137.16 14.224) (xy 138.286504 13.637579)))
  )
  (dimension 2.54 (width 0.12) (layer Cmts.User)
    (gr_text "2.540 mm" (at 118.11 12.954) (layer Cmts.User))
    (feature1 (pts (xy 119.38 15.748) (xy 119.38 13.637579)))
    (feature2 (pts (xy 116.84 15.748) (xy 116.84 13.637579)))
    (crossbar (pts (xy 116.84 14.224) (xy 119.38 14.224)))
    (arrow1a (pts (xy 119.38 14.224) (xy 118.253496 14.810421)))
    (arrow1b (pts (xy 119.38 14.224) (xy 118.253496 13.637579)))
    (arrow2a (pts (xy 116.84 14.224) (xy 117.966504 14.810421)))
    (arrow2b (pts (xy 116.84 14.224) (xy 117.966504 13.637579)))
  )
  (dimension 2.54 (width 0.12) (layer Cmts.User)
    (gr_text "2.540 mm" (at 110.998 19.812 270) (layer Cmts.User))
    (feature1 (pts (xy 114.554 21.082) (xy 111.681579 21.082)))
    (feature2 (pts (xy 114.554 18.542) (xy 111.681579 18.542)))
    (crossbar (pts (xy 112.268 18.542) (xy 112.268 21.082)))
    (arrow1a (pts (xy 112.268 21.082) (xy 111.681579 19.955496)))
    (arrow1b (pts (xy 112.268 21.082) (xy 112.854421 19.955496)))
    (arrow2a (pts (xy 112.268 18.542) (xy 111.681579 19.668504)))
    (arrow2b (pts (xy 112.268 18.542) (xy 112.854421 19.668504)))
  )
  (gr_text "the\nd-pad" (at 174.498 27.178) (layer B.SilkS))
  (gr_text www.mathcodeprint.com (at 133.985 59.69) (layer B.SilkS))
  (gr_text @mathcodeprint (at 133.35 31.115) (layer B.SilkS))
  (dimension 4.890041 (width 0.15) (layer Dwgs.User)
    (gr_text "4.890 mm" (at 134.39345 76.913976 359.7656627) (layer Dwgs.User))
    (feature1 (pts (xy 136.85 74.1) (xy 136.841368 76.210403)))
    (feature2 (pts (xy 131.96 74.08) (xy 131.951368 76.190403)))
    (crossbar (pts (xy 131.953767 75.603987) (xy 136.843767 75.623987)))
    (arrow1a (pts (xy 136.843767 75.623987) (xy 135.714874 76.205795)))
    (arrow1b (pts (xy 136.843767 75.623987) (xy 135.719671 75.032964)))
    (arrow2a (pts (xy 131.953767 75.603987) (xy 133.077863 76.19501)))
    (arrow2b (pts (xy 131.953767 75.603987) (xy 133.08266 75.022179)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 111.486 70.58 90) (layer Dwgs.User))
    (feature1 (pts (xy 114.31 69.31) (xy 112.199579 69.31)))
    (feature2 (pts (xy 114.31 71.85) (xy 112.199579 71.85)))
    (crossbar (pts (xy 112.786 71.85) (xy 112.786 69.31)))
    (arrow1a (pts (xy 112.786 69.31) (xy 113.372421 70.436504)))
    (arrow1b (pts (xy 112.786 69.31) (xy 112.199579 70.436504)))
    (arrow2a (pts (xy 112.786 71.85) (xy 113.372421 70.723496)))
    (arrow2b (pts (xy 112.786 71.85) (xy 112.199579 70.723496)))
  )
  (dimension 2.54 (width 0.15) (layer Dwgs.User)
    (gr_text "2.540 mm" (at 118.01 76.600999) (layer Dwgs.User))
    (feature1 (pts (xy 119.28 73.65) (xy 119.28 75.88742)))
    (feature2 (pts (xy 116.74 73.65) (xy 116.74 75.88742)))
    (crossbar (pts (xy 116.74 75.300999) (xy 119.28 75.300999)))
    (arrow1a (pts (xy 119.28 75.300999) (xy 118.153496 75.88742)))
    (arrow1b (pts (xy 119.28 75.300999) (xy 118.153496 74.714578)))
    (arrow2a (pts (xy 116.74 75.300999) (xy 117.866504 75.88742)))
    (arrow2b (pts (xy 116.74 75.300999) (xy 117.866504 74.714578)))
  )
  (gr_arc (start 182.16 71.19) (end 182.8 71.2) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.8 71.19) (end 182.8 19.12) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 182.160006 19.117214) (end 182.17 18.48) (angle 91.78304139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.162792 18.47722) (end 118.04 18.47) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.032792 18.47722) (end 116.77 19.74) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.77 19.75) (end 116.76 31) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 116.270489 30.99088) (end 116.757425 30.955248) (angle 45) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.65 31.29) (end 114.44 33.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 114.859999 33.99) (end 114.22 33.96329) (angle 44.99995999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.22 33.99767) (end 114.22 66.47767) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 114.879884 66.479855) (end 114.41 66.94) (angle 45) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.398802 66.933705) (end 116.562548 69.097452) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 116.11 69.55) (end 116.56 69.09) (angle 45) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.75 69.55) (end 116.75 71.19) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 117.39 71.19) (end 117.42 71.83) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.39 71.83) (end 182.16 71.83) (angle 90) (layer Edge.Cuts) (width 0.1))
)
