(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 37)
    (no_connects 0)
    (area 99.338 69.5198 178.510001 123.265001)
    (thickness 1.6)
    (drawings 49)
    (tracks 151)
    (zones 0)
    (modules 13)
    (nets 14)
  )
  (page USLetter)
  (title_block
    (title "Atmega328-based AVR Programmer")
    (date "09 Jan 2017")
    (rev v1.0)
    (company "CERN Open Hardware License v1.2")
    (comment 1 jenner@wickerbox.net)
    (comment 2 http://wickerbox.net)
    (comment 3 "Wickerbox Electronics")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 /~RESET)
  (net 2 /FTDI_RESET)
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(C3-Pad1)")
  (net 6 /FTDI_RX/D1_TX)
  (net 7 /FTDI_TX/D0_RX)
  (net 8 /MISO)
  (net 9 /SCK)
  (net 10 /MOSI)
  (net 11 VIN)
  (net 12 /ISP_RST)
  (net 13 CS_D10)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /FTDI_RESET)
    (add_net /FTDI_RX/D1_TX)
    (add_net /FTDI_TX/D0_RX)
    (add_net /ISP_RST)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /~RESET)
    (add_net CS_D10)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net VIN)
  )
  (module Wickerlib:SWITCH-OMRON-MOMENTARY-SMD-B3U-1000P (layer F.Cu) (tedit 587457BC)
    (at 110.9 77.978)
    (descr SW-B3F-10XX)
    (tags "Omron B3F-10xx")
    (fp_text reference S1 (at 1.778 0) (layer F.Fab))
    (fp_text value RESET (at 1.524 0) (layer F.Fab) hide)
    (fp_text user %R (at 5.686 0) (layer F.SilkS) hide)
    (pad 2 smd rect (at 3.4 0) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
    (pad 1 smd rect (at 0 0) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 110.732 80.772 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C1 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 2.274 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /FTDI_RESET))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 110.744 83.439)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C2 (at 0.09 0.04) (layer F.Fab))
    (fp_text value 22pF (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at -2.286 0.127 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 114.173 89.801 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C3 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 22pF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.171 -0.127 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 127.254 86.094 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C5 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.298 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 114.3 85.356 90)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C6 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.044 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x06 (layer F.Cu) (tedit 58745455)
    (at 102.997 77.47)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -0.01 6.35 180) (layer F.Fab))
    (fp_text value FTDI (at -2.63 6.86 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.14 -2.74) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /FTDI_RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /FTDI_RX/D1_TX))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /FTDI_TX/D0_RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 VIN))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Wickerlib:RLC-0805-SMD (layer F.Cu) (tedit 57904162)
    (at 132.08 78.74)
    (descr "Capacitor SMD RLC-0805-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0805-SMD")
    (attr smd)
    (fp_text reference R1 (at 0 0 180) (layer F.Fab))
    (fp_text value 10K (at 0 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.778 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
  )
  (module Wickerlib:CRYSTAL-CTS-4SMD (layer F.Cu) (tedit 58156A29)
    (at 110.5408 88.011 270)
    (fp_text reference X1 (at 0 -0.4572 360) (layer F.Fab))
    (fp_text value "16MHz 18pF" (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at -0.127 2.3368 270) (layer F.SilkS))
    (pad 3 smd rect (at 2.1844 -1.4732 270) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at -2.286 -1.4732 270) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2.1844 1.016 270) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -2.286 1.016 270) (size 1.905 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module Wickerlib:TQFP-32-7x7MM-P0.8MM (layer F.Cu) (tedit 587459A6)
    (at 120.777 85.979)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 0) (layer F.Fab))
    (fp_text value ATMEGA328 (at 0 6.05) (layer F.Fab) hide)
    (fp_text user %R (at 4.953 -4.386 180) (layer F.SilkS))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 CS_D10))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /MISO))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /SCK))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /~RESET))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /FTDI_TX/D0_RX))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /FTDI_RX/D1_TX))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 106.68 87.491 270)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C4 (at 0.09 0.04 270) (layer F.Fab))
    (fp_text value 1uF (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.012 1.397 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VIN))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-2x03 (layer F.Cu) (tedit 589D56B3)
    (at 133.35 87.63 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 1.27 2.54 180) (layer F.Fab))
    (fp_text value ISP-2560 (at 3.556 2.794 270) (layer F.Fab) hide)
    (fp_text user %R (at -0.254 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 VIN))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /ISP_RST))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Wickerlib:SWITCH-ESWITCH-SLIDE-TH-EG1218 (layer F.Cu) (tedit 589D5822)
    (at 137.9728 83.82 270)
    (fp_text reference S2 (at 0 0 360) (layer F.Fab))
    (fp_text value SLIDE (at 0 2 270) (layer F.Fab) hide)
    (fp_text user %R (at 7.0612 0 360) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /ISP_RST))
    (pad 3 thru_hole circle (at 2.4892 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 CS_D10))
    (pad 1 thru_hole circle (at -2.4892 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /~RESET))
  )
  (gr_text "PROG = Put bootloader on other board" (at 121.7422 90.424) (layer B.SilkS))
  (gr_text "TARGET = Put bootloader on this board" (at 120.8024 80.2132) (layer B.SilkS))
  (gr_text TARGET (at 137.8712 76.8604) (layer F.SilkS))
  (gr_text PROG (at 138.176 90.8304) (layer F.SilkS))
  (gr_text "Assembly Diagram\nAVR Programmer v1.1\n2/9/17" (at 141.224 71.9836) (layer F.Fab))
  (gr_text wickerbox.net (at 110.617 86.7664) (layer B.SilkS))
  (gr_text "AVR Programmer v1.1" (at 125.476 77.216) (layer B.SilkS))
  (gr_line (start 129.54 92.075) (end 102.87 92.075) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 139.7762 92.075) (end 129.54 92.075) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 141.5796 77.47) (end 141.5796 90.17) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 139.8016 75.565) (end 102.87 75.565) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 100.965 77.47) (end 100.965 90.17) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 102.87 90.17) (end 102.87 92.075) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 102.87 77.47) (end 100.965 77.47) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 139.6746 90.17) (end 141.5796 90.17) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 139.6746 77.47) (end 139.6746 75.565) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_text RESET (at 117.856 77.978) (layer F.SilkS))
  (gr_text GND (at 106.5276 90.2208) (layer F.SilkS))
  (gr_text 5V (at 106.051048 85.09) (layer F.SilkS))
  (gr_text TX (at 106.002667 82.55) (layer F.SilkS))
  (gr_text RX (at 106.123619 80.01) (layer F.SilkS))
  (gr_text RST (at 106.510667 77.47) (layer F.SilkS))
  (gr_text ICSP (at 132.1308 90.7288) (layer F.SilkS))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.5288 75.6666) (xy 101.092 75.692) (xy 101.092 91.948) (xy 141.5288 91.9226)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.5288 75.6666) (xy 101.092 75.692) (xy 101.092 91.948) (xy 141.5288 91.9226)
      )
    )
  )
)
