(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 34)
    (no_connects 0)
    (area 140.894999 89.459999 156.285001 121.360001)
    (thickness 1.6)
    (drawings 4)
    (tracks 84)
    (zones 0)
    (modules 36)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.8 2.8)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P1-Pad2)")
  (net 3 "Net-(P1-Pad3)")
  (net 4 "Net-(P1-Pad4)")
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(P1-Pad6)")
  (net 7 "Net-(P1-Pad7)")
  (net 8 "Net-(P1-Pad8)")
  (net 9 "Net-(P1-Pad9)")
  (net 10 "Net-(P1-Pad10)")
  (net 11 "Net-(P1-Pad11)")
  (net 12 "Net-(P1-Pad12)")
  (net 13 "Net-(P2-Pad1)")
  (net 14 "Net-(P2-Pad2)")
  (net 15 "Net-(P2-Pad4)")
  (net 16 "Net-(P2-Pad5)")
  (net 17 "Net-(P2-Pad6)")
  (net 18 "Net-(P2-Pad7)")
  (net 19 "Net-(P2-Pad8)")
  (net 20 "Net-(P2-Pad9)")
  (net 21 "Net-(P2-Pad10)")
  (net 22 "Net-(P2-Pad11)")
  (net 23 "Net-(P2-Pad12)")
  (net 24 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad10)")
    (add_net "Net-(P2-Pad11)")
    (add_net "Net-(P2-Pad12)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 144.78 107.95)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 152.4 100.33)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 152.4 113.03)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 144.78 119.38)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 147.32 119.38)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 151.13 118.11)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 149.86 116.84)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 147.32 116.84)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 149.86 119.38)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 152.4 119.38)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 148.59 118.11)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 146.05 118.11)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 148.59 115.57)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 147.32 110.49)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 146.05 114.3)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 151.13 92.71)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 148.59 95.25)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 148.59 92.71)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 144.78 95.25)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 144.78 92.71)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 152.273 95.504)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 150.495 97.028)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 148.717 98.806)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 152.908 97.79)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784C34)
    (at 149.352 105.918)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784C2A)
    (at 148.463 105.918)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784C23)
    (at 149.352 105.029)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784C18)
    (at 148.463 105.029)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784C09)
    (at 147.574 105.918)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784C03)
    (at 147.574 105.029)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BFD)
    (at 149.352 104.14)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BF4)
    (at 148.463 104.14)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (module lolsborn:PINHEAD_1x12 (layer F.Cu) (tedit 587849EC)
    (at 142.24 104.14 90)
    (fp_text reference P1 (at -2.54 -20.32 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 2.54 -10.16 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -15.24 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -12.7 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad3)"))
    (pad 4 thru_hole circle (at -7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at -5.08 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad5)"))
    (pad 6 thru_hole circle (at -2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad6)"))
    (pad 7 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad7)"))
    (pad 8 thru_hole circle (at 2.54 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad9)"))
    (pad 10 thru_hole circle (at 7.62 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad10)"))
    (pad 11 thru_hole circle (at 10.16 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad11)"))
    (pad 12 thru_hole circle (at 12.7 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P1-Pad12)"))
  )
  (module lolsborn:PINHEAD_1x12 (layer F.Cu) (tedit 587849E8)
    (at 154.94 106.68 270)
    (fp_text reference P2 (at -2.54 33.02 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 5.08 22.86 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -15.24 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at -12.7 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P2-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 24 GND))
    (pad 4 thru_hole circle (at -7.62 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P2-Pad4)"))
    (pad 5 thru_hole circle (at -5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P2-Pad5)"))
    (pad 6 thru_hole circle (at -2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P2-Pad6)"))
    (pad 7 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P2-Pad7)"))
    (pad 8 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P2-Pad8)"))
    (pad 9 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P2-Pad9)"))
    (pad 10 thru_hole circle (at 7.62 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P2-Pad10)"))
    (pad 11 thru_hole circle (at 10.16 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P2-Pad11)"))
    (pad 12 thru_hole circle (at 12.7 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P2-Pad12)"))
  )
  (module lolsborn:QFN50P400X400X100-25N (layer F.Cu) (tedit 58784C56)
    (at 148.5011 105.0036)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U1 (at 0.04 -3.235) (layer F.SilkS))
    (fp_text value TLC59283 (at 0.475 6.7564) (layer F.SilkS))
    (pad 1 smd rect (at -2 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P1-Pad12)") (solder_mask_margin 0.2))
    (pad 2 smd rect (at -2 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P1-Pad11)") (solder_mask_margin 0.2))
    (pad 3 smd rect (at -2 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad10)") (solder_mask_margin 0.2))
    (pad 4 smd rect (at -2 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P1-Pad9)") (solder_mask_margin 0.2))
    (pad 5 smd rect (at -2 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad8)") (solder_mask_margin 0.2))
    (pad 6 smd rect (at -2 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad7)") (solder_mask_margin 0.2))
    (pad 7 smd rect (at -1.25 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad6)") (solder_mask_margin 0.2))
    (pad 8 smd rect (at -0.75 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad5)") (solder_mask_margin 0.2))
    (pad 9 smd rect (at -0.25 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad4)") (solder_mask_margin 0.2))
    (pad 10 smd rect (at 0.25 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad3)") (solder_mask_margin 0.2))
    (pad 11 smd rect (at 0.75 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P1-Pad2)") (solder_mask_margin 0.2))
    (pad 12 smd rect (at 1.25 2 90) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(P1-Pad1)") (solder_mask_margin 0.2))
    (pad 13 smd rect (at 2 1.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(P2-Pad12)") (solder_mask_margin 0.2))
    (pad 14 smd rect (at 2 0.75 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(P2-Pad11)") (solder_mask_margin 0.2))
    (pad 15 smd rect (at 2 0.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P2-Pad10)") (solder_mask_margin 0.2))
    (pad 16 smd rect (at 2 -0.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad9)") (solder_mask_margin 0.2))
    (pad 17 smd rect (at 2 -0.75 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P2-Pad8)") (solder_mask_margin 0.2))
    (pad 18 smd rect (at 2 -1.25 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(P2-Pad7)") (solder_mask_margin 0.2))
    (pad 19 smd rect (at 1.25 -2 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(P2-Pad6)") (solder_mask_margin 0.2))
    (pad 20 smd rect (at 0.75 -2 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P2-Pad5)") (solder_mask_margin 0.2))
    (pad 21 smd rect (at 0.25 -2 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P2-Pad4)") (solder_mask_margin 0.2))
    (pad 22 smd rect (at -0.25 -2 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 GND) (solder_mask_margin 0.2))
    (pad 23 smd rect (at -0.75 -2 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P2-Pad2)") (solder_mask_margin 0.2))
    (pad 24 smd rect (at -1.25 -2 270) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P2-Pad1)") (solder_mask_margin 0.2))
    (pad 25 smd rect (at 0 0) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 24 GND) (solder_mask_margin 0.2))
  )
  (module lolsborn:via-0.6mm (layer F.Cu) (tedit 58784BE4)
    (at 147.574 104.14)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value via (at 0 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 24 GND) (zone_connect 2))
  )
  (gr_line (start 156.21 89.535) (end 140.97 89.535) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 121.285) (end 156.21 89.535) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 121.285) (end 156.21 121.285) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 89.535) (end 140.97 121.285) (layer Edge.Cuts) (width 0.15))
  (zone (net 24) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.335 89.535) (xy 156.845 89.535) (xy 156.845 121.285) (xy 140.335 121.285)
      )
    )
  )
  (zone (net 24) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.335 89.535) (xy 156.845 89.535) (xy 156.845 121.285) (xy 140.335 121.285)
      )
    )
  )
)
