(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (comment 4 "PCBWay Project ID: 445b4783-7fe5-4db3-865c-796d1ee828e5")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J3-Pad1)")
  (net 2 "Net-(R2-Pad2)")
  (net 3 "Net-(J10-Pad4)")
  (net 4 "Net-(J10-Pad3)")
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(R1-Pad1)")
  (net 8 "Net-(Q1-Pad1)")
  (net 9 "Net-(J10-Pad2)")
  (net 10 "Net-(J11-Pad2)")
  (net 11 "Net-(J10-Pad1)")
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 139.7 113.9)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -2.2 -0.1) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Female" (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 "Net-(J10-Pad4)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 153.3 103.74)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 2.3 0.06) (layer "F.SilkS"))
    (fp_text value " " (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "BC817:SOT95P230X110-3N" (layer "F.Cu")
    (tedit 63DCC9FD)
    (at 151.45 113.85)
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at -1.2 0) (layer "F.SilkS"))
    (fp_text value "MMBT3904WR" (at 7.35 2.65) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.98 -0.95) (size 1.26 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 8 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect locked (at -0.98 0.95) (size 1.26 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 11 "Net-(J10-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.98 0) (size 1.26 0.59) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.07)
      (net 5 "Net-(D1-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD_USER_3DMODELS}/MMBT3904 RF.STEP"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "SMT-0540-T-9-R:XDCR_SMT-0540-T-9-R" (layer "F.Cu")
    (tedit 63D6F9FC)
    (at 146.5 109 180)
    (property "MANUFACTURER" "Pui Audio")
    (property "MAXIMUM_PACKAGE_HEIGHT" "2.2 mm")
    (property "PARTREV" "A")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LS1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "SMT-0540-T-9-R" (at 8.515 3.775) (layer "F.Fab"))
    (pad "" smd rect locked (at -2.125 -1.75 180) (size 2.25 1.7) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "LOAD+" smd rect locked (at -2.125 1.75 180) (size 2.25 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(J3-Pad1)") (pintype "passive"))
    (pad "LOAD-" smd rect locked (at 2.125 1.75 180) (size 2.25 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD_USER_3DMODELS}/SMT-0540-T-9-R.step"
      (offset (xyz 0 -11 -5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x04_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 144.6 117.3 90)
    (descr "Through hole straight pin header, 1x04, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x04 1.27mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at -2.5 1.7) (layer "F.SilkS"))
    (fp_text value "Connector" (at 0 5.505 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.905) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 "Net-(J10-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 "Net-(J10-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x04_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.9 108.7)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -3.5 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J10-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 153.3 106.28)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 2.3 0.02) (layer "F.SilkS"))
    (fp_text value " " (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 9 "Net-(J10-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142 113.8 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 9.7) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J10-Pad4)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x02_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 140.75 117.3 90)
    (descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.27mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at -2.5 0.75) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.965 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.635) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J11-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x02_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 148.5 113.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.1 7.05) (layer "F.SilkS"))
    (fp_text value "180R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.515 0.185 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 146.5 113.8 -90)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0.05 -0.05) (layer "F.SilkS"))
    (fp_text value "DIODE" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 5 "Net-(D1-Pad1)") (pinfunction "K") (pintype "input"))
    (pad "2" smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 1 "Net-(J3-Pad1)") (pinfunction "A") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 139.7 106.28)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -2.2 0.02) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Female" (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 139.7 103.74)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -2.3 0.26) (layer "F.SilkS"))
    (fp_text value " " (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 "Net-(R1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 139.7 111.36)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -2.2 0.04) (layer "F.SilkS"))
    (fp_text value " " (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 "Net-(J10-Pad3)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x02_P1.27mm_Vertical" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 150.95 117.3 90)
    (descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.27mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at -2.5 0.65) (layer "F.SilkS"))
    (fp_text value " " (at 0 2.965 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.635) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 "Net-(J11-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 "Net-(J3-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x02_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.1 110.9)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 3.3 0.1) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.2625 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 153.3 101.2)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 2.3 0) (layer "F.SilkS"))
    (fp_text value " " (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 "Net-(R2-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.00mm:PinHeader_1x01_P1.00mm_Vertical" (layer "F.Cu")
    (tedit 59FED738)
    (at 153.3 108.82)
    (descr "Through hole straight pin header, 1x01, 1.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 1.00mm single row")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 2.3 -0.02) (layer "F.SilkS"))
    (fp_text value " " (at 0 1.56) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x01_P1.00mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.5 113.8 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "AirspeedProbe_Jan23_PCB_XiaoDaughter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -9.5) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 141 100.1) (end 142 101.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151 106.02) (end 142 106.02) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154.2 100.1) (end 154.6 100.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141 100.1) (end 138.8 100.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.4 100.5) (end 138.8 100.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 151 106.02) (end 151 101.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154.2 100.1) (end 152 100.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.4 118.02) (end 138.4 100.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154.6 118.02) (end 153.6 119.02) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 139.4 119.02) (end 153.6 119.02) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 142 106.02) (end 142 101.1) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154.6 100.5) (end 154.6 118.02) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.4 118.02) (end 139.4 119.02) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 152 100.1) (end 151 101.1) (layer "Edge.Cuts") (width 0.1))
)
