(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 38)
    (tracks 1296)
    (zones 0)
    (modules 76)
    (nets 133)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 Cin)
  (net 3 Din)
  (net 4 GND)
  (net 5 Cout)
  (net 6 Dout)
  (net 7 "Net-(U1-Pad6)")
  (net 8 "Net-(U1-Pad5)")
  (net 9 "Net-(U2-Pad6)")
  (net 10 "Net-(U2-Pad5)")
  (net 11 "Net-(U3-Pad6)")
  (net 12 "Net-(U3-Pad5)")
  (net 13 "Net-(U4-Pad6)")
  (net 14 "Net-(U4-Pad5)")
  (net 15 "Net-(U5-Pad6)")
  (net 16 "Net-(U5-Pad5)")
  (net 17 "Net-(U6-Pad6)")
  (net 18 "Net-(U6-Pad5)")
  (net 19 "Net-(U7-Pad6)")
  (net 20 "Net-(U7-Pad5)")
  (net 21 "Net-(U10-Pad2)")
  (net 22 "Net-(U10-Pad3)")
  (net 23 "Net-(U17-Pad5)")
  (net 24 "Net-(U17-Pad6)")
  (net 25 "Net-(U10-Pad6)")
  (net 26 "Net-(U10-Pad5)")
  (net 27 "Net-(U11-Pad6)")
  (net 28 "Net-(U11-Pad5)")
  (net 29 "Net-(U12-Pad6)")
  (net 30 "Net-(U12-Pad5)")
  (net 31 "Net-(U13-Pad6)")
  (net 32 "Net-(U13-Pad5)")
  (net 33 "Net-(U14-Pad6)")
  (net 34 "Net-(U14-Pad5)")
  (net 35 "Net-(U15-Pad6)")
  (net 36 "Net-(U15-Pad5)")
  (net 37 "Net-(U16-Pad6)")
  (net 38 "Net-(U16-Pad5)")
  (net 39 "Net-(U8-Pad6)")
  (net 40 "Net-(U8-Pad5)")
  (net 41 "Net-(U18-Pad6)")
  (net 42 "Net-(U18-Pad5)")
  (net 43 "Net-(U19-Pad6)")
  (net 44 "Net-(U19-Pad5)")
  (net 45 "Net-(U20-Pad6)")
  (net 46 "Net-(U20-Pad5)")
  (net 47 "Net-(U21-Pad6)")
  (net 48 "Net-(U21-Pad5)")
  (net 49 "Net-(U22-Pad6)")
  (net 50 "Net-(U22-Pad5)")
  (net 51 "Net-(U23-Pad6)")
  (net 52 "Net-(U23-Pad5)")
  (net 53 "Net-(U24-Pad6)")
  (net 54 "Net-(U24-Pad5)")
  (net 55 "Net-(U25-Pad6)")
  (net 56 "Net-(U25-Pad5)")
  (net 57 "Net-(U26-Pad6)")
  (net 58 "Net-(U26-Pad5)")
  (net 59 "Net-(U27-Pad6)")
  (net 60 "Net-(U27-Pad5)")
  (net 61 "Net-(U28-Pad6)")
  (net 62 "Net-(U28-Pad5)")
  (net 63 "Net-(U29-Pad6)")
  (net 64 "Net-(U29-Pad5)")
  (net 65 "Net-(U30-Pad6)")
  (net 66 "Net-(U30-Pad5)")
  (net 67 "Net-(U31-Pad6)")
  (net 68 "Net-(U31-Pad5)")
  (net 69 "Net-(U32-Pad6)")
  (net 70 "Net-(U32-Pad5)")
  (net 71 "Net-(U33-Pad6)")
  (net 72 "Net-(U33-Pad5)")
  (net 73 "Net-(U34-Pad6)")
  (net 74 "Net-(U34-Pad5)")
  (net 75 "Net-(U35-Pad6)")
  (net 76 "Net-(U35-Pad5)")
  (net 77 "Net-(U36-Pad6)")
  (net 78 "Net-(U36-Pad5)")
  (net 79 "Net-(U37-Pad6)")
  (net 80 "Net-(U37-Pad5)")
  (net 81 "Net-(U38-Pad6)")
  (net 82 "Net-(U38-Pad5)")
  (net 83 "Net-(U39-Pad6)")
  (net 84 "Net-(U39-Pad5)")
  (net 85 "Net-(U40-Pad6)")
  (net 86 "Net-(U40-Pad5)")
  (net 87 "Net-(U41-Pad6)")
  (net 88 "Net-(U41-Pad5)")
  (net 89 "Net-(U42-Pad6)")
  (net 90 "Net-(U42-Pad5)")
  (net 91 "Net-(U43-Pad6)")
  (net 92 "Net-(U43-Pad5)")
  (net 93 "Net-(U44-Pad6)")
  (net 94 "Net-(U44-Pad5)")
  (net 95 "Net-(U45-Pad6)")
  (net 96 "Net-(U45-Pad5)")
  (net 97 "Net-(U46-Pad6)")
  (net 98 "Net-(U46-Pad5)")
  (net 99 "Net-(U47-Pad6)")
  (net 100 "Net-(U47-Pad5)")
  (net 101 "Net-(U48-Pad6)")
  (net 102 "Net-(U48-Pad5)")
  (net 103 "Net-(U49-Pad6)")
  (net 104 "Net-(U49-Pad5)")
  (net 105 "Net-(U50-Pad6)")
  (net 106 "Net-(U50-Pad5)")
  (net 107 "Net-(U51-Pad6)")
  (net 108 "Net-(U51-Pad5)")
  (net 109 "Net-(U52-Pad6)")
  (net 110 "Net-(U52-Pad5)")
  (net 111 "Net-(U53-Pad6)")
  (net 112 "Net-(U53-Pad5)")
  (net 113 "Net-(U54-Pad6)")
  (net 114 "Net-(U54-Pad5)")
  (net 115 "Net-(U55-Pad6)")
  (net 116 "Net-(U55-Pad5)")
  (net 117 "Net-(U56-Pad6)")
  (net 118 "Net-(U56-Pad5)")
  (net 119 "Net-(U57-Pad6)")
  (net 120 "Net-(U57-Pad5)")
  (net 121 "Net-(U58-Pad6)")
  (net 122 "Net-(U58-Pad5)")
  (net 123 "Net-(U59-Pad6)")
  (net 124 "Net-(U59-Pad5)")
  (net 125 "Net-(U60-Pad6)")
  (net 126 "Net-(U60-Pad5)")
  (net 127 "Net-(U61-Pad6)")
  (net 128 "Net-(U61-Pad5)")
  (net 129 "Net-(U62-Pad6)")
  (net 130 "Net-(U62-Pad5)")
  (net 131 "Net-(U63-Pad6)")
  (net 132 "Net-(U63-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net Cin)
    (add_net Cout)
    (add_net Din)
    (add_net Dout)
    (add_net GND)
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U10-Pad2)")
    (add_net "Net-(U10-Pad3)")
    (add_net "Net-(U10-Pad5)")
    (add_net "Net-(U10-Pad6)")
    (add_net "Net-(U11-Pad5)")
    (add_net "Net-(U11-Pad6)")
    (add_net "Net-(U12-Pad5)")
    (add_net "Net-(U12-Pad6)")
    (add_net "Net-(U13-Pad5)")
    (add_net "Net-(U13-Pad6)")
    (add_net "Net-(U14-Pad5)")
    (add_net "Net-(U14-Pad6)")
    (add_net "Net-(U15-Pad5)")
    (add_net "Net-(U15-Pad6)")
    (add_net "Net-(U16-Pad5)")
    (add_net "Net-(U16-Pad6)")
    (add_net "Net-(U17-Pad5)")
    (add_net "Net-(U17-Pad6)")
    (add_net "Net-(U18-Pad5)")
    (add_net "Net-(U18-Pad6)")
    (add_net "Net-(U19-Pad5)")
    (add_net "Net-(U19-Pad6)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U20-Pad5)")
    (add_net "Net-(U20-Pad6)")
    (add_net "Net-(U21-Pad5)")
    (add_net "Net-(U21-Pad6)")
    (add_net "Net-(U22-Pad5)")
    (add_net "Net-(U22-Pad6)")
    (add_net "Net-(U23-Pad5)")
    (add_net "Net-(U23-Pad6)")
    (add_net "Net-(U24-Pad5)")
    (add_net "Net-(U24-Pad6)")
    (add_net "Net-(U25-Pad5)")
    (add_net "Net-(U25-Pad6)")
    (add_net "Net-(U26-Pad5)")
    (add_net "Net-(U26-Pad6)")
    (add_net "Net-(U27-Pad5)")
    (add_net "Net-(U27-Pad6)")
    (add_net "Net-(U28-Pad5)")
    (add_net "Net-(U28-Pad6)")
    (add_net "Net-(U29-Pad5)")
    (add_net "Net-(U29-Pad6)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U30-Pad5)")
    (add_net "Net-(U30-Pad6)")
    (add_net "Net-(U31-Pad5)")
    (add_net "Net-(U31-Pad6)")
    (add_net "Net-(U32-Pad5)")
    (add_net "Net-(U32-Pad6)")
    (add_net "Net-(U33-Pad5)")
    (add_net "Net-(U33-Pad6)")
    (add_net "Net-(U34-Pad5)")
    (add_net "Net-(U34-Pad6)")
    (add_net "Net-(U35-Pad5)")
    (add_net "Net-(U35-Pad6)")
    (add_net "Net-(U36-Pad5)")
    (add_net "Net-(U36-Pad6)")
    (add_net "Net-(U37-Pad5)")
    (add_net "Net-(U37-Pad6)")
    (add_net "Net-(U38-Pad5)")
    (add_net "Net-(U38-Pad6)")
    (add_net "Net-(U39-Pad5)")
    (add_net "Net-(U39-Pad6)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U40-Pad5)")
    (add_net "Net-(U40-Pad6)")
    (add_net "Net-(U41-Pad5)")
    (add_net "Net-(U41-Pad6)")
    (add_net "Net-(U42-Pad5)")
    (add_net "Net-(U42-Pad6)")
    (add_net "Net-(U43-Pad5)")
    (add_net "Net-(U43-Pad6)")
    (add_net "Net-(U44-Pad5)")
    (add_net "Net-(U44-Pad6)")
    (add_net "Net-(U45-Pad5)")
    (add_net "Net-(U45-Pad6)")
    (add_net "Net-(U46-Pad5)")
    (add_net "Net-(U46-Pad6)")
    (add_net "Net-(U47-Pad5)")
    (add_net "Net-(U47-Pad6)")
    (add_net "Net-(U48-Pad5)")
    (add_net "Net-(U48-Pad6)")
    (add_net "Net-(U49-Pad5)")
    (add_net "Net-(U49-Pad6)")
    (add_net "Net-(U5-Pad5)")
    (add_net "Net-(U5-Pad6)")
    (add_net "Net-(U50-Pad5)")
    (add_net "Net-(U50-Pad6)")
    (add_net "Net-(U51-Pad5)")
    (add_net "Net-(U51-Pad6)")
    (add_net "Net-(U52-Pad5)")
    (add_net "Net-(U52-Pad6)")
    (add_net "Net-(U53-Pad5)")
    (add_net "Net-(U53-Pad6)")
    (add_net "Net-(U54-Pad5)")
    (add_net "Net-(U54-Pad6)")
    (add_net "Net-(U55-Pad5)")
    (add_net "Net-(U55-Pad6)")
    (add_net "Net-(U56-Pad5)")
    (add_net "Net-(U56-Pad6)")
    (add_net "Net-(U57-Pad5)")
    (add_net "Net-(U57-Pad6)")
    (add_net "Net-(U58-Pad5)")
    (add_net "Net-(U58-Pad6)")
    (add_net "Net-(U59-Pad5)")
    (add_net "Net-(U59-Pad6)")
    (add_net "Net-(U6-Pad5)")
    (add_net "Net-(U6-Pad6)")
    (add_net "Net-(U60-Pad5)")
    (add_net "Net-(U60-Pad6)")
    (add_net "Net-(U61-Pad5)")
    (add_net "Net-(U61-Pad6)")
    (add_net "Net-(U62-Pad5)")
    (add_net "Net-(U62-Pad6)")
    (add_net "Net-(U63-Pad5)")
    (add_net "Net-(U63-Pad6)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad6)")
    (add_net "Net-(U8-Pad5)")
    (add_net "Net-(U8-Pad6)")
    (add_net VDD)
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 40.64 315)
    (fp_text reference U28 (at -0.3556 1.27 315) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 315) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 "Net-(U28-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 "Net-(U28-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(U27-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(U27-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:mountingM2 (layer F.Cu) (tedit 5EBBE67F)
    (at 156.21 67.31)
    (fp_text reference H6 (at 0 0.5) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module neonpixelmatrix:mountingM2 (layer F.Cu) (tedit 5EBBE67F)
    (at 156.21 21.59)
    (fp_text reference H5 (at 0 0.5) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module neonpixelmatrix:mountingM2 (layer F.Cu) (tedit 5EBBE67F)
    (at 110.49 67.31)
    (fp_text reference H4 (at 0 0.5) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module neonpixelmatrix:mountingM2 (layer F.Cu) (tedit 5EBBE67F)
    (at 110.49 21.59)
    (fp_text reference H3 (at 0 0.5) (layer F.Fab) hide)
    (fp_text value MountingHole_Pad (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.1) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.49 52.07)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 156.21 52.07)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 Cout))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 156.21 59.69)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 Dout))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 156.21 29.21)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 156.21 36.83)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.49 29.21)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J6 (at 1.51 -0.21) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 Cin))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.49 36.83)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Din))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.49 59.69)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Male (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 71.12 315)
    (fp_text reference U64 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 Cout))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 Dout))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 132 "Net-(U63-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 131 "Net-(U63-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 71.12 315)
    (fp_text reference U63 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 131 "Net-(U63-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 132 "Net-(U63-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 130 "Net-(U62-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 129 "Net-(U62-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 71.12 315)
    (fp_text reference U62 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 129 "Net-(U62-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 130 "Net-(U62-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 128 "Net-(U61-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 127 "Net-(U61-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 71.12 315)
    (fp_text reference U61 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 127 "Net-(U61-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 128 "Net-(U61-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 126 "Net-(U60-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 125 "Net-(U60-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 71.12 315)
    (fp_text reference U60 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 125 "Net-(U60-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 126 "Net-(U60-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 124 "Net-(U59-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 123 "Net-(U59-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 71.12 315)
    (fp_text reference U59 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 123 "Net-(U59-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 124 "Net-(U59-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 122 "Net-(U58-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 121 "Net-(U58-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 71.12 315)
    (fp_text reference U58 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 121 "Net-(U58-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 122 "Net-(U58-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 120 "Net-(U57-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 119 "Net-(U57-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 71.12 315)
    (fp_text reference U57 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 119 "Net-(U57-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 120 "Net-(U57-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 118 "Net-(U56-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 117 "Net-(U56-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 63.5 315)
    (fp_text reference U56 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 117 "Net-(U56-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 118 "Net-(U56-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 116 "Net-(U55-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 115 "Net-(U55-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 63.5 315)
    (fp_text reference U55 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 115 "Net-(U55-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 116 "Net-(U55-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 114 "Net-(U54-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 113 "Net-(U54-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 63.5 315)
    (fp_text reference U54 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 113 "Net-(U54-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 114 "Net-(U54-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 112 "Net-(U53-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 111 "Net-(U53-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 63.5 315)
    (fp_text reference U53 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 111 "Net-(U53-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 112 "Net-(U53-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 110 "Net-(U52-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 109 "Net-(U52-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 63.5 315)
    (fp_text reference U52 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 109 "Net-(U52-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 110 "Net-(U52-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 108 "Net-(U51-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 107 "Net-(U51-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 63.5 315)
    (fp_text reference U51 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 107 "Net-(U51-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 108 "Net-(U51-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 106 "Net-(U50-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 105 "Net-(U50-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 63.5 315)
    (fp_text reference U50 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 105 "Net-(U50-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 106 "Net-(U50-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 104 "Net-(U49-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 103 "Net-(U49-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 63.552102 315)
    (fp_text reference U49 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 103 "Net-(U49-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 104 "Net-(U49-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 102 "Net-(U48-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 101 "Net-(U48-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 55.88 315)
    (fp_text reference U48 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 101 "Net-(U48-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 102 "Net-(U48-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 100 "Net-(U47-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 99 "Net-(U47-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 55.88 315)
    (fp_text reference U47 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 99 "Net-(U47-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 100 "Net-(U47-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 98 "Net-(U46-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 97 "Net-(U46-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 55.88 315)
    (fp_text reference U46 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 97 "Net-(U46-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 98 "Net-(U46-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(U45-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(U45-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 55.88 315)
    (fp_text reference U45 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 95 "Net-(U45-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 96 "Net-(U45-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 94 "Net-(U44-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 93 "Net-(U44-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 55.88 315)
    (fp_text reference U44 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 93 "Net-(U44-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 94 "Net-(U44-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 "Net-(U43-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 91 "Net-(U43-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 55.88 315)
    (fp_text reference U43 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 91 "Net-(U43-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 92 "Net-(U43-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 90 "Net-(U42-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 89 "Net-(U42-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 55.88 315)
    (fp_text reference U42 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 89 "Net-(U42-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 90 "Net-(U42-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 88 "Net-(U41-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 87 "Net-(U41-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 55.88 315)
    (fp_text reference U41 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 87 "Net-(U41-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 88 "Net-(U41-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 86 "Net-(U40-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 85 "Net-(U40-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 48.26 315)
    (fp_text reference U40 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 85 "Net-(U40-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 86 "Net-(U40-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 84 "Net-(U39-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 83 "Net-(U39-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 48.26 315)
    (fp_text reference U39 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 83 "Net-(U39-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 84 "Net-(U39-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 82 "Net-(U38-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 81 "Net-(U38-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 48.26 315)
    (fp_text reference U38 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 81 "Net-(U38-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 82 "Net-(U38-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 80 "Net-(U37-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 79 "Net-(U37-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 48.26 315)
    (fp_text reference U37 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 79 "Net-(U37-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 80 "Net-(U37-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 78 "Net-(U36-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 77 "Net-(U36-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 48.26 315)
    (fp_text reference U36 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 77 "Net-(U36-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 78 "Net-(U36-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 76 "Net-(U35-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 "Net-(U35-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 48.26 315)
    (fp_text reference U35 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 "Net-(U35-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 76 "Net-(U35-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 "Net-(U34-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 "Net-(U34-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 48.26 315)
    (fp_text reference U34 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 73 "Net-(U34-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 "Net-(U34-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 "Net-(U33-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 "Net-(U33-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 48.26 315)
    (fp_text reference U33 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 71 "Net-(U33-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 72 "Net-(U33-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 "Net-(U32-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 "Net-(U32-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 40.64 315)
    (fp_text reference U32 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 69 "Net-(U32-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 70 "Net-(U32-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 "Net-(U31-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 "Net-(U31-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 40.64 315)
    (fp_text reference U31 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 67 "Net-(U31-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 68 "Net-(U31-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 "Net-(U30-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 "Net-(U30-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 40.64 315)
    (fp_text reference U30 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 65 "Net-(U30-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 66 "Net-(U30-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 "Net-(U29-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 63 "Net-(U29-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 40.64 315)
    (fp_text reference U29 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 63 "Net-(U29-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 64 "Net-(U29-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 62 "Net-(U28-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 61 "Net-(U28-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 40.64 315)
    (fp_text reference U27 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 59 "Net-(U27-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 60 "Net-(U27-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 "Net-(U26-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 "Net-(U26-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 40.64 315)
    (fp_text reference U26 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 57 "Net-(U26-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 58 "Net-(U26-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(U25-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(U25-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 40.64 315)
    (fp_text reference U25 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(U25-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 56 "Net-(U25-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(U24-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "Net-(U24-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 33.02 315)
    (fp_text reference U24 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 53 "Net-(U24-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(U24-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(U23-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(U23-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 33.02 315)
    (fp_text reference U23 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 51 "Net-(U23-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 52 "Net-(U23-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(U22-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(U22-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 33.02 315)
    (fp_text reference U22 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 49 "Net-(U22-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 50 "Net-(U22-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(U21-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(U21-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 33.02 315)
    (fp_text reference U21 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 "Net-(U21-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 48 "Net-(U21-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(U20-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(U20-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 33.02 315)
    (fp_text reference U20 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 "Net-(U20-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 46 "Net-(U20-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(U19-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(U19-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 33.02 315)
    (fp_text reference U19 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 "Net-(U19-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 44 "Net-(U19-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(U18-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(U18-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 33.02 315)
    (fp_text reference U18 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(U18-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(U18-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(U17-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(U17-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 33.02 315)
    (fp_text reference U17 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(U17-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "Net-(U17-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(U16-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(U16-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 25.4 315)
    (fp_text reference U16 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 "Net-(U16-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 "Net-(U16-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(U15-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(U15-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 25.4 315)
    (fp_text reference U15 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(U15-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(U15-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(U14-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(U14-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 25.4 315)
    (fp_text reference U14 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 33 "Net-(U14-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(U14-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 25.4 315)
    (fp_text reference U13 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 "Net-(U13-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 "Net-(U13-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(U12-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "Net-(U12-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 25.4 315)
    (fp_text reference U12 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 29 "Net-(U12-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(U12-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(U11-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 25.4 315)
    (fp_text reference U11 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(U11-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(U11-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(U10-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(U10-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 25.4 315)
    (fp_text reference U10 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(U10-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(U10-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(U10-Pad3)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(U10-Pad2)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 25.4 315)
    (fp_text reference U9 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "Net-(U10-Pad2)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(U10-Pad3)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(U8-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(U8-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 160.02 17.78 315)
    (fp_text reference U8 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(U8-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(U8-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(U7-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(U7-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 152.4 17.78 315)
    (fp_text reference U7 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 "Net-(U7-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(U7-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(U6-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(U6-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 144.78 17.78 315)
    (fp_text reference U6 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(U6-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(U6-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(U5-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(U5-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 137.16 17.78 315)
    (fp_text reference U5 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(U5-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(U5-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(U4-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(U4-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 129.54 17.78 315)
    (fp_text reference U4 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(U4-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(U4-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(U3-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(U3-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 121.92 17.78 315)
    (fp_text reference U3 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(U3-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(U3-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 114.3 17.78 315)
    (fp_text reference U2 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(U2-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(U2-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad5)"))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad6)"))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (module neonpixelmatrix:neonpixel (layer F.Cu) (tedit 5EC23CEE)
    (at 106.68 17.78 315)
    (fp_text reference U1 (at -0.3556 1.27 135) (layer F.SilkS))
    (fp_text value neonpixel (at 0 -5.079999 135) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 1.27 -2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at 1.27 2.54 315) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at -1.27 2.54 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 Din))
    (pad 2 thru_hole circle (at -1.27 0 315) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 Cin))
    (pad 1 thru_hole roundrect (at -1.27 -2.54 315) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 VDD))
  )
  (gr_text PierreMuth (at 140.97 67.564) (layer B.Mask))
  (gr_text N (at 140.97 44.45) (layer B.SilkS))
  (gr_text i (at 133.35 29.21) (layer B.SilkS))
  (gr_text l (at 133.35 52.07) (layer B.SilkS))
  (gr_text o (at 125.73 44.45) (layer B.SilkS))
  (gr_text n (at 118.11 44.45) (layer B.SilkS))
  (gr_text e (at 133.096 44.45) (layer B.SilkS))
  (gr_text P (at 133.35 21.59) (layer B.SilkS))
  (gr_text x (at 133.35 36.83) (layer B.SilkS))
  (gr_text l (at 133.35 52.07) (layer F.SilkS))
  (gr_text x (at 133.35 36.83) (layer F.SilkS))
  (gr_text i (at 133.35 29.21) (layer F.SilkS))
  (gr_text P (at 133.35 21.59) (layer F.SilkS))
  (gr_text n (at 148.59 44.45) (layer F.SilkS))
  (gr_text o (at 140.97 44.45) (layer F.SilkS))
  (gr_text e (at 133.35 44.45) (layer F.SilkS))
  (gr_text N (at 125.73 44.45) (layer F.SilkS))
  (dimension 60.96 (width 0.15) (layer Cmts.User)
    (gr_text "2.4000 in" (at 168.94 44.45 270) (layer Cmts.User))
    (feature1 (pts (xy 163.83 74.93) (xy 168.226421 74.93)))
    (feature2 (pts (xy 163.83 13.97) (xy 168.226421 13.97)))
    (crossbar (pts (xy 167.64 13.97) (xy 167.64 74.93)))
    (arrow1a (pts (xy 167.64 74.93) (xy 167.053579 73.803496)))
    (arrow1b (pts (xy 167.64 74.93) (xy 168.226421 73.803496)))
    (arrow2a (pts (xy 167.64 13.97) (xy 167.053579 15.096504)))
    (arrow2b (pts (xy 167.64 13.97) (xy 168.226421 15.096504)))
  )
  (gr_text "VCC\n" (at 116.84 52.07) (layer B.SilkS))
  (gr_text GND (at 116.84 59.69) (layer B.SilkS))
  (gr_text "DI\n" (at 116.84 36.83) (layer B.SilkS))
  (gr_text "CI\n" (at 117.094 29.21) (layer B.SilkS))
  (gr_text "CO\n" (at 149.86 52.07) (layer B.SilkS))
  (gr_text "DO\n" (at 149.86 59.69) (layer B.SilkS))
  (gr_text "VCC\n" (at 149.86 36.83) (layer B.SilkS))
  (gr_text GND (at 149.86 29.21) (layer B.SilkS))
  (gr_line (start 163.83 74.93) (end 102.87 74.93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 163.83 13.97) (end 163.83 74.93) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.87 13.97) (end 163.83 13.97) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.87 74.93) (end 102.87 13.97) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 102.87 13.97) (xy 163.83 13.97) (xy 163.83 74.93) (xy 102.87 74.93)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 102.87 13.97) (xy 163.83 13.97) (xy 163.83 74.93) (xy 102.87 74.93)
      )
    )
  )
)
