<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.1">
<drawing>
<board>
<plain>
<wire x1="45.72" y1="34.8996" x2="0" y2="34.8996" width="0.025" layer="20"/>
<wire x1="45.72" y1="0" x2="45.72" y2="34.8996" width="0.025" layer="20"/>
<wire x1="0" y1="0" x2="45.72" y2="0" width="0.025" layer="20"/>
<wire x1="0" y1="34.8996" x2="0" y2="0" width="0.025" layer="20"/>
<text>GND</text>
<text>SCR</text>
<text>XFMR</text>
<text>4KV</text>
<text>FOR USE WITH: 
TR-1795 - 600V-0.2uF
TR-1700 - 400V-0.5uF
</text>
<text>25M</text>
<text>R2</text>
<text>600V (551V)- R2=5M
400V (382V)- R2=3M</text>
<text>ASSUMING:
SCR-&gt;22M-&gt;GND</text>
<text>CHOOSY EE'S CHOOSE M6

FARNSWORTH TESTED
GLOVER APPROVED</text>
</plain>
<libraries>
<library name="ConradsNew">
<packages>
<package name="OHMITE102E-SERIES">
</package>
<package name="CUSTOM_KM8_CAP">
</package>
<package name="7466004">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="ConradsNew" package="OHMITE102E-SERIES" value="OHMITE102E-SERIES"/>
<element name="U$2" library="ConradsNew" package="OHMITE102E-SERIES" value="OHMITE102E-SERIES"/>
<element name="U$3" library="ConradsNew" package="CUSTOM_KM8_CAP" value="CUSTOM_KM8_CAP"/>
<element name="U$4" library="ConradsNew" package="7466004" value="7466004"/>
<element name="U$5" library="ConradsNew" package="7466004" value="7466004"/>
<element name="U$6" library="ConradsNew" package="7466004" value="7466004"/>
<element name="U$7" library="ConradsNew" package="7466004" value="7466004"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="P$2"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="3_8KV">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="XFMR">
<contactref element="U$3" pad="P$3"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="SCR">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$3" pad="P$5"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$4" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
