(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 143)
    (zones 0)
    (modules 26)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.08)
    (user_trace_width 0.25)
    (user_trace_width 0.37)
    (user_trace_width 0.5)
    (user_trace_width 1.08)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.5 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 GND)
  (net 4 "Net-(C4-Pad2)")
  (net 5 "Net-(C1-Pad2)")
  (net 6 "Net-(C3-Pad1)")
  (net 7 +12V)
  (net 8 "Net-(F1-Pad2)")
  (net 9 "Net-(U1-Pad6)")
  (net 10 "Net-(Fl1-PadA)")
  (net 11 "Net-(C6-Pad2)")
  (net 12 "Net-(RV1-Pad2)")
  (net 13 "Net-(J2-Pad1)")
  (net 14 "Net-(C6-Pad1)")
  (net 15 "Net-(R1-Pad1)")
  (net 16 "Net-(R2-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 1.08)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(RV1-Pad2)")
  )
  (net_class 75Ohm ""
    (clearance 0.2)
    (trace_width 0.37)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class DC ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(U1-Pad6)")
  )
  (net_class klein ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(Fl1-PadA)")
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 206.26578 94.63786 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -0.16764 -2.72542) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J2-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(Fl1-PadA)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Bauteile_Mo:F-Printbuchse (layer F.Cu) (tedit 5DF8E2BE)
    (at 178.46802 99.00412 90)
    (fp_text reference J1 (at 4.3053 1.68148 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 4.8385 11.181 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 8.4125 8.405 90) (size 2.3 2.3) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 0.0125 8.405 90) (size 2.3 2.3) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 1 thru_hole circle (at 4.2125 4.205 90) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 8.4125 0.005 90) (size 2.3 2.3) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 0.0125 0.005 90) (size 2.3 2.3) (drill 2) (layers *.Cu *.Mask)
      (net 3 GND))
  )
  (module Fuse:Fuse_Littelfuse-NANO2-451_453 (layer F.Cu) (tedit 5DA6DC9F)
    (at 204.79766 83.0707 90)
    (descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
    (tags "Fuse Nano2")
    (attr smd)
    (fp_text reference F1 (at 0.93726 -2.48412 unlocked) (layer F.SilkS))
    (fp_text value Fuse_Small (at 0 2.7 90 unlocked) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.455 0 90) (size 1.96 3.15) (layers F.Cu F.Paste F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 2.455 0 90) (size 1.96 3.15) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount (layer F.Cu) (tedit 5DAA3454)
    (at 212.6361 94.69882 90)
    (descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
    (tags "SMA Straight Samtec Edge Mount")
    (attr smd)
    (fp_text reference J2 (at -4.84632 0.8509 180) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at 0 13 90) (layer F.Fab))
    (fp_text user %R (at 0 4.79 270) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.6 90) (layer Dwgs.User))
    (fp_text user "Board Thickness: 1.57mm" (at 0 -5.45 90) (layer Cmts.User))
    (pad 2 smd rect (at -2.825 0 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 2.825 0 90) (size 1.35 4.2) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -2.825 0 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 2.825 0 90) (size 1.35 4.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 0 0.2 90) (size 1.27 3.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-X-ST-EM1_EdgeMount.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x02_P3.81mm_Drill1.2mm (layer F.Cu) (tedit 5AEE5EF3)
    (at 212.67166 81.43748 180)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference J3 (at 1.79832 1.2954) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.905 3.81) (layer F.Fab))
    (fp_text user %R (at 1.905 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 2.99974 2.99974) (drill 1.19888) (layers *.Cu *.Mask)
      (net 8 "Net-(F1-Pad2)"))
  )
  (module Package_SO:SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm (layer F.Cu) (tedit 5C56E16F)
    (at 201.40168 90.2589)
    (descr "SOIC, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ada4898-1_4898-2.pdf#page=29), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -0.06604 -3.35788) (layer F.SilkS))
    (fp_text value ADP7142ARDZ-3.3 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 9 smd roundrect (at 0 0) (size 2.29 3) (layers F.Cu F.Mask) (roundrect_rratio 0.10917)
      (net 3 GND))
    (pad "" smd roundrect (at -0.57 -0.75) (size 0.92 1.21) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.57 0.75) (size 0.92 1.21) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.57 -0.75) (size 0.92 1.21) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.57 0.75) (size 0.92 1.21) (layers F.Paste) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +12V))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(U1-Pad6)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +12V))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +12V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8-1EP_3.9x4.9mm_P1.27mm_EP2.29x3mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Bauteile_Mo:AFS14 (layer F.Cu) (tedit 5DFF9927)
    (at 203.07046 94.90202)
    (attr smd)
    (fp_text reference Fl1 (at -2.44094 1.76022) (layer F.SilkS))
    (fp_text value Bauteile_Mo_AFS14 (at -3.55 -1.9375) (layer F.Fab))
    (pad E smd rect (at -2.05 0.3) (size 0.425 0.325) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad A smd rect (at -2.05 -0.275) (size 0.425 0.325) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Fl1-PadA)"))
    (pad B smd rect (at -2.6375 -0.375) (size 0.25 0.525) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad D smd rect (at -2.6375 0.4) (size 0.25 0.525) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad C smd rect (at -3.225 0.0125) (size 0.425 0.325) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad1)"))
    (model C:/Users/dd9fj/Desktop/HamRadio/KiCad_Projekte/eigene3D/AFS14.STEP
      (offset (xyz -2.6 0 0.4))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 -180 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 190.29426 94.7928 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -0.28194 -2.29362) (layer F.SilkS))
    (fp_text value 18p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 178.96586 81.66862 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0.0254 2.04216 180) (layer F.SilkS))
    (fp_text value 44p8 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 196.088 94.80042 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -0.00762 -2.41046) (layer F.SilkS))
    (fp_text value 33p (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 186.96178 84.44484)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.11938 1.57734) (layer F.SilkS))
    (fp_text value 10n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C6-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 211.08416 88.83904 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 1n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +12V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 196.59346 90.55354 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -0.03048 -1.81102 180) (layer F.SilkS))
    (fp_text value "2,2uf 16V" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 207.05572 90.8812 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 -1.65) (layer F.SilkS))
    (fp_text value "4,7uf 25V" (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 +12V))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 191.78524 86.10346)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.01778 1.65354) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 211.1502 85.30336)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D1 (at -2.31394 2.44602) (layer F.SilkS))
    (fp_text value D (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +12V))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 179.15128 85.77326 270)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 3.02768 0.01524 180) (layer F.SilkS))
    (fp_text value 120n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 182.88254 84.4677 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 68n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(C2-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 185.70956 81.12506 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 4u7 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 +12V))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 203.55306 95.57766 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.55524 -0.14732 180) (layer F.SilkS))
    (fp_text value 82 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(Fl1-PadA)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 208.99628 95.56242 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.57048 0.13462 180) (layer F.SilkS))
    (fp_text value 82 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J2-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Oscillator:Oscillator_SMD_SeikoEpson_SG8002CE-4Pin_3.2x2.5mm (layer F.Cu) (tedit 58CD3345)
    (at 191.16802 83.4898 180)
    (descr "SMD Crystal Oscillator Seiko Epson SG-8002CE https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal oscillator")
    (attr smd)
    (fp_text reference X1 (at 0.17526 2.56794) (layer F.SilkS))
    (fp_text value ASCO (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0.95 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(RV1-Pad2)"))
    (pad 2 smd rect (at 1.2 0.95 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 1.2 -0.95 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C6-Pad2)"))
    (pad 4 smd rect (at -1.2 -0.95 180) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_SG8002CE-4Pin_3.2x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 193.18478 96.1771 90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at -3.21564 -0.0889 180) (layer F.SilkS))
    (fp_text value 47n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 GND))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 201.06386 84.62518 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.52908 90) (layer F.SilkS))
    (fp_text value 2k7 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 198.41464 86.41334)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.67462 -0.06604) (layer F.SilkS))
    (fp_text value 2k7 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C4-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3224W_Vertical (layer F.Cu) (tedit 5A3D7171)
    (at 196.75094 82.52968 270)
    (descr "Potentiometer, vertical, Bourns 3224W, https://www.bourns.com/docs/Product-Datasheets/3224.pdf")
    (tags "Potentiometer vertical Bourns 3224W")
    (attr smd)
    (fp_text reference RV1 (at -1.11252 -3.27406 90) (layer F.SilkS))
    (fp_text value 5k (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0.6 0 90) (layer F.Fab))
    (pad 1 smd rect (at 1.25 -1.45 270) (size 1.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at 0 1.45 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(RV1-Pad2)"))
    (pad 3 smd rect (at -1.25 -1.45 270) (size 1.3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3224W_Vertical.wrl
      (offset (xyz 0 0 3.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model C:/Users/dd9fj/Desktop/HamRadio/KiCad_Projekte/eigene3D/3224W.stp
      (offset (xyz 0.3 1.7 3))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (gr_text "by dd9fj" (at 180.94198 80.60436) (layer B.SilkS))
  (gr_text "Diplexer mit 25 MHz TCXO\nund SAW Filter für RX" (at 202.12812 85.10016) (layer B.SilkS))
  (gr_text "12/18V\nmax.200mA" (at 209.9437 85.36432) (layer B.SilkS))
  (gr_text LNB (at 179.07 94.64802 90) (layer B.SilkS))
  (gr_text "RX\n730MHz\n-\n760Mhz" (at 208.13014 94.5261 -90) (layer B.SilkS))
  (gr_line (start 214.884 79.21244) (end 214.78748 100.49002) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.0126 79.2226) (end 214.884 79.21244) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.01768 100.43414) (end 177.0126 79.2226) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.78748 100.49002) (end 177.01768 100.43414) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.83574 100.40112) (xy 176.93132 100.29698) (xy 176.98466 79.19212) (xy 214.83574 79.19212)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 214.8713 100.52304) (xy 176.90084 100.52304) (xy 176.91608 79.17942) (xy 214.94242 79.17942)
      )
    )
  )
)
