<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<wire x1="1" y1="4.947959375" x2="4.947959375" y2="1" width="0.01" layer="20" curve="90"/>
<wire x1="4.947959375" y1="1" x2="9" y2="5.052040625" width="0.01" layer="20" curve="90"/>
<wire x1="9" y1="5.052040625" x2="5.052040625" y2="9" width="0.01" layer="20" curve="90"/>
<wire x1="5.052040625" y1="9" x2="1" y2="4.947959375" width="0.01" layer="20" curve="90"/>
</plain>
<libraries>
<library name="MBsupply pins">
<packages>
<package name="PAD2">
<description>&lt;b&gt;Round Pad (no label) - 76mil Diameter, 39mil Drill&lt;b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN+" library="MBsupply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="IN-" library="MBsupply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="OUT+" library="MBsupply pins" package="PAD2" value="PADS.RND_NL"/>
<element name="GND" library="MBsupply pins" package="PAD2" value="PADS.RND_NL"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="IN+" pad="P$1"/>
<contactref element="OUT+" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="IN-" pad="P$1"/>
<contactref element="GND" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
