(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 101)
    (zones 0)
    (modules 24)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.99 2.26)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(Cint1-Pad1)")
  (net 3 "Net-(Csnubber1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(J1-Pad2)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J_enable1-Pad2)")
  (net 8 "Net-(Rfb1-Pad1)")
  (net 9 "Net-(Rfb1-Pad2)")
  (net 10 "Net-(Rref1-Pad2)")
  (net 11 "Net-(Rtc1-Pad1)")
  (net 12 "Net-(Rtrim1-Pad3)")
  (net 13 "Net-(U2-Pad1)")
  (net 14 "Net-(U2-Pad2)")
  (net 15 "Net-(U2-Pad4)")
  (net 16 "Net-(U2-Pad6)")
  (net 17 "Net-(U2-Pad9)")
  (net 18 "Net-(U2-Pad10)")
  (net 19 /Vin)
  (net 20 /Vout)
  (net 21 /SW)
  (net 22 GNDA)
  (net 23 "Net-(D2-Pad2)")
  (net 24 "Net-(J3-Pad1)")
  (net 25 "Net-(J4-Pad1)")
  (net 26 "Net-(J5-Pad1)")
  (net 27 "Net-(J6-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /SW)
    (add_net /Vin)
    (add_net /Vout)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(Cint1-Pad1)")
    (add_net "Net-(Csnubber1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J_enable1-Pad2)")
    (add_net "Net-(Rfb1-Pad1)")
    (add_net "Net-(Rfb1-Pad2)")
    (add_net "Net-(Rref1-Pad2)")
    (add_net "Net-(Rtc1-Pad1)")
    (add_net "Net-(Rtrim1-Pad3)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad9)")
  )
  (net_class VIN ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 142.739 113.284 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cint2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 110.49 96.266 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cin1 (at 3.801 0 90) (layer F.SilkS))
    (fp_text value 10u (at -3.302 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 /Vin))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 114.554 89.163 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cint1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 1u (at 2.803 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 "Net-(Cint1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 158.242 101.355 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Cout1 (at -2.549 -0.508) (layer F.SilkS))
    (fp_text value 330n (at 2.531 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 /Vout))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 GNDA))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 83.82 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference Csnubber1 (at 0 -5.08 180) (layer F.SilkS))
    (fp_text value 200n (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 /Vin))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(Csnubber1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B4B45C8)
    (at 115.316 100.085 270)
    (descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at -0.517 1.778 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 19 /Vin))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_PowerDI-123 (layer F.Cu) (tedit 588FC24C)
    (at 156.718 96.266 180)
    (descr http://www.diodes.com/_files/datasheets/ds30497.pdf)
    (tags "PowerDI diode vishay")
    (attr smd)
    (fp_text reference D2 (at 0.508 2.286) (layer F.SilkS))
    (fp_text value D_Schottky (at -0.254 -2.032 180) (layer F.Fab))
    (fp_text user %R (at 4.826 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.85 0) (size 2.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /Vout))
    (pad 2 smd rect (at 1.525 0) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_PowerDI-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-3_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 105.664 93.726 270)
    (descr "Terminal Block TE 282834-3, 3 pins, pitch 2.54mm, size 8.08x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-3 pitch 2.54mm size 8.08x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference Vin (at 7.874 0) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 2.54 4.37 90) (layer F.Fab))
    (fp_text user %R (at 2.54 2 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 /Vin))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-3_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-3_1x03_P2.54mm_Horizontal (layer F.Cu) (tedit 5B1EC513)
    (at 172.72 101.6 270)
    (descr "Terminal Block TE 282834-3, 3 pins, pitch 2.54mm, size 8.08x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-3 pitch 2.54mm size 8.08x6.5mm^2 drill 1.1mm pad 2.1mm")
    (fp_text reference J2 (at 7.62 3.81 180) (layer F.SilkS))
    (fp_text value Conn_01x03_Female (at 2.54 4.37 90) (layer F.Fab))
    (fp_text user %R (at 2.54 2 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 /Vout))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 GNDA))
    (model ${KISYS3DMOD}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-3_1x03_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:FanPinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5A19DCDF)
    (at 105.156 88.646 90)
    (descr "3-pin CPU fan Through hole pin header, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
    (tags "pin header 3-pin CPU fan")
    (fp_text reference "1 = on 3 = off" (at 2.921 4.191 270) (layer F.SilkS))
    (fp_text value EN_Header (at 2.55 4.5 90) (layer F.Fab))
    (fp_text user %R (at 2.45 1.8 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 /Vin))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 "Net-(J_enable1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 161.544 101.863 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -2.032 180) (layer F.SilkS))
    (fp_text value 190K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 20 /Vout))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 161.544 105.927 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -0.009 -2.032 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 6 "Net-(J2-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 22 GNDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 126.238 88.909 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rfb1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 200K (at 4.309 -0.254 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 "Net-(Rfb1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 9 "Net-(Rfb1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 115.316 94.497 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rled1 (at 0.009 -1.524 270) (layer F.SilkS))
    (fp_text value 100K (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 118.618 89.163 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rref1 (at -0.245 1.778 90) (layer F.SilkS))
    (fp_text value 10K (at -3.547 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(Rref1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 135.89 89.145 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rsnubber1 (at -0.245 -5.08 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 21 /SW))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 "Net-(Csnubber1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 122.682 89.145 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference Rtc1 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value 100K (at -4.055 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 "Net-(Rtc1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 "Net-(Rref1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Vishay_TS53YJ_Vertical (layer F.Cu) (tedit 5A3D7171)
    (at 130.81 88.392 90)
    (descr "Potentiometer, vertical, Vishay TS53YJ, https://www.vishay.com/docs/51008/ts53.pdf")
    (tags "Potentiometer vertical Vishay TS53YJ")
    (attr smd)
    (fp_text reference Rtrim1 (at 3.302 -5.08 180) (layer F.SilkS))
    (fp_text value 100K (at 3.81 0 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 1 smd rect (at 2 -1.15 90) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Rfb1-Pad2)"))
    (pad 2 smd rect (at -2 0 90) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /SW))
    (pad 3 smd rect (at 2 1.15 90) (size 2 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(Rtrim1-Pad3)"))
    (model ${KISYS3DMOD}/Potentiometer_SMD.3dshapes/Potentiometer_Vishay_TS53YJ_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HighVoltageBoard:LT8304-1 (layer F.Cu) (tedit 5E0701FB)
    (at 124.46 95.25 270)
    (fp_text reference U1 (at 0 5.08 90) (layer F.SilkS))
    (fp_text value LT8304-1 (at 0 -5.08 90) (layer F.Fab))
    (pad 1 smd rect (at -1.905 2.54 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J_enable1-Pad2)"))
    (pad 2 smd rect (at -0.635 2.54 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(Cint1-Pad1)"))
    (pad 3 smd rect (at 0.6096 2.54 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 19 /Vin))
    (pad 4 smd rect (at 1.905 2.54 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.905 -2.665 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 21 /SW))
    (pad 6 smd rect (at 0.635 -2.665 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(Rfb1-Pad1)"))
    (pad 7 smd rect (at -0.635 -2.665 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Rref1-Pad2)"))
    (pad 8 smd rect (at -1.905 -2.665 90) (size 0.76 1.143) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Rtc1-Pad1)"))
    (pad 9 smd rect (at 0 0 270) (size 2.99 2.26) (layers F.Cu F.SilkS F.Mask)
      (net 1 GND))
  )
  (module HighVoltageBoard:750315839 (layer F.Cu) (tedit 5DF08B9E)
    (at 142.24 106.68)
    (fp_text reference U2 (at 0 2.5) (layer F.SilkS))
    (fp_text value 750315839 (at 0 -12.5) (layer F.Fab))
    (pad 1 smd rect (at -8.18 0) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -8.18 -2.5) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at -8.18 -5) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 19 /Vin))
    (pad 4 smd rect (at -8.18 -7.5) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -8.18 -10) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 21 /SW))
    (pad 6 smd rect (at 8.18 -10) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at 8.18 -7.5) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D2-Pad2)"))
    (pad 8 smd rect (at 8.18 -5) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 22 GNDA))
    (pad 9 smd rect (at 8.18 -2.5) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 8.18 0) (size 1.4 0.86) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad10)"))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 175.26 114.3)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference J3 (at -3.81 0) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)"))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 112.395 84.455 90)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference J4 (at -2.667 0.127 90) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 90) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad1)"))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 175.26 83.185)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference J5 (at -3.81 -0.635) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (net 26 "Net-(J5-Pad1)"))
  )
  (module MountingHole:MountingHole_2.7mm (layer F.Cu) (tedit 56D1B4CB)
    (at 111.76 114.3 180)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (attr virtual)
    (fp_text reference J6 (at 0 2.54) (layer F.SilkS))
    (fp_text value Conn_01x01_MountingPin (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask)
      (net 27 "Net-(J6-Pad1)"))
  )
  (gr_text 1 (at 105.41 90.805 90) (layer F.SilkS))
  (gr_text "JWL HV V1" (at 125.73 113.665) (layer F.SilkS))
  (gr_text "HIGH VOLTAGE!!! " (at 161.036 87.376) (layer F.SilkS))
  (gr_text Vout/10 (at 167.64 104.14 90) (layer F.SilkS))
  (gr_text GNDA (at 172.72 110.49) (layer F.SilkS))
  (gr_text "VOUT\n" (at 172.72 97.79) (layer F.SilkS))
  (dimension 36.068 (width 0.12) (layer Dwgs.User)
    (gr_text "1.4200 in" (at 92.71 98.806 270) (layer Dwgs.User))
    (feature1 (pts (xy 101.6 116.84) (xy 93.393579 116.84)))
    (feature2 (pts (xy 101.6 80.772) (xy 93.393579 80.772)))
    (crossbar (pts (xy 93.98 80.772) (xy 93.98 116.84)))
    (arrow1a (pts (xy 93.98 116.84) (xy 93.393579 115.713496)))
    (arrow1b (pts (xy 93.98 116.84) (xy 94.566421 115.713496)))
    (arrow2a (pts (xy 93.98 80.772) (xy 93.393579 81.898504)))
    (arrow2b (pts (xy 93.98 80.772) (xy 94.566421 81.898504)))
  )
  (dimension 76.2 (width 0.15) (layer Dwgs.User)
    (gr_text "3.0000 in" (at 139.7 69.312001) (layer Dwgs.User))
    (feature1 (pts (xy 101.6 80.772) (xy 101.6 70.02558)))
    (feature2 (pts (xy 177.8 80.772) (xy 177.8 70.02558)))
    (crossbar (pts (xy 177.8 70.612001) (xy 101.6 70.612001)))
    (arrow1a (pts (xy 101.6 70.612001) (xy 102.726504 70.02558)))
    (arrow1b (pts (xy 101.6 70.612001) (xy 102.726504 71.198422)))
    (arrow2a (pts (xy 177.8 70.612001) (xy 176.673496 70.02558)))
    (arrow2b (pts (xy 177.8 70.612001) (xy 176.673496 71.198422)))
  )
  (gr_line (start 177.8 80.772) (end 101.6 80.772) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.8 116.84) (end 177.8 80.772) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 116.84) (end 177.8 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.6 80.772) (end 101.6 116.84) (layer Edge.Cuts) (width 0.05))
  (zone (net 21) (net_name /SW) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126.492 96.52) (xy 129.794 96.52) (xy 129.794 89.408) (xy 137.16 89.408) (xy 137.16 97.79)
        (xy 126.492 97.79)
      )
    )
  )
  (zone (net 23) (net_name "Net-(D2-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 155.575 97.79) (xy 155.575 94.234) (xy 153.162 94.234) (xy 148.59 94.234) (xy 148.59 100.584)
        (xy 152.654 100.584) (xy 154.559 99.187)
      )
    )
  )
  (zone (net 20) (net_name /Vout) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 157.00375 81.534) (xy 177.165 81.28) (xy 177.165 98.806) (xy 177.165 102.87) (xy 169.926 102.87)
        (xy 168.656 101.854) (xy 162.814 101.854) (xy 160.274 101.854) (xy 160.02 101.346) (xy 157.1625 101.346)
      )
    )
  )
  (zone (net 22) (net_name GNDA) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 177.165 111.9505) (xy 177.165 105.283) (xy 159.766 105.41) (xy 159.766 102.108) (xy 153.416 102.108)
        (xy 153.416 101.092) (xy 143.51 101.092) (xy 143.4465 111.1885) (xy 143.51 116.1415) (xy 177.165 116.205)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 137.16 111.252) (xy 142.113 111.252) (xy 142.113 116.205) (xy 137.16 116.332)
      )
    )
  )
  (zone (net 19) (net_name /Vin) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 102.108 96.52) (xy 109.22 96.52) (xy 120.65 96.52) (xy 120.65 98.806) (xy 130.81 98.806)
        (xy 133.096 100.33) (xy 138.43 100.33) (xy 138.43 84.328) (xy 138.43 81.407) (xy 142.113 81.407)
        (xy 142.113 109.728) (xy 102.108 109.728)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 125.476 93.69425) (xy 125.73 93.853) (xy 125.73 96.901) (xy 123.063 96.901) (xy 123.063 96.012)
        (xy 107.95 96.012) (xy 107.442 94.996) (xy 102.108 94.996) (xy 102.108 81.28) (xy 125.476 81.28)
      )
    )
  )
  (zone (net 22) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 143.51 81.28) (xy 143.51 116.332) (xy 177.165 116.332) (xy 177.165 81.28)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 1) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 103.124 81.28) (xy 142.113 81.407) (xy 142.113 116.205) (xy 102.108 116.332) (xy 102.108 81.28)
      )
    )
  )
)
