(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 54)
    (no_connects 0)
    (area 116.789999 83.769999 203.250001 119.430001)
    (thickness 1.6002)
    (drawings 34)
    (tracks 250)
    (zones 0)
    (modules 25)
    (nets 17)
  )
  (page A)
  (title_block
    (title "Interactive Rainbow")
    (date 2017-03-29)
    (rev 1.0.2)
    (company "Sembazuru Circuits")
    (comment 1 "1.0.0 Initial Release to OSHPark.")
    (comment 2 "1.0.1 Add termination resistors for differential inputs.")
    (comment 3 "1.0.2 Correct pinout of U2, relayout subcurcuit to fit. Add KiCad logo. Isolate unused gate inputs from thermals for future modification.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 0.889)
    (user_trace_width 1.016)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.7874)
    (via_drill 0.381)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 116.84 119.38)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 /~IR_Osc+)
  (net 8 /~IR_Osc-)
  (net 9 /~Sensor+)
  (net 10 /LED+)
  (net 11 /LED-)
  (net 12 /~Sensor-)
  (net 13 /LED)
  (net 14 /~IR_Osc)
  (net 15 /~Sensor)
  (net 16 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.7874)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /LED)
    (add_net /~IR_Osc)
    (add_net /~Sensor)
  )
  (net_class Differential ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.7874)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /LED+)
    (add_net /LED-)
    (add_net /~IR_Osc+)
    (add_net /~IR_Osc-)
    (add_net /~Sensor+)
    (add_net /~Sensor-)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 1.27)
    (via_dia 0.7874)
    (via_drill 0.381)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R3-Pad1)")
  )
  (module ipc-7251TH-non-standard:TO_VISHAY_TSOP3nnnnn (layer B.Cu) (tedit 58829E64)
    (at 132.08 114.3)
    (descr "SIP, 2.54 mm pitch; 3 pin, 6.20 mm L X 5.80 mm W X 8.45 mm H body")
    (fp_text reference U2 (at -2.286 -0.092) (layer B.SilkS))
    (fp_text value TSOP32138 (at -5.08 1.905) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.52 1.52) (drill 1.01) (layers *.Cu *.Mask)
      (net 15 /~Sensor))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.52 1.52) (drill 1.01) (layers *.Cu *.Mask)
      (net 16 "Net-(R3-Pad1)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.52 1.52) (drill 1.01) (layers *.Cu *.Mask)
      (net 2 GND))
    (model CDEunsorted/TO_VISHAY_TSOP3nnnnn.wrl
      (at (xyz 0.1 0.06 1))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz -90 0 0))
    )
  )
  (module ipc-7251TH-standard:RESAD1270W60L900D323 (layer F.Cu) (tedit 58157708)
    (at 165.1 101.6 270)
    (descr "Resistor, Axial; 12.70 mm C X 0.60 mm W 9.00 mm L X 3.23 mm Dia body - Standard 1/2W Resistor")
    (fp_text reference R1 (at 1.778 -3.048 360) (layer F.SilkS))
    (fp_text value "33Ω 1/2W" (at 6.35 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.28 1.28) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 12.7 0 270) (size 1.28 1.28) (drill 0.85) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model unused_3d.3dshapes/discret.resistors.horizontal.r_h_33R.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 180))
    )
  )
  (module ipc-7251TH-standard:RESAD1016W56L681D259 (layer F.Cu) (tedit 57F7175B)
    (at 190.5 109.22 270)
    (descr "Resistor, Axial; 400 mil C X 22 mil W 268 mil L X 102 mil Dia body - Standard 1/4W Resistor")
    (tags "RES 0.25 1/4")
    (fp_text reference R2 (at -3.556 -2.54 360) (layer F.SilkS))
    (fp_text value 180Ω (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.08 0 270) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model unused_3d.3dshapes/discret.resistors.horizontal.r_h_180R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module ipc-7251TH-standard:RESAD1016W56L681D259 (layer F.Cu) (tedit 57F7175B)
    (at 139.7 109.855)
    (descr "Resistor, Axial; 400 mil C X 22 mil W 268 mil L X 102 mil Dia body - Standard 1/4W Resistor")
    (tags "RES 0.25 1/4")
    (fp_text reference R3 (at -5.08 -1.905 180) (layer F.SilkS))
    (fp_text value 180Ω (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.08 0) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "Net-(R3-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.53 1.53) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model unused_3d.3dshapes/discret.resistors.horizontal.r_h_180R.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:LEDRD254W50D500H960P (layer B.Cu) (tedit 58829E6D)
    (at 185.42 114.3)
    (descr "LED 5mm Vertical")
    (tags LED)
    (fp_text reference D2 (at -4.572 0) (layer B.SilkS))
    (fp_text value "RGB Slow Flashing" (at -10.16 1.905) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.4 1.4) (drill 0.93) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.4 1.4) (drill 0.93) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:LEDRD254W50D500H960P (layer B.Cu) (tedit 58829E58)
    (at 160.02 114.3)
    (descr "LED 5mm Vertical")
    (tags LED)
    (fp_text reference D1 (at -4.572 0) (layer B.SilkS))
    (fp_text value "IR 950nm" (at -6.985 1.905) (layer B.Fab))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.4 1.4) (drill 0.93) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.4 1.4) (drill 0.93) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-5MM.wrl
      (at (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 574B292C)
    (at 158.75 96.52 90)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C1 (at -3.556 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 0)
    (at 177.8 111.76 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0.254 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_02X04 (at 1.016 -2.794 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:TO92184P520H734-3 (layer F.Cu) (tedit 0)
    (at 160.02 109.22 270)
    (descr "TO-92, 1.8415 mm pitch; 3 pin, 5.207 mm W X 7.341 mm H body")
    (tags "TO92 TO-92")
    (fp_text reference Q1 (at -1.27 3.556 360) (layer F.SilkS))
    (fp_text value VN3205 (at 0 -2.794 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.8415 0.7685 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 -1.30175 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 14 /~IR_Osc))
    (pad 3 thru_hole circle (at 1.8415 0.7685 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide.wrl
      (at (xyz 0 -0.03 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ipc-7251TH-standard:TO92184P520H734-3 (layer F.Cu) (tedit 0)
    (at 185.42 109.22 270)
    (descr "TO-92, 1.8415 mm pitch; 3 pin, 5.207 mm W X 7.341 mm H body")
    (tags "TO92 TO-92")
    (fp_text reference Q2 (at -1.27 3.556 360) (layer F.SilkS))
    (fp_text value VN3205 (at 0 -2.794 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.8415 0.7685 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 -1.30175 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 13 /LED))
    (pad 3 thru_hole circle (at 1.8415 0.7685 270) (size 1.41 1.41) (drill 0.94) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide.wrl
      (at (xyz 0 -0.03 0))
      (scale (xyz 0.8 0.8 0.8))
      (rotate (xyz 0 0 -90))
    )
  )
  (module ipc-7251TH-standard:CAPRR254W51L508T318H660P (layer F.Cu) (tedit 574B292C)
    (at 143.51 106.68 180)
    (descr "Cap Monolithic 0.1\" pitch")
    (tags "CAP mono")
    (fp_text reference C4 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.12014 1.12014) (drill 0.70104) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.19888 1.19888) (drill 0.70104) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPS762W45P254L2019H508Q16 (layer F.Cu) (tedit 5881A3C2)
    (at 147.32 93.98 180)
    (descr "DIPS, 7.62 mm lead span, 2.54 mm pitch; 16 pin, 20.19 mm L X 10.16 mm W X 5.08 mm H body")
    (fp_text reference U1 (at -11.43 3.81 180) (layer F.SilkS))
    (fp_text value 75C1168 (at 0.254 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -8.89 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 11 /LED-))
    (pad 2 thru_hole circle (at -6.35 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 10 /LED+))
    (pad 3 thru_hole circle (at -3.81 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 13 /LED))
    (pad 4 thru_hole circle (at -1.27 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole circle (at 1.27 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 14 /~IR_Osc))
    (pad 6 thru_hole circle (at 3.81 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 7 /~IR_Osc+))
    (pad 7 thru_hole circle (at 6.35 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 8 /~IR_Osc-))
    (pad 8 thru_hole circle (at 8.89 3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole circle (at 8.89 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 6.35 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 3.81 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at 1.27 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole circle (at -1.27 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 12 /~Sensor-))
    (pad 14 thru_hole circle (at -3.81 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 9 /~Sensor+))
    (pad 15 thru_hole circle (at -6.35 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 15 /~Sensor))
    (pad 16 thru_hole circle (at -8.89 -3.81 180) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model dil/sockets/dil_socket_16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:DIPfS794W45P254L1969H508Q16 (layer F.Cu) (tedit 5803B15F)
    (at 147.32 93.98 180)
    (descr "DIP for Socket, 7.94 mm lead span, 2.54 mm pitch; 16 pin, 19.69 mm L X 6.60 mm W X 5.08 mm H body")
    (fp_text reference XU1 (at -7.874 1.905 360) (layer F.SilkS))
    (fp_text value IC_Socket16 (at 0 -0.762 180) (layer F.Fab))
    (model Sockets_DIP.3dshapes/DIP-16__300.wrl
      (at (xyz 0 0 0.161))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 (layer F.Cu) (tedit 580AED82)
    (at 160.02 104.14 180)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C3 (at -2.54 2.794 180) (layer F.SilkS))
    (fp_text value 1µF (at 0 -1.27 180) (layer F.Fab))
    (fp_text user + (at -3.048 -1.016 180) (layer F.SilkS))
    (fp_text user + (at -3.048 -1.016 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-standard:CAPPRD254W50D500H850 (layer F.Cu) (tedit 580AED82)
    (at 185.42 104.14 180)
    (descr "Capacitor, Polarized, Radial (Dipped, Round); 2.54 mm C X 5.00 mm Dia X 8.50 mm H body")
    (fp_text reference C2 (at -2.794 2.54 180) (layer F.SilkS))
    (fp_text value 1µF (at 0 -1.27 180) (layer F.Fab))
    (fp_text user + (at -3.048 -1.016 180) (layer F.SilkS))
    (fp_text user + (at -3.048 -1.016 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.12 1.12) (drill 0.72) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0 0 0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ipc-7251TH-connectors:WURTH_615008144221 (layer F.Cu) (tedit 581580AA)
    (at 129.11 97.15 270)
    (descr "Modular Connector 8P/8C Vertical,1.27 mm pitch;8 pin, 17.84 mm L X 16.40 mm W X 16.38 mm H body")
    (fp_text reference J1 (at -4.186 -2.462 360) (layer F.SilkS))
    (fp_text value RJ45-Unshielded (at 4.196 13.54 450) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /~IR_Osc+))
    (pad 2 thru_hole circle (at 1.27 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /~IR_Osc-))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 /~Sensor+))
    (pad 4 thru_hole circle (at 3.81 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /LED+))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 /LED-))
    (pad 6 thru_hole circle (at 6.35 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 /~Sensor-))
    (pad 7 thru_hole circle (at 7.62 0 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 8 thru_hole circle (at 8.89 -2.54 270) (size 1.44 1.44) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 10.165 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.265 6.35 270) (size 3.17 3.17) (drill 3.17) (layers *.Cu *.Mask))
    (model connectors/WURTH_615008144221_RJ45-Vert.wrl
      (at (xyz 0.175197 -0.1830708661 0.34))
      (scale (xyz 0.408163 0.408163 0.408163))
      (rotate (xyz 90 90 0))
    )
  )
  (module logos:OSHW_03mm_copper_noMask (layer B.Cu) (tedit 0)
    (at 179.07 89.535 180)
    (fp_text reference G*** (at 0 -1.77038 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 1.77038 180) (layer B.SilkS) hide)
  )
  (module logos:crane_0.40in_silkscreen (layer B.Cu) (tedit 0)
    (at 187.325 87.63 180)
    (fp_text reference G*** (at 0 -3.64236 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 3.64236 180) (layer B.SilkS) hide)
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 5881A3E3)
    (at 143.51 88.265 180)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R4 (at -2.54 0.635 180) (layer F.SilkS))
    (fp_text value 100Ω (at 1.27 1.905 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 7 /~IR_Osc+))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 8 /~IR_Osc-))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module ipc-7251TH-standard:RESADV254W45L350D185 (layer F.Cu) (tedit 5881A3D4)
    (at 156.21 88.265 180)
    (descr "Resistor, Axial, Vertical; 100 mil C X 17.7 mil W 137.8 mil L X 72.8 mil Dia body")
    (fp_text reference R5 (at -2.54 0.635 180) (layer F.SilkS))
    (fp_text value 100Ω (at 1.27 1.905 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 11 /LED-))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.10744 1.10744) (drill 0.70104) (layers *.Cu *.Mask)
      (net 10 /LED+))
    (model unused_3d.3dshapes/discret.resistors.vertical.r_v_100R.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer B.Cu) (tedit 0)
    (at 179.07 97.155 180)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module ipc-7251TH-standard:MTGP794H326V8P (layer F.Cu) (tedit 549A50E1)
    (at 121.92 88.9)
    (descr "Mounting Hole, Plated, #4 Free Fit")
    (tags MTGP#4Free)
    (fp_text reference MH1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 PTH" (at 0 0) (layer F.SilkS) hide)
    (pad 0 thru_hole rect (at 0 0) (size 7.94 7.94) (drill 3.26) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 0 3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 3.556 3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 3.556 0) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 3.556 -3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at 0 -3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at -3.556 -3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at -3.556 0) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 0 thru_hole rect (at -3.556 3.556) (size 0.762 0.762) (drill 0.3048) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 121.92 114.3)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 198.12 88.9)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (module ipc-7251TH-standard:MTGNP794H326Z794P (layer F.Cu) (tedit 549A53B9)
    (at 198.12 114.3)
    (descr "Mounting Hole, Not Plated, #4 Free Fit")
    (tags MTGNP#4Free)
    (fp_text reference MH2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "#4 NPTH" (at 0 0) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.26 3.26) (drill 3.26) (layers *.Cu *.Mask)
      (clearance 2.34))
  )
  (gr_text "Color LED" (at 185.42 118.11) (layer B.SilkS))
  (gr_text "IR LED" (at 160.02 118.11) (layer B.SilkS))
  (gr_text "IR Sensor" (at 134.62 118.11) (layer B.SilkS))
  (gr_text "Color LED" (at 185.42 116.84) (layer F.SilkS))
  (gr_text "IR LED" (at 160.02 116.84) (layer F.SilkS))
  (gr_text "IR Sensor" (at 134.62 116.84) (layer F.SilkS))
  (gr_text - (at 180.34 111.76) (layer F.SilkS))
  (gr_text - (at 180.34 109.22) (layer F.SilkS))
  (gr_text - (at 180.34 106.68) (layer F.SilkS))
  (gr_text - (at 180.34 104.14) (layer F.SilkS))
  (gr_text + (at 172.72 111.76) (layer F.SilkS))
  (gr_text + (at 172.72 109.22) (layer F.SilkS))
  (gr_text + (at 172.72 106.68) (layer F.SilkS))
  (gr_text + (at 172.72 104.14) (layer F.SilkS))
  (gr_text "Sch V2.0.3\nPcb V1.0.2" (at 198.12 95.885) (layer F.SilkS))
  (gr_text "TrippyRGB\nSensor&LED" (at 179.07 89.535) (layer F.SilkS))
  (gr_text "Sembazuru\nCircuits" (at 187.325 92.71) (layer B.SilkS))
  (gr_text "DIY DE" (at 170.815 92.075) (layer B.SilkS))
  (gr_text BoM (at 170.815 88.265) (layer B.SilkS))
  (dimension 5.08 (width 0.064516) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 210.265 86.36 90) (layer Dwgs.User))
    (feature1 (pts (xy 203.835 83.82) (xy 211.615 83.82)))
    (feature2 (pts (xy 203.835 88.9) (xy 211.615 88.9)))
    (crossbar (pts (xy 208.915 88.9) (xy 208.915 83.82)))
    (arrow1a (pts (xy 208.915 83.82) (xy 209.501421 84.946504)))
    (arrow1b (pts (xy 208.915 83.82) (xy 208.328579 84.946504)))
    (arrow2a (pts (xy 208.915 88.9) (xy 209.501421 87.773496)))
    (arrow2b (pts (xy 208.915 88.9) (xy 208.328579 87.773496)))
  )
  (dimension 25.4 (width 0.064516) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 210.265 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 203.835 88.9) (xy 211.615 88.9)))
    (feature2 (pts (xy 203.835 114.3) (xy 211.615 114.3)))
    (crossbar (pts (xy 208.915 114.3) (xy 208.915 88.9)))
    (arrow1a (pts (xy 208.915 88.9) (xy 209.501421 90.026504)))
    (arrow1b (pts (xy 208.915 88.9) (xy 208.328579 90.026504)))
    (arrow2a (pts (xy 208.915 114.3) (xy 209.501421 113.173496)))
    (arrow2b (pts (xy 208.915 114.3) (xy 208.328579 113.173496)))
  )
  (dimension 5.08 (width 0.064516) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 210.265 116.84 90) (layer Dwgs.User))
    (feature1 (pts (xy 203.835 114.3) (xy 211.615 114.3)))
    (feature2 (pts (xy 203.835 119.38) (xy 211.615 119.38)))
    (crossbar (pts (xy 208.915 119.38) (xy 208.915 114.3)))
    (arrow1a (pts (xy 208.915 114.3) (xy 209.501421 115.426504)))
    (arrow1b (pts (xy 208.915 114.3) (xy 208.328579 115.426504)))
    (arrow2a (pts (xy 208.915 119.38) (xy 209.501421 118.253496)))
    (arrow2b (pts (xy 208.915 119.38) (xy 208.328579 118.253496)))
  )
  (dimension 25.4 (width 0.064516) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 172.72 125.81) (layer Dwgs.User))
    (feature1 (pts (xy 185.42 120.015) (xy 185.42 127.16)))
    (feature2 (pts (xy 160.02 120.015) (xy 160.02 127.16)))
    (crossbar (pts (xy 160.02 124.46) (xy 185.42 124.46)))
    (arrow1a (pts (xy 185.42 124.46) (xy 184.293496 125.046421)))
    (arrow1b (pts (xy 185.42 124.46) (xy 184.293496 123.873579)))
    (arrow2a (pts (xy 160.02 124.46) (xy 161.146504 125.046421)))
    (arrow2b (pts (xy 160.02 124.46) (xy 161.146504 123.873579)))
  )
  (dimension 25.4 (width 0.064516) (layer Dwgs.User)
    (gr_text "1.0000 in" (at 147.32 125.81) (layer Dwgs.User))
    (feature1 (pts (xy 160.02 120.015) (xy 160.02 127.16)))
    (feature2 (pts (xy 134.62 120.015) (xy 134.62 127.16)))
    (crossbar (pts (xy 134.62 124.46) (xy 160.02 124.46)))
    (arrow1a (pts (xy 160.02 124.46) (xy 158.893496 125.046421)))
    (arrow1b (pts (xy 160.02 124.46) (xy 158.893496 123.873579)))
    (arrow2a (pts (xy 134.62 124.46) (xy 135.746504 125.046421)))
    (arrow2b (pts (xy 134.62 124.46) (xy 135.746504 123.873579)))
  )
  (dimension 12.7 (width 0.064516) (layer Dwgs.User)
    (gr_text "0.5000 in" (at 191.77 125.81) (layer Dwgs.User))
    (feature1 (pts (xy 198.12 120.015) (xy 198.12 127.16)))
    (feature2 (pts (xy 185.42 120.015) (xy 185.42 127.16)))
    (crossbar (pts (xy 185.42 124.46) (xy 198.12 124.46)))
    (arrow1a (pts (xy 198.12 124.46) (xy 196.993496 125.046421)))
    (arrow1b (pts (xy 198.12 124.46) (xy 196.993496 123.873579)))
    (arrow2a (pts (xy 185.42 124.46) (xy 186.546504 125.046421)))
    (arrow2b (pts (xy 185.42 124.46) (xy 186.546504 123.873579)))
  )
  (dimension 12.7 (width 0.064516) (layer Dwgs.User)
    (gr_text "0.5000 in" (at 128.27 125.81) (layer Dwgs.User))
    (feature1 (pts (xy 134.62 120.015) (xy 134.62 127.16)))
    (feature2 (pts (xy 121.92 120.015) (xy 121.92 127.16)))
    (crossbar (pts (xy 121.92 124.46) (xy 134.62 124.46)))
    (arrow1a (pts (xy 134.62 124.46) (xy 133.493496 125.046421)))
    (arrow1b (pts (xy 134.62 124.46) (xy 133.493496 123.873579)))
    (arrow2a (pts (xy 121.92 124.46) (xy 123.046504 125.046421)))
    (arrow2b (pts (xy 121.92 124.46) (xy 123.046504 123.873579)))
  )
  (dimension 5.08 (width 0.064516) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 200.66 125.81) (layer Dwgs.User))
    (feature1 (pts (xy 203.2 120.015) (xy 203.2 127.16)))
    (feature2 (pts (xy 198.12 120.015) (xy 198.12 127.16)))
    (crossbar (pts (xy 198.12 124.46) (xy 203.2 124.46)))
    (arrow1a (pts (xy 203.2 124.46) (xy 202.073496 125.046421)))
    (arrow1b (pts (xy 203.2 124.46) (xy 202.073496 123.873579)))
    (arrow2a (pts (xy 198.12 124.46) (xy 199.246504 125.046421)))
    (arrow2b (pts (xy 198.12 124.46) (xy 199.246504 123.873579)))
  )
  (dimension 5.08 (width 0.064516) (layer Dwgs.User)
    (gr_text "0.2000 in" (at 119.38 125.81) (layer Dwgs.User))
    (feature1 (pts (xy 121.92 120.015) (xy 121.92 127.16)))
    (feature2 (pts (xy 116.84 120.015) (xy 116.84 127.16)))
    (crossbar (pts (xy 116.84 124.46) (xy 121.92 124.46)))
    (arrow1a (pts (xy 121.92 124.46) (xy 120.793496 125.046421)))
    (arrow1b (pts (xy 121.92 124.46) (xy 120.793496 123.873579)))
    (arrow2a (pts (xy 116.84 124.46) (xy 117.966504 125.046421)))
    (arrow2b (pts (xy 116.84 124.46) (xy 117.966504 123.873579)))
  )
  (dimension 35.56 (width 0.129032) (layer Dwgs.User)
    (gr_text "1.4000 in" (at 110.41 101.6 90) (layer Dwgs.User))
    (feature1 (pts (xy 116.205 83.82) (xy 109.06 83.82)))
    (feature2 (pts (xy 116.205 119.38) (xy 109.06 119.38)))
    (crossbar (pts (xy 111.76 119.38) (xy 111.76 83.82)))
    (arrow1a (pts (xy 111.76 83.82) (xy 112.346421 84.946504)))
    (arrow1b (pts (xy 111.76 83.82) (xy 111.173579 84.946504)))
    (arrow2a (pts (xy 111.76 119.38) (xy 112.346421 118.253496)))
    (arrow2b (pts (xy 111.76 119.38) (xy 111.173579 118.253496)))
  )
  (dimension 86.36 (width 0.129032) (layer Dwgs.User)
    (gr_text "3.4000 in" (at 160.02 77.39) (layer Dwgs.User))
    (feature1 (pts (xy 203.2 83.185) (xy 203.2 76.04)))
    (feature2 (pts (xy 116.84 83.185) (xy 116.84 76.04)))
    (crossbar (pts (xy 116.84 78.74) (xy 203.2 78.74)))
    (arrow1a (pts (xy 203.2 78.74) (xy 202.073496 79.326421)))
    (arrow1b (pts (xy 203.2 78.74) (xy 202.073496 78.153579)))
    (arrow2a (pts (xy 116.84 78.74) (xy 117.966504 79.326421)))
    (arrow2b (pts (xy 116.84 78.74) (xy 117.966504 78.153579)))
  )
  (gr_line (start 116.84 83.82) (end 116.84 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 203.2 83.82) (end 116.84 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 203.2 119.38) (end 203.2 83.82) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.84 119.38) (end 203.2 119.38) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 117.475 84.455) (xy 202.565 84.455) (xy 202.565 118.745) (xy 117.475 118.745)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.99 102.87) (xy 176.53 102.87) (xy 176.53 113.03) (xy 173.99 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 189.23 102.87) (xy 191.77 102.87) (xy 191.77 105.41) (xy 189.23 105.41)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 100.33) (xy 166.37 100.33) (xy 166.37 102.87) (xy 163.83 102.87)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.51 108.585) (xy 146.05 108.585) (xy 146.05 111.125) (xy 143.51 111.125)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.94 96.52) (xy 157.48 96.52) (xy 157.48 99.06) (xy 154.94 99.06)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 117.475 118.745) (xy 202.565 118.745) (xy 202.565 84.455) (xy 117.475 84.455)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 137.795 96.52) (xy 139.065 96.52) (xy 139.7 97.155) (xy 139.7 98.425) (xy 139.065 99.06)
        (xy 137.795 99.06) (xy 137.16 98.425) (xy 137.16 97.155)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 144.78 97.155) (xy 145.415 96.52) (xy 146.685 96.52) (xy 147.32 97.155) (xy 147.32 98.425)
        (xy 146.685 99.06) (xy 145.415 99.06) (xy 144.78 98.425)
      )
    )
  )
)
