(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/Pin_1")
  (net 2 "/Pin_2")
  (net 3 "/Pin_3")
  (net 4 "/Pin_4")
  (net 5 "/Pin_5")
  (net 6 "GND")
  (footprint "Package_TO_SOT_THT:TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical" (layer "F.Cu")
    (at 134.35 77.4)
    (descr "TO-220-5, Vertical, RM 1.7mm, Pentawatt, Multiwatt-5, staggered type-1, see http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-to-220/to-220_5_05-08-1421.pdf?domain=www.linear.com, https://www.diodes.com/assets/Package-Files/TO220-5.pdf")
    (tags "TO-220-5 Vertical RM 1.7mm Pentawatt Multiwatt-5 staggered type-1")
    (property "Sheetfile" "TO-220-5 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Adjustable 1.1A Single Resistor Low Dropout Regulator, TO-220")
    (property "ki_keywords" "Adjustable 1.1A Low Dropout Regulator")
    (attr through_hole)
    (fp_text reference "U101" (at 3.4 -9.32) (layer "F.SilkS"))
    (fp_text value "LT3080xT" (at 3.4 2.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.4 -9.32) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "/Pin_1") (pinfunction "NC") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.7 -3.7) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "/Pin_2") (pinfunction "SET") (pintype "input"))
    (pad "3" thru_hole oval (at 3.4 0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "/Pin_3") (pinfunction "OUT") (pintype "power_out"))
    (pad "4" thru_hole oval (at 5.1 -3.7) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "/Pin_4") (pinfunction "VCONTROL") (pintype "input"))
    (pad "5" thru_hole oval (at 6.8 0) (size 1.8 1.8) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "/Pin_5") (pinfunction "IN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-5_P3.4x3.7mm_StaggerOdd_Lead3.8mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "B.Cu")
    (at 131.45 85.7 -90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "TO-220-5 Breakout.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J101" (at 3 -6.54) (layer "B.SilkS"))
    (fp_text value "Conn_01x06" (at -3 -6.54) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -6.35) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "/Pin_1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/Pin_2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/Pin_3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/Pin_4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/Pin_5") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 125 67) (end 150 67)
    (layer "Edge.Cuts"))
  (gr_line (start 125 92) (end 125 67)
    (layer "Edge.Cuts"))
  (gr_line (start 150 92) (end 125 92)
    (layer "Edge.Cuts"))
  (gr_line (start 150 67) (end 150 92)
    (layer "Edge.Cuts"))
  (gr_text "PCB 0028 TO-220-5\nBreakout, N8FDY, 5-May-23" (at 137.6 91.3) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 125 92) (xy 150 92))
    (height 4)
    (gr_text "25.0000 mm" (at 137.5 94.85) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Cmts.User")
    (pts (xy 150 92) (xy 150 67))
    (height 9)
    (gr_text "25.0000 mm" (at 157.85 79.5 90) (layer "Cmts.User"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 6) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 124.3 66)
        (xy 150.9 66)
        (xy 150.9 92.6)
        (xy 124.7 92.6)
        (xy 124.3 92.2)
      )
    )
  )
)
