(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 34)
    (no_connects 0)
    (area 33.819048 38.3 69.35 89.000001)
    (thickness 1.6)
    (drawings 41)
    (tracks 134)
    (zones 0)
    (modules 17)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 3.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 50 45)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /i2c_bridge_common/SCL_connector)
  (net 4 /i2c_bridge_common/SDA_connector)
  (net 5 /i2c_bridge_common/SCL_inside)
  (net 6 /i2c_bridge_common/SDA_inside)
  (net 7 "Net-(R5-Pad2)")
  (net 8 "Net-(R6-Pad2)")
  (net 9 "Net-(R7-Pad1)")
  (net 10 "Net-(TRRS1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /i2c_bridge_common/SCL_connector)
    (add_net /i2c_bridge_common/SCL_inside)
    (add_net /i2c_bridge_common/SDA_connector)
    (add_net /i2c_bridge_common/SDA_inside)
    (add_net GND)
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(TRRS1-Pad2)")
  )
  (net_class power ""
    (clearance 0.3)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module myComponents:solderPads_4_Grove_I2C (layer F.Cu) (tedit 58E53D59)
    (at 50 71)
    (fp_text reference I2C1 (at 0.635 2.54) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 3) (layer F.Fab))
    (fp_text user SDA (at -3.25 0 90) (layer F.SilkS))
    (fp_text user SCL (at -4.75 0 90) (layer F.SilkS))
    (fp_text user Gnd (at 4.75 0 90) (layer F.SilkS))
    (fp_text user Vcc (at 3.25 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.905 0) (size 0.9 3) (layers F.Cu F.Paste F.Mask)
      (net 5 /i2c_bridge_common/SCL_inside))
    (pad 2 smd rect (at -0.635 0) (size 0.9 3) (layers F.Cu F.Paste F.Mask)
      (net 6 /i2c_bridge_common/SDA_inside))
    (pad 3 smd rect (at 0.635 0) (size 0.9 3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 1.905 0) (size 0.9 3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58E6699A)
    (at 55.55 52.85)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.5 0) (layer F.Fab))
    (fp_text value 10µf (at 0 -0.15 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58E669AE)
    (at 55.55 54.85)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.404999 -0.065) (layer F.Fab))
    (fp_text value 1µF (at -0.095001 -0.15 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58E669DD)
    (at 55.55 56.85)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.5 0) (layer F.Fab))
    (fp_text value 0.1µF (at 0 -0.15 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 58E7A419)
    (at 54.5 47.5 90)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at 0 0 180) (layer F.SilkS))
    (fp_text value VESD05a1 (at 5 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.7 0 270) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /i2c_bridge_common/SCL_connector))
  )
  (module Diodes_SMD:SOD-523 (layer F.Cu) (tedit 58E7A473)
    (at 44.7 50.5 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D2 (at 0 0 270) (layer F.SilkS))
    (fp_text value VESD05a1 (at 6.7 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /i2c_bridge_common/SDA_connector))
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 58E7A4A6)
    (at 50 64.575)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at -0.365 1.5) (layer F.Fab))
    (fp_text value P82B715 (at -0.865 -1.5) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 /i2c_bridge_common/SCL_connector))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 /i2c_bridge_common/SCL_inside))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 /i2c_bridge_common/SDA_inside))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 /i2c_bridge_common/SDA_connector))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E66A9B)
    (at 55.5 59.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.254999 -0.065) (layer F.Fab))
    (fp_text value 1K (at 0.004999 -0.065 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /i2c_bridge_common/SCL_connector))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E66A6F)
    (at 55.5 63.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.264999 -0.115) (layer F.Fab))
    (fp_text value 1K (at 0.014999 -0.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /i2c_bridge_common/SDA_connector))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E66AB2)
    (at 55.5 61.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.204999 0.065) (layer F.Fab))
    (fp_text value 2K2 (at -0.045001 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /i2c_bridge_common/SCL_inside))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E66AD3)
    (at 55.5 65.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.214999 -0.115) (layer F.Fab))
    (fp_text value 2K2 (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /i2c_bridge_common/SDA_inside))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myComponents:audio_smd_SJ-43514-SMT (layer F.Cu) (tedit 58E7A452)
    (at 50 45 270)
    (fp_text reference TRRS1 (at 6 2 270) (layer F.Fab))
    (fp_text value SJ-43514-SMT (at 6 -2 270) (layer F.SilkS))
    (pad "" thru_hole circle (at 4.5 0 270) (size 2 2) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at 11.5 0 270) (size 2 2) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
    (pad 4 smd rect (at 3.4 3.8 270) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 4 /i2c_bridge_common/SDA_connector))
    (pad 2 smd rect (at 12.8 3.8 270) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(TRRS1-Pad2)"))
    (pad 3 smd rect (at 5.3 -3.8 270) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 3 /i2c_bridge_common/SCL_connector))
    (pad 1 smd rect (at 0.6 3.8 270) (size 2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model /mnt/gruscht/projects/keyboard/kicad_boards/myComponents.pretty/3d-models/audio_jack_SJ-43514-SMT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E7D888)
    (at 44.8 61)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.75 0) (layer F.Fab))
    (fp_text value 10K (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E7D9AC)
    (at 44.8 63 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 2.75 0 180) (layer F.Fab))
    (fp_text value 10K (at 0.05 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E7D8B9)
    (at 44.8 65)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.75 0) (layer F.Fab))
    (fp_text value 93K1 (at 0 -0.1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 583F3ECB)
    (at 44.35 54.5)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U2 (at 0 0 90) (layer F.SilkS))
    (fp_text value AP2553W6 (at -6.35 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R6-Pad2)"))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(TRRS1-Pad2)"))
    (pad 5 smd rect (at 1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R7-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myComponents:logo (layer B.Cu) (tedit 58EA325D)
    (at 50 70.8 180)
    (descr "Imported from logo.svg")
    (tags svg2mod)
    (attr smd)
    (fp_text reference svg2mod (at 0 4.613096 180) (layer B.SilkS) hide)
    (fp_text value G*** (at 0 -4.613096 180) (layer B.SilkS) hide)
  )
  (gr_text "i2c_bridge_primary\n2017-04-09" (at 49.9 67.6) (layer B.SilkS))
  (gr_text K (at 45.5 51.5 90) (layer F.SilkS))
  (gr_text K (at 55.5 48.25) (layer F.SilkS))
  (gr_line (start 44 49) (end 42 49) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44 45) (end 44 49) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56 49) (end 56 45) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58 49) (end 56 49) (layer Edge.Cuts) (width 0.15))
  (dimension 16 (width 0.3) (layer Eco2.User)
    (gr_text "16.000 mm" (at 50 39.65) (layer Eco2.User))
    (feature1 (pts (xy 42 44) (xy 42 38.3)))
    (feature2 (pts (xy 58 44) (xy 58 38.3)))
    (crossbar (pts (xy 58 41) (xy 42 41)))
    (arrow1a (pts (xy 42 41) (xy 43.126504 40.413579)))
    (arrow1b (pts (xy 42 41) (xy 43.126504 41.586421)))
    (arrow2a (pts (xy 58 41) (xy 56.873496 40.413579)))
    (arrow2b (pts (xy 58 41) (xy 56.873496 41.586421)))
  )
  (dimension 28 (width 0.3) (layer Eco2.User)
    (gr_text "28.000 mm" (at 62.85 59 90) (layer Eco2.User))
    (feature1 (pts (xy 60 45) (xy 64.2 45)))
    (feature2 (pts (xy 60 73) (xy 64.2 73)))
    (crossbar (pts (xy 61.5 73) (xy 61.5 45)))
    (arrow1a (pts (xy 61.5 45) (xy 62.086421 46.126504)))
    (arrow1b (pts (xy 61.5 45) (xy 60.913579 46.126504)))
    (arrow2a (pts (xy 61.5 73) (xy 62.086421 71.873496)))
    (arrow2b (pts (xy 61.5 73) (xy 60.913579 71.873496)))
  )
  (gr_line (start 42 49) (end 42 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 58 69) (end 58 49) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56 69) (end 58 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56 69) (end 56 73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44 69) (end 42 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 44 69) (end 44 73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56 73) (end 44 73) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 56 45) (end 44 45) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 45) (xy 58.5 45) (xy 58.5 89) (xy 41.5 89) (xy 41.5 46)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 45) (xy 59 45) (xy 59 89) (xy 41 89)
      )
    )
  )
)
