(kicad_pcb (version 20171130) (host pcbnew 5.1.8-1.fc31)
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 30)
    (zones 0)
    (modules 13)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.54)
    (user_trace_width 0.254)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.2032)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8128)
    (via_drill 0.4064)
    (via_min_size 0.381)
    (via_min_drill 0.3)
    (uvia_size 0.8128)
    (uvia_drill 0.4064)
    (uvias_allowed no)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2032)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.1524)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 2.032)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 91.44 91.44)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gbr"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D1-Pad1)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad4)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.8128)
    (via_drill 0.4064)
    (uvia_dia 0.8128)
    (uvia_drill 0.4064)
    (diff_pair_width 0.254)
    (diff_pair_gap 0.254)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(J1-Pad1)")
  )
  (module sgt-footprints4:anderson_powerpole_1x02_Vertical (layer F.Cu) (tedit 6024A592)
    (at 101.924 86.36 180)
    (descr "Anderson Powerpole, 1x02, single row")
    (tags "Anderson Powerpole 1x02")
    (fp_text reference J1 (at -6.026 0 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 13.97) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 8.382 180) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sgt-footprints4:MountingHole-no2 (layer F.Cu) (tedit 602B226A)
    (at 94.615 88.9)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole-no2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 -3.048) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 2.413) (layers *.Cu *.Mask))
  )
  (module sgt-footprints4:MountingHole-no2 (layer F.Cu) (tedit 602B226A)
    (at 94.615 71.12)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole-no2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 -3.048) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 2.413) (layers *.Cu *.Mask))
  )
  (module sgt-footprints4:MountingHole-no2 (layer F.Cu) (tedit 602B226A)
    (at 151.765 71.755)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole-no2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 -3.048) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 2.413) (layers *.Cu *.Mask))
  )
  (module sgt-footprints4:MountingHole-no2 (layer F.Cu) (tedit 602B226A)
    (at 151.765 88.9)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole-no2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0 -3.048) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.048 3.048) (drill 2.413) (layers *.Cu *.Mask))
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294EBC)
    (at 150.495 83.185 90)
    (descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J4 (at 8.89 -1.27 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 2.54 5.66 90) (layer F.Fab))
    (fp_text user %R (at 2.54 3.2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sgt-footprints4:DPAK-handsolder (layer F.Cu) (tedit 6024A8B2)
    (at 130.81 78.74 270)
    (fp_text reference D3 (at -0.525955 -6.893605 90) (layer F.SilkS))
    (fp_text value dual-schottky-diode (at 7.4423 7.13075 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.556 270) (size 6.604 8.001) (layers F.Cu F.Mask)
      (net 4 "Net-(D3-Pad4)"))
    (pad 3 smd rect (at 2.286 4.953 270) (size 1.1176 4.3942) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -2.286 4.953 270) (size 1.1176 4.3942) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
  )
  (module sgt-footprints4:anderson_powerpole_1x02_Vertical (layer F.Cu) (tedit 6024A592)
    (at 118.11 86.36 180)
    (descr "Anderson Powerpole, 1x02, single row")
    (tags "Anderson Powerpole 1x02")
    (fp_text reference J2 (at -5.715 -3.175 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 13.97) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 8.382 180) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sgt-footprints4:anderson_powerpole_1x02_Vertical (layer F.Cu) (tedit 6024A592)
    (at 143.51 86.36 180)
    (descr "Anderson Powerpole, 1x02, single row")
    (tags "Anderson Powerpole 1x02")
    (fp_text reference J3 (at 5.715 -3.175 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 13.97) (layer F.Fab))
    (fp_text user %R (at 0 -1.016 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 8.382 180) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 5.08 5.08) (drill 2.032) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 108.458 82.27 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923076923076923)
      (net 6 "Net-(J1-Pad1)"))
    (pad 1 smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923076923076923)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 96.012 83.185 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value R_US (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0.127 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923076923076923)
      (net 6 "Net-(J1-Pad1)"))
    (pad 1 smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1923076923076923)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 112.014 78.1955 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.82 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5F68FEF0)
    (at 95.885 78.105 90)
    (descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode handsolder")
    (attr smd)
    (fp_text reference D1 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1754385964912281)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Output\n" (at 142.875 71.12) (layer F.SilkS))
  (gr_text "Input B" (at 118.11 71.12) (layer F.SilkS))
  (gr_text "Input A" (at 101.6 71.12) (layer F.SilkS))
  (gr_text "SGT-21011\nDC Dual Power" (at 130.81 85.09) (layer F.SilkS))
  (gr_line (start 154.94 68.58) (end 154.94 91.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91.44 68.58) (end 154.94 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 91.44 91.44) (end 91.44 68.58) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 154.94 91.44) (end 91.44 91.44) (layer Edge.Cuts) (width 0.05))
)
