(kicad_pcb (version 20170123) (host pcbnew "(2017-07-16 revision e797af331)-makepkg")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 335)
    (zones 0)
    (modules 20)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.1)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.6)
    (pad_drill 1.15)
    (pad_to_mask_clearance 0.1)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/Valerio/Documents/dock-new/board/gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 /UD+)
  (net 7 /UD-)
  (net 8 "Net-(J2-Pad2)")
  (net 9 /TX+)
  (net 10 /TX-)
  (net 11 /RX+)
  (net 12 /RX-)
  (net 13 /D-)
  (net 14 /D+)
  (net 15 "Net-(F1-Pad2)")
  (net 16 ETH_PWR)
  (net 17 "Net-(D1-Pad2)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(U3-Pad17)")
  (net 20 "Net-(U3-Pad18)")
  (net 21 "Net-(U3-Pad19)")
  (net 22 "Net-(U3-Pad20)")
  (net 23 "Net-(U3-Pad26)")
  (net 24 "Net-(U3-Pad27)")
  (net 25 "Net-(U3-Pad28)")
  (net 26 "Net-(U3-Pad2)")
  (net 27 "Net-(U3-Pad3)")
  (net 28 "Net-(U3-Pad4)")
  (net 29 "Net-(U3-Pad5)")
  (net 30 "Net-(U3-Pad6)")
  (net 31 "Net-(U3-Pad7)")
  (net 32 "Net-(U3-Pad8)")
  (net 33 "Net-(U3-Pad9)")
  (net 34 "Net-(U3-Pad10)")
  (net 35 "Net-(U3-Pad11)")
  (net 36 "Net-(U3-Pad12)")
  (net 37 "Net-(U3-Pad13)")
  (net 38 "Net-(U3-Pad14)")
  (net 39 "Net-(U3-Pad15)")
  (net 40 "Net-(U3-Pad16)")
  (net 41 "Net-(J3-Pad13)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /RX+)
    (add_net /RX-)
    (add_net /UD+)
    (add_net /UD-)
    (add_net ETH_PWR)
    (add_net GND)
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(U3-Pad10)")
    (add_net "Net-(U3-Pad11)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad14)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad19)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad20)")
    (add_net "Net-(U3-Pad26)")
    (add_net "Net-(U3-Pad27)")
    (add_net "Net-(U3-Pad28)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad8)")
    (add_net "Net-(U3-Pad9)")
  )
  (net_class RX ""
    (clearance 0.1)
    (trace_width 0.1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class TX ""
    (clearance 0.1)
    (trace_width 0.1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /TX+)
    (add_net /TX-)
  )
  (module logo:LOGO (layer F.Cu) (tedit 0)
    (at 191.8208 58.674)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 158.3436 65.7352)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Connectors:USB_Micro-B (layer F.Cu) (tedit 5987B4C1)
    (at 156.9 58.1 270)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J2 (at -5.68 -0.01 270) (layer F.SilkS))
    (fp_text value USB_PWR (at 0 5.01 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at 0 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 4 smd rect (at 0.65 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.35) (size 1.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.5 -1.35) (size 1.1 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.5 -1.35) (size 1.1 1.25) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -4.175 1.35) (size 2 1.6) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 4.175 1.35) (size 2 1.6) (drill 1.15) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59519441)
    (at 174.1424 50.1396 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0.1524 -1.7272 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 172.0088 64.3128 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 1.016 -4.5 270) (layer F.SilkS))
    (fp_text value AP111733 (at 0 4.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module omega:Socket_Strip_Straight_1x16_Pitch2.00mm locked (layer F.Cu) (tedit 59514D1A)
    (at 161.7 69.9 90)
    (descr "Through hole straight socket strip, 1x16, 2.00mm pitch, single row")
    (tags "Through hole socket strip THT 1x16 2.00mm single row")
    (fp_text reference U3 (at 0 -2.06 90) (layer F.Fab))
    (fp_text value OMEGA_2 (at 12.6 12 90) (layer F.Fab))
    (pad 17 thru_hole oval (at 24.4 30 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(U3-Pad17)"))
    (pad 18 thru_hole oval (at 24.4 28 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(U3-Pad18)"))
    (pad 19 thru_hole oval (at 24.4 26 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(U3-Pad19)"))
    (pad 20 thru_hole oval (at 24.4 24 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U3-Pad20)"))
    (pad 21 thru_hole oval (at 24.4 22 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /RX+))
    (pad 22 thru_hole oval (at 24.4 20 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /RX-))
    (pad 23 thru_hole oval (at 24.4 18 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /TX+))
    (pad 24 thru_hole oval (at 24.4 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /TX-))
    (pad 25 thru_hole oval (at 24.4 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 ETH_PWR))
    (pad 26 thru_hole oval (at 24.4 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U3-Pad26)"))
    (pad 27 thru_hole oval (at 24.4 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U3-Pad27)"))
    (pad 28 thru_hole oval (at 24.4 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U3-Pad28)"))
    (pad 29 thru_hole oval (at 24.4 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /D-))
    (pad 30 thru_hole oval (at 24.4 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /D+))
    (pad 31 thru_hole oval (at 24.4 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 32 thru_hole rect (at 24.4 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U3-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U3-Pad3)"))
    (pad 4 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U3-Pad4)"))
    (pad 5 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U3-Pad5)"))
    (pad 6 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad6)"))
    (pad 7 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U3-Pad7)"))
    (pad 8 thru_hole oval (at 0 14 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U3-Pad8)"))
    (pad 9 thru_hole oval (at 0 16 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U3-Pad9)"))
    (pad 10 thru_hole oval (at 0 18 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U3-Pad10)"))
    (pad 11 thru_hole oval (at 0 20 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U3-Pad11)"))
    (pad 12 thru_hole oval (at 0 22 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U3-Pad12)"))
    (pad 13 thru_hole oval (at 0 24 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U3-Pad13)"))
    (pad 14 thru_hole oval (at 0 26 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad14)"))
    (pad 15 thru_hole oval (at 0 28 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(U3-Pad15)"))
    (pad 16 thru_hole oval (at 0 30 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(U3-Pad16)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x16_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 598F2EEA)
    (at 163.7284 56.7944 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference F1 (at 0.1 2 270) (layer F.SilkS))
    (fp_text value 1.5A (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at -3.5 3.1 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_4x5.3 (layer B.Cu) (tedit 59519543)
    (at 171.0436 55.9816 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.3")
    (attr smd)
    (fp_text reference C1 (at 3.9116 0.0508) (layer B.SilkS))
    (fp_text value 10uF (at 0 3.54 90) (layer B.Fab))
    (fp_text user + (at -1.21 0.08 90) (layer B.Fab))
    (fp_text user + (at -2.77 -2.01 90) (layer B.SilkS))
    (fp_text user %R (at 0 -3.54 90) (layer B.Fab))
    (pad 1 smd rect (at -1.8 0 270) (size 2.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.8 0 270) (size 2.6 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_4x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:CP_Elec_6.3x5.3 (layer B.Cu) (tedit 59519507)
    (at 172.0596 64.1604 90)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C2 (at -3.9624 3.4544) (layer B.SilkS))
    (fp_text value 100uF (at 0 4.56 90) (layer B.Fab))
    (fp_text user + (at -1.75 0.08 90) (layer B.Fab))
    (fp_text user + (at -4.28 -3.01 90) (layer B.SilkS))
    (fp_text user %R (at 0 -4.56 90) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/CP_Elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59519446)
    (at 179.6088 48.9712)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.0308 -1.524) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59519467)
    (at 182.372 60.6352 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0.02 -1.8288 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 ETH_PWR))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:USB_A (layer B.Cu) (tedit 5951958B)
    (at 166 61.9 90)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference J1 (at 11.7096 0.3352 180) (layer B.SilkS))
    (fp_text value USB_A (at 3.84 -7.44 90) (layer B.Fab))
    (pad 4 thru_hole circle (at 7.11 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.57 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 /UD+))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 /UD-))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (pad 5 thru_hole circle (at 10.16 -2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole circle (at -3.56 -2.67 180) (size 3 3) (drill 2.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors.3dshapes/USB_A.wrl
      (at (xyz 0.14 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6_Handsoldering (layer F.Cu) (tedit 59519481)
    (at 168.7 49.6 90)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (attr smd)
    (fp_text reference U1 (at 0.43 -2.75 180) (layer F.SilkS))
    (fp_text value USBLC6-2 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /UD+))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /UD-))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 /D-))
    (pad 6 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 /D+))
    (pad 5 smd rect (at 1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer B.Cu) (tedit 595FC724)
    (at 157.988 67.4624)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at -0.1016 1.8796 180) (layer B.SilkS))
    (fp_text value PWR (at 0 -1.9) (layer B.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module RJ45-TRAFO-AMPHENOL:RJ45_TRAFO_AMPHENOL (layer B.Cu) (tedit 598679A4)
    (at 177.3936 62.4028 270)
    (tags RJ45)
    (fp_text reference J3 (at 5.0088 -2.794) (layer B.SilkS))
    (fp_text value RJ45-TRAFO (at -3.81 -13 270) (layer B.Fab))
    (pad 8 thru_hole circle (at 0.66 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 13 thru_hole circle (at -11.56 -5.84 270) (size 2.54 2.54) (drill 1.78) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(J3-Pad13)"))
    (pad 13 thru_hole circle (at 3.94 -5.84 270) (size 2.54 2.54) (drill 1.78) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(J3-Pad13)"))
    (pad 7 thru_hole circle (at -0.62 -2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.88 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 /TX-))
    (pad 5 thru_hole circle (at -3.15 -2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 ETH_PWR))
    (pad 4 thru_hole circle (at -4.42 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 /TX+))
    (pad 3 thru_hole circle (at -5.69 -2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 /RX-))
    (pad 2 thru_hole circle (at -6.96 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 16 ETH_PWR))
    (pad 1 thru_hole rect (at -8.24 -2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 /RX+))
    (pad Hole thru_hole circle (at -9.53 -8.89 270) (size 3.85 3.85) (drill 3.3) (layers *.Cu *.SilkS *.Mask))
    (pad Hole thru_hole circle (at 1.91 -8.89 270) (size 3.85 3.85) (drill 3.3) (layers *.Cu *.SilkS *.Mask))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 180.6956 50.1612 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -4.5504 -6.5024 90) (layer F.SilkS))
    (fp_text value 50R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /RX+))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 178.5112 50.1604 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -4.5512 -5.7404 90) (layer F.SilkS))
    (fp_text value 50R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 174.183217 50.162289 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 4.549311 4.257217 270) (layer F.SilkS))
    (fp_text value 50R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 176.383217 50.162289 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 4.549311 5.034817 270) (layer F.SilkS))
    (fp_text value 50R (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /TX+))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 157.988 69.7992)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.8448 0 90) (layer F.SilkS))
    (fp_text value 150R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text github.com/5N44P (at 188.0108 47.8536) (layer F.SilkS))
  (gr_text ethernet (at 192 67.9) (layer B.SilkS))
  (gr_text "usb host" (at 165.354 67.9) (layer B.SilkS))
  (gr_text "power in" (at 160.85 58 270) (layer F.SilkS))
  (gr_text omega2/2+ (at 190.7032 48.4124) (layer B.SilkS))
  (gr_text dock\new (at 165.47 47.97) (layer B.SilkS))
  (gr_line (start 194.1 70.9) (end 197 68) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 197 48.8) (end 197 68) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 192.7 44.5) (end 197 48.8) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160.7 44.5) (end 192.7 44.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.1 51.1) (end 160.7 44.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.1 70.9) (end 154.1 51.1) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 154.1 70.9) (end 194.1 70.9) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154.1 70.9) (xy 166 70.9) (xy 167.8 70.9) (xy 179.5 70.9) (xy 180.8 70.9)
        (xy 194.1 70.9) (xy 197 68) (xy 197 48.8) (xy 192.7 44.5) (xy 160.7 44.5)
        (xy 154.1 51.1)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 2))
    (polygon
      (pts
        (xy 197 48.8) (xy 197 68) (xy 194.1 70.9) (xy 154.1 70.9) (xy 154.1 51.1)
        (xy 160.7 44.5) (xy 192.7 44.5)
      )
    )
  )
)
