<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<text>G</text>
<text>3V3</text>
<text>5V</text>
<text>R</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>4</text>
<wire x1="0" y1="0" x2="43.18" y2="0" width="0" layer="20"/>
<wire x1="43.18" y1="0" x2="43.18" y2="35.56" width="0" layer="20"/>
<wire x1="43.18" y1="35.56" x2="0" y2="35.56" width="0" layer="20"/>
<wire x1="0" y1="35.56" x2="0" y2="0" width="0" layer="20"/>
<hole x="1.905" y="33.655" drill="3.2"/>
<hole x="1.905" y="1.905" drill="3.2"/>
<hole x="41.275" y="1.905" drill="3.2"/>
<hole x="41.275" y="33.655" drill="3.2"/>
<text>HelvePic32 Wing for ESP8266</text>
<text>www.boxtec.ch</text>
<text>TX</text>
<text>RX</text>
<text>G0</text>
<text>G2</text>
<text>G15</text>
<text>G13</text>
<text>G12</text>
<text>G14</text>
<text>CHPD</text>
<text>G18</text>
<text>GND</text>
<text>3v3</text>
<text>URX</text>
<text>UTX</text>
<text>G18</text>
<text>CHPD</text>
<text>G14</text>
<text>G12</text>
<text>G13</text>
<text>G15</text>
<text>G2</text>
<text>G0</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X12-CB">
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="ESP-03">
<description>ESP8266 Modules 3 &amp; 4</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="esp8266modules" package="ESP-03" value="ESP8266">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="adafruit" package="1X12-CB" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="12"/>
<contactref element="U$1" pad="GND"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="12"/>
</signal>
<signal name="3V3">
<contactref element="JP1" pad="11"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="10"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="RES">
<contactref element="JP1" pad="9"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D7">
<contactref element="JP1" pad="8"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="D6">
<contactref element="JP1" pad="7"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="D5">
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="D4">
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="D3">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="D2">
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="D1">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="UTX">
<contactref element="U$1" pad="UTXD"/>
<contactref element="JP3" pad="11"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="URX">
<contactref element="U$1" pad="URXD"/>
<contactref element="JP3" pad="10"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="G18">
<contactref element="U$1" pad="GPIO18"/>
<contactref element="JP3" pad="9"/>
<contactref element="JP5" pad="8"/>
</signal>
<signal name="CHPD">
<contactref element="U$1" pad="CH_PD"/>
<contactref element="JP3" pad="8"/>
<contactref element="JP5" pad="7"/>
</signal>
<signal name="G14">
<contactref element="U$1" pad="GPIO14"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP5" pad="6"/>
</signal>
<signal name="G12">
<contactref element="U$1" pad="GPIO12"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP5" pad="5"/>
</signal>
<signal name="G13">
<contactref element="U$1" pad="GPIO13"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP5" pad="4"/>
</signal>
<signal name="G15">
<contactref element="U$1" pad="GPIO15"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="G2">
<contactref element="U$1" pad="GPIO2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="G0">
<contactref element="U$1" pad="GPIO0"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="D0">
<contactref element="JP2" pad="12"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
