(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.5875)
    (drawings 183)
    (tracks 1286)
    (zones 0)
    (modules 96)
    (nets 164)
  )
  (page USLetter)
  (title_block
    (title Smoother)
    (date 2018-09-11)
    (company "Cafe Electric LLC")
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 1.778)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.778)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.0254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1524)
    (pcb_text_size 0.762 0.762)
    (mod_edge_width 0.15)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1524)
    (pad_size 1.6 1.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BT1-Pad1)")
  (net 3 +3V3)
  (net 4 I1)
  (net 5 I2)
  (net 6 I3)
  (net 7 I4)
  (net 8 I5)
  (net 9 I6)
  (net 10 +12V)
  (net 11 OUT6)
  (net 12 OUT5)
  (net 13 "Net-(D4-Pad1)")
  (net 14 OUT3)
  (net 15 OUT4)
  (net 16 OUT2)
  (net 17 OUT1)
  (net 18 +5V)
  (net 19 "Net-(J3-Pad2)")
  (net 20 "Net-(J3-Pad3)")
  (net 21 "Net-(J3-Pad4)")
  (net 22 "Net-(J3-Pad5)")
  (net 23 "Net-(J3-Pad6)")
  (net 24 "Net-(J3-Pad7)")
  (net 25 "Net-(J7-Pad3)")
  (net 26 "Net-(J7-Pad4)")
  (net 27 ISOSPIH)
  (net 28 CAN2H)
  (net 29 CAN1H)
  (net 30 GAS_GAUGE)
  (net 31 SPEED_OUT)
  (net 32 IN6)
  (net 33 IN4)
  (net 34 IN2)
  (net 35 ISOSPIL)
  (net 36 CAN2L)
  (net 37 CAN1L)
  (net 38 TACH_OUT)
  (net 39 IN5)
  (net 40 IN3)
  (net 41 IN1)
  (net 42 "Net-(J20-Pad3)")
  (net 43 "Net-(J20-Pad4)")
  (net 44 "Net-(J20-Pad2)")
  (net 45 "Net-(J20-Pad1)")
  (net 46 "Net-(Q1-Pad2)")
  (net 47 "Net-(Q1-Pad5)")
  (net 48 "Net-(Q2-Pad3)")
  (net 49 "Net-(Q2-Pad5)")
  (net 50 "Net-(Q2-Pad2)")
  (net 51 "Net-(Q2-Pad6)")
  (net 52 "Net-(Q3-Pad6)")
  (net 53 "Net-(Q3-Pad2)")
  (net 54 "Net-(Q3-Pad5)")
  (net 55 "Net-(Q3-Pad3)")
  (net 56 "Net-(Q4-Pad3)")
  (net 57 "Net-(Q4-Pad5)")
  (net 58 "Net-(Q4-Pad2)")
  (net 59 "Net-(Q4-Pad6)")
  (net 60 "Net-(Q5-Pad4)")
  (net 61 "Net-(Q5-Pad2)")
  (net 62 "Net-(Q6-Pad2)")
  (net 63 "Net-(Q6-Pad4)")
  (net 64 "Net-(Q7-Pad4)")
  (net 65 "Net-(Q7-Pad2)")
  (net 66 Speed)
  (net 67 Tach)
  (net 68 G6)
  (net 69 G5)
  (net 70 G4)
  (net 71 G3)
  (net 72 G2)
  (net 73 G1)
  (net 74 O5)
  (net 75 O4)
  (net 76 O3)
  (net 77 O2)
  (net 78 O1)
  (net 79 "Net-(U1-Pad26)")
  (net 80 "Net-(U1-Pad27)")
  (net 81 "Net-(U1-Pad28)")
  (net 82 "Net-(U1-Pad29)")
  (net 83 "Net-(U1-Pad30)")
  (net 84 "Net-(U1-Pad31)")
  (net 85 "Net-(U1-Pad32)")
  (net 86 "Net-(U1-Pad8)")
  (net 87 "Net-(U1-Pad6)")
  (net 88 "Net-(U1-Pad5)")
  (net 89 "Net-(U1-Pad3)")
  (net 90 "Net-(U1-Pad2)")
  (net 91 I7)
  (net 92 O6_Fuel_Lt)
  (net 93 I8)
  (net 94 "Net-(U1-Pad54)")
  (net 95 "Net-(U1-Pad63)")
  (net 96 "Net-(U1-Pad64)")
  (net 97 "Net-(U1-Pad65)")
  (net 98 "Net-(U1-Pad66)")
  (net 99 "Net-(U1-Pad67)")
  (net 100 "Net-(U1-Pad68)")
  (net 101 "Net-(U1-Pad69)")
  (net 102 "Net-(U1-Pad70)")
  (net 103 "Net-(U1-Pad71)")
  (net 104 "Net-(U1-Pad72)")
  (net 105 "Net-(U1-Pad73)")
  (net 106 "Net-(U1-Pad74)")
  (net 107 "Net-(U1-Pad75)")
  (net 108 "Net-(U1-Pad76)")
  (net 109 "Net-(U1-Pad77)")
  (net 110 "Net-(U1-Pad78)")
  (net 111 "Net-(U1-Pad79)")
  (net 112 "Net-(U1-Pad80)")
  (net 113 "Net-(U1-Pad81)")
  (net 114 "Net-(U1-Pad82)")
  (net 115 "Net-(U1-Pad83)")
  (net 116 "Net-(U1-Pad84)")
  (net 117 "Net-(U1-Pad85)")
  (net 118 "Net-(U1-Pad86)")
  (net 119 "Net-(U1-Pad58)")
  (net 120 "Net-(U1-Pad59)")
  (net 121 "Net-(U1-Pad60)")
  (net 122 "Net-(U1-Pad61)")
  (net 123 "Net-(U1-Pad62)")
  (net 124 "Net-(U2-Pad5)")
  (net 125 "Net-(U3-Pad5)")
  (net 126 "Net-(J21-Pad1)")
  (net 127 "Net-(J21-Pad2)")
  (net 128 "Net-(J21-Pad3)")
  (net 129 "Net-(J21-Pad4)")
  (net 130 "Net-(J21-Pad5)")
  (net 131 "Net-(J21-Pad6)")
  (net 132 "Net-(J21-Pad7)")
  (net 133 "Net-(J22-Pad6)")
  (net 134 "Net-(J22-Pad5)")
  (net 135 "Net-(J22-Pad4)")
  (net 136 "Net-(J22-Pad3)")
  (net 137 "Net-(J22-Pad2)")
  (net 138 "Net-(J21-Pad10)")
  (net 139 "Net-(J21-Pad9)")
  (net 140 "Net-(J21-Pad8)")
  (net 141 "Net-(J22-Pad7)")
  (net 142 "Net-(J22-Pad8)")
  (net 143 "Net-(J22-Pad9)")
  (net 144 EXT5V)
  (net 145 "Net-(JP1-Pad2)")
  (net 146 "Net-(JP2-Pad2)")
  (net 147 "Net-(C11-Pad1)")
  (net 148 "Net-(C12-Pad1)")
  (net 149 MISO)
  (net 150 "Net-(R39-Pad2)")
  (net 151 "Net-(R39-Pad1)")
  (net 152 "Net-(R41-Pad1)")
  (net 153 "Net-(R42-Pad1)")
  (net 154 "Net-(T1-Pad6)")
  (net 155 "Net-(T1-Pad7)")
  (net 156 "Net-(T1-Pad8)")
  (net 157 "Net-(T1-Pad9)")
  (net 158 "Net-(T1-Pad10)")
  (net 159 "Net-(T1-Pad11)")
  (net 160 "Net-(T1-Pad15)")
  (net 161 MOSI)
  (net 162 CS)
  (net 163 SCK)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net CAN1H)
    (add_net CAN1L)
    (add_net CAN2H)
    (add_net CAN2L)
    (add_net CS)
    (add_net EXT5V)
    (add_net G1)
    (add_net G2)
    (add_net G3)
    (add_net G4)
    (add_net G5)
    (add_net G6)
    (add_net GAS_GAUGE)
    (add_net GND)
    (add_net I1)
    (add_net I2)
    (add_net I3)
    (add_net I4)
    (add_net I5)
    (add_net I6)
    (add_net I7)
    (add_net I8)
    (add_net IN1)
    (add_net IN2)
    (add_net IN3)
    (add_net IN4)
    (add_net IN5)
    (add_net IN6)
    (add_net ISOSPIH)
    (add_net ISOSPIL)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J20-Pad2)")
    (add_net "Net-(J20-Pad3)")
    (add_net "Net-(J20-Pad4)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J21-Pad10)")
    (add_net "Net-(J21-Pad2)")
    (add_net "Net-(J21-Pad3)")
    (add_net "Net-(J21-Pad4)")
    (add_net "Net-(J21-Pad5)")
    (add_net "Net-(J21-Pad6)")
    (add_net "Net-(J21-Pad7)")
    (add_net "Net-(J21-Pad8)")
    (add_net "Net-(J21-Pad9)")
    (add_net "Net-(J22-Pad2)")
    (add_net "Net-(J22-Pad3)")
    (add_net "Net-(J22-Pad4)")
    (add_net "Net-(J22-Pad5)")
    (add_net "Net-(J22-Pad6)")
    (add_net "Net-(J22-Pad7)")
    (add_net "Net-(J22-Pad8)")
    (add_net "Net-(J22-Pad9)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J7-Pad4)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad5)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q2-Pad5)")
    (add_net "Net-(Q2-Pad6)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q3-Pad5)")
    (add_net "Net-(Q3-Pad6)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q4-Pad3)")
    (add_net "Net-(Q4-Pad5)")
    (add_net "Net-(Q4-Pad6)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(Q5-Pad4)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(Q6-Pad4)")
    (add_net "Net-(Q7-Pad2)")
    (add_net "Net-(Q7-Pad4)")
    (add_net "Net-(R39-Pad1)")
    (add_net "Net-(R39-Pad2)")
    (add_net "Net-(R41-Pad1)")
    (add_net "Net-(R42-Pad1)")
    (add_net "Net-(T1-Pad10)")
    (add_net "Net-(T1-Pad11)")
    (add_net "Net-(T1-Pad15)")
    (add_net "Net-(T1-Pad6)")
    (add_net "Net-(T1-Pad7)")
    (add_net "Net-(T1-Pad8)")
    (add_net "Net-(T1-Pad9)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad58)")
    (add_net "Net-(U1-Pad59)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad62)")
    (add_net "Net-(U1-Pad63)")
    (add_net "Net-(U1-Pad64)")
    (add_net "Net-(U1-Pad65)")
    (add_net "Net-(U1-Pad66)")
    (add_net "Net-(U1-Pad67)")
    (add_net "Net-(U1-Pad68)")
    (add_net "Net-(U1-Pad69)")
    (add_net "Net-(U1-Pad70)")
    (add_net "Net-(U1-Pad71)")
    (add_net "Net-(U1-Pad72)")
    (add_net "Net-(U1-Pad73)")
    (add_net "Net-(U1-Pad74)")
    (add_net "Net-(U1-Pad75)")
    (add_net "Net-(U1-Pad76)")
    (add_net "Net-(U1-Pad77)")
    (add_net "Net-(U1-Pad78)")
    (add_net "Net-(U1-Pad79)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad80)")
    (add_net "Net-(U1-Pad81)")
    (add_net "Net-(U1-Pad82)")
    (add_net "Net-(U1-Pad83)")
    (add_net "Net-(U1-Pad84)")
    (add_net "Net-(U1-Pad85)")
    (add_net "Net-(U1-Pad86)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad5)")
    (add_net O1)
    (add_net O2)
    (add_net O3)
    (add_net O4)
    (add_net O5)
    (add_net O6_Fuel_Lt)
    (add_net OUT1)
    (add_net OUT2)
    (add_net OUT3)
    (add_net OUT4)
    (add_net OUT5)
    (add_net OUT6)
    (add_net SCK)
    (add_net SPEED_OUT)
    (add_net Speed)
    (add_net TACH_OUT)
    (add_net Tach)
  )
  (net_class +12V ""
    (clearance 0.1524)
    (trace_width 0.889)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (net_class GND ""
    (clearance 0.1524)
    (trace_width 1.016)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module Custom:Teensy36_custom_fewpads_2 (layer F.Cu) (tedit 5BD4AF55)
    (at 43.18 49.53 270)
    (fp_text reference U1 (at -29.083 10.1981) (layer F.SilkS))
    (fp_text value "TEENSY 3.6" (at 0 10.16 270) (layer F.Fab))
    (pad 17 thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 G2))
    (pad 18 thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 G3))
    (pad 19 thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 G4))
    (pad 20 thru_hole circle (at 19.05 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 G5))
    (pad 16 thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 G1))
    (pad 15 thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 14 thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 149 MISO))
    (pad 21 thru_hole circle (at 21.59 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 G6))
    (pad 22 thru_hole circle (at 24.13 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 135 "Net-(J22-Pad4)"))
    (pad 23 thru_hole circle (at 26.67 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 134 "Net-(J22-Pad5)"))
    (pad 24 thru_hole circle (at 29.21 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 133 "Net-(J22-Pad6)"))
    (pad 25 thru_hole circle (at 16.51 5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 26 connect circle (at 16.51 2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 79 "Net-(U1-Pad26)"))
    (pad 27 connect circle (at 16.51 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 80 "Net-(U1-Pad27)"))
    (pad 28 connect circle (at 16.51 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 81 "Net-(U1-Pad28)"))
    (pad 29 connect circle (at 16.51 -5.08 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 82 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 29.21 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 83 "Net-(U1-Pad30)"))
    (pad 31 thru_hole circle (at 26.67 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 84 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at 24.13 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 85 "Net-(U1-Pad32)"))
    (pad 33 thru_hole circle (at 21.59 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 I6))
    (pad 34 thru_hole circle (at 19.05 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 I5))
    (pad 35 thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 I4))
    (pad 36 thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 I3))
    (pad 37 thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 I2))
    (pad 13 thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 161 MOSI))
    (pad 12 thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 162 CS))
    (pad 11 thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 O5))
    (pad 10 thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 O4))
    (pad 9 thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 76 O3))
    (pad 8 thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 86 "Net-(U1-Pad8)"))
    (pad 7 thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 77 O2))
    (pad 6 thru_hole circle (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "Net-(U1-Pad6)"))
    (pad 5 thru_hole circle (at -19.05 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 88 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at -21.59 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 78 O1))
    (pad 3 thru_hole circle (at -24.13 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 89 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at -26.67 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 90 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at -29.21 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 I1))
    (pad 39 thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 163 SCK))
    (pad 41 thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 91 I7))
    (pad 42 thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 92 O6_Fuel_Lt))
    (pad 43 thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 Tach))
    (pad 44 thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 Speed))
    (pad 45 thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 26 "Net-(J7-Pad4)"))
    (pad 46 thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 "Net-(J7-Pad3)"))
    (pad 47 thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 93 I8))
    (pad 48 thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad7)"))
    (pad 49 thru_hole circle (at -19.05 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad6)"))
    (pad 50 thru_hole circle (at -21.59 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad5)"))
    (pad 51 thru_hole circle (at -24.13 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 52 thru_hole circle (at -26.67 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 53 thru_hole circle (at -29.21 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 54 connect circle (at -26.67 -5.08 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 94 "Net-(U1-Pad54)"))
    (pad 55 thru_hole circle (at -21.59 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad2)"))
    (pad 56 thru_hole circle (at -19.05 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad4)"))
    (pad 57 thru_hole circle (at -16.51 -5.08 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad3)"))
    (pad 63 connect circle (at -13.97 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 95 "Net-(U1-Pad63)"))
    (pad 64 connect circle (at -11.43 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 96 "Net-(U1-Pad64)"))
    (pad 65 connect circle (at -8.89 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 97 "Net-(U1-Pad65)"))
    (pad 66 connect circle (at -6.35 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 98 "Net-(U1-Pad66)"))
    (pad 67 connect circle (at 8.89 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 99 "Net-(U1-Pad67)"))
    (pad 68 connect circle (at 11.43 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 100 "Net-(U1-Pad68)"))
    (pad 69 connect circle (at 13.97 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 101 "Net-(U1-Pad69)"))
    (pad 70 connect circle (at 19.05 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 102 "Net-(U1-Pad70)"))
    (pad 71 connect circle (at 21.59 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 103 "Net-(U1-Pad71)"))
    (pad 72 connect circle (at 24.13 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 104 "Net-(U1-Pad72)"))
    (pad 73 connect circle (at 26.67 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 105 "Net-(U1-Pad73)"))
    (pad 74 connect circle (at 29.21 0 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 106 "Net-(U1-Pad74)"))
    (pad 75 connect circle (at 29.21 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 107 "Net-(U1-Pad75)"))
    (pad 76 connect circle (at 26.67 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 108 "Net-(U1-Pad76)"))
    (pad 77 connect circle (at 24.13 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 109 "Net-(U1-Pad77)"))
    (pad 78 connect circle (at 21.59 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 110 "Net-(U1-Pad78)"))
    (pad 79 connect circle (at 19.05 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 111 "Net-(U1-Pad79)"))
    (pad 80 connect circle (at 13.97 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 112 "Net-(U1-Pad80)"))
    (pad 81 connect circle (at 11.43 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 113 "Net-(U1-Pad81)"))
    (pad 82 connect circle (at 8.89 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 114 "Net-(U1-Pad82)"))
    (pad 83 connect circle (at -6.35 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 115 "Net-(U1-Pad83)"))
    (pad 84 connect circle (at -8.89 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 116 "Net-(U1-Pad84)"))
    (pad 85 connect circle (at -11.43 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 117 "Net-(U1-Pad85)"))
    (pad 86 connect circle (at -13.97 -2.54 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 118 "Net-(U1-Pad86)"))
    (pad 58 connect circle (at -22.86 4.62 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 119 "Net-(U1-Pad58)"))
    (pad 59 connect circle (at -20.32 4.62 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 120 "Net-(U1-Pad59)"))
    (pad 60 connect circle (at -17.78 4.62 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 121 "Net-(U1-Pad60)"))
    (pad 61 connect circle (at -15.24 4.62 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 122 "Net-(U1-Pad61)"))
    (pad 62 connect circle (at -12.7 4.62 270) (size 1.6 1.6) (layers Dwgs.User)
      (net 123 "Net-(U1-Pad62)"))
  )
  (module Custom:LP-51 locked (layer F.Cu) (tedit 5BCE991B)
    (at 72.39 55.245)
    (fp_text reference J14 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "Polycase 4.55\" x 3.29\" x 1.25\" " (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 42.8498 27.051) (size 3.175 3.175) (drill 3.175) (layers *.Cu))
    (pad "" np_thru_hole circle (at 42.8498 -27.051) (size 3.175 3.175) (drill 3.175) (layers *.Cu))
    (pad "" np_thru_hole circle (at -42.8498 27.051) (size 3.175 3.175) (drill 3.175) (layers *.Cu))
    (pad "" np_thru_hole circle (at -42.8498 -27.051) (size 3.175 3.175) (drill 3.175) (layers *.Cu))
  )
  (module Custom:Keystone_3001_1x12mm-CoinCell (layer F.Cu) (tedit 58972363)
    (at 26.162 42.16 270)
    (descr http://www.keyelco.com/product-pdf.cfm?p=778)
    (tags "Keystone type 3001 coin cell retainer")
    (fp_text reference BT1 (at -7.9081 4.8895) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 7.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0 0 270) (size 4 4) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.6 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (pad 1 thru_hole circle (at -6.6 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad1)"))
    (model Battery_Holders.3dshapes/Keystone_3001_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 69.85 69.4435 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -0.1015 1.27) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 69.85 75.311 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.254 1.524) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 56.896 53.086 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -0.635 1.651) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 I1))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 56.896 56.642 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.762 -1.524 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 I2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 56.896 60.198 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at -0.635 1.397) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 I3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 56.896 63.754 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.762 -1.397 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 I4))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 56.896 68.326 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0 1.397) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 I5))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 56.896 71.882 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.889 -1.524 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 I6))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 59.436 70.104 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 2.413 0 180) (layer F.SilkS))
    (fp_text value Diode_Dual_Shottkey_Sm_CA_bas40-06hmfh (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 I6))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 I5))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 62.992 70.104)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at 1.778 -1.143) (layer F.SilkS))
    (fp_text value Diode_Dual_Shottkey_Sm_CK_bas40-05hmfh (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 I6))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 I5))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:PG-TDSON-8-4-FP (layer F.Cu) (tedit 5BCC0A1D)
    (at 78.54696 50.7492)
    (descr "PG-TDSON-8 FL")
    (tags "PG-TDSON-8 FL")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference D3 (at -2.01676 4.2672) (layer F.SilkS))
    (fp_text value Dual_Diode_Lg_Schottky_V6KL45DU (at 0.5 -0.515) (layer F.Fab) hide)
    (fp_text user H=1mm (at 0.9 0.635) (layer F.Fab))
    (fp_text user %R (at 0.25 -0.265) (layer F.Fab))
    (pad "" smd rect (at -1.33096 -0.67564) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (pad 8 smd rect (at -2 -3.175) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 7 smd rect (at -0.67 -3.175) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 6 smd rect (at 0.67 -3.175) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 5 smd rect (at 2 -3.175) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 1 smd rect (at -1.905 2.825) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 OUT5))
    (pad 2 smd rect (at -0.635 2.825) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 OUT5))
    (pad 3 smd rect (at 0.635 2.825) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 OUT6))
    (pad 4 smd rect (at 1.905 2.825) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 OUT6))
    (pad "" smd rect (at 1.33858 -0.6731) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (model C:/Cad/Footprint/Infineon/3D/TDSON-8-1.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMC (layer F.Cu) (tedit 5864295D)
    (at 96.93 32.385 180)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (attr smd)
    (fp_text reference D5 (at -5.2415 3.81) (layer F.SilkS))
    (fp_text value SMCJ18A-E3/57T (at 0 4.2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -3.4 0 270) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 2 smd rect (at 3.4 0 270) (size 3.3 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 59.436 61.976 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D6 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value Diode_Dual_Shottkey_Sm_CA_bas40-06hmfh (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 I4))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 I3))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 62.992 61.976)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D7 (at 1.651 -1.143) (layer F.SilkS))
    (fp_text value Diode_Dual_Shottkey_Sm_CK_bas40-05hmfh (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 I4))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 I3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:PG-TDSON-8-4-FP (layer F.Cu) (tedit 5BCC0A1D)
    (at 87.03564 47.56404 90)
    (descr "PG-TDSON-8 FL")
    (tags "PG-TDSON-8 FL")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference D8 (at -1.94056 4.25196 180) (layer F.SilkS))
    (fp_text value Dual_Diode_Lg_Schottky_V6KL45DU (at 0.5 -0.515 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.25 -0.265 90) (layer F.Fab))
    (fp_text user H=1mm (at 0.9 0.635 90) (layer F.Fab))
    (pad "" smd rect (at 1.33858 -0.6731 90) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (pad 4 smd rect (at 1.905 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 OUT4))
    (pad 3 smd rect (at 0.635 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 OUT4))
    (pad 2 smd rect (at -0.635 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT3))
    (pad 1 smd rect (at -1.905 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT3))
    (pad 5 smd rect (at 2 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 6 smd rect (at 0.67 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 7 smd rect (at -0.67 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 8 smd rect (at -2 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad "" smd rect (at -1.33096 -0.67564 90) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (model C:/Cad/Footprint/Infineon/3D/TDSON-8-1.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 59.436 54.864 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D9 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value Diode_Dual_Shottkey_Sm_CA_bas40-06hmfh (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 I2))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 I1))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 62.976 54.864)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D10 (at 2.302 -1.016) (layer F.SilkS))
    (fp_text value Diode_Dual_Shottkey_Sm_CK_bas40-05hmfh (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 I2))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 I1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:PG-TDSON-8-4-FP (layer F.Cu) (tedit 5BCC0A1D)
    (at 86.9569 36.12642 90)
    (descr "PG-TDSON-8 FL")
    (tags "PG-TDSON-8 FL")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference D11 (at -2.92608 4.2926 180) (layer F.SilkS))
    (fp_text value Dual_Diode_Lg_Schottky_V6KL45DU (at 0.5 -0.515 90) (layer F.Fab) hide)
    (fp_text user H=1mm (at 0.9 0.635 90) (layer F.Fab))
    (fp_text user %R (at 0.25 -0.265 90) (layer F.Fab))
    (pad "" smd rect (at -1.33096 -0.67564 90) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (pad 8 smd rect (at -2 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 7 smd rect (at -0.67 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 6 smd rect (at 0.67 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 5 smd rect (at 2 -3.175 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (pad 1 smd rect (at -1.905 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 OUT1))
    (pad 2 smd rect (at -0.635 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 OUT1))
    (pad 3 smd rect (at 0.635 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT2))
    (pad 4 smd rect (at 1.905 2.825 90) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT2))
    (pad "" smd rect (at 1.33858 -0.6731 90) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (model C:/Cad/Footprint/Infineon/3D/TDSON-8-1.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 81.28 20.32)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 58.42 27.94 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0.0381 -2.7432 180) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5BCE9CA9)
    (at 58.42 33.02)
    (descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference J7 (at -3.4036 -0.9652) (layer F.SilkS))
    (fp_text value "Conn_01x04 displays_0.96inch_I2C_OLED" (at 0 10.42) (layer F.Fab))
    (fp_text user %R (at 1.1 3.75 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 "Net-(J7-Pad4)"))
    (pad "" np_thru_hole circle (at -1.34 3.75) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Non_Placed_Part (layer F.Cu) (tedit 5BA0871D)
    (at 21.84 90.52)
    (fp_text reference J13 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "PCB Screws, #4 x 1/4\" QTY 4" (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Custom:Non_Placed_Part (layer F.Cu) (tedit 5BA0871D)
    (at 23.34 90.52)
    (fp_text reference J15 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "Mating Connector 34 pin" (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Custom:Non_Placed_Part (layer F.Cu) (tedit 5BA0871D)
    (at 22.34 91.02)
    (fp_text reference J16 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "Mating Terminals sm QTY 30" (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Custom:Non_Placed_Part (layer F.Cu) (tedit 5BA0871D)
    (at 22.84 90.52)
    (fp_text reference J17 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "Mating Termianls LG QTY 4" (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Custom:Non_Placed_Part (layer F.Cu) (tedit 5BA0871D)
    (at 21.84 91.02)
    (fp_text reference J18 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "Coin Cell CR927 or CR1025" (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Custom:Non_Placed_Part (layer F.Cu) (tedit 5BA0871D)
    (at 22.34 90.52)
    (fp_text reference J19 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "0.1 headers for Teensy Mount" (at 0 -0.5) (layer F.Fab) hide)
  )
  (module Custom:349580340 (layer F.Cu) (tedit 5BCE8B3B)
    (at 100.33 55.88 270)
    (fp_text reference J20 (at -20.6375 -6.0325) (layer F.SilkS))
    (fp_text value MOLEX_34958_X34X (at -4.40642 -11.56462 270) (layer F.Fab))
    (pad 34 thru_hole circle (at 14 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 ISOSPIH))
    (pad 33 thru_hole circle (at 12 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 CAN2H))
    (pad 32 thru_hole circle (at 10 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 29 CAN1H))
    (pad 31 thru_hole circle (at 8 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 30 GAS_GAUGE))
    (pad 30 thru_hole circle (at 6 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 31 SPEED_OUT))
    (pad 29 thru_hole circle (at 4 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 39 IN5))
    (pad 28 thru_hole circle (at 2 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 40 IN3))
    (pad 27 thru_hole circle (at 0 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 41 IN1))
    (pad 26 thru_hole circle (at -2 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 OUT6))
    (pad 25 thru_hole circle (at -4 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 OUT5))
    (pad 24 thru_hole circle (at -6 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 15 OUT4))
    (pad 23 thru_hole circle (at -8 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 OUT3))
    (pad 22 thru_hole circle (at -10 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 16 OUT2))
    (pad 21 thru_hole circle (at -12 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 17 OUT1))
    (pad 20 thru_hole circle (at -14 2.2 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole circle (at 14 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 35 ISOSPIL))
    (pad 18 thru_hole circle (at 12 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 36 CAN2L))
    (pad 17 thru_hole circle (at 10 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 37 CAN1L))
    (pad 16 thru_hole circle (at 8 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 38 TACH_OUT))
    (pad 15 thru_hole circle (at 6 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 32 IN6))
    (pad 14 thru_hole circle (at 4 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 33 IN4))
    (pad 13 thru_hole circle (at 2 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 34 IN2))
    (pad 12 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 144 EXT5V))
    (pad 11 thru_hole circle (at -2 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at -4 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -6 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at -8 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -10 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 +12V))
    (pad 6 thru_hole circle (at -12 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 +12V))
    (pad 5 thru_hole circle (at -14 0 270) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 +12V))
    (pad 3 thru_hole circle (at 8.1 -4.06 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 42 "Net-(J20-Pad3)"))
    (pad 4 thru_hole circle (at 13.35 -4.06 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 "Net-(J20-Pad4)"))
    (pad 2 thru_hole circle (at -8.1 -4.06 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "Net-(J20-Pad2)"))
    (pad 1 thru_hole circle (at -13.35 -4.06 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 45 "Net-(J20-Pad1)"))
    (pad "" np_thru_hole circle (at 16.15 5.91 270) (size 2.15 2.15) (drill 2.15) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -16.15 5.91 270) (size 2.15 2.15) (drill 2.15) (layers *.Cu *.Mask))
  )
  (module Custom:SOT563 (layer F.Cu) (tedit 0)
    (at 60.198 49.022 90)
    (descr SOT563)
    (solder_mask_margin 0.0762)
    (solder_paste_margin -0.0254)
    (attr smd)
    (fp_text reference Q1 (at 1.651 -0.508 180) (layer F.SilkS))
    (fp_text value Dual_Fet_Sm_30V_400mA_NX3008NBKV (at 0 0 90) (layer F.SilkS) hide)
    (pad 6 smd rect (at 0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 SPEED_OUT))
    (pad 4 smd rect (at 0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(Q1-Pad2)"))
    (pad 5 smd rect (at 0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(Q1-Pad5)"))
    (pad 3 smd rect (at -0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 38 TACH_OUT))
    (pad 1 smd rect (at -0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Custom:SOT563 (layer F.Cu) (tedit 0)
    (at 28.575 62.865 90)
    (descr SOT563)
    (solder_mask_margin 0.0762)
    (solder_paste_margin -0.0254)
    (attr smd)
    (fp_text reference Q2 (at -1.905 -0.635 180) (layer F.SilkS))
    (fp_text value Dual_Fet_Sm_30V_400mA_NX3008NBKV (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(Q2-Pad3)"))
    (pad 5 smd rect (at 0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q2-Pad5)"))
    (pad 2 smd rect (at -0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Q2-Pad2)"))
    (pad 4 smd rect (at 0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(Q2-Pad6)"))
  )
  (module Custom:SOT563 (layer F.Cu) (tedit 0)
    (at 26.035 62.865 90)
    (descr SOT563)
    (solder_mask_margin 0.0762)
    (solder_paste_margin -0.0254)
    (attr smd)
    (fp_text reference Q3 (at -1.7399 -1.0541 180) (layer F.SilkS))
    (fp_text value Dual_Fet_Sm_30V_400mA_NX3008NBKV (at 0 0 90) (layer F.SilkS) hide)
    (pad 6 smd rect (at 0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(Q3-Pad6)"))
    (pad 4 smd rect (at 0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(Q3-Pad2)"))
    (pad 5 smd rect (at 0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(Q3-Pad5)"))
    (pad 3 smd rect (at -0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(Q3-Pad3)"))
    (pad 1 smd rect (at -0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Custom:SOT563 (layer F.Cu) (tedit 0)
    (at 23.495 62.865 90)
    (descr SOT563)
    (solder_mask_margin 0.0762)
    (solder_paste_margin -0.0254)
    (attr smd)
    (fp_text reference Q4 (at -1.3843 -1.9558 180) (layer F.SilkS))
    (fp_text value Dual_Fet_Sm_30V_400mA_NX3008NBKV (at 0 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(Q4-Pad3)"))
    (pad 5 smd rect (at 0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(Q4-Pad5)"))
    (pad 2 smd rect (at -0.675 0 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(Q4-Pad2)"))
    (pad 4 smd rect (at 0.675 0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.675 -0.5 90) (size 0.45 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(Q4-Pad6)"))
  )
  (module Custom:PG-TDSON-8-4-FP (layer F.Cu) (tedit 5BCC0A1D)
    (at 72.71004 50.7492 180)
    (descr "PG-TDSON-8 FL")
    (tags "PG-TDSON-8 FL")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference Q5 (at -2.14376 4.1021 180) (layer F.SilkS))
    (fp_text value DualFetLg_40V_20A_IPG20N04S4L11ATMA1 (at 0.5 -0.515 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.25 -0.265 180) (layer F.Fab))
    (fp_text user H=1mm (at 0.9 0.635 180) (layer F.Fab))
    (pad "" smd rect (at 1.33858 -0.6731 180) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (pad 4 smd rect (at 1.905 2.825 180) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(Q5-Pad4)"))
    (pad 3 smd rect (at 0.635 2.825 180) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 2.825 180) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(Q5-Pad2)"))
    (pad 1 smd rect (at -1.905 2.825 180) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2 -3.175 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 OUT6))
    (pad 6 smd rect (at 0.67 -3.175 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 OUT6))
    (pad 7 smd rect (at -0.67 -3.175 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 OUT5))
    (pad 8 smd rect (at -2 -3.175 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 OUT5))
    (pad "" smd rect (at -1.33096 -0.67564 180) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (model C:/Cad/Footprint/Infineon/3D/TDSON-8-1.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:PG-TDSON-8-4-FP (layer F.Cu) (tedit 5BCC0A1D)
    (at 86.9569 53.27142 270)
    (descr "PG-TDSON-8 FL")
    (tags "PG-TDSON-8 FL")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference Q6 (at -1.88722 4.5339) (layer F.SilkS))
    (fp_text value DualFetLg_40V_20A_IPG20N04S4L11ATMA1 (at 0.5 -0.515 270) (layer F.Fab) hide)
    (fp_text user H=1mm (at 0.9 0.635 270) (layer F.Fab))
    (fp_text user %R (at 0.25 -0.265 270) (layer F.Fab))
    (pad "" smd rect (at -1.33096 -0.67564 270) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (pad 8 smd rect (at -2 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT3))
    (pad 7 smd rect (at -0.67 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 OUT3))
    (pad 6 smd rect (at 0.67 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 OUT4))
    (pad 5 smd rect (at 2 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 OUT4))
    (pad 1 smd rect (at -1.905 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(Q6-Pad2)"))
    (pad 3 smd rect (at 0.635 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.905 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(Q6-Pad4)"))
    (pad "" smd rect (at 1.33858 -0.6731 270) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (model C:/Cad/Footprint/Infineon/3D/TDSON-8-1.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:PG-TDSON-8-4-FP (layer F.Cu) (tedit 5BCC0A1D)
    (at 86.95436 41.97096 270)
    (descr "PG-TDSON-8 FL")
    (tags "PG-TDSON-8 FL")
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference Q7 (at -2.67716 5.09016) (layer F.SilkS))
    (fp_text value DualFetLg_40V_20A_IPG20N04S4L11ATMA1 (at 0.5 -0.515 270) (layer F.Fab) hide)
    (fp_text user %R (at 0.25 -0.265 270) (layer F.Fab))
    (fp_text user H=1mm (at 0.9 0.635 270) (layer F.Fab))
    (pad "" smd rect (at 1.33858 -0.6731 270) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (pad 4 smd rect (at 1.905 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(Q7-Pad4)"))
    (pad 3 smd rect (at 0.635 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(Q7-Pad2)"))
    (pad 1 smd rect (at -1.905 2.825 270) (size 0.65 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT2))
    (pad 6 smd rect (at 0.67 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 OUT2))
    (pad 7 smd rect (at -0.67 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 OUT1))
    (pad 8 smd rect (at -2 -3.175 270) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 OUT1))
    (pad "" smd rect (at -1.33096 -0.67564 270) (size 2.035 4.5) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.11))
    (model C:/Cad/Footprint/Infineon/3D/TDSON-8-1.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 57.3785 50.038)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -2.2605 0) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(Q1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 Speed))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 48.006 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 SPEED_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 57.3785 48.006)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.2605 0) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 Tach))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(Q1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 63.0175 50.292 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.1335 0 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 +12V))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 TACH_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 82.042 70.993 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -0.1651 1.8288 180) (layer F.SilkS))
    (fp_text value "R1206 120 OHM" (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 145 "Net-(JP1-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 CAN1L))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 82.042 77.343 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -0.0254 1.8796 180) (layer F.SilkS))
    (fp_text value "R1206 120 OHM" (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 CAN2L))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 146 "Net-(JP2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.9025 66.04 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at -0.8635 -3.302 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(Q2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 G6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 29.845 55.75 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -2.664 0.0127) (layer F.SilkS))
    (fp_text value 20R0 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 GAS_GAUGE))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 51 "Net-(Q2-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.9025 64.77 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -0.6095 -3.556 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(Q2-Pad5)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 69 G5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 29.845 70.485 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 2.667 -0.254 180) (layer F.SilkS))
    (fp_text value 40R2 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 48 "Net-(Q2-Pad3)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 GAS_GAUGE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.9025 63.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at -0.4825 -3.81 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 70 G4))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 55.88 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -2.667 0) (layer F.SilkS))
    (fp_text value 80R6 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 GAS_GAUGE))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 52 "Net-(Q3-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.9025 62.23 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at -0.3555 3.683 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(Q3-Pad5)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 G3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 59.436 52.324 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -0.762 1.143 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 I1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 26.67 70.485 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value 158R0 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 55 "Net-(Q3-Pad3)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 GAS_GAUGE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 59.436 57.404 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -1.143 -1.016 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 I2))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 59.436 59.436 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 1.651 0.889 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 I3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 31.9025 60.96 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -0.4825 3.429 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 G2))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 23.495 55.75 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -2.664 0) (layer F.SilkS))
    (fp_text value 316R0 (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 GAS_GAUGE))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(Q4-Pad6)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 59.436 64.516 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -0.381 -1.143 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 I4))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5BD7C4F8)
    (at 31.9025 59.69 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at -0.4825 3.175 180) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(Q4-Pad5)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 G1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 59.436 67.564 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 1.016 1.016 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 I5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 23.495 70.485 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 2.667 0 180) (layer F.SilkS))
    (fp_text value "R1206 634R0" (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 56 "Net-(Q4-Pad3)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 30 GAS_GAUGE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 59.436 72.644 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 I6))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.0305 43.815)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 2.8449 0.1651) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 92 O6_Fuel_Lt))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(Q5-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.056 42.545)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 2.8194 0.0127) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(Q5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 O5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.056 41.275)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 2.8194 0) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 O4))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(Q6-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.0305 40.005)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R30 (at 2.8195 -0.0254) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(Q6-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 76 O3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 52.324 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R31 (at -2.413 0.508 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 I1))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 IN1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 57.404 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R32 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 IN2))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 I2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.0305 38.735)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R33 (at 2.7433 0.0635) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 O2))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(Q7-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 59.436 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R34 (at -2.54 -0.127 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 I3))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 IN3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 64.516 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R35 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 IN4))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 I4))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 67.564 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R36 (at -2.54 -0.254 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 I5))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 IN5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 62.992 72.644 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R37 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 IN6))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 I6))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 67.0305 37.465)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R38 (at 2.7179 0.0762) (layer F.SilkS))
    (fp_text value 2k2 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(Q7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 78 O1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 75.405 75.692)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -3.142 -3.175) (layer F.SilkS))
    (fp_text value CAN_SN65HVD23x (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U1-Pad32)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 CAN2H))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 CAN2L))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U1-Pad31)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U1-Pad30)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 75.405 69.342)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -2.888 -3.048) (layer F.SilkS))
    (fp_text value CAN_SN65HVD23x (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U1-Pad5)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 CAN1L))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 CAN1H))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U1-Pad8)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC:Converter_DCDC_TRACO_TSR-1_THT (layer F.Cu) (tedit 59FE1FB7)
    (at 96.52 20.955 180)
    (descr "DCDC-Converter, TRACO, TSR 1-xxxx")
    (tags "DCDC-Converter TRACO TSR-1")
    (fp_text reference U4 (at -4.9276 -2.3368 180) (layer F.SilkS))
    (fp_text value traco_TSR_0.5-2450 (at 2.5 3.25 180) (layer F.Fab))
    (fp_text user %R (at 3 -3 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Converter_DCDC.3dshapes/Converter_DCDC_TRACO_TSR-1_THT.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 58.42 83.82 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J21 (at 2.0955 0 180) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J21-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 139 "Net-(J21-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 140 "Net-(J21-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(J21-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(J21-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(J21-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 "Net-(J21-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(J21-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(J21-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(J21-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 58.42 25.4 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J22 (at 0.0635 -2.8448 180) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(J22-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 136 "Net-(J22-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 135 "Net-(J22-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 134 "Net-(J22-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 133 "Net-(J22-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 141 "Net-(J22-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 142 "Net-(J22-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 "Net-(J22-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA (layer F.Cu) (tedit 586432E5)
    (at 104.14 20.32)
    (descr "Diode SMA (DO-214AC)")
    (tags "Diode SMA (DO-214AC)")
    (attr smd)
    (fp_text reference D4 (at 4.6736 -0.1778) (layer F.SilkS))
    (fp_text value B140-E3/61T (at 0 2.6) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 10 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 88.9 29.21)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.159 0.1016) (layer F.SilkS))
    (fp_text value 10R0 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 +5V))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 EXT5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:Single_43_63_PTH (layer F.Cu) (tedit 5B9B2E79)
    (at 73.66 20.32)
    (fp_text reference J4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Single_Pin (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 86.36 76.2 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 2.286 -0.0254) (layer F.SilkS))
    (fp_text value CAN_2_Term_SolderJumper (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 146 "Net-(JP2-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 28 CAN2H) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 86.36 71.755 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -2.2225 0) (layer F.SilkS))
    (fp_text value CAN_1_Term_SolderJumper (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 29 CAN1H) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 145 "Net-(JP1-Pad2)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 36.433993 86.566977)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -0.111993 -1.159477) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 47.371 88.265)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 1.3335) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 95.25 85.09 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 1.905 -0.635 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 97.155 85.09 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at 1.905 -0.0635 180) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 148 "Net-(C12-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 36.433993 88.471977)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.015007 1.253523) (layer F.SilkS))
    (fp_text value 2K21 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 149 MISO))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 47.371 86.36)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R39 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 150 "Net-(R39-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 151 "Net-(R39-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 49.911 87.4775 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R40 (at 0.0255 -1.8415) (layer F.SilkS))
    (fp_text value 1K (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 151 "Net-(R39-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 97.155 88.265 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R41 (at -1.905 -0.0635 180) (layer F.SilkS))
    (fp_text value 49R9 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 152 "Net-(R41-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.25 88.265 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R42 (at -1.9685 -0.8255 180) (layer F.SilkS))
    (fp_text value 49R9 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 147 "Net-(C11-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 153 "Net-(R42-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:SignalCommunications-7490100111A (layer F.Cu) (tedit 5BD3DAD2)
    (at 104.775 84.50072 90)
    (attr smd)
    (fp_text reference T1 (at -5.60578 -5.715 180) (layer F.SilkS))
    (fp_text value WE-LAN_7490100111A (at 1.36906 7.6835 90) (layer F.SilkS) hide)
    (fp_text user 8 (at -2.39268 4.44246 90) (layer Dwgs.User))
    (fp_text user 9 (at 2.95402 4.4831 90) (layer Dwgs.User))
    (fp_text user 16 (at 2.71272 -4.69392 90) (layer Dwgs.User))
    (pad 1 smd rect (at -4.39928 -4.445 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R41-Pad1)"))
    (pad 2 smd rect (at -4.39928 -3.175 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(C12-Pad1)"))
    (pad 3 smd rect (at -4.39928 -1.905 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R42-Pad1)"))
    (pad 4 smd rect (at -4.39928 -0.635 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -4.39928 0.635 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -4.39928 1.905 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(T1-Pad6)"))
    (pad 7 smd rect (at -4.39928 3.175 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(T1-Pad7)"))
    (pad 8 smd rect (at -4.39928 4.445 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 156 "Net-(T1-Pad8)"))
    (pad 9 smd rect (at 4.39928 4.445 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 157 "Net-(T1-Pad9)"))
    (pad 10 smd rect (at 4.39928 3.175 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 158 "Net-(T1-Pad10)"))
    (pad 11 smd rect (at 4.39928 1.905 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(T1-Pad11)"))
    (pad 12 smd rect (at 4.39928 0.635 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 4.39928 -0.635 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 4.39928 -1.905 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 35 ISOSPIL))
    (pad 15 smd rect (at 4.39928 -3.175 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 160 "Net-(T1-Pad15)"))
    (pad 16 smd rect (at 4.39928 -4.445 90) (size 1.69926 0.75946) (layers F.Cu F.Paste F.Mask)
      (net 27 ISOSPIH))
  )
  (module Package_SO:MSOP-16_3x4mm_P0.5mm (layer F.Cu) (tedit 5A02F25C)
    (at 41.275493 87.689977)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference U5 (at -2.603993 -3.425477) (layer F.SilkS))
    (fp_text value LTC6820 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.2 -1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 161 MOSI))
    (pad 3 smd rect (at -2.2 -0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 149 MISO))
    (pad 4 smd rect (at -2.2 -0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 163 SCK))
    (pad 5 smd rect (at -2.2 0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 162 CS))
    (pad 12 smd rect (at 2.2 0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +5V))
    (pad 13 smd rect (at 2.2 -0.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at 2.2 -0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 2.2 -1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R39-Pad1)"))
    (pad 16 smd rect (at 2.2 -1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R39-Pad2)"))
    (pad 6 smd rect (at -2.2 0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at -2.2 1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +5V))
    (pad 8 smd rect (at -2.2 1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +5V))
    (pad 11 smd rect (at 2.2 0.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R41-Pad1)"))
    (pad 10 smd rect (at 2.2 1.25) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R42-Pad1)"))
    (pad 9 smd rect (at 2.2 1.75) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-16_3x4mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 88.9 31.242)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 1.7145 1.27) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 144 EXT5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Here Be Relays Someday" (at 118.11 53.594 90) (layer F.SilkS))
  (gr_text "PolyCase LP-51FMBR" (at 108.0135 22.225) (layer B.SilkS))
  (gr_text "4X #4 x 1/4” Screws" (at 109.982 24.257) (layer B.SilkS))
  (gr_text +12V (at 102.489 41.0845) (layer B.SilkS))
  (gr_text +12V (at 102.9335 44.1325) (layer B.SilkS))
  (gr_text +12V (at 102.87 45.9105) (layer B.SilkS))
  (gr_text "GND\n" (at 102.235 48.514) (layer B.SilkS))
  (gr_text GND (at 102.489 51.8795) (layer B.SilkS))
  (gr_text GND (at 102.5525 49.784) (layer B.SilkS))
  (gr_text "ISO SPI L" (at 103.505 71.1835) (layer B.SilkS))
  (gr_text C2L (at 102.362 67.818) (layer B.SilkS))
  (gr_text C1L (at 102.362 65.8495) (layer B.SilkS))
  (gr_text GND (at 102.6795 53.9115) (layer B.SilkS))
  (gr_text "EXT 5V" (at 103.251 55.88) (layer B.SilkS))
  (gr_text "In 2" (at 102.6795 57.912) (layer B.SilkS))
  (gr_text "In 4" (at 102.5525 59.8805) (layer B.SilkS))
  (gr_text "In 6\n" (at 102.489 61.849) (layer B.SilkS))
  (gr_text Tach (at 102.2985 62.9285) (layer B.SilkS))
  (gr_text "ISO SPI H" (at 94.0435 69.9135) (layer B.SilkS))
  (gr_text "CAN 2 H" (at 94.4245 67.8815) (layer B.SilkS))
  (gr_text "CAN 1 H" (at 94.361 65.8495) (layer B.SilkS))
  (gr_text "Fuel Gauge" (at 93.599 63.881) (layer B.SilkS))
  (gr_text Speed (at 95.123 61.9125) (layer B.SilkS))
  (gr_text "In 5" (at 95.5675 59.8805) (layer B.SilkS))
  (gr_text "In 3" (at 95.377 57.912) (layer B.SilkS))
  (gr_text "In 1" (at 95.3135 55.88) (layer B.SilkS))
  (gr_text "Out 6" (at 95.3135 53.9115) (layer B.SilkS))
  (gr_text "Out 5" (at 95.3135 51.943) (layer B.SilkS))
  (gr_text "Out 4" (at 95.25 49.911) (layer B.SilkS))
  (gr_text "Out 3" (at 95.1865 47.9425) (layer B.SilkS))
  (gr_text "Out 2" (at 95.1865 45.847) (layer B.SilkS))
  (gr_text "Out 1" (at 95.25 43.8785) (layer B.SilkS))
  (gr_text GND (at 95.9485 41.9735) (layer B.SilkS))
  (gr_text GND (at 45.974 55.626) (layer B.SilkS))
  (gr_text 5V (at 77.6605 22.6695) (layer B.SilkS))
  (gr_text GND (at 77.597 20.32) (layer B.SilkS))
  (gr_text "OEVCI v1.0 www.CafeElectric.com " (at 69.342 89.2175) (layer B.Cu))
  (gr_text "OEVCI V1.0 10/2018\nCafe Electric LLC\nwww.CafeElectric.com" (at 80.391 59.4995) (layer F.SilkS))
  (gr_text GND (at 58.42 30.099) (layer F.SilkS))
  (gr_text 23 (at 68.58 30.099) (layer F.SilkS))
  (gr_text 22 (at 71.1835 30.0355) (layer F.SilkS))
  (gr_text 21 (at 73.66 30.0355) (layer F.SilkS))
  (gr_text A10 (at 66.1035 30.099) (layer F.SilkS))
  (gr_text A11 (at 63.5635 30.1625) (layer F.SilkS))
  (gr_text Aref (at 60.96 30.099) (layer F.SilkS))
  (gr_text 32 (at 71.12 23.368) (layer F.SilkS))
  (gr_text 31 (at 68.453 23.4315) (layer F.SilkS))
  (gr_text 30 (at 65.8495 23.495) (layer F.SilkS))
  (gr_text 3.3V (at 76.454 30.1625) (layer F.SilkS))
  (gr_text 5V (at 78.74 30.099) (layer F.SilkS))
  (gr_text GND (at 81.3435 30.099) (layer F.SilkS))
  (gr_text GND (at 81.534 23.5585) (layer F.SilkS))
  (gr_text GND (at 58.293 23.8125) (layer F.SilkS))
  (gr_text SDA (at 61.595 40.513) (layer F.SilkS))
  (gr_text SCL (at 61.595 38.0365) (layer F.SilkS))
  (gr_text GND (at 61.722 35.687) (layer F.SilkS))
  (gr_text 3.3V (at 61.6585 32.9565) (layer F.SilkS))
  (gr_text "GND\n" (at 31.496 22.7965) (layer F.SilkS))
  (gr_text "5V Switcher\nVX7805-500" (at 93.98 24.384) (layer F.SilkS))
  (gr_text "Input Protection \nDiode 18V\nSMCJ18A-E3/57T" (at 107.061 31.5595) (layer F.SilkS))
  (gr_text "EXT 5V \nOption\nPin 12" (at 85.5345 30.9245) (layer F.SilkS))
  (gr_text GND (at 77.2795 20.3835) (layer F.SilkS))
  (gr_text b5 (at 29.845 58.6105) (layer F.SilkS))
  (gr_text b4 (at 29.718 73.3425) (layer F.SilkS))
  (gr_text b3 (at 26.6065 58.674) (layer F.SilkS))
  (gr_text b2 (at 26.797 73.2155) (layer F.SilkS))
  (gr_text b1 (at 23.495 58.6105) (layer F.SilkS))
  (gr_text bit0 (at 23.368 73.279) (layer F.SilkS))
  (gr_text "Daughter Board Support" (at 70.231 85.9155) (layer F.SilkS))
  (gr_text "Output\n5 & 6" (at 74.1045 44.0055) (layer F.SilkS))
  (gr_text "Output 3 & 4" (at 75.946 40.8305) (layer F.SilkS))
  (gr_text "Output 1 & 2" (at 75.3745 37.9095) (layer F.SilkS))
  (gr_text In6 (at 66.294 70.9295) (layer F.SilkS))
  (gr_text In5 (at 66.548 66.548) (layer F.SilkS))
  (gr_text In4 (at 67.818 64.77) (layer F.SilkS))
  (gr_text In3 (at 67.818 61.341) (layer F.SilkS))
  (gr_text In2 (at 67.945 57.785) (layer F.SilkS))
  (gr_text In1 (at 67.818 54.229) (layer F.SilkS))
  (gr_text "Tach Out\nSpeed Out" (at 57.658 45.72) (layer F.SilkS))
  (gr_text "I2C Header, NanoFit" (at 66.2305 31.877) (layer F.SilkS))
  (gr_text "30x70mm Daughter Board\nPack V Sense Option" (at 64.008 21.7805) (layer F.SilkS))
  (gr_text "Teensy 3.6" (at 42.926 18.415) (layer F.SilkS))
  (gr_text "RTC Battery\nCR927/CR1025" (at 27.94 32.639) (layer F.SilkS))
  (gr_text "Fuel Gauge Driver" (at 26.416 75.311) (layer F.SilkS))
  (gr_text "ISO SPI" (at 94.869 80.645) (layer F.SilkS))
  (gr_text "ISO SPI" (at 44.323 83.82) (layer F.SilkS))
  (gr_text "CAN 1 Termination" (at 85.471 67.691) (layer F.SilkS))
  (gr_text "CAN 2 Termination" (at 84.836 74.168) (layer F.SilkS))
  (gr_text "Reserved For future dual relays" (at 116.84 54.61 90) (layer Dwgs.User))
  (gr_line (start 111.76 17.78) (end 33.02 17.78) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 125.73 31.75) (end 111.76 17.78) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 125.73 78.74) (end 125.73 31.75) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 111.76 92.71) (end 125.73 78.74) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 33.274 92.964) (end 111.76 92.71) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 19.05 78.994) (end 33.274 92.964) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 19.05 31.75) (end 19.05 78.994) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 33.02 17.78) (end 19.05 31.75) (layer Edge.Cuts) (width 0.0254))
)
