(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 87)
    (zones 0)
    (modules 26)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D4-Pad1)")
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D8-Pad1)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J1-Pad3)")
  (net 11 "Net-(J4-Pad1)")
  (net 12 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(R2-Pad2)")
  )
  (module my_shit:USB_A_Female (layer F.Cu) (tedit 5C1D515C)
    (at 65.532 64.262 180)
    (descr http://cnctech.us/pdfs/1001-011-01101.pdf)
    (tags USB-A)
    (attr smd)
    (fp_text reference J1 (at -5.08 -0.254 180) (layer F.SilkS))
    (fp_text value USB_A (at 0 8) (layer F.Fab) hide)
    (fp_text user %R (at -6 0 270) (layer F.Fab) hide)
    (fp_text user "PCB Edge" (at -1.524 -0.05 270) (layer Dwgs.User))
    (pad 5 thru_hole circle (at -6.9 5.7 180) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 5 thru_hole circle (at -6.9 -5.7 180) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at -9.65 3.5 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole circle (at -9.65 -3.5 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at -9.65 1 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -9.65 -1 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5BFDADD7)
    (at 93.98 53.34)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U2 (at -3.81 -2.54) (layer F.SilkS))
    (fp_text value LM317_3PinPackage (at 2.54 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5BFDAE6D)
    (at 69.85 53.34)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5BFDAF34)
    (at 118.11 68.58 90)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8 90) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0 90) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BFB07AB)
    (at 82.55 61 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at -1.945 -1.27) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.05 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BFB0663)
    (at 94.615 60.325 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.05 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 2.704999 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D4.0mm (layer F.Cu) (tedit 5BFB068A)
    (at 74.93 53.34)
    (descr "LED, diameter 4.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-43GD(Ver.12B).pdf")
    (tags "LED diameter 4.0mm 2 pins")
    (fp_text reference D1 (at -1.27 2.54) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.46) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D4.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5BFB0797)
    (at 82.55 69.215 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J2 (at -1.27 -0.635) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 0 5.31 270) (layer F.Fab) hide)
    (fp_text user %R (at -1.27 1.27) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5BFB078E)
    (at 88.9 62.23 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J4 (at -2.54 2.54) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 0 5.31 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5BFB0619)
    (at 107.315 69.85 270)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0.635 10.16) (layer F.SilkS))
    (fp_text value Conn_01x04_Male (at 0 10.39 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BFB07A7)
    (at 80.645 57.785 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference R1 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value 1K (at 1.25 2.05 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BFB973D)
    (at 95.25 57.15 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference R2 (at 4.445 -1.27 180) (layer F.SilkS))
    (fp_text value 330R (at 1.25 2.05 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 1.905 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BFB079E)
    (at 89.535 53.34 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference R3 (at 2.54 1.905 180) (layer F.SilkS))
    (fp_text value 1K (at 1.25 2.05 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 180) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5BFB07A2)
    (at 89.535 56.515 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference R4 (at 1.27 -1.905 180) (layer F.SilkS))
    (fp_text value 1.2K (at 1.25 2.05 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R2-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5BFB0D96)
    (at 79.06 62.4 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at 2.71 -0.32 180) (layer F.SilkS))
    (fp_text value TPS2514 (at 0 2.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 5BFDAE72)
    (at 118.11 53.34)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965 (at 0 3.8) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5BFB9461)
    (at 82.55 54.61 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at -1.905 1.905 180) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 3.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 -2.54 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_AnodeUp (layer F.Cu) (tedit 5BFC6970)
    (at 113.03 56.515 90)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D2 (at -0.635 3.175 180) (layer F.SilkS))
    (fp_text value DIODE (at 1.905 4.2535 90) (layer F.Fab) hide)
    (fp_text user A (at 1.91 1.2 90) (layer F.SilkS) hide)
    (fp_text user A (at 1.91 1.2 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_KathodeUp (layer F.Cu) (tedit 5BFC696C)
    (at 117.475 60.96 180)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D3 (at 0 -2.92 180) (layer F.SilkS))
    (fp_text value DIODE (at 1.905 4.2535 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 180) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 180) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_AnodeUp (layer F.Cu) (tedit 5BFC6996)
    (at 108.585 60.96 90)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D4 (at 1.905 1.905 180) (layer F.SilkS))
    (fp_text value DIODE (at 7.62 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 90) (layer F.Fab) hide)
    (fp_text user A (at 1.91 1.2 90) (layer F.Fab) hide)
    (fp_text user A (at 1.91 1.2 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_KathodeUp (layer F.Cu) (tedit 5BFC691A)
    (at 112.395 65.405 180)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D5 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value DIODE (at 1.905 4.2535 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 180) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 180) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_AnodeUp (layer F.Cu) (tedit 5BFC697E)
    (at 104.775 53.34)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D6 (at 4.445 -2.54) (layer F.SilkS))
    (fp_text value DIODE (at 8.89 2.54) (layer F.Fab) hide)
    (fp_text user A (at 1.91 1.2) (layer F.SilkS) hide)
    (fp_text user A (at 1.91 1.2) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_KathodeUp (layer F.Cu) (tedit 5BFC69A4)
    (at 104.14 61.595 90)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D7 (at 1.905 1.27 180) (layer F.SilkS))
    (fp_text value DIODE (at 1.905 4.2535 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 90) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 90) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_AnodeUp (layer F.Cu) (tedit 5BFC6934)
    (at 99.695 60.96 90)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D8 (at 2.54 1.905 180) (layer F.SilkS))
    (fp_text value DIODE (at 6.35 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 90) (layer F.Fab) hide)
    (fp_text user A (at 1.91 1.2 90) (layer F.Fab) hide)
    (fp_text user A (at 1.91 1.2 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 3.81 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P3.81mm_Vertical_KathodeUp (layer F.Cu) (tedit 5BFC68F2)
    (at 104.14 65.405 180)
    (descr "Diode, DO-15 series, Axial, Vertical, pin pitch=3.81mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Vertical pin pitch 3.81mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D9 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value DIODE (at 1.905 4.2535 180) (layer F.Fab) hide)
    (fp_text user K (at 1.9 1.2 180) (layer F.SilkS) hide)
    (fp_text user K (at 1.9 1.2 180) (layer F.Fab) hide)
    (fp_text user %R (at 1.905 -2.92 180) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 3.81 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(D8-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P3.81mm_Vertical_KathodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5BFC65B3)
    (at 93.98 65.405 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C4 (at 5.08 2.54) (layer F.SilkS))
    (fp_text value 470uF (at 1.25 4.4 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "github:\njonronen" (at 87.63 66.04) (layer B.SilkS))
  (gr_text 0 (at 85.09 70.485) (layer F.SilkS))
  (gr_text + (at 77.47 70.485) (layer F.SilkS))
  (gr_text OUT (at 83.82 66.04) (layer F.SilkS))
  (gr_text MOT (at 112.395 70.485) (layer F.SilkS))
  (gr_text "0=5V\n1=3.3V" (at 88.265 64.135 270) (layer F.SilkS))
  (gr_line (start 66.675 50.165) (end 121.285 50.165) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.675 71.755) (end 66.675 50.165) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 71.755) (end 66.675 71.755) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.285 50.165) (end 121.285 71.755) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.015 50.8) (xy 120.015 71.12) (xy 69.85 71.12) (xy 69.85 50.8)
      )
    )
  )
)
