(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 67)
    (no_connects 0)
    (area 76.150001 54.55 209.630476 108.300001)
    (thickness 1.6)
    (drawings 38)
    (tracks 415)
    (zones 0)
    (modules 29)
    (nets 21)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(CN1-Pad2)")
  (net 3 "Net-(CN1-Pad3)")
  (net 4 "Net-(CN2-Pad2)")
  (net 5 "Net-(CN2-Pad3)")
  (net 6 "Net-(CN6-Pad2)")
  (net 7 "Net-(CN6-Pad3)")
  (net 8 "Net-(CN11-Pad2)")
  (net 9 "Net-(CN11-Pad3)")
  (net 10 "Net-(CN15-Pad2)")
  (net 11 "Net-(CN15-Pad3)")
  (net 12 GND)
  (net 13 "Net-(CN4-Pad2)")
  (net 14 "Net-(CN4-Pad3)")
  (net 15 "Net-(CN13-Pad2)")
  (net 16 "Net-(CN13-Pad3)")
  (net 17 "Net-(CN17-Pad2)")
  (net 18 "Net-(CN17-Pad3)")
  (net 19 "Net-(MH1-Pad1)")
  (net 20 "Net-(MH2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(CN1-Pad2)")
    (add_net "Net-(CN1-Pad3)")
    (add_net "Net-(CN11-Pad2)")
    (add_net "Net-(CN11-Pad3)")
    (add_net "Net-(CN13-Pad2)")
    (add_net "Net-(CN13-Pad3)")
    (add_net "Net-(CN15-Pad2)")
    (add_net "Net-(CN15-Pad3)")
    (add_net "Net-(CN17-Pad2)")
    (add_net "Net-(CN17-Pad3)")
    (add_net "Net-(CN2-Pad2)")
    (add_net "Net-(CN2-Pad3)")
    (add_net "Net-(CN4-Pad2)")
    (add_net "Net-(CN4-Pad3)")
    (add_net "Net-(CN6-Pad2)")
    (add_net "Net-(CN6-Pad3)")
    (add_net "Net-(MH1-Pad1)")
    (add_net "Net-(MH2-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 1.7)
    (via_drill 0.8)
    (uvia_dia 1.7)
    (uvia_drill 1)
    (add_net +5V)
    (add_net GND)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 99.06 91.0082 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 122.25 91 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 131.5 91 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 155.5 91.25 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 164.5 91.25 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 189 91.75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 197.9422 91.6686 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:LETH-PowerPad (layer B.Cu) (tedit 5B44CFC8)
    (at 148 79)
    (fp_text reference J3 (at 12.954 5.842) (layer B.SilkS))
    (fp_text value CONN_01X02 (at -1.524 6.096) (layer B.Fab))
    (pad 2 smd rect (at 10.16 -2.54) (size 10 15) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.54 -2.54) (size 10 15) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
  )
  (module plan44:LETH-PowerPad locked (layer F.Cu) (tedit 5B44CFC8)
    (at 148 74)
    (fp_text reference J4 (at 12.954 -5.842) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -1.524 -6.096) (layer F.Fab))
    (pad 2 smd rect (at 10.16 2.54) (size 10 15) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.54 2.54) (size 10 15) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 104.75 91 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(CN1-Pad3)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102 91 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(CN1-Pad3)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:WS2813-CONN locked (layer F.Cu) (tedit 5B607110)
    (at 98 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN1 (at 0 10 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(CN1-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(CN1-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN locked (layer F.Cu) (tedit 5B607126)
    (at 114.7 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN2 (at 0 10.3 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CN2-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CN2-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:WS2813-CONN (layer F.Cu) (tedit 5B60712F)
    (at 131.35 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN3 (at 0 10.15 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CN2-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CN2-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN locked (layer F.Cu) (tedit 5B60713B)
    (at 148 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN4 (at 0 10 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CN4-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CN4-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:WS2813-CONN locked (layer F.Cu) (tedit 5B607146)
    (at 164.65 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN5 (at 0 9.85 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CN4-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CN4-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN locked (layer F.Cu) (tedit 5B60714E)
    (at 181.3 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN6 (at 0 10.2 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN6-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CN6-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:WS2813-CONN locked (layer F.Cu) (tedit 5B607156)
    (at 197.95 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN7 (at 0 -2.45 270) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CN6-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN6-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 105.6 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN11 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(CN11-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(CN11-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 122.3 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN12 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(CN11-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(CN11-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 138.95 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN13 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(CN13-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(CN13-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 155.6 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN14 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(CN13-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(CN13-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 172.25 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN15 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(CN15-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(CN15-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 188.9 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN16 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(CN15-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(CN15-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
  )
  (module plan44:WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 205.55 99 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN17 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(CN17-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(CN17-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 193.5 80.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 19 "Net-(MH1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 110 80.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 20 "Net-(MH2-Pad1)"))
  )
  (module plan44:STELVIO-3P-508-S locked (layer F.Cu) (tedit 5B606936)
    (at 135.55 80.7)
    (attr virtual)
    (fp_text reference J2 (at 5.334 1.016 90) (layer F.SilkS))
    (fp_text value STELVIO-3P-508 (at -2.794 -4.826) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole circle (at -10.16 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 "Net-(CN1-Pad2)"))
  )
  (module plan44:STELVIO-4P-508-S locked (layer F.Cu) (tedit 5B60697E)
    (at 183.4134 80.6704)
    (attr virtual)
    (fp_text reference J1 (at 5.334 1.016 90) (layer F.SilkS))
    (fp_text value STELVIO-4P-508 (at -2.794 -4.826) (layer F.Fab))
    (pad 4 thru_hole circle (at -15.24 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 GND))
    (pad 2 thru_hole circle (at -5.08 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 GND))
    (pad 3 thru_hole circle (at -10.16 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +5V))
  )
  (gr_text +5V (at 158 86.5) (layer F.SilkS))
  (gr_text GND (at 145.5 86.5) (layer F.SilkS))
  (gr_text DI (at 125.4 73 90) (layer F.SilkS))
  (gr_text +5V (at 130.4 73 90) (layer F.SilkS))
  (gr_text +5V (at 168 73 90) (layer F.SilkS))
  (gr_text +5V (at 173.4 73 90) (layer F.SilkS))
  (gr_text GND (at 183.5 72.9 90) (layer F.SilkS))
  (gr_text GND (at 178.3 73 90) (layer F.SilkS))
  (gr_text GND (at 135.8 73 90) (layer F.SilkS))
  (dimension 10 (width 0.3) (layer Dwgs.User)
    (gr_text "10.000 mm" (at 135.1 106.95) (layer Dwgs.User))
    (feature1 (pts (xy 140.1 99.05) (xy 140.1 108.3)))
    (feature2 (pts (xy 130.1 99.05) (xy 130.1 108.3)))
    (crossbar (pts (xy 130.1 105.6) (xy 140.1 105.6)))
    (arrow1a (pts (xy 140.1 105.6) (xy 138.973496 106.186421)))
    (arrow1b (pts (xy 140.1 105.6) (xy 138.973496 105.013579)))
    (arrow2a (pts (xy 130.1 105.6) (xy 131.226504 106.186421)))
    (arrow2b (pts (xy 130.1 105.6) (xy 131.226504 105.013579)))
  )
  (dimension 16.65 (width 0.3) (layer Dwgs.User)
    (gr_text "16.650 mm" (at 110.125 106.8) (layer Dwgs.User))
    (feature1 (pts (xy 118.45 99) (xy 118.45 108.15)))
    (feature2 (pts (xy 101.8 99) (xy 101.8 108.15)))
    (crossbar (pts (xy 101.8 105.45) (xy 118.45 105.45)))
    (arrow1a (pts (xy 118.45 105.45) (xy 117.323496 106.036421)))
    (arrow1b (pts (xy 118.45 105.45) (xy 117.323496 104.863579)))
    (arrow2a (pts (xy 101.8 105.45) (xy 102.926504 106.036421)))
    (arrow2b (pts (xy 101.8 105.45) (xy 102.926504 104.863579)))
  )
  (dimension 34 (width 0.3) (layer Dwgs.User)
    (gr_text "34.000 mm" (at 82.65 85 270) (layer Dwgs.User))
    (feature1 (pts (xy 96.75 102) (xy 81.3 102)))
    (feature2 (pts (xy 96.75 68) (xy 81.3 68)))
    (crossbar (pts (xy 84 68) (xy 84 102)))
    (arrow1a (pts (xy 84 102) (xy 83.413579 100.873496)))
    (arrow1b (pts (xy 84 102) (xy 84.586421 100.873496)))
    (arrow2a (pts (xy 84 68) (xy 83.413579 69.126504)))
    (arrow2b (pts (xy 84 68) (xy 84.586421 69.126504)))
  )
  (dimension 110 (width 0.3) (layer Dwgs.User)
    (gr_text "110.000 mm" (at 151.75 55.9) (layer Dwgs.User))
    (feature1 (pts (xy 206.75 68) (xy 206.75 54.55)))
    (feature2 (pts (xy 96.75 68) (xy 96.75 54.55)))
    (crossbar (pts (xy 96.75 57.25) (xy 206.75 57.25)))
    (arrow1a (pts (xy 206.75 57.25) (xy 205.623496 57.836421)))
    (arrow1b (pts (xy 206.75 57.25) (xy 205.623496 56.663579)))
    (arrow2a (pts (xy 96.75 57.25) (xy 97.876504 57.836421)))
    (arrow2b (pts (xy 96.75 57.25) (xy 97.876504 56.663579)))
  )
  (gr_line (start 206.75 68) (end 96.75 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.75 102) (end 206.75 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 96.75 68) (end 96.75 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 206.75 68) (end 206.75 102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.5 101) (xy 171 101) (xy 171 92) (xy 182.5 92)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149 101) (xy 137.75 101) (xy 137.75 92) (xy 149 92)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116 101) (xy 104.5 101) (xy 104.5 95.75) (xy 103 95.75) (xy 103 91.75)
        (xy 116 91.75)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 206.5 101) (xy 183.5 101) (xy 183.5 91) (xy 170 91) (xy 170 101)
        (xy 150 101) (xy 150 91) (xy 137 91) (xy 137 101) (xy 117 101)
        (xy 117 91) (xy 102 91) (xy 102 96.5) (xy 103.75 96.5) (xy 103.75 101)
        (xy 97 101) (xy 97 68.5) (xy 206.5 68.5)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.5 101) (xy 121 101) (xy 121 92.25) (xy 132.5 92)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166 101) (xy 154.5 101) (xy 154.5 92) (xy 166 92)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 199 101) (xy 188 101) (xy 188 96.5) (xy 186.75 96.5) (xy 186.75 92.75)
        (xy 199 92.75)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 206.5 101) (xy 200 101) (xy 200 91) (xy 185.5 91) (xy 185.25 101)
        (xy 167 101) (xy 167 90.5) (xy 153.25 90.5) (xy 153.25 101) (xy 133.5 101)
        (xy 133.5 90) (xy 119.75 90) (xy 119.75 101) (xy 97 101) (xy 97 68.5)
        (xy 206.5 68.5)
      )
    )
  )
)
