<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="-0.127" y1="-0.381" x2="20.244" y2="-0.381" width="0" layer="20"/>
<wire x1="20.244" y1="-0.381" x2="20.244" y2="46.853" width="0" layer="20"/>
<wire x1="20.244" y1="46.853" x2="-0.127" y2="46.853" width="0" layer="20"/>
<wire x1="-0.127" y1="46.853" x2="-0.127" y2="-0.381" width="0" layer="20"/>
<text>CANH</text>
<text>CANL</text>
<text>GND</text>
<text>ENABLE_TERM</text>
</plain>
<libraries>
<library name="Teensy_3_and_LC_Series_Boards_v1.1">
<packages>
<package name="TEENSY3-DIL">
</package>
</packages>
</library>
<library name="jpiat">
<packages>
<package name="SO08-SKINNYPADS">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 Reflow solder&lt;/b&gt;&lt;p&gt;
KEMET S / EIA 3216-12</description>
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-4">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Teensy_3_and_LC_Series_Boards_v1.1" package="TEENSY3-DIL" value="TEENSY_3.1_DIL"/>
<element name="U$2" library="jpiat" package="SO08-SKINNYPADS" value="SN65HVD232"/>
<element name="SJ1" library="jumper" package="SJ" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-wago-500" package="W237-4" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0805K" value=""/>
<element name="C4" library="adafruit" package="A/3216-18R" value=""/>
<element name="C5" library="adafruit" package="C0805K" value=""/>
<element name="C6" library="adafruit" package="A/3216-18R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT223" value="">
<attribute name="PROD_ID" value="VREG-08170"/>
</element>
</elements>
<signals>
<signal name="VIN">
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="CAN_TX">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="CAN_RX">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="C3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="+"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="-"/>
<contactref element="X2" pad="3"/>
<contactref element="C6" pad="-"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="U$1" pad="AGND"/>
</signal>
<signal name="CANH">
<contactref element="U$2" pad="7"/>
<contactref element="SJ1" pad="2"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="CANL">
<contactref element="X2" pad="1"/>
<contactref element="U$2" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="8"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="VCAN">
<contactref element="X2" pad="4"/>
<contactref element="C6" pad="+"/>
<contactref element="U1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
