(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 62)
    (no_connects 0)
    (area 144.095714 111.576666 178.404287 138.665)
    (thickness 1.6)
    (drawings 54)
    (tracks 282)
    (zones 0)
    (modules 43)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.19)
    (zone_clearance 0.19)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.3 2.3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD)
  (net 3 /A)
  (net 4 /L)
  (net 5 /LX)
  (net 6 /B)
  (net 7 /ZL)
  (net 8 /LY)
  (net 9 /MCLR)
  (net 10 /ICSPDAT)
  (net 11 /ICSPCLK)
  (net 12 "Net-(J7-Pad6)")
  (net 13 /X)
  (net 14 /R)
  (net 15 /RX)
  (net 16 /Y)
  (net 17 /ZR)
  (net 18 /RY)
  (net 19 /DU)
  (net 20 /+)
  (net 21 /LT)
  (net 22 /DD)
  (net 23 /-)
  (net 24 /RT)
  (net 25 /DR)
  (net 26 /H)
  (net 27 /DL)
  (net 28 /SDA)
  (net 29 /SCL)
  (net 30 /CS)
  (net 31 /MOSI)
  (net 32 /MISO)
  (net 33 /SCK)
  (net 34 /DET)
  (net 35 /MODE)
  (net 36 "Net-(U2-Pad4)")
  (net 37 "Net-(U2-Pad9)")
  (net 38 "Net-(U2-Pad10)")
  (net 39 "Net-(U2-Pad11)")
  (net 40 /EN)
  (net 41 "Net-(U1-Pad18)")
  (net 42 "Net-(U1-Pad19)")
  (net 43 "Net-(U1-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.19)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+)
    (add_net /-)
    (add_net /A)
    (add_net /B)
    (add_net /CS)
    (add_net /DD)
    (add_net /DET)
    (add_net /DL)
    (add_net /DR)
    (add_net /DU)
    (add_net /EN)
    (add_net /H)
    (add_net /ICSPCLK)
    (add_net /ICSPDAT)
    (add_net /L)
    (add_net /LT)
    (add_net /LX)
    (add_net /LY)
    (add_net /MCLR)
    (add_net /MISO)
    (add_net /MODE)
    (add_net /MOSI)
    (add_net /R)
    (add_net /RT)
    (add_net /RX)
    (add_net /RY)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /X)
    (add_net /Y)
    (add_net /ZL)
    (add_net /ZR)
    (add_net GND)
    (add_net "Net-(J7-Pad6)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad9)")
    (add_net VDD)
  )
  (module Classic:Screw_Hole (layer F.Cu) (tedit 5A4EC32D)
    (at 148.5 116.5)
    (fp_text reference REF** (at 0 2.6) (layer F.SilkS) hide)
    (fp_text value Screw_Hole (at 0 -2.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Classic:Screw_Hole (layer F.Cu) (tedit 5A4EC330)
    (at 148.5 135)
    (fp_text reference REF** (at 0 2.6) (layer F.SilkS) hide)
    (fp_text value Screw_Hole (at 0 -2.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Classic:Screw_Hole (layer F.Cu) (tedit 5A4EC334)
    (at 174 135)
    (fp_text reference REF** (at 0 2.6) (layer F.SilkS) hide)
    (fp_text value Screw_Hole (at 0 -2.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Classic:C_0603 (layer F.Cu) (tedit 5A4DA8EC)
    (at 165.75 119.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd oval (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd oval (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:C_0603 (layer F.Cu) (tedit 5A4DA8F1)
    (at 162.5 119.75 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd oval (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 1 smd oval (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:C_0603 (layer F.Cu) (tedit 5A4DA8F4)
    (at 165.05 125.4 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 180) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (pad 2 smd oval (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 1 smd oval (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:C_0603 (layer F.Cu) (tedit 5A4DA8F7)
    (at 154.95 126.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value C (at 0 1.5) (layer F.Fab))
    (pad 2 smd oval (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 1 smd oval (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA983)
    (at 150.25 118.75)
    (fp_text reference J1 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /A))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA986)
    (at 164.25 132.75)
    (fp_text reference J2 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /L))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA988)
    (at 170.25 132.75)
    (fp_text reference J3 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /LX))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA98A)
    (at 150.25 120.75)
    (fp_text reference J4 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /B))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA990)
    (at 162.25 132.75)
    (fp_text reference J5 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /ZL))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA992)
    (at 168.25 132.75)
    (fp_text reference J6 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /LY))
  )
  (module Classic:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A4DA8E4)
    (at 152.55 116.6 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /MCLR))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VDD))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ICSPDAT))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ICSPCLK))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J7-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA995)
    (at 150.25 122.75)
    (fp_text reference J8 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /X))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA998)
    (at 158.25 132.75)
    (fp_text reference J9 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /R))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA99E)
    (at 152.25 132.75)
    (fp_text reference J10 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /RX))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA9A0)
    (at 150.25 124.75)
    (fp_text reference J11 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /Y))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA9A2)
    (at 160.25 132.75)
    (fp_text reference J12 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /ZR))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA9A5)
    (at 154.25 132.75)
    (fp_text reference J13 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /RY))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA978)
    (at 172.25 126.75)
    (fp_text reference J14 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /DU))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA97B)
    (at 150.25 126.75)
    (fp_text reference J15 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /+))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA97D)
    (at 166.25 132.75)
    (fp_text reference J16 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /LT))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA97F)
    (at 172.25 120.75)
    (fp_text reference J17 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA96E)
    (at 172.25 128.75)
    (fp_text reference J18 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /DD))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA96F)
    (at 150.25 130.75)
    (fp_text reference J19 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /-))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA971)
    (at 156.25 132.75)
    (fp_text reference J20 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 24 /RT))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA974)
    (at 172.25 130.75)
    (fp_text reference J21 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /DR))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA976)
    (at 150.25 128.75)
    (fp_text reference J22 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /H))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA981)
    (at 172.25 118.75)
    (fp_text reference J23 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4E6884)
    (at 172.25 132.75)
    (fp_text reference J24 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /DL))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA99B)
    (at 172.25 124.75)
    (fp_text reference J25 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /SDA))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4DA9A7)
    (at 172.25 122.75)
    (fp_text reference J26 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /SCL))
  )
  (module Classic:R_0603 (layer F.Cu) (tedit 5A4DA8E9)
    (at 154 120.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /SDA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:R_0603 (layer F.Cu) (tedit 5A4DA8EF)
    (at 156 120.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 /SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A4EBE08)
    (at 170.25 118.75)
    (fp_text reference J29 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 34 /DET))
  )
  (module Classic:Screw_Hole (layer F.Cu) (tedit 5A4EC337)
    (at 174 116.5)
    (fp_text reference REF** (at 0 2.6) (layer F.SilkS) hide)
    (fp_text value Screw_Hole (at 0 -2.75) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A60B971)
    (at 150.25 132.75)
    (fp_text reference J27 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /MODE))
  )
  (module Classic:R_0603 (layer F.Cu) (tedit 5A60B97E)
    (at 155 129.25 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 /MODE))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:LGA-14_3x2.5mm_Pitch0.5mm (layer F.Cu) (tedit 5A60B981)
    (at 165.25 122.25 180)
    (descr "LGA-14 Bosch https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BMI160-DS000-07.pdf")
    (tags "lga land grid array")
    (attr smd)
    (fp_text reference U2 (at 0 -2.5 180) (layer F.SilkS) hide)
    (fp_text value LSM6DS (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 13 smd oval (at 0 -1.1 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask)
      (net 33 /SCK))
    (pad 14 smd oval (at -0.5 -1.1 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask)
      (net 31 /MOSI))
    (pad 12 smd oval (at 0.5 -1.1 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask)
      (net 30 /CS))
    (pad 5 smd oval (at -0.5 1.1 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 6 smd oval (at 0 1.1 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd oval (at 0.5 1.1 180) (size 0.25 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd oval (at -1.35 -0.75 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /MISO))
    (pad 2 smd oval (at -1.35 -0.25 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd oval (at -1.35 0.25 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd oval (at -1.35 0.75 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad4)"))
    (pad 8 smd oval (at 1.35 0.75 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 9 smd oval (at 1.35 0.25 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad9)"))
    (pad 10 smd oval (at 1.35 -0.25 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad10)"))
    (pad 11 smd oval (at 1.35 -0.75 180) (size 0.85 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad11)"))
    (model ${KISYS3DMOD}/Housings_LGA.3dshapes/Bosch_LGA-14_3x2.5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:Test_Pad (layer F.Cu) (tedit 5A60BAC7)
    (at 168.25 118.75)
    (fp_text reference J32 (at 0 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 -1.7) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /EN))
  )
  (module Classic:R_0603 (layer F.Cu) (tedit 5A60C435)
    (at 158 120.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 /EN))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Classic:QFN-40-1EP_5x5mm_Pitch0.4mm (layer F.Cu) (tedit 5A806F94)
    (at 160 126 180)
    (descr "40-Lead Plastic Quad Flat, No Lead Package (MP) - 5x5 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.4")
    (attr smd)
    (fp_text reference U1 (at 0 -3.875 180) (layer F.SilkS) hide)
    (fp_text value PIC16F18875 (at 0 3.875 180) (layer F.Fab))
    (pad 1 smd oval (at -2.45 -1.8 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /DL))
    (pad 2 smd oval (at -2.45 -1.4 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /DR))
    (pad 3 smd oval (at -2.45 -1 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /DD))
    (pad 4 smd oval (at -2.45 -0.6 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 19 /DU))
    (pad 5 smd oval (at -2.45 -0.2 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 32 /MISO))
    (pad 6 smd oval (at -2.45 0.2 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd oval (at -2.45 0.6 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 8 smd oval (at -2.45 1 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /MOSI))
    (pad 9 smd oval (at -2.45 1.4 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 33 /SCK))
    (pad 10 smd oval (at -2.45 1.8 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /CS))
    (pad 11 smd oval (at -1.8 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /SDA))
    (pad 12 smd oval (at -1.4 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /SCL))
    (pad 13 smd oval (at -1 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /DET))
    (pad 14 smd oval (at -0.6 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /ICSPCLK))
    (pad 15 smd oval (at -0.2 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /ICSPDAT))
    (pad 16 smd oval (at 0.2 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /MCLR))
    (pad 17 smd oval (at 0.6 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 40 /EN))
    (pad 18 smd oval (at 1 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U1-Pad18)"))
    (pad 19 smd oval (at 1.4 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U1-Pad19)"))
    (pad 20 smd oval (at 1.8 2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad20)"))
    (pad 21 smd oval (at 2.45 1.8 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /A))
    (pad 22 smd oval (at 2.45 1.4 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /B))
    (pad 23 smd oval (at 2.45 1 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 13 /X))
    (pad 24 smd oval (at 2.45 0.6 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 16 /Y))
    (pad 25 smd oval (at 2.45 0.2 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /+))
    (pad 26 smd oval (at 2.45 -0.2 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VDD))
    (pad 27 smd oval (at 2.45 -0.6 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd oval (at 2.45 -1 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /H))
    (pad 29 smd oval (at 2.45 -1.4 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /-))
    (pad 30 smd oval (at 2.45 -1.8 180) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 35 /MODE))
    (pad 31 smd oval (at 1.8 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 15 /RX))
    (pad 32 smd oval (at 1.4 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 18 /RY))
    (pad 33 smd oval (at 1 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 24 /RT))
    (pad 34 smd oval (at 0.6 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /R))
    (pad 35 smd oval (at 0.2 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 17 /ZR))
    (pad 36 smd oval (at -0.2 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /ZL))
    (pad 37 smd oval (at -0.6 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /L))
    (pad 38 smd oval (at -1 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /LT))
    (pad 39 smd oval (at -1.4 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /LY))
    (pad 40 smd oval (at -1.8 -2.45 270) (size 0.85 0.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /LX))
    (pad 41 smd rect (at 0 0 180) (size 2.3 2.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-40-1EP_5x5mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 148.5 114.8) (end 174 114.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.5 136.7) (end 174 136.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.8 116.5) (end 146.8 135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text MD (at 148.25 132.75) (layer F.SilkS))
  (gr_line (start 175.7 135) (end 175.7 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text R4 (at 154.3 127.95) (layer F.SilkS))
  (gr_text R3 (at 158 118.7) (layer F.SilkS))
  (gr_text C1 (at 165.85 126.55) (layer F.SilkS))
  (gr_text C2 (at 154.1 125.05) (layer F.SilkS))
  (gr_text U2 (at 167.75 121.35 270) (layer F.SilkS))
  (gr_text C3 (at 164.95 118.6) (layer F.SilkS))
  (gr_text C4 (at 160.4 119.75) (layer F.SilkS))
  (gr_text R2 (at 156 118.7) (layer F.SilkS))
  (gr_text R1 (at 154 118.7) (layer F.SilkS))
  (gr_text U1 (at 157.7 122.35) (layer F.SilkS))
  (gr_arc (start 148.5 116.5) (end 146.8 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 148.5 135) (end 148.5 136.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 135) (end 175.7 135) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 116.5) (end 174 114.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text EN (at 168.25 116.75 90) (layer F.SilkS))
  (gr_text DAT (at 160.25 119.25 90) (layer B.SilkS))
  (gr_text Classic+ (at 161.25 135.25) (layer B.SilkS))
  (gr_text DT (at 170.25 116.75 90) (layer F.SilkS))
  (gr_text VDD (at 155.25 119.5 90) (layer B.SilkS))
  (gr_text GND (at 157.75 119.25 90) (layer B.SilkS))
  (gr_text CLK (at 162.75 119.25 90) (layer B.SilkS))
  (gr_text MCLR (at 152.5 120 90) (layer B.SilkS))
  (gr_text GND (at 174.25 118.75) (layer F.SilkS))
  (gr_text 3.3V (at 174.25 120.75) (layer F.SilkS))
  (gr_text SCL (at 174.25 122.75) (layer F.SilkS))
  (gr_text SDA (at 174.25 124.75) (layer F.SilkS))
  (gr_text LX (at 170.25 134.75 270) (layer F.SilkS))
  (gr_text LY (at 168.25 134.75 270) (layer F.SilkS))
  (gr_text RX (at 152.25 134.75 270) (layer F.SilkS))
  (gr_text RY (at 154.25 134.75 270) (layer F.SilkS))
  (gr_text A (at 148.5 118.75) (layer F.SilkS))
  (gr_text B (at 148.5 120.75) (layer F.SilkS))
  (gr_text X (at 148.5 122.75) (layer F.SilkS))
  (gr_text Y (at 148.5 124.75) (layer F.SilkS))
  (gr_text DU (at 174.25 126.75) (layer F.SilkS))
  (gr_text DD (at 174.25 128.75) (layer F.SilkS))
  (gr_text DR (at 174.25 130.75) (layer F.SilkS))
  (gr_text DL (at 174.25 132.75) (layer F.SilkS))
  (gr_text H (at 148.5 128.75) (layer F.SilkS))
  (gr_text - (at 148.5 130.75) (layer F.SilkS))
  (gr_text + (at 148.5 126.75) (layer F.SilkS))
  (gr_text RT (at 156.25 134.75 270) (layer F.SilkS))
  (gr_text ZR (at 160.25 134.75 270) (layer F.SilkS))
  (gr_text R (at 158.25 134.5 270) (layer F.SilkS))
  (gr_text LT (at 166.25 134.75 270) (layer F.SilkS))
  (gr_text ZL/Z (at 162.25 135 270) (layer F.SilkS))
  (gr_text L/C (at 164.25 135 270) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.19))
    (min_thickness 0.12)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.22))
    (polygon
      (pts
        (xy 175.7 136.7) (xy 146.8 136.7) (xy 146.8 114.8) (xy 175.7 114.8)
      )
    )
  )
)
