(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 97)
    (zones 0)
    (modules 17)
    (nets 16)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 RX)
  (net 4 TX)
  (net 5 +3V3)
  (net 6 /VCAP)
  (net 7 /D+)
  (net 8 /D-)
  (net 9 /PG)
  (net 10 /EN)
  (net 11 /ID)
  (net 12 /NC)
  (net 13 /Pwr)
  (net 14 /Green)
  (net 15 /Red)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /EN)
    (add_net /Green)
    (add_net /ID)
    (add_net /NC)
    (add_net /PG)
    (add_net /Pwr)
    (add_net /Red)
    (add_net /VCAP)
    (add_net GND)
    (add_net RX)
    (add_net TX)
  )
  (module Connector_PinHeader_1.27mm:PinHeader_1x05_P1.27mm_Vertical (layer F.Cu) (tedit 5F4CCC47)
    (at 123.25 111.25 270)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x05 (at -2.25 3.25 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /Pwr))
    (pad 2 thru_hole oval (at 0 1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:Mandel_medium (layer B.Cu) (tedit 0)
    (at 113.5 116 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile (layer F.Cu) (tedit 5A0F774F)
    (at 108.1 109)
    (descr "low profile wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference Gnd (at 4.9 2) (layer F.SilkS) hide)
    (fp_text value TestPoint_Small (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile (layer F.Cu) (tedit 5A0F774F)
    (at 108.1 122.55)
    (descr "low profile wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference Gnd (at 4.9 -1.95) (layer F.SilkS) hide)
    (fp_text value TestPoint_Small (at 0 2.65) (layer F.Fab))
    (fp_text user %R (at 0 2.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile (layer F.Cu) (tedit 5A0F774F)
    (at 104.5 109)
    (descr "low profile wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference D- (at 5.5 2 unlocked) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D-))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile (layer F.Cu) (tedit 5A0F774F)
    (at 104.5 122.5)
    (descr "low profile wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference D+ (at 5.5 -1.9 unlocked) (layer F.SilkS))
    (fp_text value TestPoint_Small (at 0 2.7 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D+))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm_LowProfile.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 116.75 113 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference G-5-P (at 2.4 0.65 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0306 (layer F.Cu) (tedit 5F3D4236)
    (at 115 112.75 90)
    (fp_text reference C1 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0.03 2 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5715 0 90) (size 0.4572 1.7018) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.5715 0 90) (size 0.4572 1.7018) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Connector_USB:USB_Micro-B_Wuerth_629105150521 (layer F.Cu) (tedit 5A142044)
    (at 106.25 115.75 270)
    (descr "USB Micro-B receptacle, http://www.mouser.com/ds/2/445/629105150521-469306.pdf")
    (tags "usb micro receptacle")
    (attr smd)
    (fp_text reference J1 (at 4.75 -4.25 180) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at 0 5.6 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 3.75 90) (layer Dwgs.User))
    (fp_text user %R (at 0 1.05 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at 2.5 -0.8 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at -2.5 -0.8 270) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 3.875 1.95 270) (size 1.15 1.8) (drill oval 0.55 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -3.875 1.95 270) (size 1.15 1.8) (drill oval 0.55 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 3.725 -1.85 270) (size 1.45 2) (drill oval 0.85 1.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -3.725 -1.85 270) (size 1.45 2) (drill oval 0.85 1.4) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /ID))
    (pad 3 smd rect (at 0 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /D+))
    (pad 2 smd rect (at -0.65 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /D-))
    (pad 1 smd rect (at -1.3 -1.9 270) (size 0.45 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Wuerth_629105150521.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module JohnAdriaan:DFN-6_3x3_0.95 (layer F.Cu) (tedit 5F4C7934)
    (at 119.25 114.425 90)
    (descr "DFN6 3x3mm 0.95 Pitch")
    (tags "DFN 0.95")
    (attr smd)
    (fp_text reference U2 (at 2.675 -0.5 180) (layer F.SilkS) hide)
    (fp_text value LD39050PU33R (at -1.325 2.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 6 smd custom (at 1.275 -0.95 270) (size 0.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 -0.225) (xy -0.55 -0.225) (xy -0.55 0.225) (xy 0 0.225)) (width 0))
      ))
    (pad 5 smd custom (at 1.275 0 270) (size 0.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /NC) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 -0.225) (xy -0.55 -0.225) (xy -0.55 0.225) (xy 0 0.225)) (width 0))
      ))
    (pad 4 smd custom (at 1.275 0.95 270) (size 0.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 -0.225) (xy -0.55 -0.225) (xy -0.55 0.225) (xy 0 0.225)) (width 0))
      ))
    (pad 3 smd custom (at -1.275 0.95 90) (size 0.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /PG) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 -0.225) (xy -0.55 -0.225) (xy -0.55 0.225) (xy 0 0.225)) (width 0))
      ))
    (pad 2 smd custom (at -1.275 0 90) (size 0.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 -0.225) (xy -0.55 -0.225) (xy -0.55 0.225) (xy 0 0.225)) (width 0))
      ))
    (pad "" smd rect (at -0.425 -0.866 90) (size 0.66 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.425 -0.866 90) (size 0.66 0.73) (layers F.Paste))
    (pad "" smd rect (at -0.425 0 90) (size 0.66 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.425 0 90) (size 0.66 0.73) (layers F.Paste))
    (pad "" smd rect (at 0.425 0.866 90) (size 0.66 0.73) (layers F.Paste))
    (pad 7 thru_hole roundrect (at 0 0 90) (size 1.7 2.5) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.05)
      (net 2 GND))
    (pad "" smd rect (at -0.425 0.866 90) (size 0.66 0.73) (layers F.Paste))
    (pad 1 smd custom (at -1.275 -0.95 90) (size 0.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 /EN) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 0 -0.225) (xy -0.55 -0.225) (xy -0.55 0.225) (xy 0 0.225)) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_P0.95mm_EP1.7x2.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SO-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 113.5 116.75 180)
    (descr "SO, 8 Pin (https://www.nxp.com/docs/en/data-sheet/PCF8523.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (attr smd)
    (fp_text reference U1 (at 0 0.05) (layer F.SilkS) hide)
    (fp_text value STM8S001J3M (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.575 -1.905 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 TX))
    (pad 7 smd roundrect (at 2.575 -0.635 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /EN))
    (pad 6 smd roundrect (at 2.575 0.635 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /D-))
    (pad 5 smd roundrect (at 2.575 1.905 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /D+))
    (pad 4 smd roundrect (at -2.575 1.905 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 3 smd roundrect (at -2.575 0.635 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /VCAP))
    (pad 2 smd roundrect (at -2.575 -0.635 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -2.575 -1.905 180) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 RX))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 120.5 118 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 2.5 0.25 180) (layer F.SilkS) hide)
    (fp_text value 310 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /Red))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /PG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 126.25 111.75)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference P-3-G (at -2.15 -1.15) (layer F.SilkS))
    (fp_text value 280 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /Green))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 111.5 113)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 1K5 (at 0 -1.75) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /D-))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5F4C792B)
    (at 129.75 112)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at -2.75 8.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 3.75 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 RX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 TX))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /Pwr))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D5.0mm-3 (layer F.Cu) (tedit 587A3A7B)
    (at 124.5 118.79 90)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-59EGC(Ver.17A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins")
    (fp_text reference "R↓ G↑" (at -1.81 0 180) (layer F.SilkS))
    (fp_text value HLMP-4000#2 (at 2.54 3.96 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 /Green))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 /Red))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D5.0mm-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:C_0306 (layer F.Cu) (tedit 5F3D4236)
    (at 118.5 117.5 270)
    (fp_text reference C2 (at 2 0) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0.03 2 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.5715 0 270) (size 0.4572 1.7018) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.5715 0 270) (size 0.4572 1.7018) (layers F.Cu F.Paste F.Mask)
      (net 6 /VCAP))
  )
  (gr_text Hammerhead (at 123.5 120.25) (layer B.SilkS))
  (gr_line (start 110.1 124) (end 110.1 122) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103 124.5) (end 109.6 124.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 109.6 107) (end 103 107) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.1 109.5) (end 110.1 107.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109.6 107.5) (end 110.1 107.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 109.6 124) (end 109.6 124.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.6 122) (end 110.6 121.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.6 109.5) (end 110.1 109.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text RX (at 131.75 119.75 90) (layer F.SilkS))
  (gr_text Gnd (at 131.75 117 90) (layer F.SilkS))
  (gr_text TX (at 131.75 114.5 90) (layer F.SilkS))
  (gr_text Pwr (at 131.75 112 90) (layer F.SilkS))
  (gr_text STM8USB (at 123.5 112.75) (layer B.SilkS))
  (gr_arc (start 103 107.5) (end 103 107) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 103 124) (end 102.5 124) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 132 121) (end 132 121.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 132 110.5) (end 132.5 110.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.5 124) (end 102.5 107.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132 121.5) (end 110.6 121.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.5 110.5) (end 132.5 121) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.6 110) (end 132 110) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.5 121.5) (xy 110.1 121.5) (xy 109.6 122) (xy 109.6 124.5) (xy 102.5 124.5)
        (xy 102.5 107) (xy 109.6 107) (xy 109.6 109.5) (xy 110.1 110) (xy 132.5 110)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.5 121.5) (xy 110.1 121.5) (xy 109.6 122) (xy 109.6 124.5) (xy 102.5 124.5)
        (xy 102.5 107) (xy 109.6 107) (xy 109.6 109.5) (xy 110.1 110) (xy 132.5 110)
      )
    )
  )
)
