(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 49)
    (no_connects 0)
    (area 104.919047 70.674999 171.080953 114.325)
    (thickness 1.6)
    (drawings 14)
    (tracks 231)
    (zones 0)
    (modules 10)
    (nets 37)
  )
  (page A)
  (title_block
    (date 2017-12-09)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2286)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 2.75)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 105.5 113.75)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 GND)
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J2-Pad3)")
  (net 7 "Net-(J2-Pad5)")
  (net 8 "Net-(J2-Pad7)")
  (net 9 "Net-(J2-Pad8)")
  (net 10 "Net-(J2-Pad10)")
  (net 11 "Net-(J2-Pad11)")
  (net 12 "Net-(J2-Pad12)")
  (net 13 "Net-(J2-Pad13)")
  (net 14 "Net-(J2-Pad15)")
  (net 15 "Net-(J2-Pad16)")
  (net 16 "Net-(J2-Pad17)")
  (net 17 "Net-(J2-Pad18)")
  (net 18 "Net-(J2-Pad19)")
  (net 19 "Net-(J2-Pad21)")
  (net 20 "Net-(J2-Pad22)")
  (net 21 "Net-(J2-Pad23)")
  (net 22 "Net-(J2-Pad24)")
  (net 23 "Net-(J2-Pad26)")
  (net 24 "Net-(J2-Pad27)")
  (net 25 "Net-(J2-Pad28)")
  (net 26 "Net-(J2-Pad29)")
  (net 27 "Net-(J2-Pad31)")
  (net 28 "Net-(J2-Pad32)")
  (net 29 "Net-(J2-Pad33)")
  (net 30 "Net-(J2-Pad35)")
  (net 31 "Net-(J2-Pad36)")
  (net 32 "Net-(J2-Pad37)")
  (net 33 "Net-(J2-Pad38)")
  (net 34 "Net-(J2-Pad40)")
  (net 35 "Net-(U1-Pad8)")
  (net 36 "Net-(U1-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2286)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad29)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad35)")
    (add_net "Net-(J2-Pad36)")
    (add_net "Net-(J2-Pad37)")
    (add_net "Net-(J2-Pad38)")
    (add_net "Net-(J2-Pad40)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad8)")
    (add_net VCC)
  )
  (module LED:MountHole (layer F.Cu) (tedit 5A2C59B7)
    (at 167 89.75)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -6.35) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 -2.54) (size 6 6) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module LED:MountHole (layer F.Cu) (tedit 5A2C59C0)
    (at 167 112.75)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -6.35) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 -2.54) (size 6 6) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module LED:MountHole (layer F.Cu) (tedit 5A2C59A1)
    (at 109 89.75)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -6.35) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 -2.54) (size 6 6) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module LED:MountHole (layer F.Cu) (tedit 5A2C59AB)
    (at 109 112.75)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value MountHole (at 0 -6.35) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 -2.54) (size 6 6) (drill 2.75) (layers *.Cu *.Mask))
  )
  (module LED:Phoenix-Screw-Term-4 (layer F.Cu) (tedit 5A2C4FFB)
    (at 127 77)
    (fp_text reference J1 (at 12.5 -0.25) (layer F.SilkS))
    (fp_text value TermBlock4 (at 0 5.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -7.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at -2.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 2.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 7.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module "LED:Pi Header" (layer F.Cu) (tedit 5A2C4FE0)
    (at 139.25 88.5)
    (fp_text reference J2 (at -2.25 3.5) (layer F.SilkS))
    (fp_text value PIHeader (at -8.25 3.25) (layer F.Fab))
    (pad 1 thru_hole rect (at -25.4 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole circle (at -22.86 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at -20.32 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 7 thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at -12.7 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at -10.16 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad13)"))
    (pad 14 thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 15 thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad15)"))
    (pad 16 thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad16)"))
    (pad 17 thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad17)"))
    (pad 18 thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad18)"))
    (pad 19 thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad19)"))
    (pad 20 thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 21 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad21)"))
    (pad 22 thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad22)"))
    (pad 23 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad23)"))
    (pad 24 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad24)"))
    (pad 25 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 26 thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad26)"))
    (pad 27 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad27)"))
    (pad 28 thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad28)"))
    (pad 29 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad29)"))
    (pad 30 thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 31 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad31)"))
    (pad 32 thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad32)"))
    (pad 33 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad33)"))
    (pad 34 thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 35 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(J2-Pad35)"))
    (pad 36 thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(J2-Pad36)"))
    (pad 37 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad37)"))
    (pad 38 thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad38)"))
    (pad 39 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 40 thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(J2-Pad40)"))
  )
  (module LED:Phoenix-Screw-Term-2 (layer F.Cu) (tedit 5A2C4FF4)
    (at 150.5 77)
    (fp_text reference J3 (at 6.25 0) (layer F.SilkS))
    (fp_text value TermBlock2 (at -0.25 5.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module LED:4609X-101-RC (layer F.Cu) (tedit 5A2C4FE5)
    (at 148.25 96)
    (fp_text reference R1 (at 6.25 1.75) (layer F.SilkS))
    (fp_text value ResNetwork (at -0.25 1.75) (layer F.Fab))
    (pad 1 thru_hole rect (at -8.255 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -5.715 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 3 thru_hole circle (at -3.175 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad16)"))
    (pad 4 thru_hole circle (at -0.635 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad18)"))
    (pad 5 thru_hole circle (at 1.905 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad22)"))
    (pad 6 thru_hole circle (at 4.445 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad24)"))
    (pad 7 thru_hole circle (at 6.985 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad26)"))
    (pad 8 thru_hole circle (at 9.525 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad28)"))
    (pad 9 thru_hole circle (at 12.065 -0.635) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad32)"))
  )
  (module LED:210-008-M (layer F.Cu) (tedit 5A2C4FEC)
    (at 150.25 105.25)
    (fp_text reference SW1 (at 2.25 6) (layer F.SilkS))
    (fp_text value Dip_Switch_X8 (at -6 5.75) (layer F.Fab))
    (pad 1 thru_hole rect (at -8.89 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 2 thru_hole circle (at -6.35 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad16)"))
    (pad 3 thru_hole circle (at -3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad18)"))
    (pad 4 thru_hole circle (at -1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad22)"))
    (pad 5 thru_hole circle (at 1.27 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad24)"))
    (pad 6 thru_hole circle (at 3.81 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad26)"))
    (pad 7 thru_hole circle (at 6.35 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad28)"))
    (pad 8 thru_hole circle (at 8.89 3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad32)"))
    (pad 9 thru_hole circle (at 8.89 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 10 thru_hole circle (at 6.35 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 11 thru_hole circle (at 3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 12 thru_hole circle (at 1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 13 thru_hole circle (at -1.27 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 14 thru_hole circle (at -3.81 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 15 thru_hole circle (at -6.35 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 16 thru_hole circle (at -8.89 -3.81) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (module LED:74AHCT125 (layer F.Cu) (tedit 5A2C5008)
    (at 122 101.5)
    (fp_text reference U1 (at 6.5 1.5) (layer F.SilkS))
    (fp_text value 74AHCT125 (at 8.75 -3.25) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 2 thru_hole circle (at -3.81 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad19)"))
    (pad 3 thru_hole circle (at -3.81 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at -3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 5 thru_hole circle (at -3.81 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad23)"))
    (pad 6 thru_hole circle (at -3.81 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 7 thru_hole circle (at -3.81 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 8 thru_hole circle (at 3.81 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 3.81 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 10 thru_hole circle (at 3.81 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 11 thru_hole circle (at 3.81 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 3.81 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 13 thru_hole circle (at 3.81 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 14 thru_hole circle (at 3.81 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
  )
  (gr_text G (at 153 74) (layer B.SilkS))
  (gr_text P (at 148 74) (layer B.SilkS))
  (gr_text G (at 134.5 73.75) (layer B.SilkS))
  (gr_text P (at 119.5 73.75) (layer B.SilkS))
  (gr_text C (at 129.5 73.75) (layer B.SilkS))
  (gr_text D (at 124.5 73.75) (layer B.SilkS))
  (gr_arc (start 108.5 110.75) (end 108.5 113.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.5 110.75) (end 170.5 110.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 167.5 73.75) (end 167.5 70.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 108.5 73.75) (end 105.5 73.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.5 110.75) (end 105.5 73.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.5 113.75) (end 108.5 113.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.5 73.75) (end 170.5 110.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.5 70.75) (end 167.5 70.75) (angle 90) (layer Edge.Cuts) (width 0.15))
)
