<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="39.14" x2="0" y2="2.5" width="0" layer="20"/>
<wire x1="0" y1="2.5" x2="2.5" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.5" y1="0" x2="37.77" y2="0" width="0" layer="20"/>
<wire x1="37.77" y1="0" x2="40.27" y2="2.5" width="0" layer="20" curve="90"/>
<wire x1="40.27" y1="2.5" x2="40.27" y2="39.14" width="0" layer="20"/>
<wire x1="40.27" y1="39.14" x2="37.77" y2="41.64" width="0" layer="20" curve="90"/>
<wire x1="37.77" y1="41.64" x2="2.5" y2="41.64" width="0" layer="20"/>
<wire x1="2.5" y1="41.64" x2="0" y2="39.14" width="0" layer="20" curve="90"/>
<hole x="2.5" y="33" drill="1.4"/>
<hole x="2.5" y="30" drill="1.4"/>
<hole x="5.5" y="33" drill="1.4"/>
<hole x="5.5" y="30" drill="1.4"/>
<hole x="5.5" y="39" drill="1.4"/>
<hole x="5.5" y="36" drill="1.4"/>
<text>Pigeon FX</text>
<text>FIRENZE v1.0</text>
<text>HASTING-ENGLAND</text>
</plain>
<libraries>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="LONG">
<description>&lt;b&gt;Long Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing&lt;/b&gt;</description>
</package>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-caps-film-box">
<description>&lt;b&gt;Capacitors, Film, Box&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;1000pF - 2.2uF  (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors because they are small
&lt;li&gt;these have short leads so that pad spacing equals lead spacing
&lt;li&gt;e.g., WIMA capacitors
&lt;/ul&gt;</description>
<packages>
<package name="072X025">
<description>&lt;b&gt;7.2mm x 2.5mm&lt;/b&gt;
&lt;p&gt;WIMA MKS2, MKP2</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO35-2">
<description>&lt;b&gt;DO-35 0.2" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-switches">
<description>&lt;b&gt;Switches&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;SPST, SPDT, DPDT, 3PDT
&lt;/ul&gt;</description>
<packages>
<package name="DPDT-SLIDE">
</package>
</packages>
</library>
<library name="Logo">
<packages>
<package name="LOGO3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="gm-resistors" package="R0207/3" value=""/>
<element name="R2" library="gm-resistors" package="R0207/3" value=""/>
<element name="R3" library="gm-resistors" package="R0207/3" value=""/>
<element name="R4" library="gm-resistors" package="R0207/3" value=""/>
<element name="R5" library="gm-resistors" package="R0207/3" value=""/>
<element name="C1" library="gm-caps-electro-pol" package="050_020" value=""/>
<element name="C2" library="gm-caps-film-box" package="072X025" value=""/>
<element name="C3" library="gm-caps-electro-pol" package="063_025" value="063-EU">
<attribute name="NAME"/>
</element>
<element name="IC1" library="linear" package="DIL08" value="TL072P">
<attribute name="VALUE"/>
</element>
<element name="GND" library="gm-supply" package="LONG" value=""/>
<element name="D1" library="gm-diodes" package="DO35-2" value="1N914">
<attribute name="NAME"/>
</element>
<element name="D2" library="gm-diodes" package="DO35-2" value="1N914">
<attribute name="NAME"/>
</element>
<element name="R6" library="gm-resistors" package="R0207/3" value=""/>
<element name="LED1" library="adafruit" package="LED5MM" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="TO-92" value="">
<attribute name="VALUE"/>
</element>
<element name="OUT" library="gm-supply" package="LONG" value=""/>
<element name="IN" library="gm-supply" package="LONG" value=""/>
<element name="SW2" library="gm-switches" package="DPDT-SLIDE" value=""/>
<element name="9V" library="gm-supply" package="LONG" value=""/>
<element name="E$1" library="Logo" package="LOGO3" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="+"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="-"/>
<contactref element="R4" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="IN">
<contactref element="C2" pad="1"/>
<contactref element="SW2" pad="A3"/>
</signal>
<signal name="N$10">
<contactref element="LED1" pad="K"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="CON">
<contactref element="Q1" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="A"/>
<contactref element="SW2" pad="B1"/>
</signal>
<signal name="N$12">
<contactref element="IN" pad="1"/>
<contactref element="SW2" pad="A2"/>
</signal>
<signal name="OUT">
<contactref element="R5" pad="2"/>
<contactref element="SW2" pad="B2"/>
</signal>
<signal name="N$4">
<contactref element="SW2" pad="A1"/>
<contactref element="OUT" pad="1"/>
<contactref element="SW2" pad="B3"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="D1" pad="C"/>
<contactref element="LED1" pad="A"/>
<contactref element="9V" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
