(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 125)
    (tracks 497)
    (zones 0)
    (modules 96)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFBFF9F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 Vsense)
  (net 3 LeftIn)
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C11-Pad1)")
  (net 6 RightIn)
  (net 7 "Net-(C19-Pad1)")
  (net 8 "Net-(C20-Pad1)")
  (net 9 "Net-(C25-Pad1)")
  (net 10 +15V)
  (net 11 LeftOut)
  (net 12 "Net-(C27-Pad1)")
  (net 13 "Net-(C31-Pad1)")
  (net 14 RightOut)
  (net 15 "Net-(C36-Pad1)")
  (net 16 "Net-(C37-Pad1)")
  (net 17 "Net-(C38-Pad2)")
  (net 18 "Net-(C39-Pad2)")
  (net 19 "Net-(D1-Pad2)")
  (net 20 "Net-(D2-Pad1)")
  (net 21 "Net-(D2-Pad2)")
  (net 22 "Net-(HS1-Pad1)")
  (net 23 "Net-(HS2-Pad1)")
  (net 24 "Net-(HS3-Pad1)")
  (net 25 "Net-(HS4-Pad1)")
  (net 26 "Net-(HS5-Pad1)")
  (net 27 "Net-(J3-PadRN)")
  (net 28 "Net-(J3-PadTN)")
  (net 29 "Net-(J5-PadR)")
  (net 30 "Net-(J5-PadT)")
  (net 31 "Net-(J5-PadSN)")
  (net 32 "Net-(J5-PadRN)")
  (net 33 "Net-(J5-PadTN)")
  (net 34 "Net-(K1-Pad6)")
  (net 35 "Net-(K1-Pad11)")
  (net 36 "Net-(Q1-Pad1)")
  (net 37 "Net-(Q2-Pad1)")
  (net 38 Reset)
  (net 39 "Net-(R7-Pad2)")
  (net 40 "Net-(R9-Pad2)")
  (net 41 "Net-(R10-Pad2)")
  (net 42 "Net-(U1-Pad9)")
  (net 43 "Net-(D4-Pad1)")
  (net 44 "Net-(C10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.381)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net LeftIn)
    (add_net LeftOut)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C36-Pad1)")
    (add_net "Net-(C37-Pad1)")
    (add_net "Net-(C38-Pad2)")
    (add_net "Net-(C39-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(HS1-Pad1)")
    (add_net "Net-(HS2-Pad1)")
    (add_net "Net-(HS3-Pad1)")
    (add_net "Net-(HS4-Pad1)")
    (add_net "Net-(HS5-Pad1)")
    (add_net "Net-(J3-PadRN)")
    (add_net "Net-(J3-PadTN)")
    (add_net "Net-(J5-PadR)")
    (add_net "Net-(J5-PadRN)")
    (add_net "Net-(J5-PadSN)")
    (add_net "Net-(J5-PadT)")
    (add_net "Net-(J5-PadTN)")
    (add_net "Net-(K1-Pad11)")
    (add_net "Net-(K1-Pad6)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net Reset)
    (add_net RightIn)
    (add_net RightOut)
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net GND)
    (add_net Vsense)
  )
  (module Capacitor_THT:CP_Radial_D17.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 159.385 81.28 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=17mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 17mm Electrolytic Capacitor")
    (fp_text reference C1 (at -26.035 -2.54 270) (layer F.SilkS))
    (fp_text value 3300uF (at 3.75 9.75 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Vsense))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D17.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D17.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 221.615 81.28 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=17mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 17mm Electrolytic Capacitor")
    (fp_text reference C2 (at -26.67 -3.81 270) (layer F.SilkS))
    (fp_text value 3300uF (at 3.75 9.75 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D17.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 173.99 82.55 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C3 (at -27.305 -1.27 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Vsense))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Vsense))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 207.01 82.55 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C4 (at -27.94 1.27 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 163.195 82.55 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at -26.67 3.175 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 Vsense))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal (layer F.Cu) (tedit 5AE50EF2)
    (at 181.61 101.6 270)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=48mm, , length*diameter=40*16mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 48mm  length 40mm diameter 16mm Electrolytic Capacitor")
    (fp_text reference C6 (at 53.34 -5.715 270) (layer F.SilkS))
    (fp_text value 1uF (at 24 9.12 270) (layer F.Fab))
    (fp_text user %R (at 24 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 48 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 LeftIn))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W7.2mm_P7.50mm_MKS4 (layer F.Cu) (tedit 5AE50EF0)
    (at 181.61 101.6 270)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*7.2mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 7.2mm Capacitor")
    (fp_text reference C7 (at -47.625 -4.445 270) (layer F.SilkS))
    (fp_text value 1uF (at 3.75 4.85 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 LeftIn))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W7.2mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W11.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0)
    (at 181.61 101.6 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 11mm Capacitor")
    (fp_text reference C8 (at -46.99 -6.35 270) (layer F.SilkS))
    (fp_text value 1uF (at 2.5 6.75 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 LeftIn))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W11.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 184.15 104.3575 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -49.7475 0.635 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 3 LeftIn))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 217.805 82.55 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at -27.305 0.635 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 44 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal (layer F.Cu) (tedit 5AE50EF2)
    (at 199.39 101.6 270)
    (descr "CP, Axial series, Axial, Horizontal, pin pitch=48mm, , length*diameter=40*16mm^2, Electrolytic Capacitor")
    (tags "CP Axial series Axial Horizontal pin pitch 48mm  length 40mm diameter 16mm Electrolytic Capacitor")
    (fp_text reference C11 (at 52.705 -2.54 270) (layer F.SilkS))
    (fp_text value 1uF (at 24 9.12 270) (layer F.Fab))
    (fp_text user %R (at 24 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 48 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 RightIn))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Axial_L40.0mm_D16.0mm_P48.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L10.3mm_W7.2mm_P7.50mm_MKS4 (layer F.Cu) (tedit 5AE50EF0)
    (at 199.39 101.6 270)
    (descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=10.3*7.2mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 7.50mm  length 10.3mm width 7.2mm Capacitor")
    (fp_text reference C12 (at -49.53 -1.27 270) (layer F.SilkS))
    (fp_text value 1uF (at 3.75 4.85 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 RightIn))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L10.3mm_W7.2mm_P7.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Rect_L7.2mm_W11.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2 (layer F.Cu) (tedit 5AE50EF0)
    (at 199.39 101.6 270)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*11mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 11mm Capacitor")
    (fp_text reference C13 (at -46.355 1.27 270) (layer F.SilkS))
    (fp_text value 1uF (at 2.5 6.75 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 RightIn))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W11.0mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 196.85 104.3575 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at -50.3825 1.905 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 6 RightIn))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 165.735 82.55 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -27.94 3.81 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 Vsense))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 215.265 82.55 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at -27.305 1.27 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 44 "Net-(C10-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 168.275 82.55 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C17 (at -27.94 3.175 270) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 2 Vsense))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 212.725 82.55 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C18 (at -27.305 0.635 270) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 44 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 173.99 93.345 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C19 (at -38.735 -3.175 270) (layer F.SilkS))
    (fp_text value 470uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C19-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 207.01 93.345 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C20 (at -38.735 -5.08 270) (layer F.SilkS))
    (fp_text value 470uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 167.64 94.8325 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C21 (at 39.5875 0 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(C19-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 213.995 94.3975 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C22 (at 39.1525 1.27 90) (layer B.SilkS))
    (fp_text value 10uF (at 3.5925 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C20-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 165.1 94.8325 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C23 (at 40.2225 1.27 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 216.535 94.3975 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C24 (at 39.1525 -0.635 90) (layer B.SilkS))
    (fp_text value 1uF (at 3.5925 0 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 143.815 121.320937 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C25 (at 32.984063 0.305 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 155.9925 124.46)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C26 (at -0.4175 29.845) (layer B.SilkS))
    (fp_text value .1uF (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D17.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 159.385 100.33 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=17mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 17mm Electrolytic Capacitor")
    (fp_text reference C27 (at -45.085 0.635 270) (layer F.SilkS))
    (fp_text value 3300uF (at 3.75 9.75 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 LeftOut))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D17.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 167.945 114.3 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C28 (at 40.64 -7.95 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 LeftOut))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C27-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 LeftOut))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 170.18 122.555)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C29 (at 0 31.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 "Net-(C27-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 LeftOut))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 170.18 125.095)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C30 (at 0.635 29.21) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 11 LeftOut))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D17.0mm_P7.50mm (layer F.Cu) (tedit 5AE50EF1)
    (at 221.615 100.33 270)
    (descr "CP, Radial series, Radial, pin pitch=7.50mm, , diameter=17mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 7.50mm  diameter 17mm Electrolytic Capacitor")
    (fp_text reference C31 (at -45.085 -5.715 270) (layer F.SilkS))
    (fp_text value 3300uF (at 3.75 9.75 270) (layer F.Fab))
    (fp_text user %R (at 3.75 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 RightOut))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D17.0mm_P7.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D10.0mm_P2.50mm_P5.00mm (layer F.Cu) (tedit 5AE50EF1)
    (at 213.03 114.335937 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm 5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C32 (at 0.599063 -33.35 270) (layer F.SilkS))
    (fp_text value 100uF (at 1.25 6.25 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 RightOut))
    (pad 1 thru_hole rect (at -0.670937 -1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (pad 2 thru_hole circle (at 3.170937 1.6 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 RightOut))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P2.50mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 211.0375 125.095 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C33 (at 2.1225 -29.845 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(C31-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 RightOut))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 211.0375 122.555 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C34 (at 3.3925 -32.385 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 RightOut))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 193.04 72.1725 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C35 (at 16.9275 0 90) (layer F.SilkS))
    (fp_text value 10uF (at -0.8525 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 231.775 140.97)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C36 (at 0 13.335) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBE)
    (at 231.775 148.59)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C37 (at -0.635 5.715) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(C37-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 185.42 72.1725 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C38 (at 17.5625 -3.81 90) (layer F.SilkS))
    (fp_text value 10uF (at -1.4875 -1.905 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(C38-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 190.5 72.1725 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C39 (at 16.9275 -3.175 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(C39-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 193.8925 149.86)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at -0.2175 4.445) (layer F.SilkS))
    (fp_text value PowerLED (at 1.0525 3.175) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 186.9075 149.86)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at -0.2175 5.08) (layer F.SilkS))
    (fp_text value "Headphones Live" (at 0 4.445) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 "Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 21 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMA_Handsoldering (layer B.Cu) (tedit 58643398)
    (at 167.6 134.62)
    (descr "Diode SMA (DO-214AC) Handsoldering")
    (tags "Diode SMA (DO-214AC) Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 0 19.685) (layer B.SilkS))
    (fp_text value 1N4001 (at 0 -2.6) (layer B.Fab))
    (fp_text user %R (at 0 2.5) (layer B.Fab))
    (pad 1 smd rect (at -2.5 0) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 10 +15V))
    (pad 2 smd rect (at 2.5 0) (size 3.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 190.7175 88.9)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D4 (at -6.5675 -34.29) (layer F.SilkS))
    (fp_text value TubeLED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 43 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(C39-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:Heatsink-TO-220 (layer F.Cu) (tedit 59CF2489)
    (at 143.47 85.725 90)
    (fp_text reference HS1 (at 31.115 7.025 90) (layer F.SilkS))
    (fp_text value LeftFET (at 0 6.477 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(HS1-Pad1)"))
  )
  (module Libraries:Heatsink-TO-220 (layer F.Cu) (tedit 59CF2489)
    (at 143.47 103.505 90)
    (fp_text reference HS2 (at 48.26 -4.405 90) (layer F.SilkS))
    (fp_text value LeftCCS (at 0 6.477 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.5 90) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(HS2-Pad1)"))
  )
  (module Libraries:Heatsink-TO-220 (layer F.Cu) (tedit 59CF2489)
    (at 237.49 85.725 270)
    (fp_text reference HS3 (at -31.75 11.43 270) (layer F.SilkS))
    (fp_text value RightFET (at 0 6.477 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.5 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(HS3-Pad1)"))
  )
  (module Libraries:Heatsink-TO-220 (layer F.Cu) (tedit 59CF2489)
    (at 237.53 103.505 270)
    (fp_text reference HS4 (at -48.26 8.93 270) (layer F.SilkS))
    (fp_text value RightCCS (at 0 6.477 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.5 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(HS4-Pad1)"))
  )
  (module Libraries:Heatsink-TO-220 (layer F.Cu) (tedit 59CF2489)
    (at 190.5 63.46)
    (fp_text reference HS5 (at 0 -7.58) (layer F.SilkS))
    (fp_text value Heater (at 0 6.477) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.5) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(HS5-Pad1)"))
  )
  (module Connector_BarrelJack:BarrelJack_Horizontal (layer F.Cu) (tedit 5A1DBF6A)
    (at 168.275 67.31 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -12.065 6.35 270) (layer F.SilkS))
    (fp_text value "+15v In" (at -6.2 -5.5 270) (layer F.Fab))
    (fp_text user %R (at -3 -2.95 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 10 +15V))
    (pad 2 thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5B78013E)
    (at 158.115 67.31 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J2 (at 12.7 -4.445 90) (layer F.SilkS))
    (fp_text value "+15v In Alt" (at 1.27 4.08 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.22 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.143678)
      (net 10 +15V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:Conn-3.5mm-SJ1-3535NG (layer F.Cu) (tedit 5C312F1C)
    (at 243.84 124.46 90)
    (fp_text reference J3 (at 0 5.08 90) (layer F.SilkS))
    (fp_text value LineIn (at 0 3.81 90) (layer F.Fab))
    (pad S thru_hole oval (at 0.9 -1.2 90) (size 3 1.8) (drill oval 2 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad T thru_hole oval (at -1.1 -3.6 90) (size 3 1.8) (drill oval 2 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C37-Pad1)"))
    (pad R thru_hole oval (at -1.1 -9.1 90) (size 3 1.8) (drill oval 2 0.8 (offset -0.1 0)) (layers *.Cu *.Mask)
      (net 15 "Net-(C36-Pad1)"))
    (pad RN thru_hole oval (at 0.9 -7.3 90) (size 3 1.8) (drill oval 2 0.8 (offset 0.1 0)) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-PadRN)"))
    (pad TN thru_hole oval (at 0.9 -12.8 90) (size 3 1.8) (drill oval 2 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-PadTN)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 227.33 125.73 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at -5.715 -27.94 180) (layer F.SilkS))
    (fp_text value "LineIn Alt" (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-PadTN)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-PadRN)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:NRJ6HF (layer F.Cu) (tedit 5C313028)
    (at 152.3746 152.2222)
    (fp_text reference J5 (at -11.4046 1.4478) (layer F.SilkS))
    (fp_text value Headphones (at 0 -19.812) (layer F.Fab))
    (pad S thru_hole circle (at 7.239 -4.2418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad R thru_hole circle (at 7.239 -10.5918) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-PadR)"))
    (pad T thru_hole circle (at 7.239 -16.9418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-PadT)"))
    (pad SN thru_hole circle (at -4.191 -4.2418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-PadSN)"))
    (pad RN thru_hole circle (at -4.191 -10.5918) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-PadRN)"))
    (pad TN thru_hole circle (at -4.191 -16.9418) (size 2.54 2.54) (drill 1.4986) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-PadTN)"))
    (pad "" np_thru_hole circle (at 6.839 -7.4422) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.691 -7.4422) (size 2.032 2.032) (drill 2.032) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.1054 -13.7922) (size 2.9972 2.9972) (drill 2.9972) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.51 133.985)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 1.27 20.32) (layer F.SilkS))
    (fp_text value "Headphones Alt" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-PadRN)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-PadSN)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-PadSN)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-PadTN)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_DPDT_Omron_G5V-2 (layer F.Cu) (tedit 59D689A9)
    (at 163.83 132.08)
    (descr http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v2.pdf)
    (tags "Omron G5V-2 Relay DPDT")
    (fp_text reference K1 (at 4.445 21.59) (layer F.SilkS))
    (fp_text value G5V-2 (at -2.41 9.01 90) (layer F.Fab))
    (fp_text user %R (at 3.94 9.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 +15V))
    (pad 16 thru_hole circle (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(D2-Pad1)"))
    (pad 6 thru_hole circle (at 0 12.69) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 "Net-(K1-Pad6)"))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 30 "Net-(J5-PadT)"))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 LeftOut))
    (pad 11 thru_hole circle (at 7.63 12.71) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 "Net-(K1-Pad11)"))
    (pad 9 thru_hole circle (at 7.63 17.79) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 29 "Net-(J5-PadR)"))
    (pad 13 thru_hole circle (at 7.62 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 RightOut))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_DPDT_Omron_G5V-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 147.32 88.265 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 33.655 -4.445 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 Vsense))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 233.68 83.185 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at -28.575 0 270) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 2.54 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 171.45 128.54 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 25.765 3.81 270) (layer B.SilkS))
    (fp_text value MMBT3904 (at 0 -2.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 38 Reset))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.99 75.7825 270)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at -20.5375 -1.27 270) (layer F.SilkS))
    (fp_text value 10 (at 0 2.28 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 Vsense))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 207.01 75.565 270)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -20.955 -0.635 270) (layer F.SilkS))
    (fp_text value 10 (at 0 2.28 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 44 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 177.8 87.2125 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -31.9675 3.175 270) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 203.2 90.5875 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 35.3425 -0.635 90) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 5 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 170.18 94.8325 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at -39.5875 0.635 270) (layer B.SilkS))
    (fp_text value 150 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 211.455 94.3975 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -39.1525 -0.635 270) (layer B.SilkS))
    (fp_text value 150 (at -3.5925 0 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 8 "Net-(C20-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 155.9925 118.745 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -9.7425 -36.195 180) (layer F.SilkS))
    (fp_text value 220k (at -4.6625 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 Vsense))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 39 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 155.9925 116.205)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 4.6625 41.275) (layer F.SilkS))
    (fp_text value 10k (at 0.2175 -1.905) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 39 "Net-(R7-Pad2)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 142.875 113.665 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 1.905 -41.275 180) (layer F.SilkS))
    (fp_text value 10 (at 0 2.28 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 40 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1210_3225Metric_Pad1.42x2.65mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 237.9075 113.665 180)
    (descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -8.4725 -4.445 180) (layer F.SilkS))
    (fp_text value 10 (at 0 2.28 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 41 "Net-(R10-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 166.37 141.1875 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 13.7525 1.905 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 11 LeftOut))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 168.91 141.1875 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 14.3875 3.175 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 14 RightOut))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 167.64 129.1225 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -25.1825 1.82 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.82 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 38 Reset))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 193.8925 149.86)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -0.2175 3.81) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 19 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 186.9075 149.86)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at -0.2175 4.445) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 21 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 10 +15V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 231.775 143.51)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at 0.635 11.43) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(C36-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 231.775 146.05)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at 0.635 8.89) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 16 "Net-(C37-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 187.96 72.1725 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at 16.9275 -2.54 90) (layer F.SilkS))
    (fp_text value 150 (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(C38-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 "Net-(C39-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 166.37 146.2675 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at 9.3075 2.54 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 34 "Net-(K1-Pad6)"))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 168.91 146.2675 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at 9.9425 2.54 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 35 "Net-(K1-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 190.7175 88.9)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at -1.4875 -33.655) (layer B.SilkS))
    (fp_text value 1k (at -0.2175 -1.905) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 43 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 144.78 74.93 180)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV1 (at -2.54 19.685 180) (layer F.SilkS))
    (fp_text value 50k (at -2.54 3.67 180) (layer F.Fab))
    (fp_text user %R (at -3.175 0.005 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 Vsense))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(Q1-Pad1)"))
    (pad 3 thru_hole circle (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 236.22 74.93)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV2 (at -4.445 -19.685) (layer F.SilkS))
    (fp_text value 50k (at -2.54 3.67) (layer F.Fab))
    (fp_text user %R (at -3.175 0.005) (layer F.Fab))
    (pad 3 thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(Q2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical (layer F.Cu) (tedit 5A3D4994)
    (at 179.705 67.31 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (fp_text reference RV3 (at 12.7 -3.66 90) (layer F.SilkS))
    (fp_text value 5k (at -2.54 3.67 90) (layer F.Fab))
    (fp_text user %R (at -3.175 0.005 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(C38-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:Pot-Multiple-types (layer F.Cu) (tedit 587558CE)
    (at 222.25 153.67)
    (fp_text reference RV4 (at 8.89 0.635) (layer F.SilkS))
    (fp_text value 10k (at 0 -26.67) (layer F.Fab))
    (fp_text user RK097 (at 7.62 -8.255) (layer F.SilkS))
    (fp_text user RK27 (at -11.43 -24.13) (layer F.SilkS))
    (fp_text user DACT (at -8.89 -13.335) (layer F.SilkS))
    (pad 1 thru_hole circle (at 5.08 -5.08) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 16 "Net-(C37-Pad1)"))
    (pad 2 thru_hole circle (at 0 -5.08) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 3 LeftIn))
    (pad 3 thru_hole circle (at -5.08 -5.08) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 5.08 -12.7) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 15 "Net-(C36-Pad1)"))
    (pad 5 thru_hole circle (at 0 -12.7) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 6 RightIn))
    (pad 6 thru_hole circle (at -5.08 -12.7) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 5.08 -15.24) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 15 "Net-(C36-Pad1)"))
    (pad 5 thru_hole circle (at 0 -15.24) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 6 RightIn))
    (pad 6 thru_hole circle (at -5.08 -15.24) (size 2.286 2.286) (drill 1.27) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 2.54 -5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(C37-Pad1)"))
    (pad 3 thru_hole circle (at -2.54 -5.08) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 -7.62) (size 2.032 1.524) (drill 1.016 (offset 0.254 0)) (layers *.Cu *.Mask)
      (net 15 "Net-(C36-Pad1)"))
    (pad 5 thru_hole oval (at 0 -7.62) (size 1.524 2.032) (drill 1.016 (offset 0 -0.254)) (layers *.Cu *.Mask)
      (net 6 RightIn))
    (pad 6 thru_hole oval (at -2.54 -7.62) (size 2.032 1.524) (drill 1.016 (offset -0.254 0)) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 240.665 74.93)
    (descr "wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference TP1 (at -2.54 -19.685) (layer F.SilkS))
    (fp_text value RightBias (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 140.335 74.93)
    (descr "wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference TP2 (at 2.54 -19.685) (layer F.SilkS))
    (fp_text value LeftBias (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 140.335 70.485)
    (descr "wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference TP3 (at 0.7 -16.51) (layer F.SilkS))
    (fp_text value Ground (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Loop_D2.50mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 240.665 70.485)
    (descr "wire loop as test point, loop diameter 2.5mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (fp_text reference TP4 (at -3.81 -15.875) (layer F.SilkS))
    (fp_text value Ground (at 0 -2.8) (layer F.Fab))
    (fp_text user %R (at 0.7 2.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Loop_D2.50mm_Drill1.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Libraries:VALVE-ECC-83-Socket (layer F.Cu) (tedit 59C94D64)
    (at 190.5 88.9)
    (fp_text reference U1 (at -1.27 -33.655) (layer F.SilkS))
    (fp_text value 12AU7 (at 0 11.43) (layer F.Fab))
    (pad 1 thru_hole oval (at 6.0325 8.255 306) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 9.779 3.1115 342) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C11-Pad1)"))
    (pad 3 thru_hole oval (at 9.7155 -3.175 18) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C20-Pad1)"))
    (pad 4 thru_hole oval (at 6.0325 -8.3185 54) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C39-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.2235 90) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole oval (at -6.0325 -8.255 306) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(Q1-Pad1)"))
    (pad 7 thru_hole oval (at -9.7155 -3.175 342) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C6-Pad1)"))
    (pad 8 thru_hole oval (at -9.779 3.1115 18) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C19-Pad1)"))
    (pad 9 thru_hole oval (at -6.0325 8.255 54) (size 2.032 3.048) (drill oval 1.016 2.032) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U1-Pad9)"))
    (model Valves.3dshapes/VALVE-ECC-83-2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 147.32 106.045 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U2 (at 51.435 -1.905 90) (layer F.SilkS))
    (fp_text value LM317 (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(R9-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(C27-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 233.68 100.965 270)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U3 (at -46.355 -1.27 270) (layer F.SilkS))
    (fp_text value LM317 (at 2.54 2.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(R10-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 "Net-(C31-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 156.21 122.555)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 6.35 31.75) (layer F.SilkS))
    (fp_text value TL7700 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C25-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R7-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 +15V))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 Reset))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 187.96 67.31)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U5 (at 1.905 -12.7) (layer F.SilkS))
    (fp_text value LM317 (at 2.54 2.5) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 +15V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 18 "Net-(C39-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 17 "Net-(C38-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 240.03 148.59)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -1.27 5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 140.97 148.59)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 6.35) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 240.03 60.96)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at -0.635 -5.715) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 140.97 60.96)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.08) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text o (at 175.895 149.225) (layer F.Cu))
  (gr_text <>< (at 177.8 149.86) (layer F.Cu))
  (gr_text ><> (at 175.26 151.13) (layer F.Cu))
  (gr_text O (at 177.165 147.955) (layer F.Cu))
  (gr_text 0 (at 175.26 146.685) (layer F.Cu))
  (gr_text 0 (at 175.26 146.685) (layer F.Mask))
  (gr_text O (at 177.165 147.955) (layer F.Mask))
  (gr_text o (at 175.895 149.225) (layer F.Mask))
  (gr_text <>< (at 177.8 149.86) (layer F.Mask))
  (gr_text ><> (at 175.26 151.13) (layer F.Mask))
  (gr_text 1nF (at 234.315 143.51) (layer B.SilkS))
  (gr_text 1nF (at 234.315 146.05) (layer B.SilkS))
  (gr_text 1k (at 234.315 148.59) (layer B.SilkS))
  (gr_text 1k (at 234.315 140.97) (layer B.SilkS))
  (gr_text 1k (at 193.585 147.955) (layer B.SilkS))
  (gr_text 1k (at 188.505 147.955) (layer B.SilkS))
  (gr_text 100R (at 167.55 150.01) (layer B.SilkS))
  (gr_text 1k (at 167.55 137.795) (layer B.SilkS))
  (gr_text 1N4001 (at 167.64 132.08) (layer B.SilkS))
  (gr_text MMBT3904 (at 173.355 128.905) (layer B.SilkS))
  (gr_text 10k (at 167.64 125.73) (layer B.SilkS))
  (gr_text .1uF (at 156.21 122.555) (layer B.SilkS))
  (gr_text 10uF (at 217.805 85.09 90) (layer B.SilkS))
  (gr_text 1uF (at 215.265 85.09 90) (layer B.SilkS))
  (gr_text .1uF (at 212.725 85.09 90) (layer B.SilkS))
  (gr_text 1uF (at 216.535 97.155 90) (layer B.SilkS))
  (gr_text 10uF (at 213.995 97.155 90) (layer B.SilkS))
  (gr_text 150R (at 211.455 97.155 90) (layer B.SilkS))
  (gr_text .1uF (at 168.275 85.09 90) (layer B.SilkS))
  (gr_text 1uF (at 165.735 85.09 90) (layer B.SilkS))
  (gr_text 10uF (at 163.195 85.09 90) (layer B.SilkS))
  (gr_text 150R (at 170.18 97.155 90) (layer B.SilkS))
  (gr_text 10uF (at 167.64 97.155 90) (layer B.SilkS))
  (gr_text 1uF (at 165.1 97.155 90) (layer B.SilkS))
  (gr_text 100k (at 203.2 93.345 90) (layer B.SilkS))
  (gr_text 100k (at 177.8 89.535 90) (layer B.SilkS))
  (gr_text 1k (at 190.5 86.995) (layer B.SilkS))
  (gr_text "12AU7/IRF510 Hybrid Headphone Amp\nCC NC-BY-SA 2019\nDesign inspired by roggom@gmail.com\nBoard and mods by @SmittyHalibut ><>" (at 198.755 63.5) (layer F.SilkS))
  (gr_text GND (at 141.605 136.525) (layer F.SilkS))
  (gr_text Left (at 141.605 133.985) (layer F.SilkS))
  (gr_text Right (at 141.605 141.605) (layer F.SilkS))
  (gr_text GND (at 141.605 139.065) (layer F.SilkS))
  (gr_text "Headphones\nNRJ6HF" (at 154.305 132.715) (layer F.SilkS))
  (gr_text "Relay\nG5V 12v" (at 167.64 128.905) (layer F.SilkS))
  (gr_text 220k (at 153.67 118.745) (layer F.SilkS))
  (gr_text 10k (at 153.67 116.205) (layer F.SilkS))
  (gr_text TL7700 (at 156.21 126.365) (layer F.SilkS))
  (gr_text 100uF (at 144.145 116.84) (layer F.SilkS))
  (gr_text 1uF (at 213.36 125.095) (layer F.SilkS))
  (gr_text 10uF (at 213.36 122.555) (layer F.SilkS))
  (gr_text 1uF (at 167.64 125.095) (layer F.SilkS))
  (gr_text 10uF (at 167.64 122.555) (layer F.SilkS))
  (gr_text 100uF (at 170.815 109.855) (layer F.SilkS))
  (gr_text 100uF (at 211.455 109.855) (layer F.SilkS))
  (gr_text 10R (at 147.32 113.665) (layer F.SilkS))
  (gr_text 10R (at 233.045 113.665) (layer F.SilkS))
  (gr_text GND (at 225.425 123.19) (layer F.SilkS))
  (gr_text GND (at 225.425 120.65) (layer F.SilkS))
  (gr_text Right (at 225.425 118.11) (layer F.SilkS))
  (gr_text Left (at 225.425 125.73) (layer F.SilkS))
  (gr_text "Line In" (at 242.57 128.27 90) (layer F.SilkS))
  (gr_text 10k (at 218.44 127) (layer F.SilkS))
  (gr_text Active (at 186.69 151.765) (layer F.SilkS))
  (gr_text Power (at 193.675 151.765) (layer F.SilkS))
  (gr_text 1uF (at 199.39 99.06) (layer F.SilkS))
  (gr_text 1uF (at 181.61 99.06) (layer F.SilkS))
  (gr_text LED (at 190.5 90.805) (layer F.SilkS))
  (gr_text 12AU7 (at 190.5 100.33) (layer F.SilkS))
  (gr_text 470uF (at 208.28 100.965) (layer F.SilkS))
  (gr_text 470uF (at 172.72 100.965) (layer F.SilkS))
  (gr_text 100uF (at 202.565 78.74) (layer F.SilkS))
  (gr_text 100uF (at 169.545 78.74) (layer F.SilkS))
  (gr_text 3300uF (at 221.615 94.615) (layer F.SilkS))
  (gr_text 3300uF (at 221.615 75.565) (layer F.SilkS))
  (gr_text 3300uF (at 159.385 94.615) (layer F.SilkS))
  (gr_text 3300uF (at 159.385 75.565) (layer F.SilkS))
  (gr_text IRF510 (at 149.86 85.725 90) (layer F.SilkS))
  (gr_text IRF510 (at 231.14 85.725 270) (layer F.SilkS))
  (gr_text LM317 (at 231.14 103.505 270) (layer F.SilkS))
  (gr_text LM317 (at 149.86 103.505 90) (layer F.SilkS))
  (gr_text 150R (at 197.485 71.12 90) (layer F.SilkS))
  (gr_text 10uF (at 195.58 71.12 90) (layer F.SilkS))
  (gr_text 10uF (at 201.295 71.12 90) (layer F.SilkS))
  (gr_text 10uF (at 199.39 71.12 90) (layer F.SilkS))
  (gr_text LM317 (at 197.485 69.85) (layer F.SilkS))
  (gr_text 5k (at 179.705 64.135) (layer F.SilkS))
  (gr_text 10R (at 207.01 72.39) (layer F.SilkS))
  (gr_text 10R (at 173.99 72.39) (layer F.SilkS))
  (gr_text "Right Bias" (at 243.205 72.39 90) (layer F.SilkS))
  (gr_text GND (at 238.125 70.485 90) (layer F.SilkS))
  (gr_text GND (at 142.875 70.485 270) (layer F.SilkS))
  (gr_text "Left Bias" (at 137.795 73.025 270) (layer F.SilkS))
  (gr_text 50k (at 233.68 71.12) (layer F.SilkS))
  (gr_text 50k (at 147.32 71.12) (layer F.SilkS))
  (gr_text - (at 153.035 64.77) (layer F.SilkS))
  (gr_text + (at 153.035 67.31) (layer F.SilkS))
  (gr_text +15vDC (at 158.115 59.055 180) (layer F.SilkS))
  (dimension 95.25 (width 0.3) (layer Dwgs.User)
    (gr_text "3.7500 in" (at 252.29 104.775 90) (layer Dwgs.User))
    (feature1 (pts (xy 247.65 57.15) (xy 250.776421 57.15)))
    (feature2 (pts (xy 247.65 152.4) (xy 250.776421 152.4)))
    (crossbar (pts (xy 250.19 152.4) (xy 250.19 57.15)))
    (arrow1a (pts (xy 250.19 57.15) (xy 250.776421 58.276504)))
    (arrow1b (pts (xy 250.19 57.15) (xy 249.603579 58.276504)))
    (arrow2a (pts (xy 250.19 152.4) (xy 250.776421 151.273496)))
    (arrow2b (pts (xy 250.19 152.4) (xy 249.603579 151.273496)))
  )
  (gr_line (start 243.84 57.15) (end 243.84 152.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 57.15) (end 243.84 57.15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 152.4) (end 137.16 57.15) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 243.84 152.4) (end 137.16 152.4) (layer Edge.Cuts) (width 0.15))
  (dimension 53.34 (width 0.3) (layer Dwgs.User)
    (gr_text "2.1000 in" (at 163.83 162.12) (layer Dwgs.User))
    (feature1 (pts (xy 137.16 156.845) (xy 137.16 160.606421)))
    (feature2 (pts (xy 190.5 156.845) (xy 190.5 160.606421)))
    (crossbar (pts (xy 190.5 160.02) (xy 137.16 160.02)))
    (arrow1a (pts (xy 137.16 160.02) (xy 138.286504 159.433579)))
    (arrow1b (pts (xy 137.16 160.02) (xy 138.286504 160.606421)))
    (arrow2a (pts (xy 190.5 160.02) (xy 189.373496 159.433579)))
    (arrow2b (pts (xy 190.5 160.02) (xy 189.373496 160.606421)))
  )
  (dimension 53.34 (width 0.3) (layer Dwgs.User)
    (gr_text "2.1000 in" (at 217.17 162.119999) (layer Dwgs.User))
    (feature1 (pts (xy 243.84 156.845) (xy 243.84 160.60642)))
    (feature2 (pts (xy 190.5 156.845) (xy 190.5 160.60642)))
    (crossbar (pts (xy 190.5 160.019999) (xy 243.84 160.019999)))
    (arrow1a (pts (xy 243.84 160.019999) (xy 242.713496 160.60642)))
    (arrow1b (pts (xy 243.84 160.019999) (xy 242.713496 159.433578)))
    (arrow2a (pts (xy 190.5 160.019999) (xy 191.626504 160.60642)))
    (arrow2b (pts (xy 190.5 160.019999) (xy 191.626504 159.433578)))
  )
)
