(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 366)
    (zones 0)
    (modules 27)
    (nets 86)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 GND.Cu power)
    (2 PWR.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 1.35)
    (pad_drill 1.35)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 32 32)
    (grid_origin 32 32)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "build/"))
  )
  (net 0 "")
  (net 1 "Net-(AVR0-Pad17)")
  (net 2 "Net-(AVR0-Pad16)")
  (net 3 "Net-(AVR0-Pad6)")
  (net 4 "Net-(CPUIN0-Pad2)")
  (net 5 "Net-(CPUIN0-Pad4)")
  (net 6 "Net-(DATA2-Pad7)")
  (net 7 "Net-(DATA2-Pad6)")
  (net 8 "Net-(DATA2-Pad5)")
  (net 9 "Net-(DATA2-Pad4)")
  (net 10 "Net-(DATA2-Pad3)")
  (net 11 "Net-(DATA2-Pad2)")
  (net 12 "Net-(DATA2-Pad1)")
  (net 13 "Net-(DATA3-Pad7)")
  (net 14 "Net-(DATA3-Pad6)")
  (net 15 "Net-(DATA3-Pad5)")
  (net 16 "Net-(DATA3-Pad4)")
  (net 17 "Net-(DATA3-Pad3)")
  (net 18 "Net-(DATA3-Pad2)")
  (net 19 "Net-(DATA3-Pad1)")
  (net 20 "Net-(DATA0-Pad7)")
  (net 21 "Net-(DATA0-Pad6)")
  (net 22 "Net-(DATA0-Pad5)")
  (net 23 "Net-(DATA0-Pad4)")
  (net 24 "Net-(DATA0-Pad3)")
  (net 25 "Net-(DATA0-Pad2)")
  (net 26 "Net-(DATA0-Pad1)")
  (net 27 "Net-(DATA1-Pad7)")
  (net 28 "Net-(DATA1-Pad6)")
  (net 29 "Net-(DATA1-Pad5)")
  (net 30 "Net-(DATA1-Pad4)")
  (net 31 "Net-(DATA1-Pad3)")
  (net 32 "Net-(DATA1-Pad2)")
  (net 33 "Net-(DATA1-Pad1)")
  (net 34 "Net-(AVR0-Pad3)")
  (net 35 "Net-(AVR0-Pad4)")
  (net 36 "Net-(AVR0-Pad42)")
  (net 37 "Net-(PFP0-Pad4)")
  (net 38 "Net-(R1-Pad1)")
  (net 39 OC3A)
  (net 40 OC1B)
  (net 41 OC1A)
  (net 42 ADC10)
  (net 43 ADC9)
  (net 44 ADC8)
  (net 45 "Net-(CPUMUX0-Pad3)")
  (net 46 "Net-(CPUMUX0-Pad5)")
  (net 47 VCC)
  (net 48 PE6)
  (net 49 GND)
  (net 50 XCK1)
  (net 51 TXD1)
  (net 52 RXD1)
  (net 53 SDA)
  (net 54 SCL)
  (net 55 MISO)
  (net 56 MOSI)
  (net 57 SCLK)
  (net 58 SS)
  (net 59 "Net-(R0-Pad1)")
  (net 60 RTS)
  (net 61 HWB)
  (net 62 ADC7)
  (net 63 ADC6)
  (net 64 ADC5)
  (net 65 ADC4)
  (net 66 ADC1)
  (net 67 ADC0)
  (net 68 OC4A)
  (net 69 PB4)
  (net 70 RST)
  (net 71 +12V)
  (net 72 +5V)
  (net 73 "Net-(SATA0-Pad10)")
  (net 74 "Net-(SATA0-Pad9)")
  (net 75 "Net-(SATA0-Pad8)")
  (net 76 "Net-(SATA1-Pad10)")
  (net 77 "Net-(SATA1-Pad9)")
  (net 78 "Net-(SATA1-Pad8)")
  (net 79 "Net-(SATA2-Pad10)")
  (net 80 "Net-(SATA2-Pad9)")
  (net 81 "Net-(SATA2-Pad8)")
  (net 82 "Net-(SATA3-Pad10)")
  (net 83 "Net-(SATA3-Pad9)")
  (net 84 "Net-(SATA3-Pad8)")
  (net 85 "Net-(PMB0-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net ADC0)
    (add_net ADC1)
    (add_net ADC10)
    (add_net ADC4)
    (add_net ADC5)
    (add_net ADC6)
    (add_net ADC7)
    (add_net ADC8)
    (add_net ADC9)
    (add_net GND)
    (add_net HWB)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(AVR0-Pad16)")
    (add_net "Net-(AVR0-Pad17)")
    (add_net "Net-(AVR0-Pad3)")
    (add_net "Net-(AVR0-Pad4)")
    (add_net "Net-(AVR0-Pad42)")
    (add_net "Net-(AVR0-Pad6)")
    (add_net "Net-(CPUIN0-Pad2)")
    (add_net "Net-(CPUIN0-Pad4)")
    (add_net "Net-(CPUMUX0-Pad3)")
    (add_net "Net-(CPUMUX0-Pad5)")
    (add_net "Net-(DATA0-Pad1)")
    (add_net "Net-(DATA0-Pad2)")
    (add_net "Net-(DATA0-Pad3)")
    (add_net "Net-(DATA0-Pad4)")
    (add_net "Net-(DATA0-Pad5)")
    (add_net "Net-(DATA0-Pad6)")
    (add_net "Net-(DATA0-Pad7)")
    (add_net "Net-(DATA1-Pad1)")
    (add_net "Net-(DATA1-Pad2)")
    (add_net "Net-(DATA1-Pad3)")
    (add_net "Net-(DATA1-Pad4)")
    (add_net "Net-(DATA1-Pad5)")
    (add_net "Net-(DATA1-Pad6)")
    (add_net "Net-(DATA1-Pad7)")
    (add_net "Net-(DATA2-Pad1)")
    (add_net "Net-(DATA2-Pad2)")
    (add_net "Net-(DATA2-Pad3)")
    (add_net "Net-(DATA2-Pad4)")
    (add_net "Net-(DATA2-Pad5)")
    (add_net "Net-(DATA2-Pad6)")
    (add_net "Net-(DATA2-Pad7)")
    (add_net "Net-(DATA3-Pad1)")
    (add_net "Net-(DATA3-Pad2)")
    (add_net "Net-(DATA3-Pad3)")
    (add_net "Net-(DATA3-Pad4)")
    (add_net "Net-(DATA3-Pad5)")
    (add_net "Net-(DATA3-Pad6)")
    (add_net "Net-(DATA3-Pad7)")
    (add_net "Net-(PFP0-Pad4)")
    (add_net "Net-(PMB0-Pad3)")
    (add_net "Net-(R0-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(SATA0-Pad10)")
    (add_net "Net-(SATA0-Pad8)")
    (add_net "Net-(SATA0-Pad9)")
    (add_net "Net-(SATA1-Pad10)")
    (add_net "Net-(SATA1-Pad8)")
    (add_net "Net-(SATA1-Pad9)")
    (add_net "Net-(SATA2-Pad10)")
    (add_net "Net-(SATA2-Pad8)")
    (add_net "Net-(SATA2-Pad9)")
    (add_net "Net-(SATA3-Pad10)")
    (add_net "Net-(SATA3-Pad8)")
    (add_net "Net-(SATA3-Pad9)")
    (add_net OC1A)
    (add_net OC1B)
    (add_net OC3A)
    (add_net OC4A)
    (add_net PB4)
    (add_net PE6)
    (add_net RST)
    (add_net RTS)
    (add_net RXD1)
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net SS)
    (add_net TXD1)
    (add_net VCC)
    (add_net XCK1)
  )
  (module SATA:ATA_FLOPPY_POWER_4 (layer B.Cu) (tedit 5B98213B)
    (at 96.71 99.99 180)
    (descr "Molex ATA Power Connector")
    (attr smd)
    (fp_text reference POWER0 (at 0 4.165 180) (layer B.SilkS))
    (fp_text value ATA_FLOPPY_POWER_4 (at 0 3.5 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 3.75 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 72 +5V))
    (pad 3 thru_hole oval (at 1.25 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 2 thru_hole oval (at -1.25 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 1 thru_hole rect (at -3.75 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 71 +12V))
    (model ${KIPRJMOD}/lib/SATA/ATA_FLOPPY_POWER_4.stp
      (offset (xyz 0 0 10.4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 48.51 97.45 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (attr smd)
    (fp_text reference USB0 (at 2.54 -7.62 180) (layer B.SilkS))
    (fp_text value USB_IDC (at 0 -9.95 90) (layer B.Fab))
    (fp_text user %R (at 0 -3.81) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(R0-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(R1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 VCC))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer B.Cu) (tedit 59FED5CC)
    (at 47.18 50.46)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference ICSP0 (at 0 4.87) (layer B.SilkS))
    (fp_text value Conn_02x03_Odd_Even (at 0 -4.87) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 6 smd rect (at 2.525 -2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 5 smd rect (at -2.525 -2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 70 RST))
    (pad 4 smd rect (at 2.525 0) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 56 MOSI))
    (pad 3 smd rect (at -2.525 0) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 57 SCLK))
    (pad 2 smd rect (at 2.525 2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 1 smd rect (at -2.525 2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 55 MISO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_TL3342 (layer B.Cu) (tedit 5A02FC95)
    (at 37.15 59.35 180)
    (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
    (tags "SPST Tactile Switch")
    (attr smd)
    (fp_text reference B0 (at 0 -4.05) (layer B.SilkS))
    (fp_text value SW_SPST (at 0 -3.75 180) (layer B.Fab))
    (fp_text user %R (at 0 3.75 180) (layer B.Fab))
    (pad 2 smd rect (at 3.15 -1.9 180) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 69 PB4))
    (pad 2 smd rect (at -3.15 -1.9 180) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 69 PB4))
    (pad 1 smd rect (at 3.15 1.9 180) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 1 smd rect (at -3.15 1.9 180) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_TL3342.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SATA:SATA_DATA_7 (layer B.Cu) (tedit 5B9A7444)
    (at 61.275 52.22 180)
    (descr "SATA 7-pin Male Data Connector")
    (attr smd)
    (fp_text reference DATA1 (at 0 -7.5 180) (layer B.SilkS))
    (fp_text value SATA_DATA_7 (at 0 0.5 180) (layer B.Fab))
    (pad "" np_thru_hole oval (at -7.195 -2.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 5.635 -3.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -4.445 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(DATA1-Pad1)"))
    (pad 2 smd rect (at -3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(DATA1-Pad2)"))
    (pad 3 smd rect (at -1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(DATA1-Pad3)"))
    (pad 4 smd rect (at -0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(DATA1-Pad4)"))
    (pad 5 smd rect (at 0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(DATA1-Pad5)"))
    (pad 6 smd rect (at 1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(DATA1-Pad6)"))
    (pad 7 smd rect (at 3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(DATA1-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_DATA_7.stp
      (offset (xyz -0.82 -3.28 4.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SATA:SATA_DATA_7 (layer B.Cu) (tedit 5B9A7444)
    (at 61.275 36.22 180)
    (descr "SATA 7-pin Male Data Connector")
    (attr smd)
    (fp_text reference DATA0 (at 0 -7.5 180) (layer B.SilkS))
    (fp_text value SATA_DATA_7 (at 0 0.5 180) (layer B.Fab))
    (pad "" np_thru_hole oval (at -7.195 -2.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 5.635 -3.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -4.445 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(DATA0-Pad1)"))
    (pad 2 smd rect (at -3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(DATA0-Pad2)"))
    (pad 3 smd rect (at -1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(DATA0-Pad3)"))
    (pad 4 smd rect (at -0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(DATA0-Pad4)"))
    (pad 5 smd rect (at 0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(DATA0-Pad5)"))
    (pad 6 smd rect (at 1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(DATA0-Pad6)"))
    (pad 7 smd rect (at 3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(DATA0-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_DATA_7.stp
      (offset (xyz -0.82 -3.28 4.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SATA:SATA_DATA_7 (layer B.Cu) (tedit 5B9A7444)
    (at 61.275 84.22 180)
    (descr "SATA 7-pin Male Data Connector")
    (attr smd)
    (fp_text reference DATA3 (at 0 -7.5 180) (layer B.SilkS))
    (fp_text value SATA_DATA_7 (at 0 0.5 180) (layer B.Fab))
    (pad "" np_thru_hole oval (at -7.195 -2.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 5.635 -3.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -4.445 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(DATA3-Pad1)"))
    (pad 2 smd rect (at -3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(DATA3-Pad2)"))
    (pad 3 smd rect (at -1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(DATA3-Pad3)"))
    (pad 4 smd rect (at -0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(DATA3-Pad4)"))
    (pad 5 smd rect (at 0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(DATA3-Pad5)"))
    (pad 6 smd rect (at 1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(DATA3-Pad6)"))
    (pad 7 smd rect (at 3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(DATA3-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_DATA_7.stp
      (offset (xyz -0.82 -3.28 4.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SATA:SATA_DATA_7 (layer B.Cu) (tedit 5B9A7444)
    (at 61.275 68.57 180)
    (descr "SATA 7-pin Male Data Connector")
    (attr smd)
    (fp_text reference DATA2 (at 0 -7.5 180) (layer B.SilkS))
    (fp_text value SATA_DATA_7 (at 0 0.5 180) (layer B.Fab))
    (pad "" np_thru_hole oval (at -7.195 -2.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 5.635 -3.54 180) (size 1.35 1.35) (drill 1.35) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -4.445 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(DATA2-Pad1)"))
    (pad 2 smd rect (at -3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(DATA2-Pad2)"))
    (pad 3 smd rect (at -1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(DATA2-Pad3)"))
    (pad 4 smd rect (at -0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(DATA2-Pad4)"))
    (pad 5 smd rect (at 0.635 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(DATA2-Pad5)"))
    (pad 6 smd rect (at 1.905 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(DATA2-Pad6)"))
    (pad 7 smd rect (at 3.175 -2.54 180) (size 0.9 2.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(DATA2-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_DATA_7.stp
      (offset (xyz -0.82 -3.28 4.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 34.2 71.75)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.2) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(AVR0-Pad16)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer B.Cu) (tedit 5B301BBE)
    (at 42.7 80.305 270)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C0 (at 1.545 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(AVR0-Pad6)"))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0201_0603Metric (layer F.Cu) (tedit 5B301BBE)
    (at 34.2 70.95)
    (descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.05) (layer F.Fab))
    (fp_text user %R (at 0 -0.68) (layer F.Fab))
    (pad 2 smd roundrect (at 0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(AVR0-Pad17)"))
    (pad 1 smd roundrect (at -0.32 0) (size 0.46 0.4) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 49 GND))
    (pad "" smd roundrect (at 0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0) (size 0.318 0.36) (layers F.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_0603-2Pin_6.0x3.5mm (layer F.Cu) (tedit 5A0FD1B2)
    (at 37.4 71.35 90)
    (descr "SMD Crystal SERIES SMD0603/2 http://www.petermann-technik.de/fileadmin/petermann/pdf/SMD0603-2.pdf, 6.0x3.5mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y0 (at 4.23 0 180) (layer F.SilkS))
    (fp_text value 16MHz (at 0 2.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2.2 0 90) (size 1.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(AVR0-Pad17)"))
    (pad 1 smd rect (at -2.2 0 90) (size 1.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(AVR0-Pad16)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_0603-2Pin_6.0x3.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 43.43 94.91 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R0 (at 1.27 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(AVR0-Pad4)"))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(R0-Pad1)"))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 45.97 94.91 90)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.27 0 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.05 90) (layer B.Fab))
    (fp_text user %R (at 0 0.68 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(AVR0-Pad3)"))
    (pad 1 smd roundrect (at -0.32 0 90) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R1-Pad1)"))
    (pad "" smd roundrect (at 0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 90) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0201_0603Metric (layer B.Cu) (tedit 5B301BBD)
    (at 54.86 98.72 270)
    (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.59 0) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.05 270) (layer B.Fab))
    (fp_text user %R (at 0 0.68 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(PFP0-Pad4)"))
    (pad 1 smd roundrect (at -0.32 0 270) (size 0.46 0.4) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 68 OC4A))
    (pad "" smd roundrect (at 0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.345 0 270) (size 0.318 0.36) (layers B.Paste) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:FanPinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 5A19DE55)
    (at 77.72 99.99 180)
    (descr "4-pin CPU fan Through hole pin header, e.g. for Wieson part number 2366C888-007 Molex 47053-1000, Foxconn HF27040-M1, Tyco 1470947-1 or equivalent, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
    (tags "pin header 4-pin CPU fan")
    (attr smd)
    (fp_text reference CPUOUT0 (at 4 4.165 180) (layer B.SilkS))
    (fp_text value Fan_Tacho_PWM (at 4.05 -4.35 180) (layer B.Fab))
    (fp_text user %R (at 1.85 1.75 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.16 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 "Net-(CPUMUX0-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 65 ADC4))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 71 +12V))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:VSSOP-8_2.4x2.1mm_P0.5mm (layer B.Cu) (tedit 5A02F25C)
    (at 48.225 85.03 90)
    (descr http://www.ti.com/lit/ml/mpds050d/mpds050d.pdf)
    (tags "VSSOP DCU R-PDSO-G8 Pitch0.5mm")
    (attr smd)
    (fp_text reference CPUMUX0 (at -2.895 -0.115 180) (layer B.SilkS))
    (fp_text value 74LVC2G157 (at 0 -2.413 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 8 smd rect (at 1.55 0.75 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 7 smd rect (at 1.55 0.25 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 6 smd rect (at 1.55 -0.25 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 48 PE6))
    (pad 5 smd rect (at 1.55 -0.75 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(CPUMUX0-Pad5)"))
    (pad 4 smd rect (at -1.55 -0.75 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 3 smd rect (at -1.55 -0.25 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(CPUMUX0-Pad3)"))
    (pad 2 smd rect (at -1.55 0.25 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 41 OC1A))
    (pad 1 smd rect (at -1.55 0.75 90) (size 0.75 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(CPUIN0-Pad4)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/VSSOP-8_2.4x2.1mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-44_10x10mm_P0.8mm (layer B.Cu) (tedit 5A02F146)
    (at 42.7 70.95 90)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference AVR0 (at -7.700001 -0.0675 180) (layer B.SilkS))
    (fp_text value ATmega32U4-AU (at 0 -7.45 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 44 smd rect (at -4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 43 smd rect (at -3.2 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 42 smd rect (at -2.4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(AVR0-Pad42)"))
    (pad 41 smd rect (at -1.6 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 67 ADC0))
    (pad 40 smd rect (at -0.8 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 66 ADC1))
    (pad 39 smd rect (at 0 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 65 ADC4))
    (pad 38 smd rect (at 0.8 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 64 ADC5))
    (pad 37 smd rect (at 1.6 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 63 ADC6))
    (pad 36 smd rect (at 2.4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 62 ADC7))
    (pad 35 smd rect (at 3.2 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 34 smd rect (at 4 5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 33 smd rect (at 5.7 4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 61 HWB))
    (pad 32 smd rect (at 5.7 3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 68 OC4A))
    (pad 31 smd rect (at 5.7 2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 39 OC3A))
    (pad 30 smd rect (at 5.7 1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 40 OC1B))
    (pad 29 smd rect (at 5.7 0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 41 OC1A))
    (pad 28 smd rect (at 5.7 0 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 69 PB4))
    (pad 27 smd rect (at 5.7 -0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 42 ADC10))
    (pad 26 smd rect (at 5.7 -1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 43 ADC9))
    (pad 25 smd rect (at 5.7 -2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 44 ADC8))
    (pad 24 smd rect (at 5.7 -3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 23 smd rect (at 5.7 -4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 22 smd rect (at 4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 50 XCK1))
    (pad 21 smd rect (at 3.2 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 51 TXD1))
    (pad 20 smd rect (at 2.4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 52 RXD1))
    (pad 19 smd rect (at 1.6 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 53 SDA))
    (pad 18 smd rect (at 0.8 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 54 SCL))
    (pad 17 smd rect (at 0 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(AVR0-Pad17)"))
    (pad 16 smd rect (at -0.8 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(AVR0-Pad16)"))
    (pad 15 smd rect (at -1.6 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 14 smd rect (at -2.4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 13 smd rect (at -3.2 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 70 RST))
    (pad 12 smd rect (at -4 -5.7) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 60 RTS))
    (pad 11 smd rect (at -5.7 -4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 55 MISO))
    (pad 10 smd rect (at -5.7 -3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 56 MOSI))
    (pad 9 smd rect (at -5.7 -2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 57 SCLK))
    (pad 8 smd rect (at -5.7 -1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 58 SS))
    (pad 7 smd rect (at -5.7 -0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 6 smd rect (at -5.7 0 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(AVR0-Pad6)"))
    (pad 5 smd rect (at -5.7 0.8 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 49 GND))
    (pad 4 smd rect (at -5.7 1.6 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(AVR0-Pad4)"))
    (pad 3 smd rect (at -5.7 2.4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(AVR0-Pad3)"))
    (pad 2 smd rect (at -5.7 3.2 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 VCC))
    (pad 1 smd rect (at -5.7 4 90) (size 1.5 0.55) (layers B.Cu B.Paste B.Mask)
      (net 48 PE6))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-44_10x10mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 35.81 101.26 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (attr smd)
    (fp_text reference PMB0 (at -2.54 -1.27) (layer B.SilkS))
    (fp_text value SW_Push_LED (at 0 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 ADC0))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(PMB0-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 PB4))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:FanPinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 5A19DE55)
    (at 66.29 99.99 180)
    (descr "4-pin CPU fan Through hole pin header, e.g. for Wieson part number 2366C888-007 Molex 47053-1000, Foxconn HF27040-M1, Tyco 1470947-1 or equivalent, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
    (tags "pin header 4-pin CPU fan")
    (attr smd)
    (fp_text reference CPUIN0 (at 4 4.165 180) (layer B.SilkS))
    (fp_text value Fan_Tacho_PWM (at 4.05 -4.35 180) (layer B.Fab))
    (fp_text user %R (at 1.85 1.75 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.16 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 "Net-(CPUIN0-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 65 ADC4))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 "Net-(CPUIN0-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector:FanPinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 5A19DE55)
    (at 89.15 99.99 180)
    (descr "4-pin CPU fan Through hole pin header, e.g. for Wieson part number 2366C888-007 Molex 47053-1000, Foxconn HF27040-M1, Tyco 1470947-1 or equivalent, see http://www.formfactors.org/developer%5Cspecs%5Crev1_2_public.pdf")
    (tags "pin header 4-pin CPU fan")
    (attr smd)
    (fp_text reference INTAKE0 (at 4 4.165 180) (layer B.SilkS))
    (fp_text value Fan_Tacho_PWM (at 4.05 -4.35 180) (layer B.Fab))
    (fp_text user %R (at 1.85 1.75 180) (layer B.Fab))
    (pad "" np_thru_hole circle (at 5.08 2.16 90) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 OC1B))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 64 ADC5))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 71 +12V))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.03 1.73) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Connector.3dshapes/FanPinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 47.24 101.26 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (attr smd)
    (fp_text reference PFP0 (at -2.54 -5.08) (layer B.SilkS))
    (fp_text value SW_Push_LED (at 0 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(PFP0-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 ADC1))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SATA:SATA_COMBINED_22 (layer F.Cu) (tedit 5B98214F)
    (at 73.975 91.65)
    (descr "SATA 22-pin Female Data and Power Connector")
    (attr smd)
    (fp_text reference SATA3 (at 0 4.175) (layer F.SilkS))
    (fp_text value SATA_COMBINED_22 (at 0 -3.175) (layer F.Fab))
    (pad "" connect rect (at -21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" connect rect (at 21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -18.4 0.9) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 18.4 0.85) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad 22 smd rect (at 15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 21 smd rect (at 14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 20 smd rect (at 13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 19 smd rect (at 12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 18 smd rect (at 10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 17 smd rect (at 9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 16 smd rect (at 8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 15 smd rect (at 6.985 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 14 smd rect (at 5.715 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 13 smd rect (at 4.445 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 12 smd rect (at 3.175 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 11 smd rect (at 1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 10 smd rect (at 0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(SATA3-Pad10)"))
    (pad 9 smd rect (at -0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(SATA3-Pad9)"))
    (pad 8 smd rect (at -1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(SATA3-Pad8)"))
    (pad 7 smd rect (at -8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(DATA3-Pad1)"))
    (pad 6 smd rect (at -9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(DATA3-Pad2)"))
    (pad 5 smd rect (at -10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(DATA3-Pad3)"))
    (pad 4 smd rect (at -12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(DATA3-Pad4)"))
    (pad 3 smd rect (at -13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(DATA3-Pad5)"))
    (pad 2 smd rect (at -14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(DATA3-Pad6)"))
    (pad 1 smd rect (at -15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(DATA3-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_COMBINED_22.stp
      (offset (xyz 0 -0.6 6.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:SATA_COMBINED_22 (layer F.Cu) (tedit 5B98214F)
    (at 73.975 75.65)
    (descr "SATA 22-pin Female Data and Power Connector")
    (attr smd)
    (fp_text reference SATA2 (at 0 4.175) (layer F.SilkS))
    (fp_text value SATA_COMBINED_22 (at 0 -3.175) (layer F.Fab))
    (pad "" connect rect (at -21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" connect rect (at 21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -18.4 0.9) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 18.4 0.85) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad 22 smd rect (at 15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 21 smd rect (at 14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 20 smd rect (at 13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 19 smd rect (at 12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 18 smd rect (at 10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 17 smd rect (at 9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 16 smd rect (at 8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 15 smd rect (at 6.985 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 14 smd rect (at 5.715 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 13 smd rect (at 4.445 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 12 smd rect (at 3.175 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 11 smd rect (at 1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 10 smd rect (at 0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(SATA2-Pad10)"))
    (pad 9 smd rect (at -0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(SATA2-Pad9)"))
    (pad 8 smd rect (at -1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(SATA2-Pad8)"))
    (pad 7 smd rect (at -8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(DATA2-Pad1)"))
    (pad 6 smd rect (at -9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(DATA2-Pad2)"))
    (pad 5 smd rect (at -10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(DATA2-Pad3)"))
    (pad 4 smd rect (at -12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(DATA2-Pad4)"))
    (pad 3 smd rect (at -13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(DATA2-Pad5)"))
    (pad 2 smd rect (at -14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(DATA2-Pad6)"))
    (pad 1 smd rect (at -15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(DATA2-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_COMBINED_22.stp
      (offset (xyz 0 -0.6 6.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:SATA_COMBINED_22 (layer F.Cu) (tedit 5B98214F)
    (at 73.975 59.65)
    (descr "SATA 22-pin Female Data and Power Connector")
    (attr smd)
    (fp_text reference SATA1 (at 0 4.175) (layer F.SilkS))
    (fp_text value SATA_COMBINED_22 (at 0 -3.175) (layer F.Fab))
    (pad "" connect rect (at -21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" connect rect (at 21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -18.4 0.9) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 18.4 0.85) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad 22 smd rect (at 15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 21 smd rect (at 14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 20 smd rect (at 13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 19 smd rect (at 12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 18 smd rect (at 10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 17 smd rect (at 9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 16 smd rect (at 8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 15 smd rect (at 6.985 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 14 smd rect (at 5.715 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 13 smd rect (at 4.445 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 12 smd rect (at 3.175 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 11 smd rect (at 1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 10 smd rect (at 0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(SATA1-Pad10)"))
    (pad 9 smd rect (at -0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(SATA1-Pad9)"))
    (pad 8 smd rect (at -1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(SATA1-Pad8)"))
    (pad 7 smd rect (at -8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(DATA1-Pad1)"))
    (pad 6 smd rect (at -9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(DATA1-Pad2)"))
    (pad 5 smd rect (at -10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(DATA1-Pad3)"))
    (pad 4 smd rect (at -12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(DATA1-Pad4)"))
    (pad 3 smd rect (at -13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(DATA1-Pad5)"))
    (pad 2 smd rect (at -14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(DATA1-Pad6)"))
    (pad 1 smd rect (at -15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(DATA1-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_COMBINED_22.stp
      (offset (xyz 0 -0.6 6.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SATA:SATA_COMBINED_22 (layer F.Cu) (tedit 5B98214F)
    (at 73.975 43.65)
    (descr "SATA 22-pin Female Data and Power Connector")
    (attr smd)
    (fp_text reference SATA0 (at 0 4.175) (layer F.SilkS))
    (fp_text value SATA_COMBINED_22 (at 0 -3.175) (layer F.Fab))
    (pad "" connect rect (at -21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" connect rect (at 21.35 0.6) (size 2.1 2.2) (layers F.Cu F.Mask))
    (pad "" np_thru_hole circle (at -18.4 0.9) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 18.4 0.85) (size 2.1 2.1) (drill 2.1) (layers *.Cu *.Mask))
    (pad 22 smd rect (at 15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 21 smd rect (at 14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 20 smd rect (at 13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 71 +12V))
    (pad 19 smd rect (at 12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 18 smd rect (at 10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 17 smd rect (at 9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 16 smd rect (at 8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 15 smd rect (at 6.985 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 14 smd rect (at 5.715 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 72 +5V))
    (pad 13 smd rect (at 4.445 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 12 smd rect (at 3.175 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 11 smd rect (at 1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 49 GND))
    (pad 10 smd rect (at 0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(SATA0-Pad10)"))
    (pad 9 smd rect (at -0.635 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(SATA0-Pad9)"))
    (pad 8 smd rect (at -1.905 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(SATA0-Pad8)"))
    (pad 7 smd rect (at -8.255 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(DATA0-Pad1)"))
    (pad 6 smd rect (at -9.525 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(DATA0-Pad2)"))
    (pad 5 smd rect (at -10.795 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(DATA0-Pad3)"))
    (pad 4 smd rect (at -12.065 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(DATA0-Pad4)"))
    (pad 3 smd rect (at -13.335 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(DATA0-Pad5)"))
    (pad 2 smd rect (at -14.605 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(DATA0-Pad6)"))
    (pad 1 smd rect (at -15.875 0) (size 0.6 3.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(DATA0-Pad7)"))
    (model ${KIPRJMOD}/lib/SATA/SATA_COMBINED_22.stp
      (offset (xyz 0 -0.6 6.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Logo:System76 (layer B.Cu) (tedit 0)
    (at 87.945 37 180)
    (attr virtual)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_arc (start 107.45 85.4) (end 107.45 87) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 87) (end 107.45 87) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 48.8) (end 107.45 48.8) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 107.45 50.4) (end 109.05 50.4) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 109.05 50.4) (end 109.05 85.4) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 30.4 50.4) (end 30.4 48.8) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 28.8 85.4) (end 28.8 50.4) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 30.4 85.4) (end 28.8 85.4) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 87) (end 30.4 87) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 48.8) (end 30.4 48.8) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 87) (end 32 100.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32 48.8) (end 32 35.2) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 87) (end 105.85 100.6) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 105.85 48.8) (end 105.85 35.2) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 102.65 100.6) (end 102.65 103.8) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 35.2 100.6) (end 32 100.6) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 102.65 103.8) (end 35.2 103.8) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 35.2 35.2) (end 35.2 32) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 102.65 35.2) (end 105.85 35.2) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 35.2 32) (end 102.65 32) (layer Edge.Cuts) (width 0.2))
  (zone (net 49) (net_name GND) (layer GND.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32 32) (xy 105.85 32) (xy 105.85 104) (xy 32 104)
      )
    )
  )
  (zone (net 71) (net_name +12V) (layer PWR.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68 32) (xy 105.85 32) (xy 105.85 104) (xy 68 104)
      )
    )
  )
  (zone (net 47) (net_name VCC) (layer PWR.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.8 104) (xy 32 104) (xy 32 32) (xy 52.8 32)
      )
    )
  )
)
