(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 49)
    (tracks 831)
    (zones 0)
    (modules 46)
    (nets 93)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 89.916 40.64)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(1uF1-Pad2)")
  (net 2 "Net-(BUFFER-1-Pad1)")
  (net 3 "Net-(BUFFER-1-Pad2)")
  (net 4 "Net-(BUFFER-2-Pad1)")
  (net 5 "Net-(BUFFER-2-Pad2)")
  (net 6 "Net-(BUFFER-3-Pad1)")
  (net 7 "Net-(BUFFER-3-Pad2)")
  (net 8 "Net-(BUFFER-4-Pad1)")
  (net 9 "Net-(BUFFER-4-Pad2)")
  (net 10 "Net-(BUFFER-5-Pad2)")
  (net 11 "Net-(BUFFER-5-Pad1)")
  (net 12 "Net-(BUFFER-6-Pad2)")
  (net 13 "Net-(BUFFER-6-Pad1)")
  (net 14 "Net-(BUFFER-7-Pad2)")
  (net 15 "Net-(BUFFER-7-Pad1)")
  (net 16 "Net-(BUFFER-8-Pad2)")
  (net 17 "Net-(BUFFER-8-Pad1)")
  (net 18 "Net-(BUFFER-9-Pad1)")
  (net 19 "Net-(BUFFER-9-Pad2)")
  (net 20 "Net-(POGO-PCA-IN-1-Pad9)")
  (net 21 "Net-(POGO-PCA-IN-1-Pad8)")
  (net 22 "Net-(POGO-PCA-IN-1-Pad6)")
  (net 23 "Net-(POGO-PCA-IN-1-Pad5)")
  (net 24 "Net-(POGO-PCA-IN-1-Pad4)")
  (net 25 "Net-(POGO-PCA-IN-1-Pad2)")
  (net 26 "Net-(POGO-PCA-IN-1-Pad1)")
  (net 27 "Net-(POGO-PCA-IN-2-Pad9)")
  (net 28 "Net-(POGO-PCA-IN-2-Pad8)")
  (net 29 "Net-(POGO-PCA-IN-2-Pad6)")
  (net 30 "Net-(POGO-PCA-IN-2-Pad5)")
  (net 31 "Net-(POGO-PCA-IN-2-Pad4)")
  (net 32 "Net-(POGO-PCA-IN-2-Pad2)")
  (net 33 "Net-(POGO-PCA-IN-2-Pad1)")
  (net 34 "Net-(POGO-PCA-IN-3-Pad1)")
  (net 35 "Net-(POGO-PCA-IN-3-Pad2)")
  (net 36 "Net-(POGO-PCA-IN-3-Pad4)")
  (net 37 "Net-(POGO-PCA-IN-3-Pad5)")
  (net 38 "Net-(POGO-PCA-IN-3-Pad6)")
  (net 39 "Net-(POGO-PCA-IN-3-Pad8)")
  (net 40 "Net-(POGO-PCA-IN-3-Pad9)")
  (net 41 "Net-(POGO-PCA-IN-4-Pad1)")
  (net 42 "Net-(POGO-PCA-IN-4-Pad2)")
  (net 43 "Net-(POGO-PCA-IN-4-Pad4)")
  (net 44 "Net-(POGO-PCA-IN-4-Pad5)")
  (net 45 "Net-(POGO-PCA-IN-4-Pad6)")
  (net 46 "Net-(POGO-PCA-IN-4-Pad8)")
  (net 47 "Net-(POGO-PCA-IN-4-Pad9)")
  (net 48 "Net-(POGO-PCA-IN-5-Pad9)")
  (net 49 "Net-(POGO-PCA-IN-5-Pad8)")
  (net 50 "Net-(POGO-PCA-IN-5-Pad6)")
  (net 51 "Net-(POGO-PCA-IN-5-Pad5)")
  (net 52 "Net-(POGO-PCA-IN-5-Pad4)")
  (net 53 "Net-(POGO-PCA-IN-5-Pad2)")
  (net 54 "Net-(POGO-PCA-IN-5-Pad1)")
  (net 55 "Net-(POGO-PCA-IN-6-Pad9)")
  (net 56 "Net-(POGO-PCA-IN-6-Pad8)")
  (net 57 "Net-(POGO-PCA-IN-6-Pad6)")
  (net 58 "Net-(POGO-PCA-IN-6-Pad5)")
  (net 59 "Net-(POGO-PCA-IN-6-Pad4)")
  (net 60 "Net-(POGO-PCA-IN-6-Pad2)")
  (net 61 "Net-(POGO-PCA-IN-6-Pad1)")
  (net 62 "Net-(POGO-PCA-IN-7-Pad1)")
  (net 63 "Net-(POGO-PCA-IN-7-Pad2)")
  (net 64 "Net-(POGO-PCA-IN-7-Pad4)")
  (net 65 "Net-(POGO-PCA-IN-7-Pad5)")
  (net 66 "Net-(POGO-PCA-IN-7-Pad6)")
  (net 67 "Net-(POGO-PCA-IN-7-Pad8)")
  (net 68 "Net-(POGO-PCA-IN-7-Pad9)")
  (net 69 "Net-(POGO-PCA-IN-8-Pad9)")
  (net 70 "Net-(POGO-PCA-IN-8-Pad8)")
  (net 71 "Net-(POGO-PCA-IN-8-Pad6)")
  (net 72 "Net-(POGO-PCA-IN-8-Pad5)")
  (net 73 "Net-(POGO-PCA-IN-8-Pad4)")
  (net 74 "Net-(POGO-PCA-IN-8-Pad2)")
  (net 75 "Net-(POGO-PCA-IN-8-Pad1)")
  (net 76 "Net-(POGO-PCA-IN-9-Pad9)")
  (net 77 "Net-(POGO-PCA-IN-9-Pad8)")
  (net 78 "Net-(POGO-PCA-IN-9-Pad6)")
  (net 79 "Net-(POGO-PCA-IN-9-Pad5)")
  (net 80 "Net-(POGO-PCA-IN-9-Pad4)")
  (net 81 "Net-(POGO-PCA-IN-9-Pad2)")
  (net 82 "Net-(POGO-PCA-IN-9-Pad1)")
  (net 83 "Net-(10nF10-Pad2)")
  (net 84 "Net-(10nF10-Pad1)")
  (net 85 "Net-(10nF11-Pad2)")
  (net 86 "Net-(10nF12-Pad2)")
  (net 87 "Net-(10nF13-Pad2)")
  (net 88 "Net-(10nF14-Pad2)")
  (net 89 "Net-(10nF15-Pad2)")
  (net 90 "Net-(10nF16-Pad2)")
  (net 91 "Net-(10nF17-Pad2)")
  (net 92 "Net-(10nF18-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(10nF10-Pad1)")
    (add_net "Net-(10nF10-Pad2)")
    (add_net "Net-(10nF11-Pad2)")
    (add_net "Net-(10nF12-Pad2)")
    (add_net "Net-(10nF13-Pad2)")
    (add_net "Net-(10nF14-Pad2)")
    (add_net "Net-(10nF15-Pad2)")
    (add_net "Net-(10nF16-Pad2)")
    (add_net "Net-(10nF17-Pad2)")
    (add_net "Net-(10nF18-Pad2)")
    (add_net "Net-(1uF1-Pad2)")
    (add_net "Net-(BUFFER-1-Pad1)")
    (add_net "Net-(BUFFER-1-Pad2)")
    (add_net "Net-(BUFFER-2-Pad1)")
    (add_net "Net-(BUFFER-2-Pad2)")
    (add_net "Net-(BUFFER-3-Pad1)")
    (add_net "Net-(BUFFER-3-Pad2)")
    (add_net "Net-(BUFFER-4-Pad1)")
    (add_net "Net-(BUFFER-4-Pad2)")
    (add_net "Net-(BUFFER-5-Pad1)")
    (add_net "Net-(BUFFER-5-Pad2)")
    (add_net "Net-(BUFFER-6-Pad1)")
    (add_net "Net-(BUFFER-6-Pad2)")
    (add_net "Net-(BUFFER-7-Pad1)")
    (add_net "Net-(BUFFER-7-Pad2)")
    (add_net "Net-(BUFFER-8-Pad1)")
    (add_net "Net-(BUFFER-8-Pad2)")
    (add_net "Net-(BUFFER-9-Pad1)")
    (add_net "Net-(BUFFER-9-Pad2)")
    (add_net "Net-(POGO-PCA-IN-1-Pad1)")
    (add_net "Net-(POGO-PCA-IN-1-Pad2)")
    (add_net "Net-(POGO-PCA-IN-1-Pad4)")
    (add_net "Net-(POGO-PCA-IN-1-Pad5)")
    (add_net "Net-(POGO-PCA-IN-1-Pad6)")
    (add_net "Net-(POGO-PCA-IN-1-Pad8)")
    (add_net "Net-(POGO-PCA-IN-1-Pad9)")
    (add_net "Net-(POGO-PCA-IN-2-Pad1)")
    (add_net "Net-(POGO-PCA-IN-2-Pad2)")
    (add_net "Net-(POGO-PCA-IN-2-Pad4)")
    (add_net "Net-(POGO-PCA-IN-2-Pad5)")
    (add_net "Net-(POGO-PCA-IN-2-Pad6)")
    (add_net "Net-(POGO-PCA-IN-2-Pad8)")
    (add_net "Net-(POGO-PCA-IN-2-Pad9)")
    (add_net "Net-(POGO-PCA-IN-3-Pad1)")
    (add_net "Net-(POGO-PCA-IN-3-Pad2)")
    (add_net "Net-(POGO-PCA-IN-3-Pad4)")
    (add_net "Net-(POGO-PCA-IN-3-Pad5)")
    (add_net "Net-(POGO-PCA-IN-3-Pad6)")
    (add_net "Net-(POGO-PCA-IN-3-Pad8)")
    (add_net "Net-(POGO-PCA-IN-3-Pad9)")
    (add_net "Net-(POGO-PCA-IN-4-Pad1)")
    (add_net "Net-(POGO-PCA-IN-4-Pad2)")
    (add_net "Net-(POGO-PCA-IN-4-Pad4)")
    (add_net "Net-(POGO-PCA-IN-4-Pad5)")
    (add_net "Net-(POGO-PCA-IN-4-Pad6)")
    (add_net "Net-(POGO-PCA-IN-4-Pad8)")
    (add_net "Net-(POGO-PCA-IN-4-Pad9)")
    (add_net "Net-(POGO-PCA-IN-5-Pad1)")
    (add_net "Net-(POGO-PCA-IN-5-Pad2)")
    (add_net "Net-(POGO-PCA-IN-5-Pad4)")
    (add_net "Net-(POGO-PCA-IN-5-Pad5)")
    (add_net "Net-(POGO-PCA-IN-5-Pad6)")
    (add_net "Net-(POGO-PCA-IN-5-Pad8)")
    (add_net "Net-(POGO-PCA-IN-5-Pad9)")
    (add_net "Net-(POGO-PCA-IN-6-Pad1)")
    (add_net "Net-(POGO-PCA-IN-6-Pad2)")
    (add_net "Net-(POGO-PCA-IN-6-Pad4)")
    (add_net "Net-(POGO-PCA-IN-6-Pad5)")
    (add_net "Net-(POGO-PCA-IN-6-Pad6)")
    (add_net "Net-(POGO-PCA-IN-6-Pad8)")
    (add_net "Net-(POGO-PCA-IN-6-Pad9)")
    (add_net "Net-(POGO-PCA-IN-7-Pad1)")
    (add_net "Net-(POGO-PCA-IN-7-Pad2)")
    (add_net "Net-(POGO-PCA-IN-7-Pad4)")
    (add_net "Net-(POGO-PCA-IN-7-Pad5)")
    (add_net "Net-(POGO-PCA-IN-7-Pad6)")
    (add_net "Net-(POGO-PCA-IN-7-Pad8)")
    (add_net "Net-(POGO-PCA-IN-7-Pad9)")
    (add_net "Net-(POGO-PCA-IN-8-Pad1)")
    (add_net "Net-(POGO-PCA-IN-8-Pad2)")
    (add_net "Net-(POGO-PCA-IN-8-Pad4)")
    (add_net "Net-(POGO-PCA-IN-8-Pad5)")
    (add_net "Net-(POGO-PCA-IN-8-Pad6)")
    (add_net "Net-(POGO-PCA-IN-8-Pad8)")
    (add_net "Net-(POGO-PCA-IN-8-Pad9)")
    (add_net "Net-(POGO-PCA-IN-9-Pad1)")
    (add_net "Net-(POGO-PCA-IN-9-Pad2)")
    (add_net "Net-(POGO-PCA-IN-9-Pad4)")
    (add_net "Net-(POGO-PCA-IN-9-Pad5)")
    (add_net "Net-(POGO-PCA-IN-9-Pad6)")
    (add_net "Net-(POGO-PCA-IN-9-Pad8)")
    (add_net "Net-(POGO-PCA-IN-9-Pad9)")
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 139.166 36.59 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-3 (at 0.9 3.2) (layer F.SilkS))
    (fp_text value C (at 3.8 0.1) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 86 "Net-(10nF12-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 405.166 35.49 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-9 (at 1 3.05) (layer F.SilkS))
    (fp_text value C (at 4.15 -0.1) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 92 "Net-(10nF18-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 319.516 36.69 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-7 (at 1 3.4) (layer F.SilkS))
    (fp_text value C (at 3.8 0) (layer F.Fab))
    (fp_text user %R (at 0.8 -0.1) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 90 "Net-(10nF16-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 364.166 37.04 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-8 (at 0.9 3.35) (layer F.SilkS))
    (fp_text value C (at 4.15 0) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 91 "Net-(10nF17-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 275.116 36.49 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-6 (at 0.7 3.2) (layer F.SilkS))
    (fp_text value C (at 3.85 0.1) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 89 "Net-(10nF15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 231.216 36.64 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-5 (at 0.9 3.35) (layer F.SilkS))
    (fp_text value C (at 3.7 0) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 88 "Net-(10nF14-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 183.916 37.29 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-4 (at 0.8 3.3) (layer F.SilkS))
    (fp_text value C (at 3.9 -0.15) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 87 "Net-(10nF13-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 47.366 36.59 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-1 (at 0.8 3.2) (layer F.SilkS))
    (fp_text value C (at 4.1 0.1) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 83 "Net-(10nF10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 91.816 36.89 180)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 10nF-2 (at 0.7 3.35) (layer F.SilkS))
    (fp_text value C (at 3.8 0.05) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 85 "Net-(10nF11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 155 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-4 (at -5.41 -4.516) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(POGO-PCA-IN-4-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(POGO-PCA-IN-4-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(10nF13-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(POGO-PCA-IN-4-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(POGO-PCA-IN-4-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(POGO-PCA-IN-4-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(POGO-PCA-IN-4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(POGO-PCA-IN-4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 65 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-2 (at -5.41 -4.866 180) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(POGO-PCA-IN-2-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(POGO-PCA-IN-2-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(10nF11-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(POGO-PCA-IN-2-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(POGO-PCA-IN-2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(POGO-PCA-IN-2-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(POGO-PCA-IN-2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(POGO-PCA-IN-2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 20 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-1 (at -5.56 -4.616 180) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(POGO-PCA-IN-1-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(POGO-PCA-IN-1-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(10nF10-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(POGO-PCA-IN-1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(POGO-PCA-IN-1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(POGO-PCA-IN-1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(POGO-PCA-IN-1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(POGO-PCA-IN-1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 45.616 22.44)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-1 (at 0.966 -2.91) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 90.566 22.54)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-2 (at 0.75 -3.25) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 137.416 22.49)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-3 (at 0.75 -3.25) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 182.416 22.69)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-4 (at 0.75 -3.25) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 229.316 22.44)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-5 (at 0.75 -3.25) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 273.666 22.39)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-6 (at 0.75 -3.25) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 317.766 22.54)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-7 (at 0.75 -3.25) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 362.466 22.14)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-8 (at 0.716 -2.96) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D4.0mm_P1.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 404.016 21.19)
    (descr "CP, Radial series, Radial, pin pitch=1.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 1.50mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference 1uF-9 (at -0.884 -3.21) (layer F.SilkS))
    (fp_text value C (at 0.75 3.25) (layer F.Fab))
    (fp_text user %R (at 0.75 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.5 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 46.416 30.59)
    (fp_text reference BUFFER-1 (at 0.116 -4.66) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.266 -3.26) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(10nF10-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BUFFER-1-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(BUFFER-1-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 91.316 30.39)
    (fp_text reference BUFFER-2 (at 0.566 -4.41) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 1.066 -2.86) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(10nF11-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(BUFFER-2-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(BUFFER-2-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 138.216 30.34)
    (fp_text reference BUFFER-3 (at 0.116 -3.96) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.566 -2.61) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(10nF12-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(BUFFER-3-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(BUFFER-3-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 183.066 30.89)
    (fp_text reference BUFFER-4 (at 0.216 -4.71) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.266 -3.11) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(10nF13-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(BUFFER-4-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(BUFFER-4-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 230.266 30.34)
    (fp_text reference BUFFER-5 (at 0.216 -4.31) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.216 -2.86) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(10nF14-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(BUFFER-5-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(BUFFER-5-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 274.466 30.34)
    (fp_text reference BUFFER-6 (at 0.316 -4.51) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.566 -3.01) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(10nF15-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(BUFFER-6-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(BUFFER-6-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 318.716 30.29)
    (fp_text reference BUFFER-7 (at 0.666 -4.31) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.666 -2.81) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(10nF16-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(BUFFER-7-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(BUFFER-7-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 363.316 30.84)
    (fp_text reference BUFFER-8 (at 0.116 -4.96) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at 0.466 -3.46) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(10nF17-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(BUFFER-8-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(BUFFER-8-Pad1)"))
  )
  (module SN74LVC1G17QDBVRQ1:SN74LVC1G17QDBVRQ1 (layer F.Cu) (tedit 0)
    (at 404.666 29.44)
    (fp_text reference BUFFER-9 (at -0.184 -4.56) (layer F.SilkS))
    (fp_text value SN74LVC1G17QDBVRQ1 (at -0.334 -3.11) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.Fab))
    (fp_text user * (at -1.4478 -2.6518) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 5 smd rect (at 1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 4 smd rect (at 1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(10nF18-Pad2)"))
    (pad 3 smd rect (at -1.1938 0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 2 smd rect (at -1.1938 0) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(BUFFER-9-Pad2)"))
    (pad 1 smd rect (at -1.1938 -0.950001) (size 1.4732 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(BUFFER-9-Pad1)"))
  )
  (module Connector_Phoenix_MC_HighVoltage:PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical (layer F.Cu) (tedit 5B784ED3)
    (at 7.112 32 180)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-5.08; number of pins: 02; pin pitch: 5.08mm; Vertical || order number: 1836299 8A 320V")
    (tags "phoenix_contact connector MCV_01x02_G_5.08mm")
    (fp_text reference J1 (at -4.554 -0.29) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 2.54 4.1) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.65) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 84 "Net-(10nF10-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Phoenix_MC_HighVoltage.3dshapes/PhoenixContact_MCV_1,5_2-G-5.08_1x02_P5.08mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 20 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-1 (at -6.35 5.166 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(POGO-PCA-IN-1-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(POGO-PCA-IN-1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(BUFFER-1-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(POGO-PCA-IN-1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(POGO-PCA-IN-1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(POGO-PCA-IN-1-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(POGO-PCA-IN-1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(POGO-PCA-IN-1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 65 43 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-2 (at -6.09 5.416 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(POGO-PCA-IN-2-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(POGO-PCA-IN-2-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(BUFFER-2-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(POGO-PCA-IN-2-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(POGO-PCA-IN-2-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(POGO-PCA-IN-2-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(POGO-PCA-IN-2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(POGO-PCA-IN-2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 110 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-3 (at -6.65 6.566 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.1 5.066) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(POGO-PCA-IN-3-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(POGO-PCA-IN-3-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(BUFFER-3-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(POGO-PCA-IN-3-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(POGO-PCA-IN-3-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(POGO-PCA-IN-3-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(POGO-PCA-IN-3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(POGO-PCA-IN-3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 155 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-4 (at -5.8 5.566 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(POGO-PCA-IN-4-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(POGO-PCA-IN-4-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(BUFFER-4-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(POGO-PCA-IN-4-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(POGO-PCA-IN-4-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(POGO-PCA-IN-4-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(POGO-PCA-IN-4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(POGO-PCA-IN-4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 200 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-5 (at -5.8 5.416 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(POGO-PCA-IN-5-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(POGO-PCA-IN-5-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(BUFFER-5-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(POGO-PCA-IN-5-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(POGO-PCA-IN-5-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(POGO-PCA-IN-5-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(POGO-PCA-IN-5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(POGO-PCA-IN-5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 245 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-6 (at -5.7 5.266 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(POGO-PCA-IN-6-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(POGO-PCA-IN-6-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(BUFFER-6-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(POGO-PCA-IN-6-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(POGO-PCA-IN-6-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(POGO-PCA-IN-6-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(POGO-PCA-IN-6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(POGO-PCA-IN-6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 290 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-7 (at -5.6 4.966 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(POGO-PCA-IN-7-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(POGO-PCA-IN-7-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(BUFFER-7-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(POGO-PCA-IN-7-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(POGO-PCA-IN-7-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(POGO-PCA-IN-7-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(POGO-PCA-IN-7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(POGO-PCA-IN-7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 335 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-8 (at -5.6 5.566 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(POGO-PCA-IN-8-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(POGO-PCA-IN-8-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(BUFFER-8-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(POGO-PCA-IN-8-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(POGO-PCA-IN-8-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(POGO-PCA-IN-8-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(POGO-PCA-IN-8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(POGO-PCA-IN-8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 380 42.54 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-IN-9 (at -5.55 5.216 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 12.49 90) (layer F.Fab))
    (fp_text user %R (at 1.27 5.08) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(POGO-PCA-IN-9-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(POGO-PCA-IN-9-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(BUFFER-9-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(POGO-PCA-IN-9-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(POGO-PCA-IN-9-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(POGO-PCA-IN-9-Pad4)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(POGO-PCA-IN-9-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(POGO-PCA-IN-9-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 110 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-3 (at -5.51 -5.516 180) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(POGO-PCA-IN-3-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(POGO-PCA-IN-3-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(10nF12-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(POGO-PCA-IN-3-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(POGO-PCA-IN-3-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(POGO-PCA-IN-3-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(POGO-PCA-IN-3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(POGO-PCA-IN-3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 200 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-5 (at -5.31 -4.366 180) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(POGO-PCA-IN-5-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(POGO-PCA-IN-5-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(10nF14-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(POGO-PCA-IN-5-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(POGO-PCA-IN-5-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(POGO-PCA-IN-5-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "Net-(POGO-PCA-IN-5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(POGO-PCA-IN-5-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 245 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-6 (at -5.31 -4.816 180) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(POGO-PCA-IN-6-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(POGO-PCA-IN-6-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(10nF15-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(POGO-PCA-IN-6-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(POGO-PCA-IN-6-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(POGO-PCA-IN-6-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(POGO-PCA-IN-6-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(POGO-PCA-IN-6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 290 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-7 (at -5.21 -4.466 180) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(POGO-PCA-IN-7-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(POGO-PCA-IN-7-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(10nF16-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(POGO-PCA-IN-7-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(POGO-PCA-IN-7-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(POGO-PCA-IN-7-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(POGO-PCA-IN-7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(POGO-PCA-IN-7-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 335 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-8 (at -5.31 -4.516) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(POGO-PCA-IN-8-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(POGO-PCA-IN-8-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(10nF17-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(POGO-PCA-IN-8-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(POGO-PCA-IN-8-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(POGO-PCA-IN-8-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(POGO-PCA-IN-8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(POGO-PCA-IN-8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 380 20 270)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference POGO-PCA-OUT-9 (at -5.16 -4.466) (layer B.SilkS))
    (fp_text value Conn_02x05_Odd_Even_MountingPin (at 1.27 -12.49 270) (layer B.Fab))
    (fp_text user %R (at 1.27 -5.08) (layer B.Fab))
    (pad 10 thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(10nF10-Pad1)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(POGO-PCA-IN-9-Pad9)"))
    (pad 8 thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(POGO-PCA-IN-9-Pad8)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(10nF18-Pad2)"))
    (pad 6 thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(POGO-PCA-IN-9-Pad6)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(POGO-PCA-IN-9-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(POGO-PCA-IN-9-Pad4)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(1uF1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(POGO-PCA-IN-9-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(POGO-PCA-IN-9-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 393.316 12.44) (end 401.766 12.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 409.916 29.04) (end 409.916 20.59) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 151.816 47.44) (end 152.016 49.44) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 406.566 47.34) (end 406.566 49.34) (layer Edge.Cuts) (width 0.05))
  (gr_text 1 (at 379.966 16.44) (layer B.SilkS))
  (gr_text 10 (at 390.416 26.44) (layer B.SilkS))
  (gr_text 1 (at 334.966 16.29) (layer B.SilkS))
  (gr_text 10 (at 345.416 26.29) (layer B.SilkS))
  (gr_text 1 (at 289.966 16.44) (layer B.SilkS))
  (gr_text 10 (at 300.416 26.44) (layer B.SilkS))
  (gr_text 1 (at 244.966 16.34) (layer B.SilkS))
  (gr_text 10 (at 255.416 26.34) (layer B.SilkS))
  (gr_text 1 (at 199.916 16.44) (layer B.SilkS))
  (gr_text 10 (at 210.366 26.44) (layer B.SilkS))
  (gr_text 1 (at 154.966 16.44) (layer B.SilkS))
  (gr_text 10 (at 165.416 26.44) (layer B.SilkS))
  (gr_text 1 (at 109.866 16.39) (layer B.SilkS))
  (gr_text 10 (at 120.316 26.39) (layer B.SilkS))
  (gr_text 1 (at 64.916 16.34) (layer B.SilkS))
  (gr_text 10 (at 75.366 26.34) (layer B.SilkS))
  (gr_text 10 (at 30.266 26.29) (layer B.SilkS))
  (gr_text 1 (at 19.816 16.29) (layer B.SilkS))
  (gr_text 10 (at 390.316 35.84) (layer F.SilkS))
  (gr_text 1 (at 379.966 46.59) (layer F.SilkS))
  (gr_text 10 (at 345.166 35.79) (layer F.SilkS))
  (gr_text 1 (at 334.816 46.54) (layer F.SilkS))
  (gr_text 10 (at 300.166 35.84) (layer F.SilkS))
  (gr_text 1 (at 289.816 46.59) (layer F.SilkS))
  (gr_text 10 (at 255.216 35.79) (layer F.SilkS))
  (gr_text 1 (at 244.866 46.54) (layer F.SilkS))
  (gr_text 10 (at 210.216 35.89) (layer F.SilkS))
  (gr_text 1 (at 199.866 46.64) (layer F.SilkS))
  (gr_text 10 (at 165.316 35.84) (layer F.SilkS))
  (gr_text 1 (at 154.966 46.59) (layer F.SilkS))
  (gr_text 10 (at 120.216 35.84) (layer F.SilkS))
  (gr_text 1 (at 109.866 46.59) (layer F.SilkS))
  (gr_text 10 (at 75.266 36.24) (layer F.SilkS))
  (gr_text 1 (at 64.916 46.99) (layer F.SilkS))
  (gr_text 10 (at 30.216 35.74) (layer F.SilkS))
  (gr_text 1 (at 19.866 46.49) (layer F.SilkS))
  (gr_text VDD (at 1.466 26.59) (layer F.SilkS))
  (gr_text GND (at 7.616 38.89) (layer F.SilkS))
  (gr_line (start 409.916 50.64) (end 10.016 50.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 393.316 12.44) (end 10.016 12.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 409.916 50.64) (end 409.916 29.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 409.916 20.59) (end 401.766 12.44) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -4.084 36.54) (end -4.084 26.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 10.016 12.44) (end -4.084 26.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -4.084 36.54) (end 10.016 50.64) (layer Edge.Cuts) (width 0.05))
)
